Schema GreenBuildingXML-35.xsd

schema location: | http://www.gbxml.org/schema/GreenBuildingXML.xsd
targetNamespace: | http://www.gbxml.org/schema

Elements | Simple types
Absorptance | absorptanceUnitEnum
AdjacentSpaceId | airTemperatureTypeEnum
aecXML | areaUnitEnum
Age | blowerDoorUnitEnum
AirChangesPerHour | buildingTypeEnum
AirLoop | capacityTypeEnum
AirLoopEquipment | capacityUnitEnum
AirLoopId | conditioningTypeEnum
AirTemperature | conditioningUnitEnum
Albedo | conditionTypeEnum
AltEnergySource | conductivityFofTUnitEnum
Area | conductivityUnitEnum
AverageNumberOfFloors | controlTypeEnum
Azimuth | costTypeEnum
Ballast | currencyTypeEnum
BeginDate | dayTypeEnum
Blind | deltaPUnitEnum
BlowerDoorValue | densityFofTUnitEnum
Building | densityUnitEnum
BuildingStorey | directionUnitEnum
CADMaterialId | efficiencyTypeEnum
CADModelAzimuth | emissionUnitEnum
CADObjectId | emittanceTypeEnum
Campus | energyUnitEnum
Capacity | equipmentTypeEnum
CartesianPoint | extEquipTypeEnum
CDD | floorCategoryEnum
CDDValue | floorSlabPerimeterHeatLossCoefficientUnitTypeEnum
City | flowPerAreaUnitEnum
ClosedShell | flowUnitEnum
CLTDParameters | fluidTypeEnum
CoefficientOfUtilization | frameTypeEnum
CompanyName | fuelLoadUnitEnum
Conductivity | gasTypeEnum
ConductivityFofT | hOutsideUnitTypeEnum
Construction | hydronicEquipTypeEnum
Control | illuminanceUnitEnum
Coordinate | infiltrationTypeEnum
Cost | intEquipTypeEnum
CostValue | inverseTempUnitEnum
Country | lengthUnitEnum
CreatedBy | lifeUnitEnum
CyclesPerWeek | lightControlTypeEnum
Data | loadUnitEnum
Day | loopTypeEnum
DaylightSavings | openingTypeEnum
DaySchedule | operationTypeEnum
DDDayCool | peopleHeatGainTypeEnum
DDDayHeat | peopleHeatGainUnitEnum
DDDaylightCool | peopleNumberUnitEnum
DDDaylightHeat | permUnitEnum
DDDBCool | powerPerAreaUnitEnum
DDDBHeat | powerTypeEnum
DDDBRangeCool | powerUnitEnum
DDDBRangeHeat | powerUseTypeEnum
DDGroundTCool | pressureUnitEnum
DDGroundTHeat | radiationWavelengthTypeEnum
DDHiHrCool | reflectanceTypeEnum
DDHiHrHeat | resistanceUnitEnum
DDLoHrCool | resourceTypeEnum
DDLoHrHeat | resultsExtraResourceTypeEnum
DDMonthCool | resultsTypeEnum
DDMonthHeat | roofASHRAENumberEnum
DDPressureCool | roofCLTDIndexEnum
DDPressureHeat | roofColorEnum
DDRainCool | roofCTSTypeEnum
DDRainHeat | roughnessValueEnum
DDSkyClearnessCool | scheduleTypeEnum
DDSkyClearnessHeat | shadeOperationEnum
DDSnowCool | shadeScheduleTypeEnum
DDSnowHeat | shadeTypeEnum
DDWBCool | sinkRateUnitEnum
DDWBHeat | spaceTypeEnum
DDWindDirCool | specificHeatUnitEnum
DDWindDirHeat | stageTypeEnum
DDWindSpeedCool | standardsTypeEnum
DDWindSpeedHeat | stationIdTypeEnum
DeltaP | surfaceTypeEnum
DeltaT | systemTypeEnum
Density | temperatureUnitEnum
DensityFofT | tempTypeEnum
DependantValue | timePeriodEnum
DependantVariable | timeUnitEnum
Description | transportationTypeEnum
DesignCoolT | unitlessSmallUnitEnum
DesignFlow | unitlessUnitEnum
DesignHeatT | uValueUnitEnum
DesignPressure | valueTypeEnum
DesignTemp | vegetationTypeEnum
Dimensions | velocityUnitEnum
DocumentHistory | viscosityFofTUnitEnum
Efficiency | viscosityUnitEnum
ElecLoad | volumeUnitEnum
Elevation | wallASHRAEGroupEnum
Email1Address | wallColorEnum
EmissionRate | wallCTSTypeEnum
Emittance | wallGroupManualJEnum
EndDate | waterUseUnitEnum
Energy | weightUnitEnum
Equation |
EquipPowerPerArea |
Expression |
ExtEquip |
ExtEquipId |
FirstName |
FloorSlabHeatLossCoefficient |
Flow |
FlowControl |
FlowPerArea |
FlowPerPerson |
Frame |
FuelLoad |
Gap |
GapId |
gbXML |
GeneralGeometry |
Glare |
Glaze |
GlazeConductivity |
GlazeId |
GroundTemp |
GroundTempValue |
HDD |
HDDValue |
Height |
HighLimit |
HighValue |
HorizontalSolar |
HOutside |
HydronicLoop |
HydronicLoopEquipment |
HydronicLoopId |
Illuminance |
ImageTexture |
IndependantValue |
IndepentantVariable |
IndoorAirQuality |
InfiltrationFlow |
InputWatts |
InsideAirFilmResistance |
IntEquip |
IntEquipId |
Lamp |
LastName |
LatentLoad |
Latitude |
Layer |
LayerId |
Length |
Level |
Life |
LightControlId |
LightId |
Lighting |
LightingControl |
LightingSystem |
LightPowerPerArea |
LoadCalcInputParameters |
Location |
Longitude |
LowValue |
LumensPerLamp |
Luminaire |
ManualJ8Parameters |
Manufacturer |
Material |
MaterialId |
MaximumFlow |
MaxPressure |
MaxRelativeHumidity |
MaxTemp |
Meter |
MeterId |
MiddleName |
MinFlow |
MinimumFlow |
MinLightFrac |
MinPowerFrac |
MinPressure |
MinRelativeHumidity |
MinTemp |
Model |
ModifiedBy |
Name |
NaturalVentHiTemp |
NaturalVentLoTemp |
NaturalVentOccDep |
NumberOfLamps |
OAFlowPerArea |
OAFlowPerPerson |
ObjectId |
Opening |
OperationRange |
OperationSchedule |
PeakDomesticHotWaterFlow |
PeopleHeatGain |
PeopleNumber |
PercentAreaDaylitControled |
PercentExisting |
Performance |
Permeance |
PersonInfo |
PlanarGeometry |
Platform |
PointData |
PolyLoop |
Porosity |
Power |
PrandtlNumber |
PrandtlNumberFofT |
PressureControl |
ProductName |
ProgramInfo |
R-value |
RatedFlow |
RectangularGeometry |
RecycledContent |
Reference |
Reflectance |
RefrigerantType |
Results |
Roughness |
RTSParameters |
Schedule |
ScheduleValue |
Setback |
ShadeControl |
ShadeSchedule |
ShadingCoeff |
ShellGeometry |
SinkRate |
SolarHeatGainCoeff |
SolarOnOpening |
Space |
SpaceBoundary |
SpecificHeat |
StateOrProvince |
StationId |
StreetAddress |
Surface |
Temp |
Temperature |
TemperatureControl |
Thickness |
Tilt |
TimeIncrement |
Transmittance |
Transportation |
TypeCode |
U-value |
UtilityRate |
Value |
Vegetation |
Version |
Viscosity |
ViscosityFofT |
Volume |
WasteWaterHREff |
WaterLoss |
WaterRate |
WaterUsePerCycle |
Weather |
WebPage |
WeekSchedule |
WeekScheduleId |
Weight |
Width |
WindowType |
XAxis |
YAxis |
YearModeled |
YearSchedule |
ZipcodeOrPostalCode |
Zone |
ZoneCoolingLoad |

element Absorptance

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Construction
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | unitlessUnitEnum | required |  |  |
type | absorptanceUnitEnum | required |  |  |
annotation |
documentation
Absorptance of the outside surface
source | <xsd:element name="Absorptance"> <xsd:annotation> <xsd:documentation>Absorptance of the outside surface</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> <xsd:attribute name="type" type="absorptanceUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Absorptance/@unit

type | unitlessUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Percent
enumeration | Fraction
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

attribute Absorptance/@type

type | absorptanceUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | IntIR
enumeration | IntSolar
enumeration | IntVisible
enumeration | IntTotal
enumeration | ExtIR
enumeration | ExtSolar
enumeration | ExtVisible
enumeration | ExtTotal
source | <xsd:attribute name="type" type="absorptanceUnitEnum" use="required"/>

element AdjacentSpaceId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | Surface
attributes |
Name | Type | Use | Default | Fixed | annotation
spaceIdRef | xsd:IDREF | required |  |  |
documentation
ID for a space that is bounded by this surface.
surfaceType | surfaceTypeEnum | optional |  |  |
documentation
With interior horizontal surfaces, this attribute can distinguish between ceiling and floor surfaces to avoid double-counting of floor areas, etc. May be required in future schema versions.
source | <xsd:element name="AdjacentSpaceId"> <xsd:complexType> <xsd:attribute name="spaceIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID for a space that is bounded by this surface.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="surfaceType" type="surfaceTypeEnum" use="optional"> <xsd:annotation> <xsd:documentation>With interior horizontal surfaces, this attribute can distinguish between ceiling and floor surfaces to avoid double-counting of floor areas, etc. May be required in future schema versions.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute AdjacentSpaceId/@spaceIdRef

type | xsd:IDREF
properties |
isRef | 0
use | required
annotation |
documentation
ID for a space that is bounded by this surface.
source | <xsd:attribute name="spaceIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID for a space that is bounded by this surface.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute AdjacentSpaceId/@surfaceType

type | surfaceTypeEnum
properties |
isRef | 0
use | optional
facets |
enumeration | InteriorWall
enumeration | ExteriorWall
enumeration | Roof
enumeration | InteriorFloor
enumeration | Shade
enumeration | UndergroundWall
enumeration | UndergroundSlab
enumeration | Ceiling
enumeration | Air
enumeration | UndergroundCeiling
enumeration | RaisedFloor
enumeration | SlabOnGrade
enumeration | FreestandingColumn
enumeration | EmbeddedColumn
annotation |
documentation
With interior horizontal surfaces, this attribute can distinguish between ceiling and floor surfaces to avoid double-counting of floor areas, etc. May be required in future schema versions.
source | <xsd:attribute name="surfaceType" type="surfaceTypeEnum" use="optional"> <xsd:annotation> <xsd:documentation>With interior horizontal surfaces, this attribute can distinguish between ceiling and floor surfaces to avoid double-counting of floor areas, etc. May be required in future schema versions.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element aecXML

diagram |
namespace | http://www.gbxml.org/schema
used by |
element | gbXML
source | <xsd:element name="aecXML"/>

element Age

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:string
properties |
content | complex
used by |
elements | ExtEquip HydronicLoopEquipment IntEquip
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | derived by: xsd:NMTOKEN | required |  |  |
source | <xsd:element name="Age"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:string"> <xsd:attribute name="unit" use="required"> <xsd:simpleType> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Years"/> </xsd:restriction> </xsd:simpleType> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Age/@unit

type | restriction of xsd:NMTOKEN
properties |
isRef | 0
use | required
facets |
enumeration | Years
source | <xsd:attribute name="unit" use="required"> <xsd:simpleType> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Years"/> </xsd:restriction> </xsd:simpleType> </xsd:attribute>

element AirChangesPerHour

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Zone
source | <xsd:element name="AirChangesPerHour" type="xsd:decimal"/>

element AirLoop

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Reference AirLoopEquipment TemperatureControl PressureControl
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
controlZoneIdRef | xsd:IDREF |  |  |  |
systemType | systemTypeEnum |  |  |  |
annotation |
documentation
The AirLoop element represents the equipment serving one path of air
source | <xsd:element name="AirLoop"> <xsd:annotation> <xsd:documentation>The AirLoop element represents the equipment serving one path of air</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Reference" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="AirLoopEquipment" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="TemperatureControl" minOccurs="0"/> <xsd:element ref="PressureControl" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="controlZoneIdRef" type="xsd:IDREF"/> <xsd:attribute name="systemType" type="systemTypeEnum"/> </xsd:complexType> </xsd:element>

attribute AirLoop/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute AirLoop/@controlZoneIdRef

type | xsd:IDREF
properties |
isRef | 0
source | <xsd:attribute name="controlZoneIdRef" type="xsd:IDREF"/>

attribute AirLoop/@systemType

type | systemTypeEnum
properties |
isRef | 0
facets |
enumeration | SingleZoneReheat
enumeration | PackagedSingleZone
enumeration | SingleZoneCeilingInduction
enumeration | ReheatFan
enumeration | VariableAirVolume
enumeration | PoweredInductionUnit
enumeration | PackagedVariableAirVolume
enumeration | PackagedVariableVolumeVariableTemperature
enumeration | CeilingBypassVariableAirVolume
enumeration | EvaporativeCooling
enumeration | MultiZone
enumeration | PackagedMultiZone
enumeration | DualDuct
enumeration | FanCoil
enumeration | InductionUnit
enumeration | PackagedTerminalAirConditioner
enumeration | WaterLoopHeatPump
enumeration | ResidentialCyclingFurnaceCyclingAC
enumeration | ResidentialVariableAirVolumeVariableTemperature
enumeration | FloorPanelHeating
enumeration | HeatingAndVentilating
enumeration | UnitHeater
enumeration | UnitVentilator
source | <xsd:attribute name="systemType" type="systemTypeEnum"/>

element AirLoopEquipment

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Model Manufacturer RatedFlow MinFlow OperationSchedule Temp DeltaP DeltaT MinRelativeHumidity MaxRelativeHumidity Power Capacity Control Efficiency Performance Cost Weight Life WaterLoss Energy HydronicLoopId Reference RefrigerantType CADObjectId GeneralGeometry ShellGeometry
used by |
element | AirLoop
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
equipmentType | equipmentTypeEnum | required |  |  |
annotation |
documentation
A piece of equipment serving an air-loop. This is generalized to be able to contain any type of air loop equipment.
source | <xsd:element name="AirLoopEquipment"> <xsd:annotation> <xsd:documentation>A piece of equipment serving an air-loop. This is generalized to be able to contain any type of air loop equipment.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Model" minOccurs="0"/> <xsd:element ref="Manufacturer" minOccurs="0"/> <xsd:element ref="RatedFlow" minOccurs="0"/> <xsd:element ref="MinFlow" minOccurs="0"/> <xsd:element ref="OperationSchedule" minOccurs="0"/> <xsd:element ref="Temp" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="DeltaP" minOccurs="0"/> <xsd:element ref="DeltaT" minOccurs="0"/> <xsd:element ref="MinRelativeHumidity" minOccurs="0"/> <xsd:element ref="MaxRelativeHumidity" minOccurs="0"/> <xsd:element ref="Power" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Capacity" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Control" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Efficiency" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Performance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Cost" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Weight" minOccurs="0"/> <xsd:element ref="Life" minOccurs="0"/> <xsd:element ref="WaterLoss" minOccurs="0"/> <xsd:element ref="Energy" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="HydronicLoopId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Reference" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="RefrigerantType" minOccurs="0"/> <xsd:element ref="CADObjectId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="GeneralGeometry" minOccurs="0"/> <xsd:element ref="ShellGeometry" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="equipmentType" type="equipmentTypeEnum" use="required"/> </xsd:complexType> </xsd:element>

attribute AirLoopEquipment/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute AirLoopEquipment/@equipmentType

type | equipmentTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Fan
enumeration | HeatExchanger
enumeration | Coil
enumeration | Furnace
enumeration | Evaporative
enumeration | Radiant
enumeration | Economizer
enumeration | Duct
enumeration | Humidifier
enumeration | Dehumidifier
enumeration | UnitaryAC
enumeration | UnitaryHP
enumeration | SplitAC
enumeration | SplitHP
enumeration | TerminalUnit
enumeration | Register
enumeration | VAVBox
source | <xsd:attribute name="equipmentType" type="equipmentTypeEnum" use="required"/>

element AirLoopId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
elements | Space Zone
attributes |
Name | Type | Use | Default | Fixed | annotation
airLoopIdRef | xsd:IDREF | required |  |  |
documentation
ID pointing to an air loop
source | <xsd:element name="AirLoopId"> <xsd:complexType> <xsd:attribute name="airLoopIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID pointing to an air loop</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute AirLoopId/@airLoopIdRef

type | xsd:IDREF
properties |
isRef | 0
use | required
annotation |
documentation
ID pointing to an air loop
source | <xsd:attribute name="airLoopIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID pointing to an air loop</xsd:documentation> </xsd:annotation> </xsd:attribute>

element AirTemperature

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | ShadeControl
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | temperatureUnitEnum | required |  |  |
type | airTemperatureTypeEnum | required |  |  |
annotation |
documentation
Minimum air temperature before shades are closed.
source | <xsd:element name="AirTemperature"> <xsd:annotation> <xsd:documentation>Minimum air temperature before shades are closed.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum" use="required"/> <xsd:attribute name="type" type="airTemperatureTypeEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute AirTemperature/@unit

type | temperatureUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | F
enumeration | C
enumeration | K
enumeration | R
source | <xsd:attribute name="unit" type="temperatureUnitEnum" use="required"/>

attribute AirTemperature/@type

type | airTemperatureTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Outside
enumeration | Zone
source | <xsd:attribute name="type" type="airTemperatureTypeEnum" use="required"/>

element Albedo

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Construction
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | unitlessUnitEnum | required |  |  |
annotation |
documentation
Reflectance of solar radiation
source | <xsd:element name="Albedo"> <xsd:annotation> <xsd:documentation>Reflectance of solar radiation</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Albedo/@unit

type | unitlessUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Percent
enumeration | Fraction
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element AltEnergySource

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | MeterId
used by |
element | Campus
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
altEnergyType | derived by: xsd:NMTOKEN | required |  |  |
resourceType | resourceTypeEnum | required |  |  |
annotation |
documentation
Alternative energy source
source | <xsd:element name="AltEnergySource"> <xsd:annotation> <xsd:documentation>Alternative energy source</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="MeterId" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="altEnergyType" use="required"> <xsd:simpleType> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Solar"/> <xsd:enumeration value="Wind"/> <xsd:enumeration value="Geothermal"/> <xsd:enumeration value="HeatRecovery"/> <xsd:enumeration value="NaturalGas"/> <xsd:enumeration value="Electrical"/> </xsd:restriction> </xsd:simpleType> </xsd:attribute> <xsd:attribute name="resourceType" type="resourceTypeEnum" use="required"/> </xsd:complexType> </xsd:element>

attribute AltEnergySource/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute AltEnergySource/@altEnergyType

type | restriction of xsd:NMTOKEN
properties |
isRef | 0
use | required
facets |
enumeration | Solar
enumeration | Wind
enumeration | Geothermal
enumeration | HeatRecovery
enumeration | NaturalGas
enumeration | Electrical
source | <xsd:attribute name="altEnergyType" use="required"> <xsd:simpleType> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Solar"/> <xsd:enumeration value="Wind"/> <xsd:enumeration value="Geothermal"/> <xsd:enumeration value="HeatRecovery"/> <xsd:enumeration value="NaturalGas"/> <xsd:enumeration value="Electrical"/> </xsd:restriction> </xsd:simpleType> </xsd:attribute>

attribute AltEnergySource/@resourceType

type | resourceTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Electricity
enumeration | NaturalGas
enumeration | Propane
enumeration | FuelOil1
enumeration | FuelOil2
enumeration | FuelOil4
enumeration | Water
enumeration | ChilledWater
enumeration | HotWater
enumeration | Steam
source | <xsd:attribute name="resourceType" type="resourceTypeEnum" use="required"/>

element Area

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Building Space
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | areaUnitEnum |  |  |  |
annotation |
documentation
Specifies the area of the space or building. This value should be equal to the area enclosed by the physical boundaries of the space, as defined by the intersection of the horizontal plane at the highest floor height and the volumetric model's vertical interior surface planes. Building area should be the sum of space areas whose PeopleNumber element values are greater than zero.
source | <xsd:element name="Area"> <xsd:annotation> <xsd:documentation>Specifies the area of the space or building. This value should be equal to the area enclosed by the physical boundaries of the space, as defined by the intersection of the horizontal plane at the highest floor height and the volumetric model's vertical interior surface planes. Building area should be the sum of space areas whose PeopleNumber element values are greater than zero.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="areaUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Area/@unit

type | areaUnitEnum
properties |
isRef | 0
facets |
enumeration | SquareKilometers
enumeration | SquareMeters
enumeration | SquareCentimeters
enumeration | SquareMillimeters
enumeration | SquareMiles
enumeration | SquareYards
enumeration | SquareFeet
enumeration | SquareInches
source | <xsd:attribute name="unit" type="areaUnitEnum"/>

element AverageNumberOfFloors

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Building
source | <xsd:element name="AverageNumberOfFloors" type="xsd:decimal"/>

element Azimuth

diagram |
namespace | http://www.gbxml.org/schema
type | restriction of xsd:double
properties |
content | simple
used by |
element | RectangularGeometry
facets |
minInclusive | 0
maxInclusive | 360
annotation |
documentation
Polygon azimuth. The direction of the outward normal for the polygon (surface or opening) defined in RectangularGeometry element. Azimuth is measured in degrees clockwise from North, where North = 0 degrees. Examples: East = 90 deg, South = 180 deg, West = 270 deg. If CADModelAzimuth is defined, the Azimuth value is relative to the CADModelAzimuth value rather then North.
source | <xsd:element name="Azimuth"> <xsd:annotation> <xsd:documentation>Polygon azimuth. The direction of the outward normal for the polygon (surface or opening) defined in RectangularGeometry element. Azimuth is measured in degrees clockwise from North, where North = 0 degrees. Examples: East = 90 deg, South = 180 deg, West = 270 deg. If CADModelAzimuth is defined, the Azimuth value is relative to the CADModelAzimuth value rather then North.</xsd:documentation> </xsd:annotation> <xsd:simpleType> <xsd:restriction base="xsd:double"> <xsd:minInclusive value="0"/> <xsd:maxInclusive value="360"/> </xsd:restriction> </xsd:simpleType> </xsd:element>

element Ballast

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | LightingSystem
annotation |
documentation
Type of ballast used
source | <xsd:element name="Ballast" type="xsd:string"> <xsd:annotation> <xsd:documentation>Type of ballast used</xsd:documentation> </xsd:annotation> </xsd:element>

element BeginDate

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:date
properties |
content | simple
used by |
element | YearSchedule
annotation |
documentation
Month and day year schedule begins
source | <xsd:element name="BeginDate" type="xsd:date"> <xsd:annotation> <xsd:documentation>Month and day year schedule begins</xsd:documentation> </xsd:annotation> </xsd:element>

element Blind

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Transmittance Reflectance Emittance Thickness Conductivity
used by |
element | WindowType
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
source | <xsd:element name="Blind"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Transmittance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Reflectance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Emittance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Thickness" minOccurs="0"/> <xsd:element ref="Conductivity" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> </xsd:complexType> </xsd:element>

attribute Blind/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

element BlowerDoorValue

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | InfiltrationFlow
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | blowerDoorUnitEnum | required |  |  |
annotation |
documentation
Leakage value obtained from blower door test.
source | <xsd:element name="BlowerDoorValue"> <xsd:annotation> <xsd:documentation>Leakage value obtained from blower door test.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="blowerDoorUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute BlowerDoorValue/@unit

type | blowerDoorUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | ACH
enumeration | AirChangesPerHour
enumeration | SquareFeet
enumeration | SquareMeter
source | <xsd:attribute name="unit" type="blowerDoorUnitEnum" use="required"/>

element Building

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description StreetAddress Area Space AverageNumberOfFloors InfiltrationFlow ShellGeometry Lighting IntEquipId MeterId PeakDomesticHotWaterFlow BuildingStorey
used by |
element | Campus
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
buildingType | buildingTypeEnum | required |  |  |
ifcGUID | xsd:string | optional |  |  |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
source | <xsd:element name="Building"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="StreetAddress" minOccurs="0"/> <xsd:element ref="Area"/> <xsd:element ref="Space" maxOccurs="unbounded"/> <xsd:element ref="AverageNumberOfFloors" minOccurs="0"/> <xsd:element ref="InfiltrationFlow" minOccurs="0"/> <xsd:element ref="ShellGeometry" minOccurs="0"> <xsd:annotation> <xsd:documentation>Use this element to define the shell of the building.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="Lighting" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="IntEquipId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="MeterId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="PeakDomesticHotWaterFlow" minOccurs="0"/> <xsd:element ref="BuildingStorey" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="buildingType" type="buildingTypeEnum" use="required"/> <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Building/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Building/@buildingType

type | buildingTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | AutomotiveFacility
enumeration | ConventionCenter
enumeration | Courthouse
enumeration | DiningBarLoungeOrLeisure
enumeration | DiningCafeteriaFastFood
enumeration | DiningFamily
enumeration | Dormitory
enumeration | ExerciseCenter
enumeration | FireStation
enumeration | Gymnasium
enumeration | HospitalOrHealthcare
enumeration | Hotel
enumeration | Library
enumeration | Manufacturing
enumeration | Motel
enumeration | MotionPictureTheatre
enumeration | MultiFamily
enumeration | Museum
enumeration | Office
enumeration | ParkingGarage
enumeration | Penitentiary
enumeration | PerformingArtsTheater
enumeration | PoliceStation
enumeration | PostOffice
enumeration | ReligiousBuilding
enumeration | Retail
enumeration | SchoolOrUniversity
enumeration | SingleFamily
enumeration | SportsArena
enumeration | TownHall
enumeration | Transportation
enumeration | Unknown
enumeration | Warehouse
enumeration | Workshop
source | <xsd:attribute name="buildingType" type="buildingTypeEnum" use="required"/>

attribute Building/@ifcGUID

type | xsd:string
properties |
isRef | 0
use | optional
annotation |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
source | <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element BuildingStorey

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Level PlanarGeometry
used by |
element | Building
annotation |
documentation
Captures Building Storey Structure
source | <xsd:element name="BuildingStorey"> <xsd:annotation> <xsd:documentation>Captures Building Storey Structure</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Level"/> <xsd:element ref="PlanarGeometry" minOccurs="0"/> </xsd:choice> </xsd:complexType> </xsd:element>

element CADMaterialId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | Material
attributes |
Name | Type | Use | Default | Fixed | annotation
CADMaterialIdRef | xsd:string | required |  |  |
documentation
ID used by a CAD program to reference its internal materials library
source | <xsd:element name="CADMaterialId"> <xsd:complexType> <xsd:attribute name="CADMaterialIdRef" type="xsd:string" use="required"> <xsd:annotation> <xsd:documentation>ID used by a CAD program to reference its internal materials library</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute CADMaterialId/@CADMaterialIdRef

type | xsd:string
properties |
isRef | 0
use | required
annotation |
documentation
ID used by a CAD program to reference its internal materials library
source | <xsd:attribute name="CADMaterialIdRef" type="xsd:string" use="required"> <xsd:annotation> <xsd:documentation>ID used by a CAD program to reference its internal materials library</xsd:documentation> </xsd:annotation> </xsd:attribute>

element CADModelAzimuth

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:double
properties |
content | simple
used by |
element | Location
annotation |
documentation
The number of degrees (0 to 360) of the angle of positive Y axis from north. (Value of the of Azimuth of Model's North relative to Cardinal North)
source | <xsd:element name="CADModelAzimuth" type="xsd:double"> <xsd:annotation> <xsd:documentation>The number of degrees (0 to 360) of the angle of positive Y axis from north. (Value of the of Azimuth of Model's North relative to Cardinal North)</xsd:documentation> </xsd:annotation> </xsd:element>

element CADObjectId

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
elements | AirLoopEquipment ExtEquip HydronicLoopEquipment IntEquip Opening Results Space Surface Zone
annotation |
documentation
The CADObjectId Element is used to map unique CAD object identifiers to gbXML elements. Allows CAD tools to read results from a gbXML file and map them to their CAD objects.
source | <xsd:element name="CADObjectId" type="xsd:string"> <xsd:annotation> <xsd:documentation>The CADObjectId Element is used to map unique CAD object identifiers to gbXML elements. Allows CAD tools to read results from a gbXML file and map them to their CAD objects.</xsd:documentation> </xsd:annotation> </xsd:element>

element Campus

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Location Building Surface YearModeled DaylightSavings Life AltEnergySource ShellGeometry Vegetation Transportation MeterId ExtEquipId Lighting LightControlId
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
designHeatWeathIdRef | xsd:IDREF |  |  |  |
documentation
ID for the weather data used for a heating design day
designCoolWeathIdRef | xsd:IDREF |  |  |  |
documentation
ID for the weather data used for a cooling design day
ifcGUID | xsd:string | optional |  |  |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
annotation |
documentation
The Campus element should be used as the base for all physical objects. On a campus, place one or more buildings.
source | <xsd:element name="Campus"> <xsd:annotation> <xsd:documentation>The Campus element should be used as the base for all physical objects. On a campus, place one or more buildings.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Location"/> <xsd:element ref="Building" maxOccurs="unbounded"/> <xsd:element ref="Surface" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="YearModeled" minOccurs="0"/> <xsd:element ref="DaylightSavings" minOccurs="0"/> <xsd:element ref="Life" minOccurs="0"/> <xsd:element ref="AltEnergySource" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="ShellGeometry" minOccurs="0"/> <xsd:element ref="Vegetation" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Transportation" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="MeterId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="ExtEquipId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Lighting" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="LightControlId" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="designHeatWeathIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the weather data used for a heating design day</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="designCoolWeathIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the weather data used for a cooling design day</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Campus/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Campus/@designHeatWeathIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID for the weather data used for a heating design day
source | <xsd:attribute name="designHeatWeathIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the weather data used for a heating design day</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Campus/@designCoolWeathIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID for the weather data used for a cooling design day
source | <xsd:attribute name="designCoolWeathIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the weather data used for a cooling design day</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Campus/@ifcGUID

type | xsd:string
properties |
isRef | 0
use | optional
annotation |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
source | <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Capacity

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | AirLoopEquipment HydronicLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | capacityUnitEnum | required |  |  |
capacityType | capacityTypeEnum | required |  |  |
source | <xsd:element name="Capacity"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="capacityUnitEnum" use="required"/> <xsd:attribute name="capacityType" type="capacityTypeEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Capacity/@unit

type | capacityUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Tons
enumeration | kW
enumeration | BtuPerHour
enumeration | kBtuPerHour
enumeration | Gallons
enumeration | Liters
enumeration | CubicMeters
enumeration | CubicFeet
source | <xsd:attribute name="unit" type="capacityUnitEnum" use="required"/>

attribute Capacity/@capacityType

type | capacityTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Heating
enumeration | CoolingTotal
enumeration | CoolingSensible
enumeration | CoolingLatent
enumeration | CoolingSHR
enumeration | Volume
source | <xsd:attribute name="capacityType" type="capacityTypeEnum" use="required"/>

element CartesianPoint

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Coordinate
used by |
elements | LightingControl PolyLoop RectangularGeometry Results
annotation |
documentation
This is the x, y, and z distances from the origin. This element must have three Coordinate elements when representing 3-d space, which represent x, y and z in order. This element must have two Coordinate elements when representing 2-d space.
appinfo
<xhtml:a href="http://cig.bre.co.uk/iai_uk/documentation/IfcR2x_Final/ifcgeometryresource/lexical/ifccartesianpoint.html">IfcCartesianPoint</xhtml:a>
source | <xsd:element name="CartesianPoint"> <xsd:annotation> <xsd:documentation>This is the x, y, and z distances from the origin. This element must have three Coordinate elements when representing 3-d space, which represent x, y and z in order. This element must have two Coordinate elements when representing 2-d space.</xsd:documentation> <xsd:appinfo> <xhtml:a href="http://cig.bre.co.uk/iai_uk/documentation/IfcR2x_Final/ifcgeometryresource/lexical/ifccartesianpoint.html">IfcCartesianPoint</xhtml:a> </xsd:appinfo> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Coordinate" minOccurs="2" maxOccurs="3"/> </xsd:choice> </xsd:complexType> </xsd:element>

element CDD

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Temperature CDDValue
used by |
element | Weather
annotation |
documentation
Cooling degree days. CDD is calculated as the number of degrees a mean daily temperature is above a value (specified as the Temperature element), for each day. For example, if the mean temperature in a region rises to 77 degrees for three days during a year, the rest of the time staying below 75, and the Temperature element is set at 75, then CDD = 6.
source | <xsd:element name="CDD"> <xsd:annotation> <xsd:documentation>Cooling degree days. CDD is calculated as the number of degrees a mean daily temperature is above a value (specified as the Temperature element), for each day. For example, if the mean temperature in a region rises to 77 degrees for three days during a year, the rest of the time staying below 75, and the Temperature element is set at 75, then CDD = 6.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Temperature"/> <xsd:element ref="CDDValue"/> </xsd:choice> </xsd:complexType> </xsd:element>

element CDDValue

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | CDD
annotation |
documentation
Cooling degree day value
source | <xsd:element name="CDDValue" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Cooling degree day value</xsd:documentation> </xsd:annotation> </xsd:element>

element City

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | Weather
source | <xsd:element name="City" type="xsd:string"/>

element ClosedShell

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | PolyLoop
used by |
element | ShellGeometry
annotation |
documentation
This is an element from ifcXML that describes a collection of faces that make up a closed shell.
appinfo
<xhtml:a href="http://cig.bre.co.uk/iai_uk/documentation/IfcR2x_Final/IFCTOPOLOGYRESOURCE/lexical/ifcclosedshell">IfcClosedShell</xhtml:a>
source | <xsd:element name="ClosedShell"> <xsd:annotation> <xsd:documentation>This is an element from ifcXML that describes a collection of faces that make up a closed shell.</xsd:documentation> <xsd:appinfo> <xhtml:a href="http://cig.bre.co.uk/iai_uk/documentation/IfcR2x_Final/IFCTOPOLOGYRESOURCE/lexical/ifcclosedshell">IfcClosedShell</xhtml:a> </xsd:appinfo> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="PolyLoop" minOccurs="4" maxOccurs="unbounded"/> </xsd:choice> </xsd:complexType> </xsd:element>

element CLTDParameters

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | LoadCalcInputParameters
attributes |
Name | Type | Use | Default | Fixed | annotation
roofASHRAENumber | roofASHRAENumberEnum |  |  |  |
documentation
Specifies the number 1 to 13 to use for a roof. See Table 29 page 26.34, 1989 ASHRAE Handbook, Fundamentals volume.
wallASHRAEGroup | wallASHRAEGroupEnum |  |  |  |
documentation
Specifies the wall group code A to G to use for a wall. See Table 31, page 26.36, 1989 ASHRAE Handbook, Fundamentals volume.
roofColor | roofColorEnum |  |  |  |
documentation
Specifies the effective roof color, which depends on the actual color and whether the location is industrial or rural. See page 26.34, 1989 ASHRAE Handbook, Fundamentals volume.
roofHasSuspendedCeiling | xsd:boolean |  |  |  |
documentation
Specifies whether or not a roof has a suspended ceiling under it. See table 29, page 26.34, 1989 ASHRAE Handbook, Fundamentals volume.
wallColor | wallColorEnum |  |  |  |
documentation
Specifies the effective wall color, which depends on the actual color and whether the location is industrial or rural. See page 26.36, 1989 ASHRAE Handbook, Fundamentals volume.
annotation |
documentation
Parameters required by CLTD load calculation method, as described in the 1989 ASHRAE Handbook, Fundamentals volume, pages 26.32 and following. Ignore this element and all elements under it if you are not planning to use that method.
source | <xsd:element name="CLTDParameters"> <xsd:annotation> <xsd:documentation>Parameters required by CLTD load calculation method, as described in the 1989 ASHRAE Handbook, Fundamentals volume, pages 26.32 and following. Ignore this element and all elements under it if you are not planning to use that method.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:attribute name="roofASHRAENumber" type="roofASHRAENumberEnum"> <xsd:annotation> <xsd:documentation>Specifies the number 1 to 13 to use for a roof. See Table 29 page 26.34, 1989 ASHRAE Handbook, Fundamentals volume.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="wallASHRAEGroup" type="wallASHRAEGroupEnum"> <xsd:annotation> <xsd:documentation>Specifies the wall group code A to G to use for a wall. See Table 31, page 26.36, 1989 ASHRAE Handbook, Fundamentals volume.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="roofColor" type="roofColorEnum"> <xsd:annotation> <xsd:documentation>Specifies the effective roof color, which depends on the actual color and whether the location is industrial or rural. See page 26.34, 1989 ASHRAE Handbook, Fundamentals volume.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="roofHasSuspendedCeiling" type="xsd:boolean"> <xsd:annotation> <xsd:documentation>Specifies whether or not a roof has a suspended ceiling under it. See table 29, page 26.34, 1989 ASHRAE Handbook, Fundamentals volume.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="wallColor" type="wallColorEnum"> <xsd:annotation> <xsd:documentation>Specifies the effective wall color, which depends on the actual color and whether the location is industrial or rural. See page 26.36, 1989 ASHRAE Handbook, Fundamentals volume.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute CLTDParameters/@roofASHRAENumber

type | roofASHRAENumberEnum
properties |
isRef | 0
facets |
enumeration | 0
enumeration | 1
enumeration | 2
enumeration | 3
enumeration | 4
enumeration | 5
enumeration | 6
enumeration | 7
enumeration | 8
enumeration | 9
enumeration | 10
enumeration | 11
enumeration | 12
enumeration | 13
annotation |
documentation
Specifies the number 1 to 13 to use for a roof. See Table 29 page 26.34, 1989 ASHRAE Handbook, Fundamentals volume.
source | <xsd:attribute name="roofASHRAENumber" type="roofASHRAENumberEnum"> <xsd:annotation> <xsd:documentation>Specifies the number 1 to 13 to use for a roof. See Table 29 page 26.34, 1989 ASHRAE Handbook, Fundamentals volume.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute CLTDParameters/@wallASHRAEGroup

type | wallASHRAEGroupEnum
properties |
isRef | 0
facets |
enumeration | A
enumeration | B
enumeration | C
enumeration | D
enumeration | E
enumeration | F
enumeration | G
annotation |
documentation
Specifies the wall group code A to G to use for a wall. See Table 31, page 26.36, 1989 ASHRAE Handbook, Fundamentals volume.
source | <xsd:attribute name="wallASHRAEGroup" type="wallASHRAEGroupEnum"> <xsd:annotation> <xsd:documentation>Specifies the wall group code A to G to use for a wall. See Table 31, page 26.36, 1989 ASHRAE Handbook, Fundamentals volume.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute CLTDParameters/@roofColor

type | roofColorEnum
properties |
isRef | 0
facets |
enumeration | Dark
enumeration | Light
annotation |
documentation
Specifies the effective roof color, which depends on the actual color and whether the location is industrial or rural. See page 26.34, 1989 ASHRAE Handbook, Fundamentals volume.
source | <xsd:attribute name="roofColor" type="roofColorEnum"> <xsd:annotation> <xsd:documentation>Specifies the effective roof color, which depends on the actual color and whether the location is industrial or rural. See page 26.34, 1989 ASHRAE Handbook, Fundamentals volume.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute CLTDParameters/@roofHasSuspendedCeiling

type | xsd:boolean
properties |
isRef | 0
annotation |
documentation
Specifies whether or not a roof has a suspended ceiling under it. See table 29, page 26.34, 1989 ASHRAE Handbook, Fundamentals volume.
source | <xsd:attribute name="roofHasSuspendedCeiling" type="xsd:boolean"> <xsd:annotation> <xsd:documentation>Specifies whether or not a roof has a suspended ceiling under it. See table 29, page 26.34, 1989 ASHRAE Handbook, Fundamentals volume.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute CLTDParameters/@wallColor

type | wallColorEnum
properties |
isRef | 0
facets |
enumeration | Dark
enumeration | Medium
enumeration | Light
annotation |
documentation
Specifies the effective wall color, which depends on the actual color and whether the location is industrial or rural. See page 26.36, 1989 ASHRAE Handbook, Fundamentals volume.
source | <xsd:attribute name="wallColor" type="wallColorEnum"> <xsd:annotation> <xsd:documentation>Specifies the effective wall color, which depends on the actual color and whether the location is industrial or rural. See page 26.36, 1989 ASHRAE Handbook, Fundamentals volume.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element CoefficientOfUtilization

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | LightingSystem
attributes |
Name | Type | Use | Default | Fixed | annotation
wallReflectance | xsd:decimal |  |  |  |
ceilingCavityReflectance | xsd:decimal |  |  |  |
floorReflectance | xsd:decimal |  |  |  |
roomCavityRatio | xsd:decimal |  |  |  |
documentation
Room cavity ratio is a measure of the room cavity proportions.
annotation |
documentation
The coefficient of utilization is the ratio of luminous flux on a work plane to the luminous flux emitted by the lamps alone.
source | <xsd:element name="CoefficientOfUtilization"> <xsd:annotation> <xsd:documentation>The coefficient of utilization is the ratio of luminous flux on a work plane to the luminous flux emitted by the lamps alone. </xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="wallReflectance" type="xsd:decimal"/> <xsd:attribute name="ceilingCavityReflectance" type="xsd:decimal"/> <xsd:attribute name="floorReflectance" type="xsd:decimal"/> <xsd:attribute name="roomCavityRatio" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Room cavity ratio is a measure of the room cavity proportions.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute CoefficientOfUtilization/@wallReflectance

type | xsd:decimal
properties |
isRef | 0
source | <xsd:attribute name="wallReflectance" type="xsd:decimal"/>

attribute CoefficientOfUtilization/@ceilingCavityReflectance

type | xsd:decimal
properties |
isRef | 0
source | <xsd:attribute name="ceilingCavityReflectance" type="xsd:decimal"/>

attribute CoefficientOfUtilization/@floorReflectance

type | xsd:decimal
properties |
isRef | 0
source | <xsd:attribute name="floorReflectance" type="xsd:decimal"/>

attribute CoefficientOfUtilization/@roomCavityRatio

type | xsd:decimal
properties |
isRef | 0
annotation |
documentation
Room cavity ratio is a measure of the room cavity proportions.
source | <xsd:attribute name="roomCavityRatio" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Room cavity ratio is a measure of the room cavity proportions.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element CompanyName

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
elements | PersonInfo ProgramInfo
source | <xsd:element name="CompanyName" type="xsd:string"/>

element Conductivity

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Blind Gap Glaze Material
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | conductivityUnitEnum | required |  |  |
source | <xsd:element name="Conductivity"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="conductivityUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Conductivity/@unit

type | conductivityUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | WPerCmC
enumeration | WPerMeterK
enumeration | BtuPerHourFtF
source | <xsd:attribute name="unit" type="conductivityUnitEnum" use="required"/>

element ConductivityFofT

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Gap
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | conductivityFofTUnitEnum | required |  |  |
annotation |
documentation
Conductivity as a function of temperature
source | <xsd:element name="ConductivityFofT"> <xsd:annotation> <xsd:documentation>Conductivity as a function of temperature</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="conductivityFofTUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute ConductivityFofT/@unit

type | conductivityFofTUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | WPerMSquareK
enumeration | BtuPerHourFtSquareF
source | <xsd:attribute name="unit" type="conductivityFofTUnitEnum" use="required"/>

element Construction

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description U-value Absorptance Roughness Albedo Reflectance Transmittance Emittance Cost PercentExisting LayerId LoadCalcInputParameters
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
DOELibIdRef | xsd:string |  |  |  |
documentation
Use this attribute to reference objects in the DOE2 library
annotation |
documentation
A Construction is a combination of layers, such as a wall or a roof
source | <xsd:element name="Construction"> <xsd:annotation> <xsd:documentation>A Construction is a combination of layers, such as a wall or a roof</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="U-value" minOccurs="0"/> <xsd:element ref="Absorptance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Roughness" minOccurs="0"/> <xsd:element ref="Albedo" minOccurs="0"/> <xsd:element ref="Reflectance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Transmittance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Emittance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Cost" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="PercentExisting" minOccurs="0"/> <xsd:element ref="LayerId" minOccurs="0" maxOccurs="unbounded"> <xsd:annotation> <xsd:documentation>Reference to layers that comprise this construction. Multiple LayerId's order is important and specifies the layering of the layer's referenced materials. The first Surface/AdjacentSpaceId entered will determine how the referenced construction layers are ordered with the first construction layer being in contact with the outside or 2nd Surface/AdjacentSpaceId listed and the last layer in contact with the first Surface/AdjacentSpaceId listed.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="LoadCalcInputParameters" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Construction/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Construction/@DOELibIdRef

type | xsd:string
properties |
isRef | 0
annotation |
documentation
Use this attribute to reference objects in the DOE2 library
source | <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Control

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
elements | AirLoopEquipment HydronicLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | annotation
controlType | controlTypeEnum |  |  |  |
stages | stageTypeEnum | optional |  |  |
minPowerRatio | xsd:float |  |  |  |
operationType | operationTypeEnum |  |  |  |
performanceIdRef | xsd:IDREF |  |  |  |
annotation |
documentation
The Control element should be used for describing how this equipment is controlled.
source | <xsd:element name="Control"> <xsd:annotation> <xsd:documentation>The Control element should be used for describing how this equipment is controlled.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:attribute name="controlType" type="controlTypeEnum"/> <xsd:attribute name="stages" type="stageTypeEnum" use="optional"/> <xsd:attribute name="minPowerRatio" type="xsd:float"/> <xsd:attribute name="operationType" type="operationTypeEnum"/> <xsd:attribute name="performanceIdRef" type="xsd:IDREF"/> </xsd:complexType> </xsd:element>

attribute Control/@controlType

type | controlTypeEnum
properties |
isRef | 0
facets |
enumeration | Fan
enumeration | Pump
enumeration | Valve
source | <xsd:attribute name="controlType" type="controlTypeEnum"/>

attribute Control/@stages

type | stageTypeEnum
properties |
isRef | 0
use | optional
facets |
enumeration | 1Stage
enumeration | 2Stage
enumeration | Variable
source | <xsd:attribute name="stages" type="stageTypeEnum" use="optional"/>

attribute Control/@minPowerRatio

type | xsd:float
properties |
isRef | 0
source | <xsd:attribute name="minPowerRatio" type="xsd:float"/>

attribute Control/@operationType

type | operationTypeEnum
properties |
isRef | 0
facets |
enumeration | Cycling
enumeration | Continuous
source | <xsd:attribute name="operationType" type="operationTypeEnum"/>

attribute Control/@performanceIdRef

type | xsd:IDREF
properties |
isRef | 0
source | <xsd:attribute name="performanceIdRef" type="xsd:IDREF"/>

element Coordinate

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | CartesianPoint
annotation |
documentation
This is the an x, y, or z length measurement from the origin.
appinfo
<xhtml:a href="http://cig.bre.co.uk/iai_uk/documentation/IfcR2x_Final/ifcmeasureresource/lexical/ifclengthmeasure.html">IfcLengthMeasure</xhtml:a>
source | <xsd:element name="Coordinate"> <xsd:annotation> <xsd:documentation>This is the an x, y, or z length measurement from the origin.</xsd:documentation> <xsd:appinfo> <xhtml:a href="http://cig.bre.co.uk/iai_uk/documentation/IfcR2x_Final/ifcmeasureresource/lexical/ifclengthmeasure.html">IfcLengthMeasure</xhtml:a> </xsd:appinfo> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"/> </xsd:simpleContent> </xsd:complexType> </xsd:element>

element Cost

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | CostValue Reference
used by |
elements | AirLoopEquipment Construction ExtEquip HydronicLoop HydronicLoopEquipment IntEquip Layer LightingSystem Material Transportation Vegetation WindowType
attributes |
Name | Type | Use | Default | Fixed | annotation
costType | costTypeEnum | required |  |  |
source | <xsd:element name="Cost"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="CostValue"/> <xsd:element ref="Reference" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="costType" type="costTypeEnum" use="required"/> </xsd:complexType> </xsd:element>

attribute Cost/@costType

type | costTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | CO2
enumeration | SOx
enumeration | NOx
enumeration | EmbodiedEnergyTransportation
enumeration | EmbodiedEnergyManufacture
enumeration | EmbodiedEnergyInstallation
enumeration | EmbodiedEnergyTotal
enumeration | PurchaseCost
enumeration | DeliveryCost
enumeration | FirstCost
enumeration | MonthlyCost
enumeration | AnnualCost
enumeration | MaintenanceCost
enumeration | OverhaulCost
enumeration | InstallationCost
source | <xsd:attribute name="costType" type="costTypeEnum" use="required"/>

element CostValue

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Cost
attributes |
Name | Type | Use | Default | Fixed | annotation
currency | currencyTypeEnum |  |  |  |
unit | xsd:string | optional |  |  |
source | <xsd:element name="CostValue"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="currency" type="currencyTypeEnum"/> <xsd:attribute name="unit" type="xsd:string" use="optional"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute CostValue/@currency

type | currencyTypeEnum
properties |
isRef | 0
facets |
enumeration | USDollars
enumeration | CanadianDollars
enumeration | Pesos
enumeration | Euros
enumeration | Yen
enumeration | IndianRupee
enumeration | Yuan
enumeration | TaiwanDollar
enumeration | EnglishPound
enumeration | Mark
enumeration | Franc
enumeration | Ruble
enumeration | Real
enumeration | NewZealandDollar
enumeration | AustralianDollar
source | <xsd:attribute name="currency" type="currencyTypeEnum"/>

attribute CostValue/@unit

type | xsd:string
properties |
isRef | 0
use | optional
source | <xsd:attribute name="unit" type="xsd:string" use="optional"/>

element Country

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | Weather
source | <xsd:element name="Country" type="xsd:string"/>

element CreatedBy

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | DocumentHistory
attributes |
Name | Type | Use | Default | Fixed | annotation
personId | xsd:IDREF | required |  |  |
programId | xsd:IDREF | required |  |  |
date | xsd:dateTime | required |  |  |
annotation |
documentation
Denotes the time this file has been created, as well as the person and program used to create this file.
source | <xsd:element name="CreatedBy"> <xsd:annotation> <xsd:documentation>Denotes the time this file has been created, as well as the person and program used to create this file.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:attribute name="personId" type="xsd:IDREF" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="required"/> <xsd:attribute name="date" type="xsd:dateTime" use="required"/> </xsd:complexType> </xsd:element>

attribute CreatedBy/@personId

type | xsd:IDREF
properties |
isRef | 0
use | required
source | <xsd:attribute name="personId" type="xsd:IDREF" use="required"/>

attribute CreatedBy/@programId

type | xsd:IDREF
properties |
isRef | 0
use | required
source | <xsd:attribute name="programId" type="xsd:IDREF" use="required"/>

attribute CreatedBy/@date

type | xsd:dateTime
properties |
isRef | 0
use | required
source | <xsd:attribute name="date" type="xsd:dateTime" use="required"/>

element CyclesPerWeek

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
elements | ExtEquip IntEquip
annotation |
documentation
Number of operation cycles per week.
source | <xsd:element name="CyclesPerWeek" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Number of operation cycles per week.</xsd:documentation> </xsd:annotation> </xsd:element>

element Data

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | IndependantValue DependantValue
used by |
element | PointData
source | <xsd:element name="Data"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="IndependantValue" maxOccurs="2"/> <xsd:element ref="DependantValue" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> </xsd:complexType> </xsd:element>

element Day

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:string
properties |
content | complex
used by |
element | WeekSchedule
attributes |
Name | Type | Use | Default | Fixed | annotation
dayScheduleIdRef | xsd:IDREF | required |  |  |
documentation
ID for operation schedules
dayType | dayTypeEnum | required |  |  |
source | <xsd:element name="Day"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:string"> <xsd:attribute name="dayScheduleIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID for operation schedules</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="dayType" type="dayTypeEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Day/@dayScheduleIdRef

type | xsd:IDREF
properties |
isRef | 0
use | required
annotation |
documentation
ID for operation schedules
source | <xsd:attribute name="dayScheduleIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID for operation schedules</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Day/@dayType

type | dayTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Weekday
enumeration | Weekend
enumeration | Holiday
enumeration | WeekendOrHoliday
enumeration | HeatingDesignDay
enumeration | CoolingDesignDay
enumeration | Sun
enumeration | Mon
enumeration | Tue
enumeration | Wed
enumeration | Thu
enumeration | Fri
enumeration | Sat
enumeration | All
source | <xsd:attribute name="dayType" type="dayTypeEnum" use="required"/>

element DaylightSavings

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:boolean
properties |
content | simple
used by |
element | Campus
annotation |
documentation
Allows for including daylight savings time
source | <xsd:element name="DaylightSavings" type="xsd:boolean"> <xsd:annotation> <xsd:documentation>Allows for including daylight savings time</xsd:documentation> </xsd:annotation> </xsd:element>

element DaySchedule

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description ScheduleValue
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
type | scheduleTypeEnum | required |  |  |
annotation |
documentation
Set of values that define the profile of one 24 hour period divided equally to the number of values entered.
source | <xsd:element name="DaySchedule"> <xsd:annotation> <xsd:documentation>Set of values that define the profile of one 24 hour period divided equally to the number of values entered.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="ScheduleValue" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="type" type="scheduleTypeEnum" use="required"/> </xsd:complexType> </xsd:element>

attribute DaySchedule/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute DaySchedule/@type

type | scheduleTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Temp
enumeration | Fraction
enumeration | OnOff
source | <xsd:attribute name="type" type="scheduleTypeEnum" use="required"/>

element DDDayCool

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Heating design day dry bulb temperature range
source | <xsd:element name="DDDayCool" type="xsd:integer"> <xsd:annotation> <xsd:documentation>Heating design day dry bulb temperature range</xsd:documentation> </xsd:annotation> </xsd:element>

element DDDayHeat

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Day of the month that the heating design day occurs on
source | <xsd:element name="DDDayHeat" type="xsd:integer"> <xsd:annotation> <xsd:documentation>Day of the month that the heating design day occurs on</xsd:documentation> </xsd:annotation> </xsd:element>

element DDDaylightCool

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Flag for daylight savings on the cooling design day
source | <xsd:element name="DDDaylightCool" type="xsd:integer"> <xsd:annotation> <xsd:documentation>Flag for daylight savings on the cooling design day</xsd:documentation> </xsd:annotation> </xsd:element>

element DDDaylightHeat

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Flag for daylight savings for the heating design day
source | <xsd:element name="DDDaylightHeat" type="xsd:integer"> <xsd:annotation> <xsd:documentation>Flag for daylight savings for the heating design day</xsd:documentation> </xsd:annotation> </xsd:element>

element DDDBCool

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | temperatureUnitEnum |  |  |  |
annotation |
documentation
Cooling design day dry bulb temperature
source | <xsd:element name="DDDBCool"> <xsd:annotation> <xsd:documentation>Cooling design day dry bulb temperature</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDDBCool/@unit

type | temperatureUnitEnum
properties |
isRef | 0
facets |
enumeration | F
enumeration | C
enumeration | K
enumeration | R
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element DDDBHeat

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | temperatureUnitEnum |  |  |  |
annotation |
documentation
Heating design day dry bulb temperature
source | <xsd:element name="DDDBHeat"> <xsd:annotation> <xsd:documentation>Heating design day dry bulb temperature</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDDBHeat/@unit

type | temperatureUnitEnum
properties |
isRef | 0
facets |
enumeration | F
enumeration | C
enumeration | K
enumeration | R
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element DDDBRangeCool

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | temperatureUnitEnum |  |  |  |
annotation |
documentation
Cooling design day dry bulb temperature range
source | <xsd:element name="DDDBRangeCool"> <xsd:annotation> <xsd:documentation>Cooling design day dry bulb temperature range</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDDBRangeCool/@unit

type | temperatureUnitEnum
properties |
isRef | 0
facets |
enumeration | F
enumeration | C
enumeration | K
enumeration | R
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element DDDBRangeHeat

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | temperatureUnitEnum |  |  |  |
annotation |
documentation
Heating design day dry bulb temperature range
source | <xsd:element name="DDDBRangeHeat"> <xsd:annotation> <xsd:documentation>Heating design day dry bulb temperature range</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDDBRangeHeat/@unit

type | temperatureUnitEnum
properties |
isRef | 0
facets |
enumeration | F
enumeration | C
enumeration | K
enumeration | R
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element DDGroundTCool

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | temperatureUnitEnum |  |  |  |
annotation |
documentation
Ground temperature on the cooling design day
source | <xsd:element name="DDGroundTCool"> <xsd:annotation> <xsd:documentation>Ground temperature on the cooling design day</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDGroundTCool/@unit

type | temperatureUnitEnum
properties |
isRef | 0
facets |
enumeration | F
enumeration | C
enumeration | K
enumeration | R
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element DDGroundTHeat

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | temperatureUnitEnum |  |  |  |
annotation |
documentation
Ground temperature for the heating design day
source | <xsd:element name="DDGroundTHeat"> <xsd:annotation> <xsd:documentation>Ground temperature for the heating design day</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDGroundTHeat/@unit

type | temperatureUnitEnum
properties |
isRef | 0
facets |
enumeration | F
enumeration | C
enumeration | K
enumeration | R
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element DDHiHrCool

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Cooling design day hour of high temperature
source | <xsd:element name="DDHiHrCool" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Cooling design day hour of high temperature</xsd:documentation> </xsd:annotation> </xsd:element>

element DDHiHrHeat

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Heating design day hour of high temperature
source | <xsd:element name="DDHiHrHeat" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Heating design day hour of high temperature</xsd:documentation> </xsd:annotation> </xsd:element>

element DDLoHrCool

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Cooling design day hour of low temperature
source | <xsd:element name="DDLoHrCool" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Cooling design day hour of low temperature</xsd:documentation> </xsd:annotation> </xsd:element>

element DDLoHrHeat

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Heating design day hour of low temperature
source | <xsd:element name="DDLoHrHeat" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Heating design day hour of low temperature</xsd:documentation> </xsd:annotation> </xsd:element>

element DDMonthCool

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Month the cooling design day lands on. 1=Jan 12=Dec
source | <xsd:element name="DDMonthCool" type="xsd:integer"> <xsd:annotation> <xsd:documentation>Month the cooling design day lands on. 1=Jan 12=Dec</xsd:documentation> </xsd:annotation> </xsd:element>

element DDMonthHeat

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Month that the heating design day occurs on. 1=Jan 12=Dec
source | <xsd:element name="DDMonthHeat" type="xsd:integer"> <xsd:annotation> <xsd:documentation>Month that the heating design day occurs on. 1=Jan 12=Dec</xsd:documentation> </xsd:annotation> </xsd:element>

element DDPressureCool

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | pressureUnitEnum |  |  |  |
annotation |
documentation
Cooling design day atmospheric pressure
source | <xsd:element name="DDPressureCool"> <xsd:annotation> <xsd:documentation>Cooling design day atmospheric pressure</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="pressureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDPressureCool/@unit

type | pressureUnitEnum
properties |
isRef | 0
facets |
enumeration | PSI
enumeration | kPa
enumeration | Atmospheres
enumeration | InchesOfH2O
enumeration | CentimetersOfH2O
enumeration | InchesOfMercury
enumeration | CentimetersOfMercury
enumeration | MillimetersOfMercury
enumeration | Pascals
source | <xsd:attribute name="unit" type="pressureUnitEnum"/>

element DDPressureHeat

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | pressureUnitEnum |  |  |  |
annotation |
documentation
Heating design day atmospheric pressure
source | <xsd:element name="DDPressureHeat"> <xsd:annotation> <xsd:documentation>Heating design day atmospheric pressure</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="pressureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDPressureHeat/@unit

type | pressureUnitEnum
properties |
isRef | 0
facets |
enumeration | PSI
enumeration | kPa
enumeration | Atmospheres
enumeration | InchesOfH2O
enumeration | CentimetersOfH2O
enumeration | InchesOfMercury
enumeration | CentimetersOfMercury
enumeration | MillimetersOfMercury
enumeration | Pascals
source | <xsd:attribute name="unit" type="pressureUnitEnum"/>

element DDRainCool

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Flag for rain on the cooling design day. 0=no rain 1=rain
source | <xsd:element name="DDRainCool" type="xsd:integer"> <xsd:annotation> <xsd:documentation>Flag for rain on the cooling design day. 0=no rain 1=rain</xsd:documentation> </xsd:annotation> </xsd:element>

element DDRainHeat

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Heating design day rain flag. 0=no rain, 1=rain
source | <xsd:element name="DDRainHeat" type="xsd:integer"> <xsd:annotation> <xsd:documentation>Heating design day rain flag. 0=no rain, 1=rain</xsd:documentation> </xsd:annotation> </xsd:element>

element DDSkyClearnessCool

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | unitlessUnitEnum | required |  |  |
annotation |
documentation
Cooling design day sky clearness
source | <xsd:element name="DDSkyClearnessCool"> <xsd:annotation> <xsd:documentation>Cooling design day sky clearness</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDSkyClearnessCool/@unit

type | unitlessUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Percent
enumeration | Fraction
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element DDSkyClearnessHeat

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | unitlessUnitEnum | required |  |  |
annotation |
documentation
Heating design day sky clearness
source | <xsd:element name="DDSkyClearnessHeat"> <xsd:annotation> <xsd:documentation>Heating design day sky clearness</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDSkyClearnessHeat/@unit

type | unitlessUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Percent
enumeration | Fraction
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element DDSnowCool

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Flag for snow on the cooling design day. 0=not snowing 1=snowing
source | <xsd:element name="DDSnowCool" type="xsd:integer"> <xsd:annotation> <xsd:documentation>Flag for snow on the cooling design day. 0=not snowing 1=snowing</xsd:documentation> </xsd:annotation> </xsd:element>

element DDSnowHeat

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Heating design day snow flag. 0=not snowing 1=snowing
source | <xsd:element name="DDSnowHeat" type="xsd:integer"> <xsd:annotation> <xsd:documentation>Heating design day snow flag. 0=not snowing 1=snowing</xsd:documentation> </xsd:annotation> </xsd:element>

element DDWBCool

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | temperatureUnitEnum |  |  |  |
annotation |
documentation
Cooling design day wet bulb temperature
source | <xsd:element name="DDWBCool"> <xsd:annotation> <xsd:documentation>Cooling design day wet bulb temperature</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDWBCool/@unit

type | temperatureUnitEnum
properties |
isRef | 0
facets |
enumeration | F
enumeration | C
enumeration | K
enumeration | R
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element DDWBHeat

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | temperatureUnitEnum |  |  |  |
annotation |
documentation
Heating design day wet bulb temperature
source | <xsd:element name="DDWBHeat"> <xsd:annotation> <xsd:documentation>Heating design day wet bulb temperature</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDWBHeat/@unit

type | temperatureUnitEnum
properties |
isRef | 0
facets |
enumeration | F
enumeration | C
enumeration | K
enumeration | R
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element DDWindDirCool

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | directionUnitEnum | required |  |  |
annotation |
documentation
Cooing design day wind direction
source | <xsd:element name="DDWindDirCool"> <xsd:annotation> <xsd:documentation>Cooing design day wind direction</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="directionUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDWindDirCool/@unit

type | directionUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | DegreeDecimalFromNorth
source | <xsd:attribute name="unit" type="directionUnitEnum" use="required"/>

element DDWindDirHeat

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | directionUnitEnum | required |  |  |
annotation |
documentation
Heating design day wind direction
source | <xsd:element name="DDWindDirHeat"> <xsd:annotation> <xsd:documentation>Heating design day wind direction</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="directionUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDWindDirHeat/@unit

type | directionUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | DegreeDecimalFromNorth
source | <xsd:attribute name="unit" type="directionUnitEnum" use="required"/>

element DDWindSpeedCool

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | velocityUnitEnum | required |  |  |
annotation |
documentation
Cooling design day wind speed
source | <xsd:element name="DDWindSpeedCool"> <xsd:annotation> <xsd:documentation>Cooling design day wind speed</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="velocityUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDWindSpeedCool/@unit

type | velocityUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | MetersPerSecond
enumeration | MilesPerHour
enumeration | Knots
source | <xsd:attribute name="unit" type="velocityUnitEnum" use="required"/>

element DDWindSpeedHeat

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | velocityUnitEnum | required |  |  |
annotation |
documentation
Heating design day wind speed
source | <xsd:element name="DDWindSpeedHeat"> <xsd:annotation> <xsd:documentation>Heating design day wind speed</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="velocityUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDWindSpeedHeat/@unit

type | velocityUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | MetersPerSecond
enumeration | MilesPerHour
enumeration | Knots
source | <xsd:attribute name="unit" type="velocityUnitEnum" use="required"/>

element DeltaP

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | AirLoopEquipment HydronicLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | deltaPUnitEnum | required |  |  |
hydronicLoopType | loopTypeEnum |  |  |  |
hydronicLoopIdRef | xsd:IDREF |  |  |  |
conditioningType | conditioningTypeEnum |  |  |  |
documentation
Use this attribute for conditioning units with both heating and cooling.
performanceId | xsd:IDREF |  |  |  |
documentation
Use this attribute to point to a performance curve if one is provided
annotation |
documentation
Difference in pressure
source | <xsd:element name="DeltaP"> <xsd:annotation> <xsd:documentation>Difference in pressure</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="deltaPUnitEnum" use="required"/> <xsd:attribute name="hydronicLoopType" type="loopTypeEnum"/> <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF"/> <xsd:attribute name="conditioningType" type="conditioningTypeEnum"> <xsd:annotation> <xsd:documentation>Use this attribute for conditioning units with both heating and cooling.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="performanceId" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Use this attribute to point to a performance curve if one is provided</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DeltaP/@unit

type | deltaPUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | PSI
enumeration | kPa
enumeration | Atmospheres
enumeration | InchesOfH2O
enumeration | CentimetersOfH2O
enumeration | InchesOfMercury
enumeration | CentimetersOfMercury
enumeration | MillimetersOfMercury
enumeration | Pascals
source | <xsd:attribute name="unit" type="deltaPUnitEnum" use="required"/>

attribute DeltaP/@hydronicLoopType

type | loopTypeEnum
properties |
isRef | 0
facets |
enumeration | PrimaryChilledWater
enumeration | SecondaryChilledWater
enumeration | HotWater
enumeration | CondenserWater
enumeration | DomesticHotWater
enumeration | WaterLoopHeatPump
enumeration | TwoPipe
enumeration | PotableWaterLoop
source | <xsd:attribute name="hydronicLoopType" type="loopTypeEnum"/>

attribute DeltaP/@hydronicLoopIdRef

type | xsd:IDREF
properties |
isRef | 0
source | <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF"/>

attribute DeltaP/@conditioningType

type | conditioningTypeEnum
properties |
isRef | 0
facets |
enumeration | Heating
enumeration | Cooling
enumeration | HeatingAndCooling
annotation |
documentation
Use this attribute for conditioning units with both heating and cooling.
source | <xsd:attribute name="conditioningType" type="conditioningTypeEnum"> <xsd:annotation> <xsd:documentation>Use this attribute for conditioning units with both heating and cooling.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute DeltaP/@performanceId

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
Use this attribute to point to a performance curve if one is provided
source | <xsd:attribute name="performanceId" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Use this attribute to point to a performance curve if one is provided</xsd:documentation> </xsd:annotation> </xsd:attribute>

element DeltaT

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | AirLoopEquipment HydronicLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | temperatureUnitEnum |  |  |  |
conditioningType | conditioningTypeEnum |  |  |  |
documentation
Use this attribute for conditioning units with both heating and cooling.
annotation |
documentation
Difference in temperature
source | <xsd:element name="DeltaT"> <xsd:annotation> <xsd:documentation>Difference in temperature</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> <xsd:attribute name="conditioningType" type="conditioningTypeEnum"> <xsd:annotation> <xsd:documentation>Use this attribute for conditioning units with both heating and cooling.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DeltaT/@unit

type | temperatureUnitEnum
properties |
isRef | 0
facets |
enumeration | F
enumeration | C
enumeration | K
enumeration | R
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

attribute DeltaT/@conditioningType

type | conditioningTypeEnum
properties |
isRef | 0
facets |
enumeration | Heating
enumeration | Cooling
enumeration | HeatingAndCooling
annotation |
documentation
Use this attribute for conditioning units with both heating and cooling.
source | <xsd:attribute name="conditioningType" type="conditioningTypeEnum"> <xsd:annotation> <xsd:documentation>Use this attribute for conditioning units with both heating and cooling.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Density

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Gap Material
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | densityUnitEnum | required |  |  |
source | <xsd:element name="Density"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="densityUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Density/@unit

type | densityUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | GramsPerCubicCm
enumeration | LbsPerCubicIn
enumeration | LbsPerCubicFt
enumeration | KgPerCubicM
source | <xsd:attribute name="unit" type="densityUnitEnum" use="required"/>

element DensityFofT

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Gap
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | densityFofTUnitEnum | required |  |  |
annotation |
documentation
Density as a function of temperature
source | <xsd:element name="DensityFofT"> <xsd:annotation> <xsd:documentation>Density as a function of temperature</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="densityFofTUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DensityFofT/@unit

type | densityFofTUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | LbsPerCubicFtF
enumeration | KgPerCubicMK
source | <xsd:attribute name="unit" type="densityFofTUnitEnum" use="required"/>

element DependantValue

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Data
annotation |
documentation
Value of a dependant variable for this data point
source | <xsd:element name="DependantValue" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Value of a dependant variable for this data point</xsd:documentation> </xsd:annotation> </xsd:element>

element DependantVariable

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description
used by |
elements | Equation PointData
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | xsd:string | required |  |  |
dataType | xsd:string | required |  |  |
minValue | xsd:decimal |  |  |  |
documentation
Use minValue and maxValue to define constraints on the curve.
maxValue | xsd:decimal |  |  |  |
source | <xsd:element name="DependantVariable"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="unit" type="xsd:string" use="required"/> <xsd:attribute name="dataType" type="xsd:string" use="required"/> <xsd:attribute name="minValue" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Use minValue and maxValue to define constraints on the curve.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="maxValue" type="xsd:decimal"/> </xsd:complexType> </xsd:element>

attribute DependantVariable/@unit

type | xsd:string
properties |
isRef | 0
use | required
source | <xsd:attribute name="unit" type="xsd:string" use="required"/>

attribute DependantVariable/@dataType

type | xsd:string
properties |
isRef | 0
use | required
source | <xsd:attribute name="dataType" type="xsd:string" use="required"/>

attribute DependantVariable/@minValue

type | xsd:decimal
properties |
isRef | 0
annotation |
documentation
Use minValue and maxValue to define constraints on the curve.
source | <xsd:attribute name="minValue" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Use minValue and maxValue to define constraints on the curve.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute DependantVariable/@maxValue

type | xsd:decimal
properties |
isRef | 0
source | <xsd:attribute name="maxValue" type="xsd:decimal"/>

element Description

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
elements | AirLoop AirLoopEquipment Blind Building Campus Construction DaySchedule DependantVariable ExtEquip Frame Gap Glaze HydronicLoop HydronicLoopEquipment IndepentantVariable IntEquip Layer Location Material Meter Opening Results Schedule ShellGeometry Space Surface Weather WeekSchedule WindowType XAxis YAxis YearSchedule Zone
source | <xsd:element name="Description" type="xsd:string"/>

element DesignCoolT

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Zone
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | temperatureUnitEnum |  |  |  |
annotation |
documentation
Design temperature for cooling
source | <xsd:element name="DesignCoolT"> <xsd:annotation> <xsd:documentation>Design temperature for cooling</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DesignCoolT/@unit

type | temperatureUnitEnum
properties |
isRef | 0
facets |
enumeration | F
enumeration | C
enumeration | K
enumeration | R
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element DesignFlow

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | FlowControl
source | <xsd:element name="DesignFlow" type="xsd:decimal"/>

element DesignHeatT

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Zone
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | temperatureUnitEnum |  |  |  |
annotation |
documentation
Design temperature for heating
source | <xsd:element name="DesignHeatT"> <xsd:annotation> <xsd:documentation>Design temperature for heating</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DesignHeatT/@unit

type | temperatureUnitEnum
properties |
isRef | 0
facets |
enumeration | F
enumeration | C
enumeration | K
enumeration | R
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element DesignPressure

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | PressureControl
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | pressureUnitEnum |  |  |  |
source | <xsd:element name="DesignPressure"> <xsd:complexType> <xsd:attribute name="unit" type="pressureUnitEnum"/> </xsd:complexType> </xsd:element>

attribute DesignPressure/@unit

type | pressureUnitEnum
properties |
isRef | 0
facets |
enumeration | PSI
enumeration | kPa
enumeration | Atmospheres
enumeration | InchesOfH2O
enumeration | CentimetersOfH2O
enumeration | InchesOfMercury
enumeration | CentimetersOfMercury
enumeration | MillimetersOfMercury
enumeration | Pascals
source | <xsd:attribute name="unit" type="pressureUnitEnum"/>

element DesignTemp

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | TemperatureControl
source | <xsd:element name="DesignTemp" type="xsd:decimal"/>

element Dimensions

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Height Width Length
used by |
element | LightingSystem
source | <xsd:element name="Dimensions"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Height" minOccurs="0"/> <xsd:element ref="Width" minOccurs="0"/> <xsd:element ref="Length" minOccurs="0"/> </xsd:choice> </xsd:complexType> </xsd:element>

element DocumentHistory

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | ProgramInfo PersonInfo CreatedBy ModifiedBy
used by |
element | gbXML
annotation |
documentation
Contains details about people and programs that created and modified this file
source | <xsd:element name="DocumentHistory"> <xsd:annotation> <xsd:documentation>Contains details about people and programs that created and modified this file</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="ProgramInfo" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="PersonInfo" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="CreatedBy" minOccurs="0"/> <xsd:element ref="ModifiedBy" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> </xsd:complexType> </xsd:element>

element Efficiency

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | AirLoopEquipment ExtEquip HydronicLoopEquipment IntEquip
attributes |
Name | Type | Use | Default | Fixed | annotation
standardsType | standardsTypeEnum |  |  |  |
documentation
Use the standardsType attribute when the efficiency is measured at standard conditions.
efficiencyType | efficiencyTypeEnum | required |  |  |
operationType | conditioningTypeEnum |  |  |  |
documentation
Use this attribute for conditioning units with both heating and cooling.
performanceId | xsd:IDREF |  |  |  |
documentation
Use this attribute to point to a performance curve if one is provided
source | <xsd:element name="Efficiency"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="standardsType" type="standardsTypeEnum"> <xsd:annotation> <xsd:documentation>Use the standardsType attribute when the efficiency is measured at standard conditions.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="efficiencyType" type="efficiencyTypeEnum" use="required"/> <xsd:attribute name="operationType" type="conditioningTypeEnum"> <xsd:annotation> <xsd:documentation>Use this attribute for conditioning units with both heating and cooling.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="performanceId" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Use this attribute to point to a performance curve if one is provided</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Efficiency/@standardsType

type | standardsTypeEnum
properties |
isRef | 0
facets |
enumeration | DOE
enumeration | ARI
enumeration | ANSI
enumeration | NEMA
annotation |
documentation
Use the standardsType attribute when the efficiency is measured at standard conditions.
source | <xsd:attribute name="standardsType" type="standardsTypeEnum"> <xsd:annotation> <xsd:documentation>Use the standardsType attribute when the efficiency is measured at standard conditions.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Efficiency/@efficiencyType

type | efficiencyTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | COP
enumeration | EER
enumeration | SEER
enumeration | AFUE
enumeration | HSPF
enumeration | effectiveness
enumeration | EnergyFactor
enumeration | ThermalEff
enumeration | MotorEff
enumeration | FanEff
enumeration | MechanicalEff
enumeration | BoilerEff
enumeration | kWPerTon
enumeration | kWPerkW
source | <xsd:attribute name="efficiencyType" type="efficiencyTypeEnum" use="required"/>

attribute Efficiency/@operationType

type | conditioningTypeEnum
properties |
isRef | 0
facets |
enumeration | Heating
enumeration | Cooling
enumeration | HeatingAndCooling
annotation |
documentation
Use this attribute for conditioning units with both heating and cooling.
source | <xsd:attribute name="operationType" type="conditioningTypeEnum"> <xsd:annotation> <xsd:documentation>Use this attribute for conditioning units with both heating and cooling.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Efficiency/@performanceId

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
Use this attribute to point to a performance curve if one is provided
source | <xsd:attribute name="performanceId" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Use this attribute to point to a performance curve if one is provided</xsd:documentation> </xsd:annotation> </xsd:attribute>

element ElecLoad

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | ExtEquip IntEquip
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | powerUnitEnum | required |  |  |
annotation |
documentation
Electric load
source | <xsd:element name="ElecLoad"> <xsd:annotation> <xsd:documentation>Electric load</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="powerUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute ElecLoad/@unit

type | powerUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Watt
enumeration | Kilowatt
enumeration | Horsepower
enumeration | KilogramForceMeterPerSecond
enumeration | BtuPerSecond
enumeration | FootPoundForcePerSecond
enumeration | KilocaloriesPerSecond
enumeration | BtuPerHour
source | <xsd:attribute name="unit" type="powerUnitEnum" use="required"/>

element Elevation

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Location
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | lengthUnitEnum |  |  |  |
annotation |
documentation
Height above sea level
source | <xsd:element name="Elevation"> <xsd:annotation> <xsd:documentation>Height above sea level</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="lengthUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Elevation/@unit

type | lengthUnitEnum
properties |
isRef | 0
facets |
enumeration | Kilometers
enumeration | Meters
enumeration | Centimeters
enumeration | Millimeters
enumeration | Miles
enumeration | Yards
enumeration | Feet
enumeration | Inches
source | <xsd:attribute name="unit" type="lengthUnitEnum"/>

element Email1Address

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | PersonInfo
source | <xsd:element name="Email1Address" type="xsd:string"/>

element EmissionRate

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | IndoorAirQuality
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | emissionUnitEnum | required |  |  |
source | <xsd:element name="EmissionRate"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="emissionUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute EmissionRate/@unit

type | emissionUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | PoundsPerHour
enumeration | KilogramsPerHour
enumeration | GramsPerHour
source | <xsd:attribute name="unit" type="emissionUnitEnum" use="required"/>

element Emittance

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Blind Construction Glaze Opening WindowType
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | unitlessUnitEnum | required |  |  |
type | emittanceTypeEnum | required |  |  |
annotation |
documentation
Infra-red emissivity
source | <xsd:element name="Emittance"> <xsd:annotation> <xsd:documentation>Infra-red emissivity</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> <xsd:attribute name="type" type="emittanceTypeEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Emittance/@unit

type | unitlessUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Percent
enumeration | Fraction
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

attribute Emittance/@type

type | emittanceTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | IntIR
enumeration | ExtIR
source | <xsd:attribute name="type" type="emittanceTypeEnum" use="required"/>

element EndDate

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:date
properties |
content | simple
used by |
element | YearSchedule
annotation |
documentation
Month and day year schedule ends
source | <xsd:element name="EndDate" type="xsd:date"> <xsd:annotation> <xsd:documentation>Month and day year schedule ends</xsd:documentation> </xsd:annotation> </xsd:element>

element Energy

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | AirLoopEquipment ExtEquip HydronicLoopEquipment IntEquip
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | energyUnitEnum | required |  |  |
valueType | valueTypeEnum | required |  |  |
timePeriod | timePeriodEnum | required |  |  |
resourceType | resourceTypeEnum | required |  |  |
meterIdRef | xsd:IDREF |  |  |  |
documentation
ID for a resource meter
source | <xsd:element name="Energy"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="energyUnitEnum" use="required"/> <xsd:attribute name="valueType" type="valueTypeEnum" use="required"/> <xsd:attribute name="timePeriod" type="timePeriodEnum" use="required"/> <xsd:attribute name="resourceType" type="resourceTypeEnum" use="required"/> <xsd:attribute name="meterIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for a resource meter</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Energy/@unit

type | energyUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | KilowattHours
enumeration | Joules
enumeration | BTU
enumeration | Therms
source | <xsd:attribute name="unit" type="energyUnitEnum" use="required"/>

attribute Energy/@valueType

type | valueTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Historical
enumeration | Simulated
enumeration | Rated
enumeration | Measured
source | <xsd:attribute name="valueType" type="valueTypeEnum" use="required"/>

attribute Energy/@timePeriod

type | timePeriodEnum
properties |
isRef | 0
use | required
facets |
enumeration | Annual
enumeration | Jan
enumeration | Feb
enumeration | Mar
enumeration | Apr
enumeration | May
enumeration | Jun
enumeration | Jul
enumeration | Aug
enumeration | Sep
enumeration | Oct
enumeration | Nov
enumeration | Dec
source | <xsd:attribute name="timePeriod" type="timePeriodEnum" use="required"/>

attribute Energy/@resourceType

type | resourceTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Electricity
enumeration | NaturalGas
enumeration | Propane
enumeration | FuelOil1
enumeration | FuelOil2
enumeration | FuelOil4
enumeration | Water
enumeration | ChilledWater
enumeration | HotWater
enumeration | Steam
source | <xsd:attribute name="resourceType" type="resourceTypeEnum" use="required"/>

attribute Energy/@meterIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID for a resource meter
source | <xsd:attribute name="meterIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for a resource meter</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Equation

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Expression IndepentantVariable DependantVariable
used by |
element | Performance
annotation |
documentation
The Equation element allows data for n-dimensional algebraic data to be entered. The Expression element should contain an independent variable followed by an = sign and an equation containing dependant variables. The independent and dependant variables are then defined by their respective tags. The only mathematical operations allowed are ^ (power), + (addition), - (subtraction), / (division), and * (multiplication). Example: z=x+2*y^2 would have an IndependantVariable with a name = z, and two DependantVariables with names of x and y. Descriptions would be included for each variable, along with unit and dataType information identifying the variable and its role.
source | <xsd:element name="Equation"> <xsd:annotation> <xsd:documentation>The Equation element allows data for n-dimensional algebraic data to be entered. The Expression element should contain an independent variable followed by an = sign and an equation containing dependant variables. The independent and dependant variables are then defined by their respective tags. The only mathematical operations allowed are ^ (power), + (addition), - (subtraction), / (division), and * (multiplication). Example: z=x+2*y^2 would have an IndependantVariable with a name = z, and two DependantVariables with names of x and y. Descriptions would be included for each variable, along with unit and dataType information identifying the variable and its role. </xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Expression"/> <xsd:element ref="IndepentantVariable" maxOccurs="2"/> <xsd:element ref="DependantVariable" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> </xsd:complexType> </xsd:element>

element EquipPowerPerArea

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Space
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | powerPerAreaUnitEnum | required |  |  |
annotation |
documentation
Amount of power used by equipment in a given area
source | <xsd:element name="EquipPowerPerArea"> <xsd:annotation> <xsd:documentation>Amount of power used by equipment in a given area</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="powerPerAreaUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute EquipPowerPerArea/@unit

type | powerPerAreaUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | WattPerSquareMeter
enumeration | WattPerSquareFoot
source | <xsd:attribute name="unit" type="powerPerAreaUnitEnum" use="required"/>

element Expression

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | Equation
source | <xsd:element name="Expression" type="xsd:string"/>

element ExtEquip

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Manufacturer Model ElecLoad FuelLoad LatentLoad Efficiency Performance Cost WasteWaterHREff WaterUsePerCycle RatedFlow Power CyclesPerWeek Energy GeneralGeometry ShellGeometry IndoorAirQuality Age Reference CADObjectId
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
scheduleIdRef | xsd:IDREF |  |  |  |
documentation
ID for the schedule of transmittance of a shading surface
waterTempScheduleIdRef | xsd:IDREF |  |  |  |
hydronicLoopIdRef | xsd:IDREF |  |  |  |
documentation
ID pointing to a hydronic loop
waterScheduleIdRef | xsd:IDREF |  |  |  |
waterMeterIdRef | xsd:IDREF |  |  |  |
type | extEquipTypeEnum | required |  |  |
airLoopIdRef | xsd:IDREF |  |  |  |
documentation
ID pointing to an air loop
annotation |
documentation
External equipment. This is generalized to be able to contain any type of external equipment.
source | <xsd:element name="ExtEquip"> <xsd:annotation> <xsd:documentation>External equipment. This is generalized to be able to contain any type of external equipment.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Manufacturer" minOccurs="0"/> <xsd:element ref="Model" minOccurs="0"/> <xsd:element ref="ElecLoad" minOccurs="0"/> <xsd:element ref="FuelLoad" minOccurs="0"/> <xsd:element ref="LatentLoad" minOccurs="0"/> <xsd:element ref="Efficiency" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Performance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Cost" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="WasteWaterHREff" minOccurs="0"/> <xsd:element ref="WaterUsePerCycle" minOccurs="0"/> <xsd:element ref="RatedFlow" minOccurs="0"/> <xsd:element ref="Power" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="CyclesPerWeek" minOccurs="0"/> <xsd:element ref="Energy" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="GeneralGeometry" minOccurs="0"/> <xsd:element ref="ShellGeometry" minOccurs="0"/> <xsd:element ref="IndoorAirQuality" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Age" minOccurs="0"/> <xsd:element ref="Reference" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="CADObjectId" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="waterTempScheduleIdRef" type="xsd:IDREF"/> <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID pointing to a hydronic loop </xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="waterScheduleIdRef" type="xsd:IDREF"/> <xsd:attribute name="waterMeterIdRef" type="xsd:IDREF"/> <xsd:attribute name="type" type="extEquipTypeEnum" use="required"/> <xsd:attribute name="airLoopIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID pointing to an air loop</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute ExtEquip/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute ExtEquip/@scheduleIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID for the schedule of transmittance of a shading surface
source | <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute ExtEquip/@waterTempScheduleIdRef

type | xsd:IDREF
properties |
isRef | 0
source | <xsd:attribute name="waterTempScheduleIdRef" type="xsd:IDREF"/>

attribute ExtEquip/@hydronicLoopIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID pointing to a hydronic loop
source | <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID pointing to a hydronic loop </xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute ExtEquip/@waterScheduleIdRef

type | xsd:IDREF
properties |
isRef | 0
source | <xsd:attribute name="waterScheduleIdRef" type="xsd:IDREF"/>

attribute ExtEquip/@waterMeterIdRef

type | xsd:IDREF
properties |
isRef | 0
source | <xsd:attribute name="waterMeterIdRef" type="xsd:IDREF"/>

attribute ExtEquip/@type

type | extEquipTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Sprinkler
enumeration | LawnMower
enumeration | GeneralPlugload
enumeration | Fountain
enumeration | Refrigerator
enumeration | Freezer
enumeration | Pool
enumeration | HotTub
enumeration | Pump
enumeration | Sauna
enumeration | BatteryCharger
enumeration | Furnace
enumeration | IndustrialEquip
enumeration | Irrigation
enumeration | MiscEquip
enumeration | Vending
enumeration | Elevator
enumeration | Escalator
source | <xsd:attribute name="type" type="extEquipTypeEnum" use="required"/>

attribute ExtEquip/@airLoopIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID pointing to an air loop
source | <xsd:attribute name="airLoopIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID pointing to an air loop</xsd:documentation> </xsd:annotation> </xsd:attribute>

element ExtEquipId

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:string
properties |
content | complex
used by |
element | Campus
attributes |
Name | Type | Use | Default | Fixed | annotation
extEquipIdRef | xsd:IDREF |  |  |  |
source | <xsd:element name="ExtEquipId"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:string"> <xsd:attribute name="extEquipIdRef" type="xsd:IDREF"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute ExtEquipId/@extEquipIdRef

type | xsd:IDREF
properties |
isRef | 0
source | <xsd:attribute name="extEquipIdRef" type="xsd:IDREF"/>

element FirstName

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | PersonInfo
source | <xsd:element name="FirstName" type="xsd:string"/>

element FloorSlabHeatLossCoefficient

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:float
properties |
content | complex
used by |
element | LoadCalcInputParameters
attributes |
Name | Type | Use | Default | Fixed | annotation
floorSlabPerimeterHeatLossCoefficientUnitTypeEnum | floorSlabPerimeterHeatLossCoefficientUnitTypeEnum |  |  |  |
annotation |
documentation
Specifies the heat loss from a floor in terms of the amount of heat lost per length of exposed perimeter. Used with both commercial and residential load calculation methods.
source | <xsd:element name="FloorSlabHeatLossCoefficient"> <xsd:annotation> <xsd:documentation>Specifies the heat loss from a floor in terms of the amount of heat lost per length of exposed perimeter. Used with both commercial and residential load calculation methods.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:float"> <xsd:attribute name="floorSlabPerimeterHeatLossCoefficientUnitTypeEnum" type="floorSlabPerimeterHeatLossCoefficientUnitTypeEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute FloorSlabHeatLossCoefficient/@floorSlabPerimeterHeatLossCoefficientUnitTypeEnum

type | floorSlabPerimeterHeatLossCoefficientUnitTypeEnum
properties |
isRef | 0
facets |
enumeration | btuPerHourDegreeFPerLinearFoot
enumeration | wattDegreeCPerLinearMeter
source | <xsd:attribute name="floorSlabPerimeterHeatLossCoefficientUnitTypeEnum" type="floorSlabPerimeterHeatLossCoefficientUnitTypeEnum"/>

element Flow

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Zone
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | flowUnitEnum | required |  |  |
source | <xsd:element name="Flow"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="flowUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Flow/@unit

type | flowUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | CFM
enumeration | LPerSec
enumeration | CubicMPerHr
enumeration | GPM
enumeration | GPH
source | <xsd:attribute name="unit" type="flowUnitEnum" use="required"/>

element FlowControl

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | DesignFlow MinimumFlow MaximumFlow
used by |
element | HydronicLoop
annotation |
documentation
Use this element to describe how the fluid flow is controlled. The temperatures specified in this element should be measured just upstream of the chiller.
source | <xsd:element name="FlowControl"> <xsd:annotation> <xsd:documentation>Use this element to describe how the fluid flow is controlled. The temperatures specified in this element should be measured just upstream of the chiller.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="DesignFlow" minOccurs="0"/> <xsd:element ref="MinimumFlow" minOccurs="0"/> <xsd:element ref="MaximumFlow" minOccurs="0"/> </xsd:choice> </xsd:complexType> </xsd:element>

element FlowPerArea

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Zone
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | flowPerAreaUnitEnum | required |  |  |
source | <xsd:element name="FlowPerArea"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="flowPerAreaUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute FlowPerArea/@unit

type | flowPerAreaUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | CFMPerSquareFoot
enumeration | LPerSecPerSquareM
enumeration | CubicMPerSecPerSquareM
source | <xsd:attribute name="unit" type="flowPerAreaUnitEnum" use="required"/>

element FlowPerPerson

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Zone
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | flowUnitEnum | required |  |  |
source | <xsd:element name="FlowPerPerson"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="flowUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute FlowPerPerson/@unit

type | flowUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | CFM
enumeration | LPerSec
enumeration | CubicMPerHr
enumeration | GPM
enumeration | GPH
source | <xsd:attribute name="unit" type="flowUnitEnum" use="required"/>

element Frame

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Width
used by |
element | WindowType
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
type | frameTypeEnum | required |  |  |
DOELibIdRef | xsd:string |  |  |  |
documentation
Use this attribute to reference objects in the DOE2 library
source | <xsd:element name="Frame"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Width" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="type" type="frameTypeEnum" use="required"/> <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Frame/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Frame/@type

type | frameTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Wood
enumeration | Vinyl
enumeration | Aluminum
enumeration | AluminumWithBreak
enumeration | Insulated
source | <xsd:attribute name="type" type="frameTypeEnum" use="required"/>

attribute Frame/@DOELibIdRef

type | xsd:string
properties |
isRef | 0
annotation |
documentation
Use this attribute to reference objects in the DOE2 library
source | <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute>

element FuelLoad

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | ExtEquip IntEquip
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | fuelLoadUnitEnum | required |  |  |
source | <xsd:element name="FuelLoad"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="fuelLoadUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute FuelLoad/@unit

type | fuelLoadUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | BtuPerHour
enumeration | kBtuPerHour
enumeration | MBtuPerHour
enumeration | Watts
enumeration | kW
source | <xsd:attribute name="unit" type="fuelLoadUnitEnum" use="required"/>

element Gap

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Thickness Density DensityFofT Conductivity ConductivityFofT Viscosity ViscosityFofT PrandtlNumber PrandtlNumberFofT
used by |
element | WindowType
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
gas | gasTypeEnum | required |  |  |
DOELibIdRef | xsd:string |  |  |  |
documentation
Use this attribute to reference objects in the DOE2 library
annotation |
documentation
Space between window panes
source | <xsd:element name="Gap"> <xsd:annotation> <xsd:documentation>Space between window panes</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Thickness" minOccurs="0"/> <xsd:element ref="Density" minOccurs="0"/> <xsd:element ref="DensityFofT" minOccurs="0"/> <xsd:element ref="Conductivity" minOccurs="0"/> <xsd:element ref="ConductivityFofT" minOccurs="0"/> <xsd:element ref="Viscosity" minOccurs="0"/> <xsd:element ref="ViscosityFofT" minOccurs="0"/> <xsd:element ref="PrandtlNumber" minOccurs="0"/> <xsd:element ref="PrandtlNumberFofT" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="gas" type="gasTypeEnum" use="required"/> <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Gap/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Gap/@gas

type | gasTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Air
enumeration | Argon
enumeration | Krypton
enumeration | CO2
enumeration | SF6
enumeration | Custom
source | <xsd:attribute name="gas" type="gasTypeEnum" use="required"/>

attribute Gap/@DOELibIdRef

type | xsd:string
properties |
isRef | 0
annotation |
documentation
Use this attribute to reference objects in the DOE2 library
source | <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute>

element GapId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
attributes |
Name | Type | Use | Default | Fixed | annotation
gapIdRef | xsd:IDREF | required |  |  |
documentation
ID for a gap between window panes
source | <xsd:element name="GapId"> <xsd:complexType> <xsd:attribute name="gapIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID for a gap between window panes</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute GapId/@gapIdRef

type | xsd:IDREF
properties |
isRef | 0
use | required
annotation |
documentation
ID for a gap between window panes
source | <xsd:attribute name="gapIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID for a gap between window panes</xsd:documentation> </xsd:annotation> </xsd:attribute>

element gbXML

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | aecXML Campus LightingSystem LightingControl Construction Layer Material WindowType Schedule WeekSchedule DaySchedule Zone AirLoop HydronicLoop IntEquip ExtEquip Weather Meter Results DocumentHistory
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID |  |  |  |
engine | derived by: xsd:NMTOKEN |  |  |  |
documentation
Analysis engine used
temperatureUnit | temperatureUnitEnum | required |  |  |
documentation
This attribute specifies the default temperature unit for the entire gbXML document, wherever the temperatureUnit simple type is used.
lengthUnit | lengthUnitEnum | required |  |  |
documentation
This attribute specifies the default length unit for the entire gbXML document, wherever the lengthUnit simple type is used.
areaUnit | areaUnitEnum | required |  |  |
documentation
This attribute specifies the default area unit for the entire gbXML document, wherever the areaUnit simple type is used.
volumeUnit | volumeUnitEnum | required |  |  |
documentation
This attribute specifies the default volume unit for the entire gbXML document, wherever the volumeUnit simple type is used.
useSIUnitsForResults | xsd:boolean | required |  |  |
documentation
Results will be given in SI or IP units. True = SI units which is the implied default. If False, results will be in english units.
source | <xsd:element name="gbXML"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="aecXML" minOccurs="0"/> <xsd:element ref="Campus"/> <xsd:element ref="LightingSystem" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="LightingControl" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Construction" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Layer" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Material" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="WindowType" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Schedule" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="WeekSchedule" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="DaySchedule" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Zone" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="AirLoop" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="HydronicLoop" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="IntEquip" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="ExtEquip" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Weather" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Meter" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Results" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="DocumentHistory" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID"/> <xsd:attribute name="engine"> <xsd:annotation> <xsd:documentation>Analysis engine used</xsd:documentation> </xsd:annotation> <xsd:simpleType> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="DOE2.1e"/> <xsd:enumeration value="DOE2.2"/> <xsd:enumeration value="EnergyPlus"/> </xsd:restriction> </xsd:simpleType> </xsd:attribute> <xsd:attribute name="temperatureUnit" type="temperatureUnitEnum" use="required"> <xsd:annotation> <xsd:documentation>This attribute specifies the default temperature unit for the entire gbXML document, wherever the temperatureUnit simple type is used.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="lengthUnit" type="lengthUnitEnum" use="required"> <xsd:annotation> <xsd:documentation>This attribute specifies the default length unit for the entire gbXML document, wherever the lengthUnit simple type is used.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="areaUnit" type="areaUnitEnum" use="required"> <xsd:annotation> <xsd:documentation>This attribute specifies the default area unit for the entire gbXML document, wherever the areaUnit simple type is used.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="volumeUnit" type="volumeUnitEnum" use="required"> <xsd:annotation> <xsd:documentation>This attribute specifies the default volume unit for the entire gbXML document, wherever the volumeUnit simple type is used.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="useSIUnitsForResults" type="xsd:boolean" use="required"> <xsd:annotation> <xsd:documentation>Results will be given in SI or IP units. True = SI units which is the implied default. If False, results will be in english units.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute gbXML/@id

type | xsd:ID
properties |
isRef | 0
source | <xsd:attribute name="id" type="xsd:ID"/>

attribute gbXML/@engine

type | restriction of xsd:NMTOKEN
properties |
isRef | 0
facets |
enumeration | DOE2.1e
enumeration | DOE2.2
enumeration | EnergyPlus
annotation |
documentation
Analysis engine used
source | <xsd:attribute name="engine"> <xsd:annotation> <xsd:documentation>Analysis engine used</xsd:documentation> </xsd:annotation> <xsd:simpleType> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="DOE2.1e"/> <xsd:enumeration value="DOE2.2"/> <xsd:enumeration value="EnergyPlus"/> </xsd:restriction> </xsd:simpleType> </xsd:attribute>

attribute gbXML/@temperatureUnit

type | temperatureUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | F
enumeration | C
enumeration | K
enumeration | R
annotation |
documentation
This attribute specifies the default temperature unit for the entire gbXML document, wherever the temperatureUnit simple type is used.
source | <xsd:attribute name="temperatureUnit" type="temperatureUnitEnum" use="required"> <xsd:annotation> <xsd:documentation>This attribute specifies the default temperature unit for the entire gbXML document, wherever the temperatureUnit simple type is used.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute gbXML/@lengthUnit

type | lengthUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Kilometers
enumeration | Meters
enumeration | Centimeters
enumeration | Millimeters
enumeration | Miles
enumeration | Yards
enumeration | Feet
enumeration | Inches
annotation |
documentation
This attribute specifies the default length unit for the entire gbXML document, wherever the lengthUnit simple type is used.
source | <xsd:attribute name="lengthUnit" type="lengthUnitEnum" use="required"> <xsd:annotation> <xsd:documentation>This attribute specifies the default length unit for the entire gbXML document, wherever the lengthUnit simple type is used.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute gbXML/@areaUnit

type | areaUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | SquareKilometers
enumeration | SquareMeters
enumeration | SquareCentimeters
enumeration | SquareMillimeters
enumeration | SquareMiles
enumeration | SquareYards
enumeration | SquareFeet
enumeration | SquareInches
annotation |
documentation
This attribute specifies the default area unit for the entire gbXML document, wherever the areaUnit simple type is used.
source | <xsd:attribute name="areaUnit" type="areaUnitEnum" use="required"> <xsd:annotation> <xsd:documentation>This attribute specifies the default area unit for the entire gbXML document, wherever the areaUnit simple type is used.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute gbXML/@volumeUnit

type | volumeUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | CubicKilometers
enumeration | CubicMeters
enumeration | CubicCentimeters
enumeration | CubicMillimeters
enumeration | CubicMiles
enumeration | CubicYards
enumeration | CubicFeet
enumeration | CubicInches
annotation |
documentation
This attribute specifies the default volume unit for the entire gbXML document, wherever the volumeUnit simple type is used.
source | <xsd:attribute name="volumeUnit" type="volumeUnitEnum" use="required"> <xsd:annotation> <xsd:documentation>This attribute specifies the default volume unit for the entire gbXML document, wherever the volumeUnit simple type is used.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute gbXML/@useSIUnitsForResults

type | xsd:boolean
properties |
isRef | 0
use | required
annotation |
documentation
Results will be given in SI or IP units. True = SI units which is the implied default. If False, results will be in english units.
source | <xsd:attribute name="useSIUnitsForResults" type="xsd:boolean" use="required"> <xsd:annotation> <xsd:documentation>Results will be given in SI or IP units. True = SI units which is the implied default. If False, results will be in english units.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element GeneralGeometry

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
elements | AirLoopEquipment ExtEquip HydronicLoopEquipment IntEquip Lighting LightingControl LightingSystem Transportation Vegetation
annotation |
documentation
This element has been left open for use with other geometry definitions, such as X3D or BLISXML.
source | <xsd:element name="GeneralGeometry"> <xsd:annotation> <xsd:documentation>This element has been left open for use with other geometry definitions, such as X3D or BLISXML.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:any namespace="##other" processContents="lax" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> </xsd:complexType> </xsd:element>

element Glare

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | ShadeControl
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | unitlessUnitEnum |  |  |  |
annotation |
documentation
Minimum amount of glare to trigger the shades to close
source | <xsd:element name="Glare"> <xsd:annotation> <xsd:documentation>Minimum amount of glare to trigger the shades to close</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Glare/@unit

type | unitlessUnitEnum
properties |
isRef | 0
facets |
enumeration | Percent
enumeration | Fraction
source | <xsd:attribute name="unit" type="unitlessUnitEnum"/>

element Glaze

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Transmittance Reflectance Emittance Thickness Conductivity Reference
used by |
element | WindowType
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
DOELibIdRef | xsd:string |  |  |  |
documentation
Use this attribute to reference objects in the DOE2 library
annotation |
documentation
Properties of one layer of a window
source | <xsd:element name="Glaze"> <xsd:annotation> <xsd:documentation>Properties of one layer of a window</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Transmittance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Reflectance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Emittance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Thickness" minOccurs="0"/> <xsd:element ref="Conductivity" minOccurs="0"/> <xsd:element ref="Reference" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Glaze/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Glaze/@DOELibIdRef

type | xsd:string
properties |
isRef | 0
annotation |
documentation
Use this attribute to reference objects in the DOE2 library
source | <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute>

element GlazeConductivity

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Opening
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | conductivityUnitEnum | required |  |  |
source | <xsd:element name="GlazeConductivity"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="conductivityUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute GlazeConductivity/@unit

type | conductivityUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | WPerCmC
enumeration | WPerMeterK
enumeration | BtuPerHourFtF
source | <xsd:attribute name="unit" type="conductivityUnitEnum" use="required"/>

element GlazeId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
attributes |
Name | Type | Use | Default | Fixed | annotation
glazeIdRef | xsd:IDREF | required |  |  |
documentation
ID indicating the type of glaze used
source | <xsd:element name="GlazeId"> <xsd:complexType> <xsd:attribute name="glazeIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID indicating the type of glaze used</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute GlazeId/@glazeIdRef

type | xsd:IDREF
properties |
isRef | 0
use | required
annotation |
documentation
ID indicating the type of glaze used
source | <xsd:attribute name="glazeIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID indicating the type of glaze used</xsd:documentation> </xsd:annotation> </xsd:attribute>

element GroundTemp

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | temperatureUnitEnum |  |  |  |
annotation |
documentation
Monthly ground temperatures, 12 values
source | <xsd:element name="GroundTemp"> <xsd:annotation> <xsd:documentation>Monthly ground temperatures, 12 values</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute GroundTemp/@unit

type | temperatureUnitEnum
properties |
isRef | 0
facets |
enumeration | F
enumeration | C
enumeration | K
enumeration | R
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element GroundTempValue

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
source | <xsd:element name="GroundTempValue" type="xsd:decimal"/>

element HDD

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Temperature HDDValue
used by |
element | Weather
annotation |
documentation
Heating degree days. HDD is calculated as the number of degrees a mean daily temperature is below a value (specified as the Temperature element), for each day. For example, if the mean temperature in a region drops to 64 degrees for four days during a year, the rest of the time staying above 65, and the Temperature element is set at 65, then HDD = 4.
source | <xsd:element name="HDD"> <xsd:annotation> <xsd:documentation>Heating degree days. HDD is calculated as the number of degrees a mean daily temperature is below a value (specified as the Temperature element), for each day. For example, if the mean temperature in a region drops to 64 degrees for four days during a year, the rest of the time staying above 65, and the Temperature element is set at 65, then HDD = 4.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Temperature"/> <xsd:element ref="HDDValue"/> </xsd:choice> </xsd:complexType> </xsd:element>

element HDDValue

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | HDD
source | <xsd:element name="HDDValue" type="xsd:decimal"/>

element Height

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Dimensions RectangularGeometry
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | lengthUnitEnum |  |  |  |
source | <xsd:element name="Height"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="lengthUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Height/@unit

type | lengthUnitEnum
properties |
isRef | 0
facets |
enumeration | Kilometers
enumeration | Meters
enumeration | Centimeters
enumeration | Millimeters
enumeration | Miles
enumeration | Yards
enumeration | Feet
enumeration | Inches
source | <xsd:attribute name="unit" type="lengthUnitEnum"/>

element HighLimit

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | IndoorAirQuality
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | unitlessSmallUnitEnum | required |  |  |
source | <xsd:element name="HighLimit"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessSmallUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute HighLimit/@unit

type | unitlessSmallUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Percent
enumeration | PartPerMillionByVolume
enumeration | milliGramsPerCubicMeter
source | <xsd:attribute name="unit" type="unitlessSmallUnitEnum" use="required"/>

element HighValue

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | OperationRange
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | conditioningUnitEnum | required |  |  |
source | <xsd:element name="HighValue"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="conditioningUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute HighValue/@unit

type | conditioningUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | kBtu
enumeration | Btu
enumeration | kW
enumeration | Tons
source | <xsd:attribute name="unit" type="conditioningUnitEnum" use="required"/>

element HorizontalSolar

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | ShadeControl
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | powerPerAreaUnitEnum | required |  |  |
annotation |
documentation
Amount of horizontal solar radiation striking the opening before a shade is closed.
source | <xsd:element name="HorizontalSolar"> <xsd:annotation> <xsd:documentation>Amount of horizontal solar radiation striking the opening before a shade is closed.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="powerPerAreaUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute HorizontalSolar/@unit

type | powerPerAreaUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | WattPerSquareMeter
enumeration | WattPerSquareFoot
source | <xsd:attribute name="unit" type="powerPerAreaUnitEnum" use="required"/>

element HOutside

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:float
properties |
content | complex
used by |
element | RTSParameters
attributes |
Name | Type | Use | Default | Fixed | annotation
hOutsideUnitTypeEnum | hOutsideUnitTypeEnum |  |  |  |
documentation
Used by the hOutsideUnitType attribute.
annotation |
documentation
h (Outside) is the combined coefficient of heat transfer by long-wave radiation and convection at outer surface, Btu/h-sf-F. See 2001 HoF Chapter 25 Table 1.
source | <xsd:element name="HOutside"> <xsd:annotation> <xsd:documentation>h (Outside) is the combined coefficient of heat transfer by long-wave radiation and convection at outer surface, Btu/h-sf-F. See 2001 HoF Chapter 25 Table 1.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:float"> <xsd:attribute name="hOutsideUnitTypeEnum" type="hOutsideUnitTypeEnum"> <xsd:annotation> <xsd:documentation>Used by the hOutsideUnitType attribute.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute HOutside/@hOutsideUnitTypeEnum

type | hOutsideUnitTypeEnum
properties |
isRef | 0
facets |
enumeration | BTUPerHourSquareFootDegreeF
enumeration | WattsPerSecondSquareMeterDegreeC
annotation |
documentation
Used by the hOutsideUnitType attribute.
source | <xsd:attribute name="hOutsideUnitTypeEnum" type="hOutsideUnitTypeEnum"> <xsd:annotation> <xsd:documentation>Used by the hOutsideUnitType attribute.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element HydronicLoop

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Cost Reference HydronicLoopEquipment FlowControl TemperatureControl
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | annotation
loopType | loopTypeEnum | required |  |  |
controlZoneIdRef | xsd:IDREF |  |  |  |
fluidType | fluidTypeEnum | required |  |  |
id | xsd:ID | required |  |  |
documentation
Only use this attribute for secondary loops to reference the primary loop.
annotation |
documentation
The HydronicLoop element represents the equipment serving one path of water, or other liquid
source | <xsd:element name="HydronicLoop"> <xsd:annotation> <xsd:documentation>The HydronicLoop element represents the equipment serving one path of water, or other liquid</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Cost" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Reference" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="HydronicLoopEquipment" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="FlowControl" minOccurs="0"/> <xsd:element ref="TemperatureControl" minOccurs="0"/> </xsd:choice> <xsd:attribute name="loopType" type="loopTypeEnum" use="required"/> <xsd:attribute name="controlZoneIdRef" type="xsd:IDREF"/> <xsd:attribute name="fluidType" type="fluidTypeEnum" use="required"/> <xsd:attribute name="id" type="xsd:ID" use="required"> <xsd:annotation> <xsd:documentation>Only use this attribute for secondary loops to reference the primary loop.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute HydronicLoop/@loopType

type | loopTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | PrimaryChilledWater
enumeration | SecondaryChilledWater
enumeration | HotWater
enumeration | CondenserWater
enumeration | DomesticHotWater
enumeration | WaterLoopHeatPump
enumeration | TwoPipe
enumeration | PotableWaterLoop
source | <xsd:attribute name="loopType" type="loopTypeEnum" use="required"/>

attribute HydronicLoop/@controlZoneIdRef

type | xsd:IDREF
properties |
isRef | 0
source | <xsd:attribute name="controlZoneIdRef" type="xsd:IDREF"/>

attribute HydronicLoop/@fluidType

type | fluidTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Water
enumeration | Brine
enumeration | Glycol
source | <xsd:attribute name="fluidType" type="fluidTypeEnum" use="required"/>

attribute HydronicLoop/@id

type | xsd:ID
properties |
isRef | 0
use | required
annotation |
documentation
Only use this attribute for secondary loops to reference the primary loop.
source | <xsd:attribute name="id" type="xsd:ID" use="required"> <xsd:annotation> <xsd:documentation>Only use this attribute for secondary loops to reference the primary loop.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element HydronicLoopEquipment

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Manufacturer Model OperationSchedule Temp HydronicLoopId RatedFlow MinFlow DeltaT DeltaP Power Capacity Efficiency Control Performance Cost Weight Life RefrigerantType Energy Age Reference CADObjectId GeneralGeometry ShellGeometry
used by |
element | HydronicLoop
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
equipmentType | hydronicEquipTypeEnum | required |  |  |
waterMeterIdRef | xsd:IDREF |  |  |  |
waterScheduleIdRef | xsd:IDREF |  |  |  |
primaryLoopId | xsd:IDREF |  |  |  |
annotation |
documentation
A piece of equipment serving a hydronic loop (most commonly a water loop). This is generalized to be able to contain any type of hydronic loop equipment.
source | <xsd:element name="HydronicLoopEquipment"> <xsd:annotation> <xsd:documentation>A piece of equipment serving a hydronic loop (most commonly a water loop). This is generalized to be able to contain any type of hydronic loop equipment.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Manufacturer" minOccurs="0"/> <xsd:element ref="Model" minOccurs="0"/> <xsd:element ref="OperationSchedule" minOccurs="0"/> <xsd:element ref="Temp" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="HydronicLoopId" minOccurs="0" maxOccurs="unbounded"> <xsd:annotation> <xsd:documentation>Use this element to point to another loop. For instance if this is a chiller and is a child of a chilled water loop, use this element to point at a cooling water loop.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="RatedFlow" minOccurs="0" maxOccurs="2"/> <xsd:element ref="MinFlow" minOccurs="0" maxOccurs="2"/> <xsd:element ref="DeltaT" minOccurs="0" maxOccurs="2"/> <xsd:element ref="DeltaP" minOccurs="0" maxOccurs="2"/> <xsd:element ref="Power" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Capacity" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Efficiency" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Control" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Performance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Cost" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Weight" minOccurs="0"/> <xsd:element ref="Life" minOccurs="0"/> <xsd:element ref="RefrigerantType" minOccurs="0"/> <xsd:element ref="Energy" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Age" minOccurs="0"/> <xsd:element ref="Reference" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="CADObjectId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="GeneralGeometry" minOccurs="0"/> <xsd:element ref="ShellGeometry" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="equipmentType" type="hydronicEquipTypeEnum" use="required"/> <xsd:attribute name="waterMeterIdRef" type="xsd:IDREF"/> <xsd:attribute name="waterScheduleIdRef" type="xsd:IDREF"/> <xsd:attribute name="primaryLoopId" type="xsd:IDREF"/> </xsd:complexType> </xsd:element>

attribute HydronicLoopEquipment/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute HydronicLoopEquipment/@equipmentType

type | hydronicEquipTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Chiller
enumeration | CoolingTower
enumeration | Condenser
enumeration | Boiler
enumeration | HeatExchanger
enumeration | Pump
enumeration | RadiantPanel
enumeration | HotWaterHeater
enumeration | SolarPanels
enumeration | Earth
enumeration | Pipe
enumeration | Storage
enumeration | Coil
source | <xsd:attribute name="equipmentType" type="hydronicEquipTypeEnum" use="required"/>

attribute HydronicLoopEquipment/@waterMeterIdRef

type | xsd:IDREF
properties |
isRef | 0
source | <xsd:attribute name="waterMeterIdRef" type="xsd:IDREF"/>

attribute HydronicLoopEquipment/@waterScheduleIdRef

type | xsd:IDREF
properties |
isRef | 0
source | <xsd:attribute name="waterScheduleIdRef" type="xsd:IDREF"/>

attribute HydronicLoopEquipment/@primaryLoopId

type | xsd:IDREF
properties |
isRef | 0
source | <xsd:attribute name="primaryLoopId" type="xsd:IDREF"/>

element HydronicLoopId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
elements | AirLoopEquipment HydronicLoopEquipment Space Zone
attributes |
Name | Type | Use | Default | Fixed | annotation
hydronicLoopIdRef | xsd:IDREF | required |  |  |
documentation
ID pointing to a hydronic loop
hydronicLoopType | loopTypeEnum | required |  |  |
documentation
Type of hydronic loop
source | <xsd:element name="HydronicLoopId"> <xsd:complexType> <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID pointing to a hydronic loop </xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="hydronicLoopType" type="loopTypeEnum" use="required"> <xsd:annotation> <xsd:documentation>Type of hydronic loop </xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute HydronicLoopId/@hydronicLoopIdRef

type | xsd:IDREF
properties |
isRef | 0
use | required
annotation |
documentation
ID pointing to a hydronic loop
source | <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID pointing to a hydronic loop </xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute HydronicLoopId/@hydronicLoopType

type | loopTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | PrimaryChilledWater
enumeration | SecondaryChilledWater
enumeration | HotWater
enumeration | CondenserWater
enumeration | DomesticHotWater
enumeration | WaterLoopHeatPump
enumeration | TwoPipe
enumeration | PotableWaterLoop
annotation |
documentation
Type of hydronic loop
source | <xsd:attribute name="hydronicLoopType" type="loopTypeEnum" use="required"> <xsd:annotation> <xsd:documentation>Type of hydronic loop </xsd:documentation> </xsd:annotation> </xsd:attribute>

element Illuminance

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | LightingControl
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | illuminanceUnitEnum | required |  |  |
source | <xsd:element name="Illuminance"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="illuminanceUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Illuminance/@unit

type | illuminanceUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Footcandles
source | <xsd:attribute name="unit" type="illuminanceUnitEnum" use="required"/>

element ImageTexture

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | Material
attributes |
Name | Type | Use | Default | Fixed | annotation
url | xsd:string | required |  |  |
documentation
Specifies location of the image. From X3D specification: The texture is read from the URL specified by the url field. When the url field contains no values, texturing is disabled. Browsers shall support the JPEG and PNG image file formats. In addition, browsers may support other image formats (e.g. CGM) which can be rendered into a 2D image. Support for the GIF format is also recommended (including transparency).
repeatS | xsd:boolean | required |  |  |
documentation
From X3D specification: If repeatS is TRUE, the texture map is repeated outside the [0.0, 1.0] texture coordinate range in the S direction so that it fills the shape. If repeatS is FALSE, the texture coordinates are clamped in the S direction to lie within the [0.0, 1.0] range.
repeatT | xsd:boolean | required |  |  |
documentation
From X3D specification: If repeatT is TRUE, the texture map is repeated outside the [0.0, 1.0] texture coordinate range in the T direction so that it fills the shape. If repeatT is FALSE, the texture coordinates are clamped in the T direction to lie within the [0.0, 1.0] range.
annotation |
documentation
This is an X3D element to map a texture to this material. From X3D specification: The ImageTexture node defines a texture map by specifying an image file and general parameters for mapping to geometry. Texture maps are defined in a 2D coordinate system (s, t) that ranges from [0.0, 1.0] in both directions. The bottom edge of the image corresponds to the S-axis of the texture map, and left edge of the image corresponds to the T-axis of the texture map. The lower-left pixel of the image corresponds to s=0, t=0, and the top-right pixel of the image corresponds to s=1, t=1. <!--When fixed: add type="x3d:ImageTexture"-->
source | <xsd:element name="ImageTexture"> <xsd:annotation> <xsd:documentation>This is an X3D element to map a texture to this material. From X3D specification: The ImageTexture node defines a texture map by specifying an image file and general parameters for mapping to geometry. Texture maps are defined in a 2D coordinate system (s, t) that ranges from [0.0, 1.0] in both directions. The bottom edge of the image corresponds to the S-axis of the texture map, and left edge of the image corresponds to the T-axis of the texture map. The lower-left pixel of the image corresponds to s=0, t=0, and the top-right pixel of the image corresponds to s=1, t=1. <!--When fixed: add type="x3d:ImageTexture"--> </xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:attribute name="url" type="xsd:string" use="required"> <xsd:annotation> <xsd:documentation>Specifies location of the image. From X3D specification: The texture is read from the URL specified by the url field. When the url field contains no values, texturing is disabled. Browsers shall support the JPEG and PNG image file formats. In addition, browsers may support other image formats (e.g. CGM) which can be rendered into a 2D image. Support for the GIF format is also recommended (including transparency). </xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="repeatS" type="xsd:boolean" use="required"> <xsd:annotation> <xsd:documentation>From X3D specification: If repeatS is TRUE, the texture map is repeated outside the [0.0, 1.0] texture coordinate range in the S direction so that it fills the shape. If repeatS is FALSE, the texture coordinates are clamped in the S direction to lie within the [0.0, 1.0] range. </xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="repeatT" type="xsd:boolean" use="required"> <xsd:annotation> <xsd:documentation>From X3D specification: If repeatT is TRUE, the texture map is repeated outside the [0.0, 1.0] texture coordinate range in the T direction so that it fills the shape. If repeatT is FALSE, the texture coordinates are clamped in the T direction to lie within the [0.0, 1.0] range. </xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute ImageTexture/@url

type | xsd:string
properties |
isRef | 0
use | required
annotation |
documentation
Specifies location of the image. From X3D specification: The texture is read from the URL specified by the url field. When the url field contains no values, texturing is disabled. Browsers shall support the JPEG and PNG image file formats. In addition, browsers may support other image formats (e.g. CGM) which can be rendered into a 2D image. Support for the GIF format is also recommended (including transparency).
source | <xsd:attribute name="url" type="xsd:string" use="required"> <xsd:annotation> <xsd:documentation>Specifies location of the image. From X3D specification: The texture is read from the URL specified by the url field. When the url field contains no values, texturing is disabled. Browsers shall support the JPEG and PNG image file formats. In addition, browsers may support other image formats (e.g. CGM) which can be rendered into a 2D image. Support for the GIF format is also recommended (including transparency). </xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute ImageTexture/@repeatS

type | xsd:boolean
properties |
isRef | 0
use | required
annotation |
documentation
From X3D specification: If repeatS is TRUE, the texture map is repeated outside the [0.0, 1.0] texture coordinate range in the S direction so that it fills the shape. If repeatS is FALSE, the texture coordinates are clamped in the S direction to lie within the [0.0, 1.0] range.
source | <xsd:attribute name="repeatS" type="xsd:boolean" use="required"> <xsd:annotation> <xsd:documentation>From X3D specification: If repeatS is TRUE, the texture map is repeated outside the [0.0, 1.0] texture coordinate range in the S direction so that it fills the shape. If repeatS is FALSE, the texture coordinates are clamped in the S direction to lie within the [0.0, 1.0] range. </xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute ImageTexture/@repeatT

type | xsd:boolean
properties |
isRef | 0
use | required
annotation |
documentation
From X3D specification: If repeatT is TRUE, the texture map is repeated outside the [0.0, 1.0] texture coordinate range in the T direction so that it fills the shape. If repeatT is FALSE, the texture coordinates are clamped in the T direction to lie within the [0.0, 1.0] range.
source | <xsd:attribute name="repeatT" type="xsd:boolean" use="required"> <xsd:annotation> <xsd:documentation>From X3D specification: If repeatT is TRUE, the texture map is repeated outside the [0.0, 1.0] texture coordinate range in the T direction so that it fills the shape. If repeatT is FALSE, the texture coordinates are clamped in the T direction to lie within the [0.0, 1.0] range. </xsd:documentation> </xsd:annotation> </xsd:attribute>

element IndependantValue

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Data
annotation |
documentation
Value of the independent variable for this data point
source | <xsd:element name="IndependantValue" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Value of the independent variable for this data point</xsd:documentation> </xsd:annotation> </xsd:element>

element IndepentantVariable

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description
used by |
elements | Equation PointData
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | xsd:string | required |  |  |
dataType | xsd:string | required |  |  |
source | <xsd:element name="IndepentantVariable"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> </xsd:choice> <xsd:attribute name="unit" type="xsd:string" use="required"/> <xsd:attribute name="dataType" type="xsd:string" use="required"/> </xsd:complexType> </xsd:element>

attribute IndepentantVariable/@unit

type | xsd:string
properties |
isRef | 0
use | required
source | <xsd:attribute name="unit" type="xsd:string" use="required"/>

attribute IndepentantVariable/@dataType

type | xsd:string
properties |
isRef | 0
use | required
source | <xsd:attribute name="dataType" type="xsd:string" use="required"/>

element IndoorAirQuality

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | EmissionRate SinkRate HighLimit
used by |
elements | ExtEquip IntEquip Material Zone
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
scheduleIdRef | xsd:IDREF |  |  |  |
documentation
ID for the schedule of transmittance of a shading surface
source | <xsd:element name="IndoorAirQuality"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="EmissionRate" minOccurs="0"/> <xsd:element ref="SinkRate" minOccurs="0"/> <xsd:element ref="HighLimit" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute IndoorAirQuality/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute IndoorAirQuality/@scheduleIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID for the schedule of transmittance of a shading surface
source | <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute>

element InfiltrationFlow

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | BlowerDoorValue Reference
used by |
elements | Building Space
attributes |
Name | Type | Use | Default | Fixed | annotation
type | infiltrationTypeEnum |  |  |  |
annotation |
documentation
Flow of air through building envelope
source | <xsd:element name="InfiltrationFlow"> <xsd:annotation> <xsd:documentation>Flow of air through building envelope</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="BlowerDoorValue" minOccurs="0"/> <xsd:element ref="Reference" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="type" type="infiltrationTypeEnum"/> </xsd:complexType> </xsd:element>

attribute InfiltrationFlow/@type

type | infiltrationTypeEnum
properties |
isRef | 0
facets |
enumeration | Loose
enumeration | Average
enumeration | Tight
source | <xsd:attribute name="type" type="infiltrationTypeEnum"/>

element InputWatts

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | LightingSystem
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | powerUnitEnum | required |  |  |
source | <xsd:element name="InputWatts"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="powerUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute InputWatts/@unit

type | powerUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Watt
enumeration | Kilowatt
enumeration | Horsepower
enumeration | KilogramForceMeterPerSecond
enumeration | BtuPerSecond
enumeration | FootPoundForcePerSecond
enumeration | KilocaloriesPerSecond
enumeration | BtuPerHour
source | <xsd:attribute name="unit" type="powerUnitEnum" use="required"/>

element InsideAirFilmResistance

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Layer
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | resistanceUnitEnum | required |  |  |
annotation |
documentation
Thermal resistance of the internal air film in a layer
source | <xsd:element name="InsideAirFilmResistance"> <xsd:annotation> <xsd:documentation>Thermal resistance of the internal air film in a layer</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="resistanceUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute InsideAirFilmResistance/@unit

type | resistanceUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | SquareMeterKPerW
enumeration | HrSquareFtFPerBTU
source | <xsd:attribute name="unit" type="resistanceUnitEnum" use="required"/>

element IntEquip

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Manufacturer Model ElecLoad FuelLoad LatentLoad Efficiency Performance Cost WasteWaterHREff WaterUsePerCycle RatedFlow Power CyclesPerWeek Energy GeneralGeometry ShellGeometry IndoorAirQuality Age Reference CADObjectId
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
scheduleIdRef | xsd:IDREF |  |  |  |
documentation
ID for the schedule of transmittance of a shading surface
waterTempScheduleIdRef | xsd:IDREF |  |  |  |
hydronicLoopIdRef | xsd:IDREF |  |  |  |
documentation
ID pointing to a hydronic loop
waterScheduleIdRef | xsd:IDREF |  |  |  |
waterMeterIdRef | xsd:IDREF |  |  |  |
type | intEquipTypeEnum | required |  |  |
airLoopIdRef | xsd:IDREF |  |  |  |
documentation
ID pointing to an air loop
annotation |
documentation
Interior equipment. This is generalized to be able to contain any type of internal equipment.
source | <xsd:element name="IntEquip"> <xsd:annotation> <xsd:documentation>Interior equipment. This is generalized to be able to contain any type of internal equipment.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Manufacturer" minOccurs="0"/> <xsd:element ref="Model" minOccurs="0"/> <xsd:element ref="ElecLoad" minOccurs="0"/> <xsd:element ref="FuelLoad" minOccurs="0"/> <xsd:element ref="LatentLoad" minOccurs="0"/> <xsd:element ref="Efficiency" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Performance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Cost" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="WasteWaterHREff" minOccurs="0"/> <xsd:element ref="WaterUsePerCycle" minOccurs="0"/> <xsd:element ref="RatedFlow" minOccurs="0"/> <xsd:element ref="Power" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="CyclesPerWeek" minOccurs="0"/> <xsd:element ref="Energy" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="GeneralGeometry" minOccurs="0"/> <xsd:element ref="ShellGeometry" minOccurs="0"/> <xsd:element ref="IndoorAirQuality" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Age" minOccurs="0"/> <xsd:element ref="Reference" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="CADObjectId" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="waterTempScheduleIdRef" type="xsd:IDREF"/> <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID pointing to a hydronic loop </xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="waterScheduleIdRef" type="xsd:IDREF"/> <xsd:attribute name="waterMeterIdRef" type="xsd:IDREF"/> <xsd:attribute name="type" type="intEquipTypeEnum" use="required"/> <xsd:attribute name="airLoopIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID pointing to an air loop</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute IntEquip/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute IntEquip/@scheduleIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID for the schedule of transmittance of a shading surface
source | <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute IntEquip/@waterTempScheduleIdRef

type | xsd:IDREF
properties |
isRef | 0
source | <xsd:attribute name="waterTempScheduleIdRef" type="xsd:IDREF"/>

attribute IntEquip/@hydronicLoopIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID pointing to a hydronic loop
source | <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID pointing to a hydronic loop </xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute IntEquip/@waterScheduleIdRef

type | xsd:IDREF
properties |
isRef | 0
source | <xsd:attribute name="waterScheduleIdRef" type="xsd:IDREF"/>

attribute IntEquip/@waterMeterIdRef

type | xsd:IDREF
properties |
isRef | 0
source | <xsd:attribute name="waterMeterIdRef" type="xsd:IDREF"/>

attribute IntEquip/@type

type | intEquipTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | GeneralPlugload
enumeration | Computer
enumeration | Copier
enumeration | Refrigerator
enumeration | Stove
enumeration | Cooktop
enumeration | Fryer
enumeration | Freezer
enumeration | ClothesDryer
enumeration | ClothesWasher
enumeration | Dishwasher
enumeration | TV
enumeration | VCR
enumeration | Microwave
enumeration | Fan
enumeration | AudioEquip
enumeration | MiscEquip
enumeration | Toilet
enumeration | Urinal
enumeration | Shower
enumeration | Sink
enumeration | Pool
enumeration | HotTub
enumeration | Sauna
enumeration | BatteryCharger
enumeration | Furnace
enumeration | IndustrialEquip
enumeration | Printer
enumeration | Vending
enumeration | Elevator
enumeration | Escalator
enumeration | GeneralLaundryEquip
enumeration | GeneralKitchenEquip
enumeration | GeneralMedicalEquip
enumeration | GeneralOfficeEquip
enumeration | GeneralEntertainmentEquip
enumeration | GeneralRefrigerationEquip
enumeration | GeneralFitnessEquip
enumeration | GeneralVideoEquip
enumeration | GeneralToilet
source | <xsd:attribute name="type" type="intEquipTypeEnum" use="required"/>

attribute IntEquip/@airLoopIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID pointing to an air loop
source | <xsd:attribute name="airLoopIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID pointing to an air loop</xsd:documentation> </xsd:annotation> </xsd:attribute>

element IntEquipId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
elements | Building Space
attributes |
Name | Type | Use | Default | Fixed | annotation
intEquipIdRef | xsd:IDREF | required |  |  |
documentation
ID pointing at an interior equipment object
source | <xsd:element name="IntEquipId"> <xsd:complexType> <xsd:attribute name="intEquipIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID pointing at an interior equipment object</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute IntEquipId/@intEquipIdRef

type | xsd:IDREF
properties |
isRef | 0
use | required
annotation |
documentation
ID pointing at an interior equipment object
source | <xsd:attribute name="intEquipIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID pointing at an interior equipment object</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Lamp

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | LightingSystem
annotation |
documentation
Type of lamp used
source | <xsd:element name="Lamp" type="xsd:string"> <xsd:annotation> <xsd:documentation>Type of lamp used</xsd:documentation> </xsd:annotation> </xsd:element>

element LastName

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | PersonInfo
source | <xsd:element name="LastName" type="xsd:string"/>

element LatentLoad

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | ExtEquip IntEquip
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | loadUnitEnum | required |  |  |
source | <xsd:element name="LatentLoad"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="loadUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute LatentLoad/@unit

type | loadUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | BtuPerHour
enumeration | Watt
source | <xsd:attribute name="unit" type="loadUnitEnum" use="required"/>

element Latitude

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Location
annotation |
documentation
Degrees east of Greenwich, in decimal degrees. Locations west of Greenwich are negative.
source | <xsd:element name="Latitude" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Degrees east of Greenwich, in decimal degrees. Locations west of Greenwich are negative.</xsd:documentation> </xsd:annotation> </xsd:element>

element Layer

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Cost InsideAirFilmResistance MaterialId
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
DOELibIdRef | xsd:string |  |  |  |
documentation
Use this attribute to reference objects in the DOE2 library
annotation |
documentation
A Layer is a combination of one of more materials
source | <xsd:element name="Layer"> <xsd:annotation> <xsd:documentation>A Layer is a combination of one of more materials</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Cost" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="InsideAirFilmResistance" minOccurs="0"/> <xsd:element ref="MaterialId" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Layer/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Layer/@DOELibIdRef

type | xsd:string
properties |
isRef | 0
annotation |
documentation
Use this attribute to reference objects in the DOE2 library
source | <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute>

element LayerId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | Construction
attributes |
Name | Type | Use | Default | Fixed | annotation
layerIdRef | xsd:IDREF | required |  |  |
documentation
ID identifying a layer in this construction. Multiple layers in Constructions are in order from outside to inside.
source | <xsd:element name="LayerId"> <xsd:complexType> <xsd:attribute name="layerIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID identifying a layer in this construction. Multiple layers in Constructions are in order from outside to inside.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute LayerId/@layerIdRef

type | xsd:IDREF
properties |
isRef | 0
use | required
annotation |
documentation
ID identifying a layer in this construction. Multiple layers in Constructions are in order from outside to inside.
source | <xsd:attribute name="layerIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID identifying a layer in this construction. Multiple layers in Constructions are in order from outside to inside.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Length

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Dimensions
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | lengthUnitEnum |  |  |  |
source | <xsd:element name="Length"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="lengthUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Length/@unit

type | lengthUnitEnum
properties |
isRef | 0
facets |
enumeration | Kilometers
enumeration | Meters
enumeration | Centimeters
enumeration | Millimeters
enumeration | Miles
enumeration | Yards
enumeration | Feet
enumeration | Inches
source | <xsd:attribute name="unit" type="lengthUnitEnum"/>

element Level

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | BuildingStorey
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | lengthUnitEnum |  |  |  |
annotation |
documentation
Building storey Local Placement Z coordinate.
source | <xsd:element name="Level"> <xsd:annotation> <xsd:documentation>Building storey Local Placement Z coordinate.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="lengthUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Level/@unit

type | lengthUnitEnum
properties |
isRef | 0
facets |
enumeration | Kilometers
enumeration | Meters
enumeration | Centimeters
enumeration | Millimeters
enumeration | Miles
enumeration | Yards
enumeration | Feet
enumeration | Inches
source | <xsd:attribute name="unit" type="lengthUnitEnum"/>

element Life

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | AirLoopEquipment Campus HydronicLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | lifeUnitEnum | required |  |  |
source | <xsd:element name="Life"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="lifeUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Life/@unit

type | lifeUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Months
enumeration | Years
enumeration | Cycles
enumeration | MillionCycles
source | <xsd:attribute name="unit" type="lifeUnitEnum" use="required"/>

element LightControlId

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:string
properties |
content | complex
used by |
element | Campus
attributes |
Name | Type | Use | Default | Fixed | annotation
scheduleIdRef | xsd:IDREF |  |  |  |
documentation
ID for the schedule of transmittance of a shading surface
source | <xsd:element name="LightControlId"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:string"> <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute LightControlId/@scheduleIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID for the schedule of transmittance of a shading surface
source | <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute>

element LightId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
attributes |
Name | Type | Use | Default | Fixed | annotation
lightIdRef | xsd:IDREF | required |  |  |
documentation
Identifier pointing at a light object
source | <xsd:element name="LightId"> <xsd:complexType> <xsd:attribute name="lightIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>Identifier pointing at a light object</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute LightId/@lightIdRef

type | xsd:IDREF
properties |
isRef | 0
use | required
annotation |
documentation
Identifier pointing at a light object
source | <xsd:attribute name="lightIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>Identifier pointing at a light object</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Lighting

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | GeneralGeometry ShellGeometry
used by |
elements | Building Campus Space
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
lightingSystemIdRef | xsd:IDREF |  |  |  |
lightingControlIdRef | xsd:IDREF |  |  |  |
meterIdRef | xsd:IDREF |  |  |  |
documentation
ID for a resource meter
source | <xsd:element name="Lighting"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="GeneralGeometry" minOccurs="0"/> <xsd:element ref="ShellGeometry" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="lightingSystemIdRef" type="xsd:IDREF"/> <xsd:attribute name="lightingControlIdRef" type="xsd:IDREF"/> <xsd:attribute name="meterIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for a resource meter</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Lighting/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Lighting/@lightingSystemIdRef

type | xsd:IDREF
properties |
isRef | 0
source | <xsd:attribute name="lightingSystemIdRef" type="xsd:IDREF"/>

attribute Lighting/@lightingControlIdRef

type | xsd:IDREF
properties |
isRef | 0
source | <xsd:attribute name="lightingControlIdRef" type="xsd:IDREF"/>

attribute Lighting/@meterIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID for a resource meter
source | <xsd:attribute name="meterIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for a resource meter</xsd:documentation> </xsd:annotation> </xsd:attribute>

element LightingControl

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | GeneralGeometry ShellGeometry Illuminance CartesianPoint MinPowerFrac MinLightFrac PercentAreaDaylitControled
used by |
elements | gbXML Space
attributes |
Name | Type | Use | Default | Fixed | annotation
type | lightControlTypeEnum | required |  |  |
id | xsd:ID | required |  |  |
lightingSystemIdRef | xsd:IDREF |  |  |  |
source | <xsd:element name="LightingControl"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="GeneralGeometry" minOccurs="0"/> <xsd:element ref="ShellGeometry" minOccurs="0"/> <xsd:element ref="Illuminance" minOccurs="0"> <xsd:annotation> <xsd:documentation>Illuminance level that the lights are maintained if daylighting controls present (lightControlTypeEnum not equal to on off).</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="CartesianPoint" minOccurs="0"> <xsd:annotation> <xsd:documentation>Location where Illuminance value is specified.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="MinPowerFrac" minOccurs="0"/> <xsd:element ref="MinLightFrac" minOccurs="0"/> <xsd:element ref="PercentAreaDaylitControled" minOccurs="0"/> </xsd:choice> <xsd:attribute name="type" type="lightControlTypeEnum" use="required"/> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="lightingSystemIdRef" type="xsd:IDREF"/> </xsd:complexType> </xsd:element>

attribute LightingControl/@type

type | lightControlTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Continuous
enumeration | OnOff
enumeration | Stepped2
enumeration | Stepped3
enumeration | Stepped4
enumeration | Stepped5
enumeration | Stepped6
enumeration | Stepped7
enumeration | Stepped8
enumeration | Stepped9
enumeration | Stepped10
enumeration | Stepped11
enumeration | Stepped12
enumeration | Stepped13
enumeration | Stepped14
enumeration | Stepped15
enumeration | Stepped16
enumeration | Stepped17
enumeration | Stepped18
enumeration | Stepped19
enumeration | Stepped20
enumeration | ContinuousOff
enumeration | MotionSensor
enumeration | Photocell
source | <xsd:attribute name="type" type="lightControlTypeEnum" use="required"/>

attribute LightingControl/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute LightingControl/@lightingSystemIdRef

type | xsd:IDREF
properties |
isRef | 0
source | <xsd:attribute name="lightingSystemIdRef" type="xsd:IDREF"/>

element LightingSystem

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Manufacturer NumberOfLamps LumensPerLamp Dimensions InputWatts Ballast Lamp Luminaire CoefficientOfUtilization Cost GeneralGeometry ShellGeometry Reference
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
source | <xsd:element name="LightingSystem"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Manufacturer" minOccurs="0"/> <xsd:element ref="NumberOfLamps" minOccurs="0"/> <xsd:element ref="LumensPerLamp" minOccurs="0"/> <xsd:element ref="Dimensions" minOccurs="0"/> <xsd:element ref="InputWatts" minOccurs="0"/> <xsd:element ref="Ballast" minOccurs="0"/> <xsd:element ref="Lamp" maxOccurs="unbounded"/> <xsd:element ref="Luminaire" minOccurs="0"/> <xsd:element ref="CoefficientOfUtilization" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Cost" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="GeneralGeometry" minOccurs="0"/> <xsd:element ref="ShellGeometry" minOccurs="0"/> <xsd:element ref="Reference" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> </xsd:complexType> </xsd:element>

attribute LightingSystem/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

element LightPowerPerArea

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Space
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | powerPerAreaUnitEnum | required |  |  |
annotation |
documentation
Amount of power used by lighting in a given area
source | <xsd:element name="LightPowerPerArea"> <xsd:annotation> <xsd:documentation>Amount of power used by lighting in a given area</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="powerPerAreaUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute LightPowerPerArea/@unit

type | powerPerAreaUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | WattPerSquareMeter
enumeration | WattPerSquareFoot
source | <xsd:attribute name="unit" type="powerPerAreaUnitEnum" use="required"/>

element LoadCalcInputParameters

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | RTSParameters CLTDParameters ManualJ8Parameters FloorSlabHeatLossCoefficient
used by |
element | Construction
source | <xsd:element name="LoadCalcInputParameters"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="RTSParameters" minOccurs="0"/> <xsd:element ref="CLTDParameters" minOccurs="0"/> <xsd:element ref="ManualJ8Parameters" minOccurs="0"/> <xsd:element ref="FloorSlabHeatLossCoefficient" minOccurs="0"/> </xsd:choice> </xsd:complexType> </xsd:element>

element Location

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | StationId Name Description ZipcodeOrPostalCode Longitude Latitude Elevation CADModelAzimuth
used by |
element | Campus
annotation |
documentation
The Location element describes the location of the global origin for this campus. This element can be used in a general sense by using the Name and Description elements for a physical address or landmark, or Location can be made precise by specifying the Elevation, Longitude, and Latitude of the origin.
source | <xsd:element name="Location"> <xsd:annotation> <xsd:documentation>The Location element describes the location of the global origin for this campus. This element can be used in a general sense by using the Name and Description elements for a physical address or landmark, or Location can be made precise by specifying the Elevation, Longitude, and Latitude of the origin.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="StationId" minOccurs="0"/> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="ZipcodeOrPostalCode"/> <xsd:element ref="Longitude" minOccurs="0"/> <xsd:element ref="Latitude" minOccurs="0"/> <xsd:element ref="Elevation" minOccurs="0"/> <xsd:element ref="CADModelAzimuth" minOccurs="0"/> </xsd:choice> </xsd:complexType> </xsd:element>

element Longitude

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Location
annotation |
documentation
Degrees north of the equator, in decimal degrees. Locations south of the equator are negative.
source | <xsd:element name="Longitude" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Degrees north of the equator, in decimal degrees. Locations south of the equator are negative.</xsd:documentation> </xsd:annotation> </xsd:element>

element LowValue

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | OperationRange
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | conditioningUnitEnum | required |  |  |
source | <xsd:element name="LowValue"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="conditioningUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute LowValue/@unit

type | conditioningUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | kBtu
enumeration | Btu
enumeration | kW
enumeration | Tons
source | <xsd:attribute name="unit" type="conditioningUnitEnum" use="required"/>

element LumensPerLamp

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | LightingSystem
source | <xsd:element name="LumensPerLamp" type="xsd:decimal"/>

element Luminaire

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | LightingSystem
annotation |
documentation
Type of luminaire used
source | <xsd:element name="Luminaire" type="xsd:string"> <xsd:annotation> <xsd:documentation>Type of luminaire used</xsd:documentation> </xsd:annotation> </xsd:element>

element ManualJ8Parameters

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | LoadCalcInputParameters
attributes |
Name | Type | Use | Default | Fixed | annotation
wallGroupManualJ | wallGroupManualJEnum |  |  |  |
documentation
Specifies the group code for the wall, which determines how quickly the wall delivers heat into the space. See Table 4C, page T4C-1 ACCA Manual J Eighth Edition.
roofCLTDIndex | roofCLTDIndexEnum |  |  |  |
documentation
Specifies the array of CLTD values to use for the roof, which determines how quickly the roof delivers heat into the space. See Table 4A page T4A-18 and following, ACCA Manual J Eighth Edition.
floorIsRadiant | xsd:boolean |  |  |  |
documentation
Specifies whether or not to use a higher heating temperature difference value in calculating the heating loss for a floor (25 degrees F higher value is used in formula if floor is radiant). See Figure A5-5, page A5-8, ACCA Manual J Eighth Edition.
floorCrawlSpaceWallUValue | xsd:float |  |  |  |
documentation
Specifies the u-value of the crawl space wall that is associated with the floor, which affects both the heating and cooling load. See Figure A5-5, page A5-8, and Figure A5-17, page A5-16, ACCA Manual J Eighth Edition.
floorCrawlSpaceIsSealed | xsd:boolean |  |  |  |
documentation
Specifies whether or not the crawl space wall associated with this floor is well sealed from the outdoor air, which affects both the heating and cooling loads. See Figure A5-5, page A5-8, and Figure A5-17 page A5-16, ACCA Manual J Eighth Edition.
floorCategory | floorCategoryEnum |  |  |  |
documentation
Specifies the type of floor being considered, which affects both the heating and the cooling loads. See Table 4A, pages T4A-27 and following, ACCA Manual J Eighth Edition.
annotation |
documentation
Parameters required by the ACCA Manual J Eighth Edition load calculation method. Ignore this element and all elements under it if you are not planning to use that method.
source | <xsd:element name="ManualJ8Parameters"> <xsd:annotation> <xsd:documentation>Parameters required by the ACCA Manual J Eighth Edition load calculation method. Ignore this element and all elements under it if you are not planning to use that method.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:attribute name="wallGroupManualJ" type="wallGroupManualJEnum"> <xsd:annotation> <xsd:documentation>Specifies the group code for the wall, which determines how quickly the wall delivers heat into the space. See Table 4C, page T4C-1 ACCA Manual J Eighth Edition.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="roofCLTDIndex" type="roofCLTDIndexEnum"> <xsd:annotation> <xsd:documentation>Specifies the array of CLTD values to use for the roof, which determines how quickly the roof delivers heat into the space. See Table 4A page T4A-18 and following, ACCA Manual J Eighth Edition.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="floorIsRadiant" type="xsd:boolean"> <xsd:annotation> <xsd:documentation>Specifies whether or not to use a higher heating temperature difference value in calculating the heating loss for a floor (25 degrees F higher value is used in formula if floor is radiant). See Figure A5-5, page A5-8, ACCA Manual J Eighth Edition.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="floorCrawlSpaceWallUValue" type="xsd:float"> <xsd:annotation> <xsd:documentation>Specifies the u-value of the crawl space wall that is associated with the floor, which affects both the heating and cooling load. See Figure A5-5, page A5-8, and Figure A5-17, page A5-16, ACCA Manual J Eighth Edition.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="floorCrawlSpaceIsSealed" type="xsd:boolean"> <xsd:annotation> <xsd:documentation>Specifies whether or not the crawl space wall associated with this floor is well sealed from the outdoor air, which affects both the heating and cooling loads. See Figure A5-5, page A5-8, and Figure A5-17 page A5-16, ACCA Manual J Eighth Edition.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="floorCategory" type="floorCategoryEnum"> <xsd:annotation> <xsd:documentation>Specifies the type of floor being considered, which affects both the heating and the cooling loads. See Table 4A, pages T4A-27 and following, ACCA Manual J Eighth Edition.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute ManualJ8Parameters/@wallGroupManualJ

type | wallGroupManualJEnum
properties |
isRef | 0
facets |
enumeration | A
enumeration | B
enumeration | C
enumeration | D
enumeration | E
enumeration | F
enumeration | G
enumeration | H
enumeration | I
enumeration | J
enumeration | K
annotation |
documentation
Specifies the group code for the wall, which determines how quickly the wall delivers heat into the space. See Table 4C, page T4C-1 ACCA Manual J Eighth Edition.
source | <xsd:attribute name="wallGroupManualJ" type="wallGroupManualJEnum"> <xsd:annotation> <xsd:documentation>Specifies the group code for the wall, which determines how quickly the wall delivers heat into the space. See Table 4C, page T4C-1 ACCA Manual J Eighth Edition.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute ManualJ8Parameters/@roofCLTDIndex

type | roofCLTDIndexEnum
properties |
isRef | 0
facets |
enumeration | 1
enumeration | 2
enumeration | 3
enumeration | 4
enumeration | 5
enumeration | 6
enumeration | 7
enumeration | 8
enumeration | 9
enumeration | 10
enumeration | 11
enumeration | 12
enumeration | 13
enumeration | 14
enumeration | 15
enumeration | 16
enumeration | 17
enumeration | 18
enumeration | 19
enumeration | 20
enumeration | 21
enumeration | 22
enumeration | 23
enumeration | 24
enumeration | 25
enumeration | 26
enumeration | 27
enumeration | 28
enumeration | 29
enumeration | 30
enumeration | 31
enumeration | 32
enumeration | 33
enumeration | 34
enumeration | 35
enumeration | 36
enumeration | 37
enumeration | 38
enumeration | 39
enumeration | 40
enumeration | 41
enumeration | 42
enumeration | 43
enumeration | 44
enumeration | 45
enumeration | 46
enumeration | 47
annotation |
documentation
Specifies the array of CLTD values to use for the roof, which determines how quickly the roof delivers heat into the space. See Table 4A page T4A-18 and following, ACCA Manual J Eighth Edition.
source | <xsd:attribute name="roofCLTDIndex" type="roofCLTDIndexEnum"> <xsd:annotation> <xsd:documentation>Specifies the array of CLTD values to use for the roof, which determines how quickly the roof delivers heat into the space. See Table 4A page T4A-18 and following, ACCA Manual J Eighth Edition.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute ManualJ8Parameters/@floorIsRadiant

type | xsd:boolean
properties |
isRef | 0
annotation |
documentation
Specifies whether or not to use a higher heating temperature difference value in calculating the heating loss for a floor (25 degrees F higher value is used in formula if floor is radiant). See Figure A5-5, page A5-8, ACCA Manual J Eighth Edition.
source | <xsd:attribute name="floorIsRadiant" type="xsd:boolean"> <xsd:annotation> <xsd:documentation>Specifies whether or not to use a higher heating temperature difference value in calculating the heating loss for a floor (25 degrees F higher value is used in formula if floor is radiant). See Figure A5-5, page A5-8, ACCA Manual J Eighth Edition.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute ManualJ8Parameters/@floorCrawlSpaceWallUValue

type | xsd:float
properties |
isRef | 0
annotation |
documentation
Specifies the u-value of the crawl space wall that is associated with the floor, which affects both the heating and cooling load. See Figure A5-5, page A5-8, and Figure A5-17, page A5-16, ACCA Manual J Eighth Edition.
source | <xsd:attribute name="floorCrawlSpaceWallUValue" type="xsd:float"> <xsd:annotation> <xsd:documentation>Specifies the u-value of the crawl space wall that is associated with the floor, which affects both the heating and cooling load. See Figure A5-5, page A5-8, and Figure A5-17, page A5-16, ACCA Manual J Eighth Edition.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute ManualJ8Parameters/@floorCrawlSpaceIsSealed

type | xsd:boolean
properties |
isRef | 0
annotation |
documentation
Specifies whether or not the crawl space wall associated with this floor is well sealed from the outdoor air, which affects both the heating and cooling loads. See Figure A5-5, page A5-8, and Figure A5-17 page A5-16, ACCA Manual J Eighth Edition.
source | <xsd:attribute name="floorCrawlSpaceIsSealed" type="xsd:boolean"> <xsd:annotation> <xsd:documentation>Specifies whether or not the crawl space wall associated with this floor is well sealed from the outdoor air, which affects both the heating and cooling loads. See Figure A5-5, page A5-8, and Figure A5-17 page A5-16, ACCA Manual J Eighth Edition.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute ManualJ8Parameters/@floorCategory

type | floorCategoryEnum
properties |
isRef | 0
facets |
enumeration | OverEnclosedCrawlSpaceOrBasement
enumeration | OverOpenCrawlSpaceOrGarage
enumeration | Basement
enumeration | SlabOnGrade
annotation |
documentation
Specifies the type of floor being considered, which affects both the heating and the cooling loads. See Table 4A, pages T4A-27 and following, ACCA Manual J Eighth Edition.
source | <xsd:attribute name="floorCategory" type="floorCategoryEnum"> <xsd:annotation> <xsd:documentation>Specifies the type of floor being considered, which affects both the heating and the cooling loads. See Table 4A, pages T4A-27 and following, ACCA Manual J Eighth Edition.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Manufacturer

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
elements | AirLoopEquipment ExtEquip HydronicLoopEquipment IntEquip LightingSystem
source | <xsd:element name="Manufacturer" type="xsd:string"/>

element Material

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description ImageTexture R-value Thickness Conductivity Density SpecificHeat Permeance Porosity RecycledContent Cost IndoorAirQuality CADMaterialId Reference
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
DOELibIdRef | xsd:string |  |  |  |
documentation
Use this attribute to reference objects in the DOE2 library
source | <xsd:element name="Material"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="ImageTexture" minOccurs="0"/> <xsd:element ref="R-value" minOccurs="0"/> <xsd:element ref="Thickness" minOccurs="0"/> <xsd:element ref="Conductivity" minOccurs="0"/> <xsd:element ref="Density" minOccurs="0"/> <xsd:element ref="SpecificHeat" minOccurs="0"/> <xsd:element ref="Permeance" minOccurs="0"/> <xsd:element ref="Porosity" minOccurs="0"/> <xsd:element ref="RecycledContent" minOccurs="0"/> <xsd:element ref="Cost" minOccurs="0"/> <xsd:element ref="IndoorAirQuality" minOccurs="0"/> <xsd:element ref="CADMaterialId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Reference" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Material/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Material/@DOELibIdRef

type | xsd:string
properties |
isRef | 0
annotation |
documentation
Use this attribute to reference objects in the DOE2 library
source | <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute>

element MaterialId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | Layer
attributes |
Name | Type | Use | Default | Fixed | annotation
materialIdRef | xsd:IDREF | required |  |  |
documentation
ID identifying a material in this layer. Multiple materials in layers are in order from outside to inside.
percentOfLayer | xsd:double |  |  |  |
documentation
Percentage (1-100%) of this layer that this material is made from.
source | <xsd:element name="MaterialId"> <xsd:complexType> <xsd:attribute name="materialIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID identifying a material in this layer. Multiple materials in layers are in order from outside to inside.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="percentOfLayer" type="xsd:double"> <xsd:annotation> <xsd:documentation>Percentage (1-100%) of this layer that this material is made from. </xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute MaterialId/@materialIdRef

type | xsd:IDREF
properties |
isRef | 0
use | required
annotation |
documentation
ID identifying a material in this layer. Multiple materials in layers are in order from outside to inside.
source | <xsd:attribute name="materialIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID identifying a material in this layer. Multiple materials in layers are in order from outside to inside.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute MaterialId/@percentOfLayer

type | xsd:double
properties |
isRef | 0
annotation |
documentation
Percentage (1-100%) of this layer that this material is made from.
source | <xsd:attribute name="percentOfLayer" type="xsd:double"> <xsd:annotation> <xsd:documentation>Percentage (1-100%) of this layer that this material is made from. </xsd:documentation> </xsd:annotation> </xsd:attribute>

element MaximumFlow

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | FlowControl
source | <xsd:element name="MaximumFlow" type="xsd:decimal"/>

element MaxPressure

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | PressureControl
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | pressureUnitEnum |  |  |  |
source | <xsd:element name="MaxPressure"> <xsd:complexType> <xsd:attribute name="unit" type="pressureUnitEnum"/> </xsd:complexType> </xsd:element>

attribute MaxPressure/@unit

type | pressureUnitEnum
properties |
isRef | 0
facets |
enumeration | PSI
enumeration | kPa
enumeration | Atmospheres
enumeration | InchesOfH2O
enumeration | CentimetersOfH2O
enumeration | InchesOfMercury
enumeration | CentimetersOfMercury
enumeration | MillimetersOfMercury
enumeration | Pascals
source | <xsd:attribute name="unit" type="pressureUnitEnum"/>

element MaxRelativeHumidity

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | AirLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | unitlessUnitEnum | required |  |  |
source | <xsd:element name="MaxRelativeHumidity"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute MaxRelativeHumidity/@unit

type | unitlessUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Percent
enumeration | Fraction
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element MaxTemp

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | TemperatureControl
source | <xsd:element name="MaxTemp" type="xsd:decimal"/>

element Meter

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description UtilityRate
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
resourceType | resourceTypeEnum | required |  |  |
annotation |
documentation
Description of a resource measurement
source | <xsd:element name="Meter"> <xsd:annotation> <xsd:documentation>Description of a resource measurement</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="UtilityRate" minOccurs="0"/> <xsd:any namespace="##other" processContents="lax" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="resourceType" type="resourceTypeEnum" use="required"/> </xsd:complexType> </xsd:element>

attribute Meter/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Meter/@resourceType

type | resourceTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Electricity
enumeration | NaturalGas
enumeration | Propane
enumeration | FuelOil1
enumeration | FuelOil2
enumeration | FuelOil4
enumeration | Water
enumeration | ChilledWater
enumeration | HotWater
enumeration | Steam
source | <xsd:attribute name="resourceType" type="resourceTypeEnum" use="required"/>

element MeterId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
elements | AltEnergySource Building Campus Space
attributes |
Name | Type | Use | Default | Fixed | annotation
meterIdRef | xsd:IDREF |  |  |  |
documentation
ID for a resource meter
source | <xsd:element name="MeterId"> <xsd:complexType> <xsd:attribute name="meterIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for a resource meter</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute MeterId/@meterIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID for a resource meter
source | <xsd:attribute name="meterIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for a resource meter</xsd:documentation> </xsd:annotation> </xsd:attribute>

element MiddleName

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | PersonInfo
source | <xsd:element name="MiddleName" type="xsd:string"/>

element MinFlow

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | AirLoopEquipment HydronicLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | derived by: flowUnitEnum | required |  |  |
hydronicLoopIdRef | xsd:IDREF |  |  |  |
hydronicLoopType | loopTypeEnum |  |  |  |
annotation |
documentation
Minimum flow
source | <xsd:element name="MinFlow"> <xsd:annotation> <xsd:documentation>Minimum flow</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" use="required"> <xsd:simpleType> <xsd:union memberTypes="flowUnitEnum unitlessUnitEnum"/> </xsd:simpleType> </xsd:attribute> <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF"/> <xsd:attribute name="hydronicLoopType" type="loopTypeEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute MinFlow/@unit

type | union of (flowUnitEnum, unitlessUnitEnum)
properties |
isRef | 0
use | required
source | <xsd:attribute name="unit" use="required"> <xsd:simpleType> <xsd:union memberTypes="flowUnitEnum unitlessUnitEnum"/> </xsd:simpleType> </xsd:attribute>

attribute MinFlow/@hydronicLoopIdRef

type | xsd:IDREF
properties |
isRef | 0
source | <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF"/>

attribute MinFlow/@hydronicLoopType

type | loopTypeEnum
properties |
isRef | 0
facets |
enumeration | PrimaryChilledWater
enumeration | SecondaryChilledWater
enumeration | HotWater
enumeration | CondenserWater
enumeration | DomesticHotWater
enumeration | WaterLoopHeatPump
enumeration | TwoPipe
enumeration | PotableWaterLoop
source | <xsd:attribute name="hydronicLoopType" type="loopTypeEnum"/>

element MinimumFlow

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | FlowControl
source | <xsd:element name="MinimumFlow" type="xsd:decimal"/>

element MinLightFrac

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | LightingControl
annotation |
documentation
Fraction of light illuminance used at minimum setting.
source | <xsd:element name="MinLightFrac" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Fraction of light illuminance used at minimum setting.</xsd:documentation> </xsd:annotation> </xsd:element>

element MinPowerFrac

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | LightingControl
annotation |
documentation
Fraction of power used at minimum setting.
source | <xsd:element name="MinPowerFrac" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Fraction of power used at minimum setting.</xsd:documentation> </xsd:annotation> </xsd:element>

element MinPressure

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | PressureControl
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | pressureUnitEnum |  |  |  |
source | <xsd:element name="MinPressure"> <xsd:complexType> <xsd:attribute name="unit" type="pressureUnitEnum"/> </xsd:complexType> </xsd:element>

attribute MinPressure/@unit

type | pressureUnitEnum
properties |
isRef | 0
facets |
enumeration | PSI
enumeration | kPa
enumeration | Atmospheres
enumeration | InchesOfH2O
enumeration | CentimetersOfH2O
enumeration | InchesOfMercury
enumeration | CentimetersOfMercury
enumeration | MillimetersOfMercury
enumeration | Pascals
source | <xsd:attribute name="unit" type="pressureUnitEnum"/>

element MinRelativeHumidity

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | AirLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | unitlessUnitEnum | required |  |  |
source | <xsd:element name="MinRelativeHumidity"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute MinRelativeHumidity/@unit

type | unitlessUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Percent
enumeration | Fraction
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element MinTemp

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | TemperatureControl
source | <xsd:element name="MinTemp" type="xsd:decimal"/>

element Model

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
elements | AirLoopEquipment ExtEquip HydronicLoopEquipment IntEquip
source | <xsd:element name="Model" type="xsd:string"/>

element ModifiedBy

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | DocumentHistory
attributes |
Name | Type | Use | Default | Fixed | annotation
personId | xsd:IDREF | required |  |  |
programId | xsd:IDREF | required |  |  |
date | xsd:dateTime | required |  |  |
annotation |
documentation
Denotes the time this file has been modified, as well as the person and program used to modify this file.
source | <xsd:element name="ModifiedBy"> <xsd:annotation> <xsd:documentation>Denotes the time this file has been modified, as well as the person and program used to modify this file.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:attribute name="personId" type="xsd:IDREF" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="required"/> <xsd:attribute name="date" type="xsd:dateTime" use="required"/> </xsd:complexType> </xsd:element>

attribute ModifiedBy/@personId

type | xsd:IDREF
properties |
isRef | 0
use | required
source | <xsd:attribute name="personId" type="xsd:IDREF" use="required"/>

attribute ModifiedBy/@programId

type | xsd:IDREF
properties |
isRef | 0
use | required
source | <xsd:attribute name="programId" type="xsd:IDREF" use="required"/>

attribute ModifiedBy/@date

type | xsd:dateTime
properties |
isRef | 0
use | required
source | <xsd:attribute name="date" type="xsd:dateTime" use="required"/>

element Name

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
elements | AirLoop AirLoopEquipment Blind Building BuildingStorey Campus Construction DaySchedule DependantVariable ExtEquip Frame Gap Glaze HydronicLoop HydronicLoopEquipment IndepentantVariable IntEquip Layer Location Material Meter Opening Results Schedule ShellGeometry Space Surface Weather WeekSchedule WindowType XAxis YAxis YearSchedule Zone
source | <xsd:element name="Name" type="xsd:string"/>

element NaturalVentHiTemp

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Opening
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | temperatureUnitEnum |  |  |  |
annotation |
documentation
Natural ventilation does not occur above this temperature.
source | <xsd:element name="NaturalVentHiTemp"> <xsd:annotation> <xsd:documentation>Natural ventilation does not occur above this temperature.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute NaturalVentHiTemp/@unit

type | temperatureUnitEnum
properties |
isRef | 0
facets |
enumeration | F
enumeration | C
enumeration | K
enumeration | R
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element NaturalVentLoTemp

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Opening
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | temperatureUnitEnum |  |  |  |
annotation |
documentation
Natural ventilation does not occur below this temperature.
source | <xsd:element name="NaturalVentLoTemp"> <xsd:annotation> <xsd:documentation>Natural ventilation does not occur below this temperature.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute NaturalVentLoTemp/@unit

type | temperatureUnitEnum
properties |
isRef | 0
facets |
enumeration | F
enumeration | C
enumeration | K
enumeration | R
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element NaturalVentOccDep

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:boolean
properties |
content | simple
used by |
element | Opening
annotation |
documentation
Occupancy dependence of natural ventilation. If true, then natural ventilation only occurs when people are present.
source | <xsd:element name="NaturalVentOccDep" type="xsd:boolean"> <xsd:annotation> <xsd:documentation>Occupancy dependence of natural ventilation. If true, then natural ventilation only occurs when people are present.</xsd:documentation> </xsd:annotation> </xsd:element>

element NumberOfLamps

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | LightingSystem
source | <xsd:element name="NumberOfLamps" type="xsd:integer"/>

element OAFlowPerArea

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Zone
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | flowPerAreaUnitEnum | required |  |  |
annotation |
documentation
Outside air flow per area
source | <xsd:element name="OAFlowPerArea"> <xsd:annotation> <xsd:documentation>Outside air flow per area</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="flowPerAreaUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute OAFlowPerArea/@unit

type | flowPerAreaUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | CFMPerSquareFoot
enumeration | LPerSecPerSquareM
enumeration | CubicMPerSecPerSquareM
source | <xsd:attribute name="unit" type="flowPerAreaUnitEnum" use="required"/>

element OAFlowPerPerson

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Zone
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | flowUnitEnum | required |  |  |
annotation |
documentation
Outside air flow per person
source | <xsd:element name="OAFlowPerPerson"> <xsd:annotation> <xsd:documentation>Outside air flow per person</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="flowUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute OAFlowPerPerson/@unit

type | flowUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | CFM
enumeration | LPerSec
enumeration | CubicMPerHr
enumeration | GPM
enumeration | GPH
source | <xsd:attribute name="unit" type="flowUnitEnum" use="required"/>

element ObjectId

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | Results
annotation |
documentation
Indicates which object or objects the results apply to, if any
source | <xsd:element name="ObjectId" type="xsd:string"> <xsd:annotation> <xsd:documentation>Indicates which object or objects the results apply to, if any</xsd:documentation> </xsd:annotation> </xsd:element>

element Opening

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description ShadeControl U-value ShadingCoeff SolarHeatGainCoeff Transmittance Reflectance GlazeConductivity Emittance Setback NaturalVentHiTemp NaturalVentLoTemp NaturalVentOccDep RectangularGeometry PlanarGeometry CADObjectId
used by |
element | Surface
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
interiorShadeType | shadeOperationEnum |  |  |  |
exteriorShadeType | shadeOperationEnum |  |  |  |
windowTypeIdRef | xsd:IDREF |  |  |  |
constructionIdRef | xsd:IDREF |  |  |  |
documentation
Identifier pointing to a construction
openingType | openingTypeEnum | required |  |  |
ifcGUID | xsd:string | optional |  |  |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
source | <xsd:element name="Opening"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="ShadeControl" minOccurs="0"/> <xsd:element ref="U-value" minOccurs="0"/> <xsd:element ref="ShadingCoeff" minOccurs="0"/> <xsd:element ref="SolarHeatGainCoeff" minOccurs="0"/> <xsd:element ref="Transmittance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Reflectance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="GlazeConductivity" minOccurs="0"/> <xsd:element ref="Emittance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Setback" minOccurs="0"/> <xsd:element ref="NaturalVentHiTemp" minOccurs="0"/> <xsd:element ref="NaturalVentLoTemp" minOccurs="0"/> <xsd:element ref="NaturalVentOccDep" minOccurs="0"/> <xsd:element ref="RectangularGeometry"/> <xsd:element ref="PlanarGeometry"/> <xsd:element ref="CADObjectId" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="interiorShadeType" type="shadeOperationEnum"/> <xsd:attribute name="exteriorShadeType" type="shadeOperationEnum"/> <xsd:attribute name="windowTypeIdRef" type="xsd:IDREF"/> <xsd:attribute name="constructionIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Identifier pointing to a construction</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="openingType" type="openingTypeEnum" use="required"/> <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Opening/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Opening/@interiorShadeType

type | shadeOperationEnum
properties |
isRef | 0
facets |
enumeration | Fixed
enumeration | Operable
source | <xsd:attribute name="interiorShadeType" type="shadeOperationEnum"/>

attribute Opening/@exteriorShadeType

type | shadeOperationEnum
properties |
isRef | 0
facets |
enumeration | Fixed
enumeration | Operable
source | <xsd:attribute name="exteriorShadeType" type="shadeOperationEnum"/>

attribute Opening/@windowTypeIdRef

type | xsd:IDREF
properties |
isRef | 0
source | <xsd:attribute name="windowTypeIdRef" type="xsd:IDREF"/>

attribute Opening/@constructionIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
Identifier pointing to a construction
source | <xsd:attribute name="constructionIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Identifier pointing to a construction</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Opening/@openingType

type | openingTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | FixedWindow
enumeration | OperableWindow
enumeration | FixedSkylight
enumeration | OperableSkylight
enumeration | SlidingDoor
enumeration | NonSlidingDoor
enumeration | Air
source | <xsd:attribute name="openingType" type="openingTypeEnum" use="required"/>

attribute Opening/@ifcGUID

type | xsd:string
properties |
isRef | 0
use | optional
annotation |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
source | <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element OperationRange

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | LowValue HighValue
used by |
element | OperationSchedule
source | <xsd:element name="OperationRange"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="LowValue"/> <xsd:element ref="HighValue"/> </xsd:choice> </xsd:complexType> </xsd:element>

element OperationSchedule

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | OperationRange
used by |
elements | AirLoopEquipment HydronicLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | annotation
scheduleIdRef | xsd:IDREF |  |  |  |
documentation
Schedule of operation for a piece of equipment. For heating and cooling equipment (such as a boiler or chiller) this is the availability schedule, the schedule of temperatures that, when reached, the piece of equipment will be available.
source | <xsd:element name="OperationSchedule"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="OperationRange"/> </xsd:choice> <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Schedule of operation for a piece of equipment. For heating and cooling equipment (such as a boiler or chiller) this is the availability schedule, the schedule of temperatures that, when reached, the piece of equipment will be available.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute OperationSchedule/@scheduleIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
Schedule of operation for a piece of equipment. For heating and cooling equipment (such as a boiler or chiller) this is the availability schedule, the schedule of temperatures that, when reached, the piece of equipment will be available.
source | <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Schedule of operation for a piece of equipment. For heating and cooling equipment (such as a boiler or chiller) this is the availability schedule, the schedule of temperatures that, when reached, the piece of equipment will be available.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element PeakDomesticHotWaterFlow

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Building
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | flowUnitEnum | required |  |  |
hydronicLoopIdRef | xsd:IDREF | required |  |  |
waterUseScheduleIdRef | xsd:IDREF | required |  |  |
annotation |
documentation
Use this element to report overall domestic hot water use for the domestic hot water loop referenced with the hydronicLoopIdRef attribute. The schedule referenced by waterUseScheduleIdRef defines a hot water use fraction schedule, which when combined with the value of PeakDomesticHotWaterFlow fully describe the hot water use of this building.
source | <xsd:element name="PeakDomesticHotWaterFlow"> <xsd:annotation> <xsd:documentation>Use this element to report overall domestic hot water use for the domestic hot water loop referenced with the hydronicLoopIdRef attribute. The schedule referenced by waterUseScheduleIdRef defines a hot water use fraction schedule, which when combined with the value of PeakDomesticHotWaterFlow fully describe the hot water use of this building.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="flowUnitEnum" use="required"/> <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF" use="required"/> <xsd:attribute name="waterUseScheduleIdRef" type="xsd:IDREF" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute PeakDomesticHotWaterFlow/@unit

type | flowUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | CFM
enumeration | LPerSec
enumeration | CubicMPerHr
enumeration | GPM
enumeration | GPH
source | <xsd:attribute name="unit" type="flowUnitEnum" use="required"/>

attribute PeakDomesticHotWaterFlow/@hydronicLoopIdRef

type | xsd:IDREF
properties |
isRef | 0
use | required
source | <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF" use="required"/>

attribute PeakDomesticHotWaterFlow/@waterUseScheduleIdRef

type | xsd:IDREF
properties |
isRef | 0
use | required
source | <xsd:attribute name="waterUseScheduleIdRef" type="xsd:IDREF" use="required"/>

element PeopleHeatGain

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Space
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | peopleHeatGainUnitEnum | required |  |  |
heatGainType | peopleHeatGainTypeEnum | required |  |  |
annotation |
documentation
Amount of heat added to the space by people
source | <xsd:element name="PeopleHeatGain"> <xsd:annotation> <xsd:documentation>Amount of heat added to the space by people</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="peopleHeatGainUnitEnum" use="required"/> <xsd:attribute name="heatGainType" type="peopleHeatGainTypeEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute PeopleHeatGain/@unit

type | peopleHeatGainUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | WattPerPerson
enumeration | BtuPerHourPerson
source | <xsd:attribute name="unit" type="peopleHeatGainUnitEnum" use="required"/>

attribute PeopleHeatGain/@heatGainType

type | peopleHeatGainTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Total
enumeration | Sensible
enumeration | Latent
source | <xsd:attribute name="heatGainType" type="peopleHeatGainTypeEnum" use="required"/>

element PeopleNumber

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Space
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | peopleNumberUnitEnum | required |  |  |
annotation |
documentation
Occupancy of the space
source | <xsd:element name="PeopleNumber"> <xsd:annotation> <xsd:documentation>Occupancy of the space</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="peopleNumberUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute PeopleNumber/@unit

type | peopleNumberUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | NumberOfPeople
enumeration | SquareFtPerPerson
enumeration | SquareMPerPerson
source | <xsd:attribute name="unit" type="peopleNumberUnitEnum" use="required"/>

element PercentAreaDaylitControled

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | LightingControl
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | unitlessUnitEnum | required |  |  |
annotation |
documentation
Percent of space area whose lights are controled by a daylight sensor. Only applicable when LightPowerPerArea is used at the space level and not Lighting Systems.
source | <xsd:element name="PercentAreaDaylitControled"> <xsd:annotation> <xsd:documentation>Percent of space area whose lights are controled by a daylight sensor. Only applicable when LightPowerPerArea is used at the space level and not Lighting Systems.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute PercentAreaDaylitControled/@unit

type | unitlessUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Percent
enumeration | Fraction
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element PercentExisting

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Construction
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | unitlessUnitEnum | required |  |  |
annotation |
documentation
Percent of original building shell used in renovation
source | <xsd:element name="PercentExisting"> <xsd:annotation> <xsd:documentation>Percent of original building shell used in renovation</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute PercentExisting/@unit

type | unitlessUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Percent
enumeration | Fraction
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element Performance

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | PointData Equation
used by |
elements | AirLoopEquipment ExtEquip HydronicLoopEquipment IntEquip
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID |  |  |  |
performanceType | xsd:string |  |  |  |
annotation |
documentation
Used to represent part load performance
source | <xsd:element name="Performance"> <xsd:annotation> <xsd:documentation>Used to represent part load performance</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="PointData" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Equation" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID"/> <xsd:attribute name="performanceType" type="xsd:string"/> </xsd:complexType> </xsd:element>

attribute Performance/@id

type | xsd:ID
properties |
isRef | 0
source | <xsd:attribute name="id" type="xsd:ID"/>

attribute Performance/@performanceType

type | xsd:string
properties |
isRef | 0
source | <xsd:attribute name="performanceType" type="xsd:string"/>

element Permeance

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Material
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | permUnitEnum | required |  |  |
annotation |
documentation
The rate water vapor is allowed through a surface
source | <xsd:element name="Permeance"> <xsd:annotation> <xsd:documentation>The rate water vapor is allowed through a surface</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="permUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Permeance/@unit

type | permUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | PermSI
enumeration | PermIP
source | <xsd:attribute name="unit" type="permUnitEnum" use="required"/>

element PersonInfo

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | FirstName LastName MiddleName Email1Address WebPage CompanyName
used by |
element | DocumentHistory
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
annotation |
documentation
Contains information about people that created and modified this file
source | <xsd:element name="PersonInfo"> <xsd:annotation> <xsd:documentation>Contains information about people that created and modified this file</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="FirstName"/> <xsd:element ref="LastName"/> <xsd:element ref="MiddleName" minOccurs="0"/> <xsd:element ref="Email1Address" minOccurs="0"/> <xsd:element ref="WebPage" minOccurs="0"/> <xsd:element ref="CompanyName" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> </xsd:complexType> </xsd:element>

attribute PersonInfo/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

element PlanarGeometry

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | PolyLoop
used by |
elements | BuildingStorey Opening Space SpaceBoundary Surface
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID |  |  |  |
unit | lengthUnitEnum |  |  |  |
annotation |
documentation
List of points defining a loop. There are no repeated points in the list. All data are global, with the assumption that positive Z is up, and if CADModelAzimuth is undefined or zero, positive X is East and positive Y is North. If CADModelAzimuth is defined it is the angle of positive Y to North, positive X is the vectorial product of Y and Z. If geometry is to be precise, use Longitude, Latitude and Elevation in the Location element to define the origin. Otherwise the origin is an arbitrary point. Use PlanarGeometry to define a three dimensional polygon that lies on a plane, and has no self-intersection.
source | <xsd:element name="PlanarGeometry"> <xsd:annotation> <xsd:documentation>List of points defining a loop. There are no repeated points in the list. All data are global, with the assumption that positive Z is up, and if CADModelAzimuth is undefined or zero, positive X is East and positive Y is North. If CADModelAzimuth is defined it is the angle of positive Y to North, positive X is the vectorial product of Y and Z. If geometry is to be precise, use Longitude, Latitude and Elevation in the Location element to define the origin. Otherwise the origin is an arbitrary point. Use PlanarGeometry to define a three dimensional polygon that lies on a plane, and has no self-intersection.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="PolyLoop"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID"/> <xsd:attribute name="unit" type="lengthUnitEnum"/> </xsd:complexType> </xsd:element>

attribute PlanarGeometry/@id

type | xsd:ID
properties |
isRef | 0
source | <xsd:attribute name="id" type="xsd:ID"/>

attribute PlanarGeometry/@unit

type | lengthUnitEnum
properties |
isRef | 0
facets |
enumeration | Kilometers
enumeration | Meters
enumeration | Centimeters
enumeration | Millimeters
enumeration | Miles
enumeration | Yards
enumeration | Feet
enumeration | Inches
source | <xsd:attribute name="unit" type="lengthUnitEnum"/>

element Platform

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | ProgramInfo
source | <xsd:element name="Platform" type="xsd:string"/>

element PointData

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | IndepentantVariable DependantVariable Data
used by |
element | Performance
annotation |
documentation
The PointData element allows for graph or tabular information to be entered. The data type and units of the independent and dependant variables are defined in their respective elements. Each Data element represent a data point, with each Value element representing the value of a variable - starting with the independent variable, then each dependant variable listed in the order defined.
source | <xsd:element name="PointData"> <xsd:annotation> <xsd:documentation>The PointData element allows for graph or tabular information to be entered. The data type and units of the independent and dependant variables are defined in their respective elements. Each Data element represent a data point, with each Value element representing the value of a variable - starting with the independent variable, then each dependant variable listed in the order defined.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="IndepentantVariable" maxOccurs="2"/> <xsd:element ref="DependantVariable" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Data" maxOccurs="unbounded"/> </xsd:choice> </xsd:complexType> </xsd:element>

element PolyLoop

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | CartesianPoint
used by |
elements | ClosedShell PlanarGeometry RectangularGeometry
annotation |
documentation
This is a list of coordinates that make up a polygon in three-dimensional space. All coordinates must lie on the same plane. The right-hand rule applies for defining the outward normal of a surface: For every surface, points must be defined in order, such that the direction of (the average cross-product between (any point, the centroid of the surface, and the next point)) points in the direction of the outward normal, which is a vector pointing away from the associated space. Of course, this must only hold for surfaces touching the exterior (only one SpaceId element).
appinfo
<xhtml:a href="http://cig.bre.co.uk/iai_uk/documentation/IfcR2x_Final/ifctopologyresource/lexical/ifcpolyloop.html">IfcPolyLoop</xhtml:a>
source | <xsd:element name="PolyLoop"> <xsd:annotation> <xsd:documentation>This is a list of coordinates that make up a polygon in three-dimensional space. All coordinates must lie on the same plane. The right-hand rule applies for defining the outward normal of a surface: For every surface, points must be defined in order, such that the direction of (the average cross-product between (any point, the centroid of the surface, and the next point)) points in the direction of the outward normal, which is a vector pointing away from the associated space. Of course, this must only hold for surfaces touching the exterior (only one SpaceId element).</xsd:documentation> <xsd:appinfo> <xhtml:a href="http://cig.bre.co.uk/iai_uk/documentation/IfcR2x_Final/ifctopologyresource/lexical/ifcpolyloop.html">IfcPolyLoop</xhtml:a> </xsd:appinfo> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="CartesianPoint" minOccurs="3" maxOccurs="unbounded"/> </xsd:choice> </xsd:complexType> </xsd:element>

element Porosity

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Material
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | unitlessUnitEnum | required |  |  |
annotation |
documentation
the ratio of the total amount of void space in a material (due to poses, small channels, and so on) to the bulk volume occupied by the material.
source | <xsd:element name="Porosity"> <xsd:annotation> <xsd:documentation>the ratio of the total amount of void space in a material (due to poses, small channels, and so on) to the bulk volume occupied by the material. </xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Porosity/@unit

type | unitlessUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Percent
enumeration | Fraction
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element Power

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | AirLoopEquipment ExtEquip HydronicLoopEquipment IntEquip
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | powerUnitEnum | required |  |  |
powerType | powerTypeEnum | required |  |  |
useType | powerUseTypeEnum | required |  |  |
meterIdRef | xsd:IDREF |  |  |  |
documentation
ID for a resource meter
annotation |
documentation
Maximum consumption of energy (power input)
source | <xsd:element name="Power"> <xsd:annotation> <xsd:documentation>Maximum consumption of energy (power input)</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="powerUnitEnum" use="required"/> <xsd:attribute name="powerType" type="powerTypeEnum" use="required"/> <xsd:attribute name="useType" type="powerUseTypeEnum" use="required"/> <xsd:attribute name="meterIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for a resource meter</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Power/@unit

type | powerUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Watt
enumeration | Kilowatt
enumeration | Horsepower
enumeration | KilogramForceMeterPerSecond
enumeration | BtuPerSecond
enumeration | FootPoundForcePerSecond
enumeration | KilocaloriesPerSecond
enumeration | BtuPerHour
source | <xsd:attribute name="unit" type="powerUnitEnum" use="required"/>

attribute Power/@powerType

type | powerTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Electricity
enumeration | NaturalGas
enumeration | Propane
enumeration | FuelOil1
enumeration | FuelOil2
enumeration | FuelOil4
enumeration | Water
enumeration | ChilledWater
enumeration | HotWater
enumeration | Steam
source | <xsd:attribute name="powerType" type="powerTypeEnum" use="required"/>

attribute Power/@useType

type | powerUseTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Heating
enumeration | Cooling
enumeration | Both
enumeration | Other
source | <xsd:attribute name="useType" type="powerUseTypeEnum" use="required"/>

attribute Power/@meterIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID for a resource meter
source | <xsd:attribute name="meterIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for a resource meter</xsd:documentation> </xsd:annotation> </xsd:attribute>

element PrandtlNumber

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Gap
source | <xsd:element name="PrandtlNumber" type="xsd:decimal"/>

element PrandtlNumberFofT

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Gap
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | inverseTempUnitEnum | required |  |  |
annotation |
documentation
Prandtl number as a function of temperature
source | <xsd:element name="PrandtlNumberFofT"> <xsd:annotation> <xsd:documentation>Prandtl number as a function of temperature</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="inverseTempUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute PrandtlNumberFofT/@unit

type | inverseTempUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | PerK
enumeration | PerF
source | <xsd:attribute name="unit" type="inverseTempUnitEnum" use="required"/>

element PressureControl

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | DesignPressure MinPressure MaxPressure
used by |
element | AirLoop
annotation |
documentation
Use this element to describe how the air pressure is controlled. The temperatures specified in this element should be measured just upstream of the air handlers.
source | <xsd:element name="PressureControl"> <xsd:annotation> <xsd:documentation>Use this element to describe how the air pressure is controlled. The temperatures specified in this element should be measured just upstream of the air handlers.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="DesignPressure" minOccurs="0"/> <xsd:element ref="MinPressure" minOccurs="0"/> <xsd:element ref="MaxPressure" minOccurs="0"/> </xsd:choice> </xsd:complexType> </xsd:element>

element ProductName

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | ProgramInfo
source | <xsd:element name="ProductName" type="xsd:string"/>

element ProgramInfo

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | CompanyName ProductName Version Platform
used by |
element | DocumentHistory
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
annotation |
documentation
Contains information about programs that created and modified this file
source | <xsd:element name="ProgramInfo"> <xsd:annotation> <xsd:documentation>Contains information about programs that created and modified this file</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="CompanyName" minOccurs="0"/> <xsd:element ref="ProductName" minOccurs="0"/> <xsd:element ref="Version" minOccurs="0"/> <xsd:element ref="Platform" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> </xsd:complexType> </xsd:element>

attribute ProgramInfo/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

element R-value

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Material
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | resistanceUnitEnum | required |  |  |
annotation |
documentation
Resistance of material
source | <xsd:element name="R-value"> <xsd:annotation> <xsd:documentation>Resistance of material</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="resistanceUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute R-value/@unit

type | resistanceUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | SquareMeterKPerW
enumeration | HrSquareFtFPerBTU
source | <xsd:attribute name="unit" type="resistanceUnitEnum" use="required"/>

element RatedFlow

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | AirLoopEquipment ExtEquip HydronicLoopEquipment IntEquip
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | flowUnitEnum | required |  |  |
hydronicLoopIdRef | xsd:IDREF |  |  |  |
hydronicLoopType | loopTypeEnum |  |  |  |
source | <xsd:element name="RatedFlow"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="flowUnitEnum" use="required"/> <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF"/> <xsd:attribute name="hydronicLoopType" type="loopTypeEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute RatedFlow/@unit

type | flowUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | CFM
enumeration | LPerSec
enumeration | CubicMPerHr
enumeration | GPM
enumeration | GPH
source | <xsd:attribute name="unit" type="flowUnitEnum" use="required"/>

attribute RatedFlow/@hydronicLoopIdRef

type | xsd:IDREF
properties |
isRef | 0
source | <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF"/>

attribute RatedFlow/@hydronicLoopType

type | loopTypeEnum
properties |
isRef | 0
facets |
enumeration | PrimaryChilledWater
enumeration | SecondaryChilledWater
enumeration | HotWater
enumeration | CondenserWater
enumeration | DomesticHotWater
enumeration | WaterLoopHeatPump
enumeration | TwoPipe
enumeration | PotableWaterLoop
source | <xsd:attribute name="hydronicLoopType" type="loopTypeEnum"/>

element RectangularGeometry

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Azimuth CartesianPoint Tilt Height Width PolyLoop
used by |
elements | Opening Surface
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID |  |  |  |
unit | lengthUnitEnum |  |  |  |
annotation |
documentation
Geometry data in a form typically used in simulation engines. For surfaces, specify the location of the bottom-left corner with the CartesianPoint element when facing it from the outside. Also for surfaces, Tilt and Azimuth must be specified. If CADModelAzimuth is defined, the Azimuth value is relative to the CADModelAzimuth value rather then North. For openings, the third Coordinate should be zero or left missing. For openings, these Coordinates represent the distance of the bottom-left of the opening to the bottom-left corner of the parent surface. Azimuth and Tilt should not be specified for opening. There is an optional PolyLoop element, which may be used for describing the polygon shape of the surface.
source | <xsd:element name="RectangularGeometry"> <xsd:annotation> <xsd:documentation>Geometry data in a form typically used in simulation engines. For surfaces, specify the location of the bottom-left corner with the CartesianPoint element when facing it from the outside. Also for surfaces, Tilt and Azimuth must be specified. If CADModelAzimuth is defined, the Azimuth value is relative to the CADModelAzimuth value rather then North. For openings, the third Coordinate should be zero or left missing. For openings, these Coordinates represent the distance of the bottom-left of the opening to the bottom-left corner of the parent surface. Azimuth and Tilt should not be specified for opening. There is an optional PolyLoop element, which may be used for describing the polygon shape of the surface.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Azimuth"/> <xsd:element ref="CartesianPoint"/> <xsd:element ref="Tilt"/> <xsd:element ref="Height"/> <xsd:element ref="Width"/> <xsd:element ref="PolyLoop" minOccurs="0"> <xsd:annotation> <xsd:documentation>This is a two-dimensional polygon, with the origin at the point specified with RectangularGeometry/CartesianPoint. </xsd:documentation> </xsd:annotation> </xsd:element> </xsd:choice> <xsd:attribute name="id" type="xsd:ID"/> <xsd:attribute name="unit" type="lengthUnitEnum"/> </xsd:complexType> </xsd:element>

attribute RectangularGeometry/@id

type | xsd:ID
properties |
isRef | 0
source | <xsd:attribute name="id" type="xsd:ID"/>

attribute RectangularGeometry/@unit

type | lengthUnitEnum
properties |
isRef | 0
facets |
enumeration | Kilometers
enumeration | Meters
enumeration | Centimeters
enumeration | Millimeters
enumeration | Miles
enumeration | Yards
enumeration | Feet
enumeration | Inches
source | <xsd:attribute name="unit" type="lengthUnitEnum"/>

element RecycledContent

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Material
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | unitlessUnitEnum | required |  |  |
source | <xsd:element name="RecycledContent"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute RecycledContent/@unit

type | unitlessUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Percent
enumeration | Fraction
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element Reference

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
elements | AirLoop AirLoopEquipment Cost ExtEquip Glaze HydronicLoop HydronicLoopEquipment InfiltrationFlow IntEquip LightingSystem Material Weather
source | <xsd:element name="Reference" type="xsd:string"/>

element Reflectance

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Blind Construction Glaze Opening WindowType
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | unitlessUnitEnum | required |  |  |
type | reflectanceTypeEnum | required |  |  |
source | <xsd:element name="Reflectance"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> <xsd:attribute name="type" type="reflectanceTypeEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Reflectance/@unit

type | unitlessUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Percent
enumeration | Fraction
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

attribute Reflectance/@type

type | reflectanceTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Ground
enumeration | IntSolar
enumeration | IntIR
enumeration | IntVisible
enumeration | ExtSolar
enumeration | ExtVisible
enumeration | ExtIR
source | <xsd:attribute name="type" type="reflectanceTypeEnum" use="required"/>

element RefrigerantType

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
elements | AirLoopEquipment HydronicLoopEquipment
source | <xsd:element name="RefrigerantType" type="xsd:string"/>

element Results

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Value ObjectId CADObjectId CartesianPoint
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
unit | derived by: loadUnitEnum | required |  |  |
currency | currencyTypeEnum |  |  |  |
resultsType | resultsTypeEnum |  |  |  |
resourceType | resourceTypeEnum | required |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that generated the results using the id of the ProgramInfo element.
valueType | valueTypeEnum |  |  |  |
documentation
Please specify how the values were obtained.
startTime | xsd:dateTime | required |  |  |
documentation
Use the startTime attribute to define the start of the first Value element.
timeIncrement | xsd:duration | optional |  |  |
documentation
This specifies the duration of time between each Value element. This is required if more than one Value element exists in a this Results element.
source | <xsd:element name="Results"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Value" maxOccurs="unbounded"/> <xsd:element ref="ObjectId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="CADObjectId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="CartesianPoint" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="unit" use="required"> <xsd:simpleType> <xsd:union memberTypes="loadUnitEnum unitlessSmallUnitEnum energyUnitEnum powerUnitEnum temperatureUnitEnum unitlessUnitEnum illuminanceUnitEnum flowUnitEnum"/> </xsd:simpleType> </xsd:attribute> <xsd:attribute name="currency" type="currencyTypeEnum"/> <xsd:attribute name="resultsType" type="resultsTypeEnum"/> <xsd:attribute name="resourceType" type="resourceTypeEnum" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that generated the results using the id of the ProgramInfo element.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="valueType" type="valueTypeEnum"> <xsd:annotation> <xsd:documentation>Please specify how the values were obtained.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="startTime" type="xsd:dateTime" use="required"> <xsd:annotation> <xsd:documentation>Use the startTime attribute to define the start of the first Value element.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="timeIncrement" type="xsd:duration" use="optional"> <xsd:annotation> <xsd:documentation>This specifies the duration of time between each Value element. This is required if more than one Value element exists in a this Results element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Results/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Results/@unit

type | union of (loadUnitEnum, unitlessSmallUnitEnum, energyUnitEnum, powerUnitEnum, temperatureUnitEnum, unitlessUnitEnum, illuminanceUnitEnum, flowUnitEnum)
properties |
isRef | 0
use | required
source | <xsd:attribute name="unit" use="required"> <xsd:simpleType> <xsd:union memberTypes="loadUnitEnum unitlessSmallUnitEnum energyUnitEnum powerUnitEnum temperatureUnitEnum unitlessUnitEnum illuminanceUnitEnum flowUnitEnum"/> </xsd:simpleType> </xsd:attribute>

attribute Results/@currency

type | currencyTypeEnum
properties |
isRef | 0
facets |
enumeration | USDollars
enumeration | CanadianDollars
enumeration | Pesos
enumeration | Euros
enumeration | Yen
enumeration | IndianRupee
enumeration | Yuan
enumeration | TaiwanDollar
enumeration | EnglishPound
enumeration | Mark
enumeration | Franc
enumeration | Ruble
enumeration | Real
enumeration | NewZealandDollar
enumeration | AustralianDollar
source | <xsd:attribute name="currency" type="currencyTypeEnum"/>

attribute Results/@resultsType

type | resultsTypeEnum
properties |
isRef | 0
facets |
enumeration | HeatLoad
enumeration | CoolingLoad
enumeration | CO2
enumeration | SO2
enumeration | NOx
enumeration | Energy
enumeration | Power
enumeration | Cost
enumeration | EnergyCost
enumeration | DemandCost
enumeration | CommodityCost
enumeration | TransportationCost
enumeration | DryBulbTemperature
enumeration | WetBulbTemperature
enumeration | DewPointTemperature
enumeration | FootCandles
enumeration | Humidity
enumeration | MoistureContent
enumeration | Flow
enumeration | Capacity
source | <xsd:attribute name="resultsType" type="resultsTypeEnum"/>

attribute Results/@resourceType

type | resourceTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Electricity
enumeration | NaturalGas
enumeration | Propane
enumeration | FuelOil1
enumeration | FuelOil2
enumeration | FuelOil4
enumeration | Water
enumeration | ChilledWater
enumeration | HotWater
enumeration | Steam
source | <xsd:attribute name="resourceType" type="resourceTypeEnum" use="required"/>

attribute Results/@programId

type | xsd:IDREF
properties |
isRef | 0
use | optional
annotation |
documentation
Please specify the program that generated the results using the id of the ProgramInfo element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that generated the results using the id of the ProgramInfo element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Results/@valueType

type | valueTypeEnum
properties |
isRef | 0
facets |
enumeration | Historical
enumeration | Simulated
enumeration | Rated
enumeration | Measured
annotation |
documentation
Please specify how the values were obtained.
source | <xsd:attribute name="valueType" type="valueTypeEnum"> <xsd:annotation> <xsd:documentation>Please specify how the values were obtained.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Results/@startTime

type | xsd:dateTime
properties |
isRef | 0
use | required
annotation |
documentation
Use the startTime attribute to define the start of the first Value element.
source | <xsd:attribute name="startTime" type="xsd:dateTime" use="required"> <xsd:annotation> <xsd:documentation>Use the startTime attribute to define the start of the first Value element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Results/@timeIncrement

type | xsd:duration
properties |
isRef | 0
use | optional
annotation |
documentation
This specifies the duration of time between each Value element. This is required if more than one Value element exists in a this Results element.
source | <xsd:attribute name="timeIncrement" type="xsd:duration" use="optional"> <xsd:annotation> <xsd:documentation>This specifies the duration of time between each Value element. This is required if more than one Value element exists in a this Results element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Roughness

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | Construction
attributes |
Name | Type | Use | Default | Fixed | annotation
value | roughnessValueEnum | required |  |  |
annotation |
documentation
Roughness of the outside surface
source | <xsd:element name="Roughness"> <xsd:annotation> <xsd:documentation>Roughness of the outside surface</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:attribute name="value" type="roughnessValueEnum" use="required"/> </xsd:complexType> </xsd:element>

attribute Roughness/@value

type | roughnessValueEnum
properties |
isRef | 0
use | required
facets |
enumeration | VeryRough
enumeration | MediumRough
enumeration | Rough
enumeration | Smooth
enumeration | MediumSmooth
enumeration | VerySmooth
source | <xsd:attribute name="value" type="roughnessValueEnum" use="required"/>

element RTSParameters

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | HOutside
used by |
element | LoadCalcInputParameters
attributes |
Name | Type | Use | Default | Fixed | annotation
roofCTSType | roofCTSTypeEnum |  |  |  |
documentation
Specifies which Conduction Time Series to use for the roof. See Table 21, page 29.30, 2001 ASHRAE Handbook, Fundamentals volume. Only used if the construction is a roof and you are using the RTS calculation method.
wallCTSType | wallCTSTypeEnum |  |  |  |
documentation
Specifies which Conduction Time Series to use for the wall. See Table 20, page 29.28, 2001 ASHRAE Handbook, Fundamentals volume. Only used if the construction is a wall and you are using the RTS calculation method.
annotation |
documentation
Parameters required by RTS load calculation method, as described in pages 29.25 and following of the 2001 ASHRAE Handbook, Fundamentals volume. Ignore this element and all elements under it if you are not planning to use that method.
source | <xsd:element name="RTSParameters"> <xsd:annotation> <xsd:documentation>Parameters required by RTS load calculation method, as described in pages 29.25 and following of the 2001 ASHRAE Handbook, Fundamentals volume. Ignore this element and all elements under it if you are not planning to use that method.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice> <xsd:element ref="HOutside"/> </xsd:choice> <xsd:attribute name="roofCTSType" type="roofCTSTypeEnum"> <xsd:annotation> <xsd:documentation>Specifies which Conduction Time Series to use for the roof. See Table 21, page 29.30, 2001 ASHRAE Handbook, Fundamentals volume. Only used if the construction is a roof and you are using the RTS calculation method.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="wallCTSType" type="wallCTSTypeEnum"> <xsd:annotation> <xsd:documentation>Specifies which Conduction Time Series to use for the wall. See Table 20, page 29.28, 2001 ASHRAE Handbook, Fundamentals volume. Only used if the construction is a wall and you are using the RTS calculation method.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute RTSParameters/@roofCTSType

type | roofCTSTypeEnum
properties |
isRef | 0
facets |
enumeration | 1
enumeration | 2
enumeration | 3
enumeration | 4
enumeration | 5
enumeration | 6
enumeration | 7
enumeration | 8
enumeration | 9
enumeration | 10
enumeration | 11
enumeration | 12
enumeration | 13
enumeration | 14
enumeration | 15
enumeration | 16
enumeration | 17
enumeration | 18
enumeration | 19
annotation |
documentation
Specifies which Conduction Time Series to use for the roof. See Table 21, page 29.30, 2001 ASHRAE Handbook, Fundamentals volume. Only used if the construction is a roof and you are using the RTS calculation method.
source | <xsd:attribute name="roofCTSType" type="roofCTSTypeEnum"> <xsd:annotation> <xsd:documentation>Specifies which Conduction Time Series to use for the roof. See Table 21, page 29.30, 2001 ASHRAE Handbook, Fundamentals volume. Only used if the construction is a roof and you are using the RTS calculation method.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute RTSParameters/@wallCTSType

type | wallCTSTypeEnum
properties |
isRef | 0
facets |
enumeration | 1
enumeration | 2
enumeration | 3
enumeration | 4
enumeration | 5
enumeration | 6
enumeration | 7
enumeration | 8
enumeration | 9
enumeration | 10
enumeration | 11
enumeration | 12
enumeration | 13
enumeration | 14
enumeration | 15
enumeration | 16
enumeration | 17
enumeration | 18
enumeration | 19
enumeration | 20
enumeration | 21
enumeration | 22
enumeration | 23
enumeration | 24
enumeration | 25
enumeration | 26
enumeration | 27
enumeration | 28
enumeration | 29
enumeration | 30
enumeration | 31
enumeration | 32
enumeration | 33
enumeration | 34
enumeration | 35
annotation |
documentation
Specifies which Conduction Time Series to use for the wall. See Table 20, page 29.28, 2001 ASHRAE Handbook, Fundamentals volume. Only used if the construction is a wall and you are using the RTS calculation method.
source | <xsd:attribute name="wallCTSType" type="wallCTSTypeEnum"> <xsd:annotation> <xsd:documentation>Specifies which Conduction Time Series to use for the wall. See Table 20, page 29.28, 2001 ASHRAE Handbook, Fundamentals volume. Only used if the construction is a wall and you are using the RTS calculation method.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Schedule

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description YearSchedule
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
type | scheduleTypeEnum | required |  |  |
annotation |
documentation
List of year schedules that make up an entire calendar year.
source | <xsd:element name="Schedule"> <xsd:annotation> <xsd:documentation>List of year schedules that make up an entire calendar year.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="YearSchedule" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="type" type="scheduleTypeEnum" use="required"/> </xsd:complexType> </xsd:element>

attribute Schedule/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Schedule/@type

type | scheduleTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Temp
enumeration | Fraction
enumeration | OnOff
source | <xsd:attribute name="type" type="scheduleTypeEnum" use="required"/>

element ScheduleValue

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | DaySchedule
annotation |
documentation
Value for one block of time. Divides a day evenly into number of ScheduleValue elements defined in DaySchedule. Example: If 12 ScheduleValue elements are defined, each will represent two hours
source | <xsd:element name="ScheduleValue" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Value for one block of time. Divides a day evenly into number of ScheduleValue elements defined in DaySchedule. Example: If 12 ScheduleValue elements are defined, each will represent two hours</xsd:documentation> </xsd:annotation> </xsd:element>

element Setback

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Opening
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | lengthUnitEnum |  |  |  |
annotation |
documentation
Distance from outside surface of window to outside surface of wall
source | <xsd:element name="Setback"> <xsd:annotation> <xsd:documentation>Distance from outside surface of window to outside surface of wall</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="lengthUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Setback/@unit

type | lengthUnitEnum
properties |
isRef | 0
facets |
enumeration | Kilometers
enumeration | Meters
enumeration | Centimeters
enumeration | Millimeters
enumeration | Miles
enumeration | Yards
enumeration | Feet
enumeration | Inches
source | <xsd:attribute name="unit" type="lengthUnitEnum"/>

element ShadeControl

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | ShadeSchedule SolarOnOpening HorizontalSolar AirTemperature ZoneCoolingLoad Glare
used by |
element | Opening
attributes |
Name | Type | Use | Default | Fixed | annotation
type | shadeTypeEnum | required |  |  |
source | <xsd:element name="ShadeControl"> <xsd:complexType> <xsd:annotation> <xsd:documentation>The ShadeControl element is a bit complex, as shading control is handled differently in different simulation engines. Each child of ShadeControl represents a criteria to help determine if the shades will be open or closed. The resulting shade action should be a union of these. Example: You have included a ShadeSchedule, which is a 1 on weekdays and a 0 on weekends, and a SolarOnOpening. The shade will be drawn when the solar radiation on this opening is greater than SolarOnOpening and it is a weekday.</xsd:documentation> </xsd:annotation> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="ShadeSchedule" minOccurs="0"/> <xsd:element ref="SolarOnOpening" minOccurs="0"/> <xsd:element ref="HorizontalSolar" minOccurs="0"/> <xsd:element ref="AirTemperature" minOccurs="0"/> <xsd:element ref="ZoneCoolingLoad" minOccurs="0"/> <xsd:element ref="Glare" minOccurs="0"/> </xsd:choice> <xsd:attribute name="type" type="shadeTypeEnum" use="required"/> </xsd:complexType> </xsd:element>

attribute ShadeControl/@type

type | shadeTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | InteriorInsulated
enumeration | InteriorUnInsulated
enumeration | ExternalInsulated
enumeration | ExternalUnInsulated
source | <xsd:attribute name="type" type="shadeTypeEnum" use="required"/>

element ShadeSchedule

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | ShadeControl
attributes |
Name | Type | Use | Default | Fixed | annotation
scheduleIdRef | xsd:ID | required |  |  |
annotation |
documentation
Use this element to define schedules for a shade.
source | <xsd:element name="ShadeSchedule"> <xsd:annotation> <xsd:documentation>Use this element to define schedules for a shade.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:attribute name="scheduleIdRef" type="xsd:ID" use="required"/> </xsd:complexType> </xsd:element>

attribute ShadeSchedule/@scheduleIdRef

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="scheduleIdRef" type="xsd:ID" use="required"/>

element ShadingCoeff

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Opening WindowType
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | unitlessUnitEnum | required |  |  |
annotation |
documentation
Shading Coefficient: The ratio of total solar transmittance for the specified glazing system to the total solar transmittance for the standard reference glazing (1/8" clear).
source | <xsd:element name="ShadingCoeff"> <xsd:annotation> <xsd:documentation>Shading Coefficient: The ratio of total solar transmittance for the specified glazing system to the total solar transmittance for the standard reference glazing (1/8" clear).</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute ShadingCoeff/@unit

type | unitlessUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Percent
enumeration | Fraction
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element ShellGeometry

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description ClosedShell
used by |
elements | AirLoopEquipment Building Campus ExtEquip HydronicLoopEquipment IntEquip Lighting LightingControl LightingSystem Space Transportation Vegetation
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
unit | lengthUnitEnum |  | Meters |  |
annotation |
documentation
All data are global, with the assumption that positive Z is up, and if CADModelAzimuth is undefined or zero, positive X is East and positive Y is North. If CADModelAzimuth is defined it is the angle of positive Y to North, positive X is the vectorial product of Y and Z. If geometry is to be precise, use Longitude Latitude, and Elevation in the Location element to define the origin. Otherwise the origin is an arbitrary point. ShellGeometry is used to define a union of closed shells, where there is no intersection of any two of the given shells.
source | <xsd:element name="ShellGeometry"> <xsd:annotation> <xsd:documentation>All data are global, with the assumption that positive Z is up, and if CADModelAzimuth is undefined or zero, positive X is East and positive Y is North. If CADModelAzimuth is defined it is the angle of positive Y to North, positive X is the vectorial product of Y and Z. If geometry is to be precise, use Longitude Latitude, and Elevation in the Location element to define the origin. Otherwise the origin is an arbitrary point. ShellGeometry is used to define a union of closed shells, where there is no intersection of any two of the given shells.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="ClosedShell"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="unit" type="lengthUnitEnum" default="Meters"/> </xsd:complexType> </xsd:element>

attribute ShellGeometry/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute ShellGeometry/@unit

type | lengthUnitEnum
properties |
isRef | 0
default | Meters
facets |
enumeration | Kilometers
enumeration | Meters
enumeration | Centimeters
enumeration | Millimeters
enumeration | Miles
enumeration | Yards
enumeration | Feet
enumeration | Inches
source | <xsd:attribute name="unit" type="lengthUnitEnum" default="Meters"/>

element SinkRate

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | IndoorAirQuality
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | sinkRateUnitEnum | required |  |  |
source | <xsd:element name="SinkRate"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="sinkRateUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute SinkRate/@unit

type | sinkRateUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | PoundsPerHour
enumeration | KilogramsPerHour
enumeration | GramsPerHour
source | <xsd:attribute name="unit" type="sinkRateUnitEnum" use="required"/>

element SolarHeatGainCoeff

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Opening WindowType
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | unitlessUnitEnum | required |  |  |
annotation |
documentation
When element is a child of WindowType: The center of glass solar heat gain coefficient. When element is a child of Opening: The overall solar heat gain coefficient for the window assembly.
source | <xsd:element name="SolarHeatGainCoeff"> <xsd:annotation> <xsd:documentation>When element is a child of WindowType: The center of glass solar heat gain coefficient. When element is a child of Opening: The overall solar heat gain coefficient for the window assembly.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute SolarHeatGainCoeff/@unit

type | unitlessUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Percent
enumeration | Fraction
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element SolarOnOpening

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | ShadeControl
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | powerPerAreaUnitEnum | required |  |  |
annotation |
documentation
Amount of solar radiation striking the opening before a shade is closed.
source | <xsd:element name="SolarOnOpening"> <xsd:annotation> <xsd:documentation>Amount of solar radiation striking the opening before a shade is closed.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="powerPerAreaUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute SolarOnOpening/@unit

type | powerPerAreaUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | WattPerSquareMeter
enumeration | WattPerSquareFoot
source | <xsd:attribute name="unit" type="powerPerAreaUnitEnum" use="required"/>

element Space

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Lighting LightingControl InfiltrationFlow PeopleNumber PeopleHeatGain LightPowerPerArea EquipPowerPerArea Area Temperature Volume PlanarGeometry ShellGeometry AirLoopId HydronicLoopId MeterId IntEquipId CADObjectId TypeCode SpaceBoundary
used by |
element | Building
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
spaceType | spaceTypeEnum |  |  |  |
documentation
spaceType represents how a space is used.
appinfo
<xhtml:a href="http://206.55.31.90/cgi-bin/lpd/ShowSpaceTypes.pl">IfcPolyLoop</xhtml:a>, an IESNA and ASHRAE project for determining lighting power density for individual spaces.
zoneIdRef | xsd:IDREF |  |  |  |
scheduleIdRef | xsd:IDREF |  |  |  |
documentation
ID for the schedule of transmittance of a shading surface
lightScheduleIdRef | xsd:IDREF |  |  |  |
documentation
ID of the schedule for lights contained in this space
equipmentScheduleIdRef | xsd:IDREF |  |  |  |
documentation
ID for schedule of equipment use
peopleScheduleIdRef | xsd:IDREF |  |  |  |
documentation
ID for schedule of people in this space
conditionType | conditionTypeEnum |  |  |  |
buildingStoreyIdRef | xsd:IDREF |  |  |  |
documentation
ID for BuildingStorey this space is on.
ifcGUID | xsd:string | optional |  |  |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
annotation |
documentation
A space represents a volume enclosed by surfaces.
source | <xsd:element name="Space"> <xsd:annotation> <xsd:documentation>A space represents a volume enclosed by surfaces.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Lighting" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="LightingControl" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="InfiltrationFlow" minOccurs="0"/> <xsd:element ref="PeopleNumber" minOccurs="0"/> <xsd:element ref="PeopleHeatGain" minOccurs="0" maxOccurs="3"/> <xsd:element ref="LightPowerPerArea" minOccurs="0"/> <xsd:element ref="EquipPowerPerArea" minOccurs="0"/> <xsd:element ref="Area" minOccurs="0"/> <xsd:element ref="Temperature" minOccurs="0"/> <xsd:element ref="Volume" minOccurs="0"/> <xsd:element ref="PlanarGeometry" minOccurs="0"> <xsd:annotation> <xsd:documentation>Planar polygon that represents the perimeter of space and whose area is equal to the floor area of the space.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="ShellGeometry" minOccurs="0"> <xsd:annotation> <xsd:documentation>Use this element to define the shell of the space.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="AirLoopId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="HydronicLoopId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="MeterId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="IntEquipId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="CADObjectId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="TypeCode" minOccurs="0"/> <xsd:element ref="SpaceBoundary" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="spaceType" type="spaceTypeEnum"> <xsd:annotation> <xsd:documentation>spaceType represents how a space is used.</xsd:documentation> <xsd:appinfo> <xhtml:a href="http://206.55.31.90/cgi-bin/lpd/ShowSpaceTypes.pl">IfcPolyLoop</xhtml:a>, an IESNA and ASHRAE project for determining lighting power density for individual spaces. </xsd:appinfo> </xsd:annotation> </xsd:attribute> <xsd:attribute name="zoneIdRef" type="xsd:IDREF"/> <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="lightScheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID of the schedule for lights contained in this space</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="equipmentScheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for schedule of equipment use</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="peopleScheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for schedule of people in this space</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="conditionType" type="conditionTypeEnum"/> <xsd:attribute name="buildingStoreyIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for BuildingStorey this space is on.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Space/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Space/@spaceType

type | spaceTypeEnum
properties |
isRef | 0
facets |
enumeration | ActiveStorage
enumeration | ActiveStorageHospitalOrHealthcare
enumeration | AirOrTrainOrBusBaggageArea
enumeration | AirportConcourse
enumeration | AtriumEachAdditionalFloor
enumeration | AtriumFirstThreeFloors
enumeration | AudienceOrSeatingAreaPenitentiary
enumeration | AudienceOrSeatingAreaExerciseCenter
enumeration | AudienceOrSeatingAreaGymnasium
enumeration | AudienceOrSeatingAreaSportsArena
enumeration | AudienceOrSeatingAreaConventionCenter
enumeration | AudienceOrSeatingAreaMotionPictureTheatre
enumeration | AudienceOrSeatingAreaPerformingArtsTheatre
enumeration | AudienceOrSeatingAreaReligious
enumeration | AudienceOrSeatingAreaPoliceOrFireStations
enumeration | AudienceOrSeatingAreaCourtHouse
enumeration | AudienceOrSeatingAreaAuditorium
enumeration | BankCustomerArea
enumeration | BankingActivityAreaOffice
enumeration | BarberAndBeautyParlor
enumeration | CardFileAndCataloguingLibrary
enumeration | ClassroomOrLectureOrTrainingPenitentiary
enumeration | ClassroomOrLectureOrTraining
enumeration | ComfinementCellsPenitentiary
enumeration | ComfinementCellsCourtHouse
enumeration | ConferenceMeetingOrMultipurpose
enumeration | CorridorOrTransition
enumeration | CorridorOrTransitionManufacturingFacility
enumeration | CorridorsWithPatientWaitingExamHospitalOrHealthcare
enumeration | CourtSportsAreaSportsArena
enumeration | CourtroomCourtHouse
enumeration | DepartmentStoreSalesAreaRetail
enumeration | DetailedManufacturingFacility
enumeration | DiningArea
enumeration | DiningAreaHotel
enumeration | DiningAreaFamilyDining
enumeration | DiningAreaLoungeOrLeisureDining
enumeration | DiningAreaMotel
enumeration | DiningAreaTransportation
enumeration | DiningAreaPenitentiary
enumeration | DiningAreaCivilServices
enumeration | DormitoryBedroom
enumeration | DormitoryStudyHall
enumeration | DressingOrLockerOrFittingRoomGymnasium
enumeration | DressingOrLockerOrFittingRoomCourtHouse
enumeration | DressingOrLockerOrFittingRoomPerformingArtsTheatre
enumeration | DressingOrLockerOrFittingRoomAuditorium
enumeration | DressingOrLockerOrFittingRoomExerciseCenter
enumeration | ElectricalOrMechanical
enumeration | ElevatorLobbies
enumeration | EmergencyHospitalOrHealthcare
enumeration | EquipmentRoomManufacturingFacility
enumeration | ExamOrTreatmentHospitalOrHealthcare
enumeration | ExcerciseAreaExerciseCenter
enumeration | ExcerciseAreaGymnasium
enumeration | ExhibitSpaceConventionCenter
enumeration | FellowshipHallReligiousBuildings
enumeration | FineMaterialWarehouse
enumeration | FineMerchandiseSalesAreaRetail
enumeration | FireStationEngineRoomPoliceOrFireStation
enumeration | FoodPreparation
enumeration | GarageServiceOrRepairAutomotiveFacility
enumeration | GeneralHighBayManufacturingFacility
enumeration | GeneralLowBayManufacturingFacility
enumeration | GeneralExhibitionMuseum
enumeration | HospitalNurseryHospitalOrHealthcare
enumeration | HospitalOrMedicalSuppliesHospitalOrHealthcare
enumeration | HospitalOrRadiologyHospitalOrHealthcare
enumeration | HotelOrConferenceCenterConferenceOrMeeting
enumeration | InactiveStorage
enumeration | JudgesChambersCourtHouse
enumeration | LaboratoryOffice
enumeration | LaundryIroningAndSorting
enumeration | LaundryWashingHospitalOrHealthcare
enumeration | LibraryAudioVisualLibraryAudioVisual
enumeration | LivingQuartersDormitory
enumeration | LivingQuartersMotel
enumeration | LivingQuartersHotel
enumeration | Lobby
enumeration | LobbyReligiousBuildings
enumeration | LobbyMotionPictureTheatre
enumeration | LobbyAuditorium
enumeration | LobbyPerformingArtsTheatre
enumeration | LobbyPostOffice
enumeration | LobbyHotel
enumeration | LoungeOrRecreation
enumeration | MallConcourseSalesAreaRetail
enumeration | MassMerchandisingSalesAreaRetail
enumeration | MediumOrBulkyMaterialWarehouse
enumeration | MerchandisingSalesAreaRetail
enumeration | MuseumAndGalleryStorage
enumeration | NurseStationHospitalOrHealthcare
enumeration | OfficeEnclosed
enumeration | OfficeOpenPlan
enumeration | OfficeCommonActivityAreasInactiveStorage
enumeration | OperatingRoomHospitalOrHealthcare
enumeration | OtherTelevisedPlayingAreaSportsArena
enumeration | ParkingAreaAttendantOnlyParkingGarage
enumeration | ParkingAreaPedestrianParkingGarage
enumeration | PatientRoomHospitalOrHealthcare
enumeration | PersonalServicesSalesAreaRetail
enumeration | PharmacyHospitalOrHealthcare
enumeration | PhysicalTherapyHospitalOrHealthcare
enumeration | PlayingAreaGymnasium
enumeration | Plenum
enumeration | PoliceStationLaboratoryPoliceOrFireStations
enumeration | PublicAndStaffLoungeHospitalOrHealthcare
enumeration | ReadingAreaLibrary
enumeration | ReceptionOrWaitingTransportation
enumeration | ReceptionOrWaitingMotel
enumeration | ReceptionOrWaitingHotel
enumeration | RecoveryHospitalOrHealthcare
enumeration | RestorationMuseum
enumeration | Restrooms
enumeration | RingSportsAreaSportsArena
enumeration | SleepingQuartersPoliceOrFireStation
enumeration | SortingAreaPostOffice
enumeration | SpecialtyStoreSalesAreaRetail
enumeration | StacksLibrary
enumeration | StairsInactive
enumeration | Stairway
enumeration | SupermarketSalesAreaRetail
enumeration | TerminalTicketCounterTransportation
enumeration | WorkshopWorkshop
enumeration | WorshipPulpitChoirReligious
annotation |
documentation
spaceType represents how a space is used.
appinfo
<xhtml:a href="http://206.55.31.90/cgi-bin/lpd/ShowSpaceTypes.pl">IfcPolyLoop</xhtml:a>, an IESNA and ASHRAE project for determining lighting power density for individual spaces.
source | <xsd:attribute name="spaceType" type="spaceTypeEnum"> <xsd:annotation> <xsd:documentation>spaceType represents how a space is used.</xsd:documentation> <xsd:appinfo> <xhtml:a href="http://206.55.31.90/cgi-bin/lpd/ShowSpaceTypes.pl">IfcPolyLoop</xhtml:a>, an IESNA and ASHRAE project for determining lighting power density for individual spaces. </xsd:appinfo> </xsd:annotation> </xsd:attribute>

attribute Space/@zoneIdRef

type | xsd:IDREF
properties |
isRef | 0
source | <xsd:attribute name="zoneIdRef" type="xsd:IDREF"/>

attribute Space/@scheduleIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID for the schedule of transmittance of a shading surface
source | <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Space/@lightScheduleIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID of the schedule for lights contained in this space
source | <xsd:attribute name="lightScheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID of the schedule for lights contained in this space</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Space/@equipmentScheduleIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID for schedule of equipment use
source | <xsd:attribute name="equipmentScheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for schedule of equipment use</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Space/@peopleScheduleIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID for schedule of people in this space
source | <xsd:attribute name="peopleScheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for schedule of people in this space</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Space/@conditionType

type | conditionTypeEnum
properties |
isRef | 0
facets |
enumeration | Heated
enumeration | Cooled
enumeration | HeatedAndCooled
enumeration | Unconditioned
enumeration | Vented
enumeration | NaturallyVentedOnly
source | <xsd:attribute name="conditionType" type="conditionTypeEnum"/>

attribute Space/@buildingStoreyIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID for BuildingStorey this space is on.
source | <xsd:attribute name="buildingStoreyIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for BuildingStorey this space is on.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Space/@ifcGUID

type | xsd:string
properties |
isRef | 0
use | optional
annotation |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
source | <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element SpaceBoundary

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | PlanarGeometry
used by |
element | Space
attributes |
Name | Type | Use | Default | Fixed | annotation
ifcGUID | xsd:string | optional |  |  |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
isSecondLevelBoundary | xsd:boolean | optional |  |  |
documentation
If this attribute is set to true, the boundary is important in heat flow calculation.
surfaceIdRef | xsd:IDREF | optional |  |  |
documentation
Connects the space boundary to a surface representing a building element (or representing the open air).
annotation |
documentation
This element establishes the logical relation of a given part of the space geometry to the building constructions through its surfaceIdRef attribute. One Surface may be referenced by more space boundaries of one space.
source | <xsd:element name="SpaceBoundary"> <xsd:annotation> <xsd:documentation>This element establishes the logical relation of a given part of the space geometry to the building constructions through its surfaceIdRef attribute. One Surface may be referenced by more space boundaries of one space.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice> <xsd:element ref="PlanarGeometry"/> </xsd:choice> <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="isSecondLevelBoundary" type="xsd:boolean" use="optional"> <xsd:annotation> <xsd:documentation>If this attribute is set to true, the boundary is important in heat flow calculation.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="surfaceIdRef" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Connects the space boundary to a surface representing a building element (or representing the open air).</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute SpaceBoundary/@ifcGUID

type | xsd:string
properties |
isRef | 0
use | optional
annotation |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
source | <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute SpaceBoundary/@isSecondLevelBoundary

type | xsd:boolean
properties |
isRef | 0
use | optional
annotation |
documentation
If this attribute is set to true, the boundary is important in heat flow calculation.
source | <xsd:attribute name="isSecondLevelBoundary" type="xsd:boolean" use="optional"> <xsd:annotation> <xsd:documentation>If this attribute is set to true, the boundary is important in heat flow calculation.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute SpaceBoundary/@surfaceIdRef

type | xsd:IDREF
properties |
isRef | 0
use | optional
annotation |
documentation
Connects the space boundary to a surface representing a building element (or representing the open air).
source | <xsd:attribute name="surfaceIdRef" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Connects the space boundary to a surface representing a building element (or representing the open air).</xsd:documentation> </xsd:annotation> </xsd:attribute>

element SpecificHeat

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Material
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | specificHeatUnitEnum | required |  |  |
source | <xsd:element name="SpecificHeat"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="specificHeatUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute SpecificHeat/@unit

type | specificHeatUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | JPerKgK
enumeration | BTUPerLbF
source | <xsd:attribute name="unit" type="specificHeatUnitEnum" use="required"/>

element StateOrProvince

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | Weather
source | <xsd:element name="StateOrProvince" type="xsd:string"/>

element StationId

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:string
properties |
content | complex
used by |
element | Location
attributes |
Name | Type | Use | Default | Fixed | annotation
IDType | stationIdTypeEnum |  |  |  |
source | <xsd:element name="StationId"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:string"> <xsd:attribute name="IDType" type="stationIdTypeEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute StationId/@IDType

type | stationIdTypeEnum
properties |
isRef | 0
facets |
enumeration | WMO
enumeration | WBAN
enumeration | ICAO
enumeration | NWSLI
enumeration | FAACallSign
enumeration | COOP
source | <xsd:attribute name="IDType" type="stationIdTypeEnum"/>

element StreetAddress

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | Building
source | <xsd:element name="StreetAddress" type="xsd:string"/>

element Surface

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description AdjacentSpaceId RectangularGeometry PlanarGeometry Opening CADObjectId
used by |
element | Campus
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
surfaceType | surfaceTypeEnum | required |  |  |
constructionIdRef | xsd:IDREF |  |  |  |
documentation
Identifier pointing to a construction
scheduleShadeIdRef | xsd:IDREF |  |  |  |
documentation
ID for the schedule of transmittance of a shading surface
exposedToSun | xsd:boolean |  | true |  |
documentation
This attribute specifies whether or not direct beam radiation from the sun will ever hit this surface. Only relevant to exterior surface types.
ifcGUID | xsd:string | optional |  |  |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
source | <xsd:element name="Surface"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="AdjacentSpaceId" minOccurs="0" maxOccurs="2"> <xsd:annotation> <xsd:documentation>First AdjacentSpaceId entered will determine how the referenced construction layers are ordered with the first construction layer being in contact with the outside or 2nd space listed and the last layer in contact with the first space listed. </xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="RectangularGeometry"/> <xsd:element ref="PlanarGeometry"/> <xsd:element ref="Opening" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="CADObjectId" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="surfaceType" type="surfaceTypeEnum" use="required"/> <xsd:attribute name="constructionIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Identifier pointing to a construction</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="scheduleShadeIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="exposedToSun" type="xsd:boolean" default="true"> <xsd:annotation> <xsd:documentation>This attribute specifies whether or not direct beam radiation from the sun will ever hit this surface. Only relevant to exterior surface types.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Surface/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Surface/@surfaceType

type | surfaceTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | InteriorWall
enumeration | ExteriorWall
enumeration | Roof
enumeration | InteriorFloor
enumeration | Shade
enumeration | UndergroundWall
enumeration | UndergroundSlab
enumeration | Ceiling
enumeration | Air
enumeration | UndergroundCeiling
enumeration | RaisedFloor
enumeration | SlabOnGrade
enumeration | FreestandingColumn
enumeration | EmbeddedColumn
source | <xsd:attribute name="surfaceType" type="surfaceTypeEnum" use="required"/>

attribute Surface/@constructionIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
Identifier pointing to a construction
source | <xsd:attribute name="constructionIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Identifier pointing to a construction</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Surface/@scheduleShadeIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID for the schedule of transmittance of a shading surface
source | <xsd:attribute name="scheduleShadeIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Surface/@exposedToSun

type | xsd:boolean
properties |
isRef | 0
default | true
annotation |
documentation
This attribute specifies whether or not direct beam radiation from the sun will ever hit this surface. Only relevant to exterior surface types.
source | <xsd:attribute name="exposedToSun" type="xsd:boolean" default="true"> <xsd:annotation> <xsd:documentation>This attribute specifies whether or not direct beam radiation from the sun will ever hit this surface. Only relevant to exterior surface types.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Surface/@ifcGUID

type | xsd:string
properties |
isRef | 0
use | optional
annotation |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
source | <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Temp

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | AirLoopEquipment HydronicLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | temperatureUnitEnum |  |  |  |
tempType | tempTypeEnum | required |  |  |
annotation |
documentation
Temperature
source | <xsd:element name="Temp"> <xsd:annotation> <xsd:documentation>Temperature</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> <xsd:attribute name="tempType" type="tempTypeEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Temp/@unit

type | temperatureUnitEnum
properties |
isRef | 0
facets |
enumeration | F
enumeration | C
enumeration | K
enumeration | R
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

attribute Temp/@tempType

type | tempTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Max
enumeration | Min
enumeration | Design
enumeration | CoolDesign
enumeration | HeatDesign
enumeration | Throttle
enumeration | Range
enumeration | Approach
enumeration | EnteringWetBulb
enumeration | LeavingDryBulb
enumeration | EnteringDryBulb
enumeration | LeavingWetBulb
enumeration | ChilledWaterSupply
enumeration | CondenserWaterSupply
enumeration | LeavingChilledWater
enumeration | LeavingCondenserWater
source | <xsd:attribute name="tempType" type="tempTypeEnum" use="required"/>

element Temperature

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | CDD HDD Space
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | temperatureUnitEnum |  |  |  |
source | <xsd:element name="Temperature"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Temperature/@unit

type | temperatureUnitEnum
properties |
isRef | 0
facets |
enumeration | F
enumeration | C
enumeration | K
enumeration | R
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element TemperatureControl

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | DesignTemp MinTemp MaxTemp
used by |
elements | AirLoop HydronicLoop
annotation |
documentation
Use this element to describe how the temperature is controlled. The temperatures specified in this element should be measured just upstream of the most critical piece of equipment (air handlers for a chilled water and hot water loops the chiller for the cooling water loop).
source | <xsd:element name="TemperatureControl"> <xsd:annotation> <xsd:documentation>Use this element to describe how the temperature is controlled. The temperatures specified in this element should be measured just upstream of the most critical piece of equipment (air handlers for a chilled water and hot water loops the chiller for the cooling water loop).</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="DesignTemp" minOccurs="0"/> <xsd:element ref="MinTemp" minOccurs="0"/> <xsd:element ref="MaxTemp" minOccurs="0"/> </xsd:choice> </xsd:complexType> </xsd:element>

element Thickness

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Blind Gap Glaze Material
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | lengthUnitEnum |  |  |  |
source | <xsd:element name="Thickness"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="lengthUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Thickness/@unit

type | lengthUnitEnum
properties |
isRef | 0
facets |
enumeration | Kilometers
enumeration | Meters
enumeration | Centimeters
enumeration | Millimeters
enumeration | Miles
enumeration | Yards
enumeration | Feet
enumeration | Inches
source | <xsd:attribute name="unit" type="lengthUnitEnum"/>

element Tilt

diagram |
namespace | http://www.gbxml.org/schema
type | restriction of xsd:double
properties |
content | simple
used by |
element | RectangularGeometry
facets |
minInclusive | 0
maxInclusive | 180
annotation |
documentation
The number of degrees from up that the outside of the surface is tilted in relation to the bottom-left corner.
source | <xsd:element name="Tilt"> <xsd:annotation> <xsd:documentation>The number of degrees from up that the outside of the surface is tilted in relation to the bottom-left corner.</xsd:documentation> </xsd:annotation> <xsd:simpleType> <xsd:restriction base="xsd:double"> <xsd:minInclusive value="0"/> <xsd:maxInclusive value="180"/> </xsd:restriction> </xsd:simpleType> </xsd:element>

element TimeIncrement

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
attributes |
Name | Type | Use | Default | Fixed | annotation
timeUnit | timeUnitEnum | required |  |  |
annotation |
documentation
Time or period that results represent. Example: if timeType = Month and TimeIncrement = 1 the Value would be for the month of January or if timeType = Hour and TimeIncrement = 4 the 81st the Value would be for January 14 at noon.
source | <xsd:element name="TimeIncrement"> <xsd:annotation> <xsd:documentation>Time or period that results represent. Example: if timeType = Month and TimeIncrement = 1 the Value would be for the month of January or if timeType = Hour and TimeIncrement = 4 the 81st the Value would be for January 14 at noon.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="timeUnit" type="timeUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute TimeIncrement/@timeUnit

type | timeUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Year
enumeration | Month
enumeration | Week
enumeration | Day
enumeration | Hour
enumeration | Minute
source | <xsd:attribute name="timeUnit" type="timeUnitEnum" use="required"/>

element Transmittance

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Blind Construction Glaze Opening WindowType
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | unitlessUnitEnum | required |  |  |
type | radiationWavelengthTypeEnum | required |  |  |
annotation |
documentation
Transmittance of shading surface
source | <xsd:element name="Transmittance"> <xsd:annotation> <xsd:documentation>Transmittance of shading surface</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> <xsd:attribute name="type" type="radiationWavelengthTypeEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Transmittance/@unit

type | unitlessUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Percent
enumeration | Fraction
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

attribute Transmittance/@type

type | radiationWavelengthTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Solar
enumeration | IR
enumeration | Visible
source | <xsd:attribute name="type" type="radiationWavelengthTypeEnum" use="required"/>

element Transportation

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | GeneralGeometry ShellGeometry Cost
used by |
element | Campus
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
transportationType | transportationTypeEnum | required |  |  |
scheduleIdRef | xsd:IDREF |  |  |  |
documentation
ID for the schedule of transmittance of a shading surface
annotation |
documentation
Public transportation
source | <xsd:element name="Transportation"> <xsd:annotation> <xsd:documentation>Public transportation</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="GeneralGeometry" minOccurs="0"/> <xsd:element ref="ShellGeometry" minOccurs="0"/> <xsd:element ref="Cost" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="transportationType" type="transportationTypeEnum" use="required"/> <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Transportation/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Transportation/@transportationType

type | transportationTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Bus
enumeration | Train
enumeration | Car
enumeration | LightRail
enumeration | Ferry
enumeration | Airplane
enumeration | Monorail
enumeration | Bike
source | <xsd:attribute name="transportationType" type="transportationTypeEnum" use="required"/>

attribute Transportation/@scheduleIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID for the schedule of transmittance of a shading surface
source | <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute>

element TypeCode

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
elements | Space Zone
annotation |
documentation
User/project defined Code for Space or Zone.
source | <xsd:element name="TypeCode" type="xsd:string"> <xsd:annotation> <xsd:documentation>User/project defined Code for Space or Zone.</xsd:documentation> </xsd:annotation> </xsd:element>

element U-value

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Construction Opening WindowType
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | uValueUnitEnum | required |  |  |
annotation |
documentation
Overall conductance
source | <xsd:element name="U-value"> <xsd:annotation> <xsd:documentation>Overall conductance</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="uValueUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute U-value/@unit

type | uValueUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | WPerSquareMeterK
enumeration | BtuPerHourSquareFtF
source | <xsd:attribute name="unit" type="uValueUnitEnum" use="required"/>

element UtilityRate

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | Meter
annotation |
documentation
We have left the UtilityRate element open to allow for use with billing schemas.
source | <xsd:element name="UtilityRate"> <xsd:annotation> <xsd:documentation>We have left the UtilityRate element open to allow for use with billing schemas.</xsd:documentation> </xsd:annotation> <xsd:complexType/> </xsd:element>

element Value

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Results
annotation |
documentation
Contains the actual numerical result value. If series result type each Value element contains the one value and is in sequential order for the series.
source | <xsd:element name="Value" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Contains the actual numerical result value. If series result type each Value element contains the one value and is in sequential order for the series.</xsd:documentation> </xsd:annotation> </xsd:element>

element Vegetation

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | GeneralGeometry ShellGeometry WaterRate Cost
used by |
element | Campus
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
vegetationType | vegetationTypeEnum | required |  |  |
waterScheduleIdRef | xsd:IDREF |  |  |  |
waterMeterIdRef | xsd:IDREF |  |  |  |
shadeScheduleIdRef | xsd:IDREF |  |  |  |
documentation
Refers to a building-level surface.
annotation |
documentation
Plants, trees, etc. on a campus
source | <xsd:element name="Vegetation"> <xsd:annotation> <xsd:documentation>Plants, trees, etc. on a campus</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="GeneralGeometry" minOccurs="0"/> <xsd:element ref="ShellGeometry" minOccurs="0"/> <xsd:element ref="WaterRate" minOccurs="0"/> <xsd:element ref="Cost" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="vegetationType" type="vegetationTypeEnum" use="required"/> <xsd:attribute name="waterScheduleIdRef" type="xsd:IDREF"/> <xsd:attribute name="waterMeterIdRef" type="xsd:IDREF"/> <xsd:attribute name="shadeScheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Refers to a building-level surface.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Vegetation/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Vegetation/@vegetationType

type | vegetationTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Trees
enumeration | Bushes
enumeration | Plants
enumeration | Grass
enumeration | Moss
enumeration | EvergreenTrees
enumeration | EvergreenShrubs
enumeration | DeciduousTrees
enumeration | DeciduousShrubs
source | <xsd:attribute name="vegetationType" type="vegetationTypeEnum" use="required"/>

attribute Vegetation/@waterScheduleIdRef

type | xsd:IDREF
properties |
isRef | 0
source | <xsd:attribute name="waterScheduleIdRef" type="xsd:IDREF"/>

attribute Vegetation/@waterMeterIdRef

type | xsd:IDREF
properties |
isRef | 0
source | <xsd:attribute name="waterMeterIdRef" type="xsd:IDREF"/>

attribute Vegetation/@shadeScheduleIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
Refers to a building-level surface.
source | <xsd:attribute name="shadeScheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Refers to a building-level surface.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Version

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | ProgramInfo
source | <xsd:element name="Version" type="xsd:string"/>

element Viscosity

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Gap
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | viscosityUnitEnum | required |  |  |
source | <xsd:element name="Viscosity"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="viscosityUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Viscosity/@unit

type | viscosityUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | KgPerMSec
enumeration | PoundPerFootSec
source | <xsd:attribute name="unit" type="viscosityUnitEnum" use="required"/>

element ViscosityFofT

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Gap
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | viscosityFofTUnitEnum | required |  |  |
annotation |
documentation
Viscosity as a function of temperature
source | <xsd:element name="ViscosityFofT"> <xsd:annotation> <xsd:documentation>Viscosity as a function of temperature</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="viscosityFofTUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute ViscosityFofT/@unit

type | viscosityFofTUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | KgPerMSecK
enumeration | PoundPerFootSecF
source | <xsd:attribute name="unit" type="viscosityFofTUnitEnum" use="required"/>

element Volume

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Space
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | volumeUnitEnum |  |  |  |
annotation |
documentation
Specifies the volume of the space. This value should be equal to the volume enclosed by the actual physical boundaries of the space, as defined by the volumetric model's interior surfaces bounding that space.
source | <xsd:element name="Volume"> <xsd:annotation> <xsd:documentation>Specifies the volume of the space. This value should be equal to the volume enclosed by the actual physical boundaries of the space, as defined by the volumetric model's interior surfaces bounding that space.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="volumeUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Volume/@unit

type | volumeUnitEnum
properties |
isRef | 0
facets |
enumeration | CubicKilometers
enumeration | CubicMeters
enumeration | CubicCentimeters
enumeration | CubicMillimeters
enumeration | CubicMiles
enumeration | CubicYards
enumeration | CubicFeet
enumeration | CubicInches
source | <xsd:attribute name="unit" type="volumeUnitEnum"/>

element WasteWaterHREff

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | ExtEquip IntEquip
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | unitlessUnitEnum | required |  |  |
airLoopIdRef | xsd:IDREF |  |  |  |
documentation
ID pointing to an air loop
hydronicLoopIdRef | xsd:IDREF |  |  |  |
documentation
ID pointing to a hydronic loop
annotation |
documentation
Waste water heat recovery efficiency
source | <xsd:element name="WasteWaterHREff"> <xsd:annotation> <xsd:documentation>Waste water heat recovery efficiency</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> <xsd:attribute name="airLoopIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID pointing to an air loop</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID pointing to a hydronic loop </xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute WasteWaterHREff/@unit

type | unitlessUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Percent
enumeration | Fraction
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

attribute WasteWaterHREff/@airLoopIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID pointing to an air loop
source | <xsd:attribute name="airLoopIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID pointing to an air loop</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute WasteWaterHREff/@hydronicLoopIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID pointing to a hydronic loop
source | <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID pointing to a hydronic loop </xsd:documentation> </xsd:annotation> </xsd:attribute>

element WaterLoss

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | AirLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | unitlessUnitEnum | required |  |  |
annotation |
documentation
This includes blowdown (draining a cooling tower to clean), drift (water loss from water sprayed), and evaporation in cooling towers.
source | <xsd:element name="WaterLoss"> <xsd:annotation> <xsd:documentation>This includes blowdown (draining a cooling tower to clean), drift (water loss from water sprayed), and evaporation in cooling towers.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute WaterLoss/@unit

type | unitlessUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Percent
enumeration | Fraction
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element WaterRate

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Vegetation
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | flowUnitEnum | required |  |  |
source | <xsd:element name="WaterRate"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="flowUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute WaterRate/@unit

type | flowUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | CFM
enumeration | LPerSec
enumeration | CubicMPerHr
enumeration | GPM
enumeration | GPH
source | <xsd:attribute name="unit" type="flowUnitEnum" use="required"/>

element WaterUsePerCycle

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | ExtEquip IntEquip
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | waterUseUnitEnum | required |  |  |
annotation |
documentation
Amount of water used for water using equipment per cycle of operation.
source | <xsd:element name="WaterUsePerCycle"> <xsd:annotation> <xsd:documentation>Amount of water used for water using equipment per cycle of operation.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="waterUseUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute WaterUsePerCycle/@unit

type | waterUseUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | CubicMeters
enumeration | Gallons
enumeration | Tons
enumeration | Kilograms
enumeration | Liters
source | <xsd:attribute name="unit" type="waterUseUnitEnum" use="required"/>

element Weather

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description City StateOrProvince Country HDD CDD DDDBCool DDHiHrCool DDWBCool DDDBRangeCool DDLoHrCool DDPressureCool DDWindSpeedCool DDWindDirCool DDSkyClearnessCool DDRainCool DDSnowCool DDMonthCool DDDayCool DDDaylightCool DDGroundTCool DDDBHeat DDHiHrHeat DDWBHeat DDDBRangeHeat DDLoHrHeat DDPressureHeat DDWindSpeedHeat DDWindDirHeat DDSkyClearnessHeat DDRainHeat DDSnowHeat DDMonthHeat DDDayHeat DDDaylightHeat DDGroundTHeat GroundTemp Reference
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
source | <xsd:element name="Weather"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="City" minOccurs="0"/> <xsd:element ref="StateOrProvince" minOccurs="0"/> <xsd:element ref="Country" minOccurs="0"/> <xsd:element ref="HDD" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="CDD" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="DDDBCool" minOccurs="0"/> <xsd:element ref="DDHiHrCool" minOccurs="0"/> <xsd:element ref="DDWBCool" minOccurs="0"/> <xsd:element ref="DDDBRangeCool" minOccurs="0"/> <xsd:element ref="DDLoHrCool" minOccurs="0"/> <xsd:element ref="DDPressureCool" minOccurs="0"/> <xsd:element ref="DDWindSpeedCool" minOccurs="0"/> <xsd:element ref="DDWindDirCool" minOccurs="0"/> <xsd:element ref="DDSkyClearnessCool" minOccurs="0"/> <xsd:element ref="DDRainCool" minOccurs="0"/> <xsd:element ref="DDSnowCool" minOccurs="0"/> <xsd:element ref="DDMonthCool" minOccurs="0"/> <xsd:element ref="DDDayCool" minOccurs="0"/> <xsd:element ref="DDDaylightCool" minOccurs="0"/> <xsd:element ref="DDGroundTCool" minOccurs="0"/> <xsd:element ref="DDDBHeat" minOccurs="0"/> <xsd:element ref="DDHiHrHeat" minOccurs="0"/> <xsd:element ref="DDWBHeat" minOccurs="0"/> <xsd:element ref="DDDBRangeHeat" minOccurs="0"/> <xsd:element ref="DDLoHrHeat" minOccurs="0"/> <xsd:element ref="DDPressureHeat" minOccurs="0"/> <xsd:element ref="DDWindSpeedHeat" minOccurs="0"/> <xsd:element ref="DDWindDirHeat" minOccurs="0"/> <xsd:element ref="DDSkyClearnessHeat" minOccurs="0"/> <xsd:element ref="DDRainHeat" minOccurs="0"/> <xsd:element ref="DDSnowHeat" minOccurs="0"/> <xsd:element ref="DDMonthHeat" minOccurs="0"/> <xsd:element ref="DDDayHeat" minOccurs="0"/> <xsd:element ref="DDDaylightHeat" minOccurs="0"/> <xsd:element ref="DDGroundTHeat" minOccurs="0"/> <xsd:element ref="GroundTemp" minOccurs="0"/> <xsd:element ref="Reference" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> </xsd:complexType> </xsd:element>

attribute Weather/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

element WebPage

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | PersonInfo
source | <xsd:element name="WebPage" type="xsd:string"/>

element WeekSchedule

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Day
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
type | scheduleTypeEnum | required |  |  |
annotation |
documentation
Set of day schedules all assigned to a unique particular period of the week using the day type attribute. Do not schedule conflicting day types to the same week schedule.
source | <xsd:element name="WeekSchedule"> <xsd:annotation> <xsd:documentation>Set of day schedules all assigned to a unique particular period of the week using the day type attribute. Do not schedule conflicting day types to the same week schedule.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Day" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="type" type="scheduleTypeEnum" use="required"/> </xsd:complexType> </xsd:element>

attribute WeekSchedule/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute WeekSchedule/@type

type | scheduleTypeEnum
properties |
isRef | 0
use | required
facets |
enumeration | Temp
enumeration | Fraction
enumeration | OnOff
source | <xsd:attribute name="type" type="scheduleTypeEnum" use="required"/>

element WeekScheduleId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | YearSchedule
attributes |
Name | Type | Use | Default | Fixed | annotation
weekScheduleIdRef | xsd:IDREF | required |  |  |
source | <xsd:element name="WeekScheduleId"> <xsd:complexType> <xsd:attribute name="weekScheduleIdRef" type="xsd:IDREF" use="required"/> </xsd:complexType> </xsd:element>

attribute WeekScheduleId/@weekScheduleIdRef

type | xsd:IDREF
properties |
isRef | 0
use | required
source | <xsd:attribute name="weekScheduleIdRef" type="xsd:IDREF" use="required"/>

element Weight

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | AirLoopEquipment HydronicLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | weightUnitEnum | required |  |  |
source | <xsd:element name="Weight"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="weightUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Weight/@unit

type | weightUnitEnum
properties |
isRef | 0
use | required
facets |
enumeration | Pounds
enumeration | Kilograms
enumeration | Tons
source | <xsd:attribute name="unit" type="weightUnitEnum" use="required"/>

element Width

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Dimensions Frame RectangularGeometry
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | lengthUnitEnum |  |  |  |
source | <xsd:element name="Width"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="lengthUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Width/@unit

type | lengthUnitEnum
properties |
isRef | 0
facets |
enumeration | Kilometers
enumeration | Meters
enumeration | Centimeters
enumeration | Millimeters
enumeration | Miles
enumeration | Yards
enumeration | Feet
enumeration | Inches
source | <xsd:attribute name="unit" type="lengthUnitEnum"/>

element WindowType

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description U-value ShadingCoeff SolarHeatGainCoeff Transmittance Reflectance Emittance Blind Frame Gap Glaze Cost
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
DOELibIdRef | xsd:string |  |  |  |
documentation
Use this attribute to reference objects in the DOE2 library
annotation |
documentation
One WindowType should be created for each type of window. Create a Blind, Frame, and Cost for each OpeningType, and then add as many Glaze and Gaps as exist in the window. Place these Glaze and Gap elements in order from outside to inside. For instance, a two pane window will have Glaze Gap Glaze, where the first Glaze represents the outside surface.
source | <xsd:element name="WindowType"> <xsd:annotation> <xsd:documentation>One WindowType should be created for each type of window. Create a Blind, Frame, and Cost for each OpeningType, and then add as many Glaze and Gaps as exist in the window. Place these Glaze and Gap elements in order from outside to inside. For instance, a two pane window will have Glaze Gap Glaze, where the first Glaze represents the outside surface.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="U-value" minOccurs="0"/> <xsd:element ref="ShadingCoeff" minOccurs="0"/> <xsd:element ref="SolarHeatGainCoeff" minOccurs="0"/> <xsd:element ref="Transmittance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Reflectance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Emittance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Blind" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Frame" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Gap" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Glaze" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Cost" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute WindowType/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute WindowType/@DOELibIdRef

type | xsd:string
properties |
isRef | 0
annotation |
documentation
Use this attribute to reference objects in the DOE2 library
source | <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute>

element XAxis

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | xsd:string | required |  |  |
dataType | xsd:string | required |  |  |
source | <xsd:element name="XAxis"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name"/> <xsd:element ref="Description" minOccurs="0"/> </xsd:choice> <xsd:attribute name="unit" type="xsd:string" use="required"/> <xsd:attribute name="dataType" type="xsd:string" use="required"/> </xsd:complexType> </xsd:element>

attribute XAxis/@unit

type | xsd:string
properties |
isRef | 0
use | required
source | <xsd:attribute name="unit" type="xsd:string" use="required"/>

attribute XAxis/@dataType

type | xsd:string
properties |
isRef | 0
use | required
source | <xsd:attribute name="dataType" type="xsd:string" use="required"/>

element YAxis

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | xsd:string | required |  |  |
dataType | xsd:string | required |  |  |
source | <xsd:element name="YAxis"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name"/> <xsd:element ref="Description" minOccurs="0"/> </xsd:choice> <xsd:attribute name="unit" type="xsd:string" use="required"/> <xsd:attribute name="dataType" type="xsd:string" use="required"/> </xsd:complexType> </xsd:element>

attribute YAxis/@unit

type | xsd:string
properties |
isRef | 0
use | required
source | <xsd:attribute name="unit" type="xsd:string" use="required"/>

attribute YAxis/@dataType

type | xsd:string
properties |
isRef | 0
use | required
source | <xsd:attribute name="dataType" type="xsd:string" use="required"/>

element YearModeled

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:date
properties |
content | simple
used by |
element | Campus
annotation |
documentation
Year of simulation to use
source | <xsd:element name="YearModeled" type="xsd:date"> <xsd:annotation> <xsd:documentation>Year of simulation to use</xsd:documentation> </xsd:annotation> </xsd:element>

element YearSchedule

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description BeginDate EndDate WeekScheduleId
used by |
element | Schedule
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
annotation |
documentation
Set of week schedules all assigned for a particular time period during the year defined by the begin and end date elements. These must not span more than one calendar year.
source | <xsd:element name="YearSchedule"> <xsd:annotation> <xsd:documentation>Set of week schedules all assigned for a particular time period during the year defined by the begin and end date elements. These must not span more than one calendar year.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="BeginDate"/> <xsd:element ref="EndDate"/> <xsd:element ref="WeekScheduleId"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> </xsd:complexType> </xsd:element>

attribute YearSchedule/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

element ZipcodeOrPostalCode

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | Location
source | <xsd:element name="ZipcodeOrPostalCode" type="xsd:string"/>

element Zone

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Flow AirChangesPerHour FlowPerArea FlowPerPerson OAFlowPerArea OAFlowPerPerson DesignHeatT DesignCoolT IndoorAirQuality HydronicLoopId AirLoopId CADObjectId TypeCode
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | annotation
id | xsd:ID | required |  |  |
heatSchedIdRef | xsd:IDREF |  |  |  |
documentation
ID of heating schedule
coolSchedIdRef | xsd:IDREF |  |  |  |
documentation
Design temperature for cooling
outAirSchedIdRef | xsd:IDREF |  |  |  |
documentation
Outside air schedule ID
fanSchedIdRef | xsd:IDREF |  |  |  |
documentation
ID of the fan schedule for this zone
ifcGUID | xsd:string | optional |  |  |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
source | <xsd:element name="Zone"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Flow" minOccurs="0"/> <xsd:element ref="AirChangesPerHour" minOccurs="0"/> <xsd:element ref="FlowPerArea" minOccurs="0"/> <xsd:element ref="FlowPerPerson" minOccurs="0"/> <xsd:element ref="OAFlowPerArea" minOccurs="0"/> <xsd:element ref="OAFlowPerPerson" minOccurs="0"/> <xsd:element ref="DesignHeatT" minOccurs="0"/> <xsd:element ref="DesignCoolT" minOccurs="0"/> <xsd:element ref="IndoorAirQuality" minOccurs="0"/> <xsd:element ref="HydronicLoopId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="AirLoopId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="CADObjectId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="TypeCode" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="heatSchedIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID of heating schedule</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="coolSchedIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Design temperature for cooling</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="outAirSchedIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Outside air schedule ID</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="fanSchedIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID of the fan schedule for this zone</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Zone/@id

type | xsd:ID
properties |
isRef | 0
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Zone/@heatSchedIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID of heating schedule
source | <xsd:attribute name="heatSchedIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID of heating schedule</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Zone/@coolSchedIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
Design temperature for cooling
source | <xsd:attribute name="coolSchedIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Design temperature for cooling</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Zone/@outAirSchedIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
Outside air schedule ID
source | <xsd:attribute name="outAirSchedIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Outside air schedule ID</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Zone/@fanSchedIdRef

type | xsd:IDREF
properties |
isRef | 0
annotation |
documentation
ID of the fan schedule for this zone
source | <xsd:attribute name="fanSchedIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID of the fan schedule for this zone</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Zone/@ifcGUID

type | xsd:string
properties |
isRef | 0
use | optional
annotation |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
source | <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element ZoneCoolingLoad

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | ShadeControl
attributes |
Name | Type | Use | Default | Fixed | annotation
unit | loadUnitEnum |  |  |  |
annotation |
documentation
Minimum cooling load that triggers the shades to close
source | <xsd:element name="ZoneCoolingLoad"> <xsd:annotation> <xsd:documentation>Minimum cooling load that triggers the shades to close</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="loadUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute ZoneCoolingLoad/@unit

type | loadUnitEnum
properties |
isRef | 0
facets |
enumeration | BtuPerHour
enumeration | Watt
source | <xsd:attribute name="unit" type="loadUnitEnum"/>

simpleType absorptanceUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Absorptance/@type
facets |
enumeration | IntIR
enumeration | IntSolar
enumeration | IntVisible
enumeration | IntTotal
enumeration | ExtIR
enumeration | ExtSolar
enumeration | ExtVisible
enumeration | ExtTotal
source | <xsd:simpleType name="absorptanceUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="IntIR"/> <xsd:enumeration value="IntSolar"/> <xsd:enumeration value="IntVisible"/> <xsd:enumeration value="IntTotal"/> <xsd:enumeration value="ExtIR"/> <xsd:enumeration value="ExtSolar"/> <xsd:enumeration value="ExtVisible"/> <xsd:enumeration value="ExtTotal"/> </xsd:restriction> </xsd:simpleType>

simpleType airTemperatureTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | AirTemperature/@type
facets |
enumeration | Outside
enumeration | Zone
source | <xsd:simpleType name="airTemperatureTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Outside"/> <xsd:enumeration value="Zone"/> </xsd:restriction> </xsd:simpleType>

simpleType areaUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attributes | gbXML/@areaUnit Area/@unit
facets |
enumeration | SquareKilometers
enumeration | SquareMeters
enumeration | SquareCentimeters
enumeration | SquareMillimeters
enumeration | SquareMiles
enumeration | SquareYards
enumeration | SquareFeet
enumeration | SquareInches
source | <xsd:simpleType name="areaUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="SquareKilometers"/> <xsd:enumeration value="SquareMeters"/> <xsd:enumeration value="SquareCentimeters"/> <xsd:enumeration value="SquareMillimeters"/> <xsd:enumeration value="SquareMiles"/> <xsd:enumeration value="SquareYards"/> <xsd:enumeration value="SquareFeet"/> <xsd:enumeration value="SquareInches"/> </xsd:restriction> </xsd:simpleType>

simpleType blowerDoorUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | BlowerDoorValue/@unit
facets |
enumeration | ACH
enumeration | AirChangesPerHour
enumeration | SquareFeet
enumeration | SquareMeter
source | <xsd:simpleType name="blowerDoorUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="ACH"/> <xsd:enumeration value="AirChangesPerHour"/> <xsd:enumeration value="SquareFeet"/> <xsd:enumeration value="SquareMeter"/> </xsd:restriction> </xsd:simpleType>

simpleType buildingTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Building/@buildingType
facets |
enumeration | AutomotiveFacility
enumeration | ConventionCenter
enumeration | Courthouse
enumeration | DiningBarLoungeOrLeisure
enumeration | DiningCafeteriaFastFood
enumeration | DiningFamily
enumeration | Dormitory
enumeration | ExerciseCenter
enumeration | FireStation
enumeration | Gymnasium
enumeration | HospitalOrHealthcare
enumeration | Hotel
enumeration | Library
enumeration | Manufacturing
enumeration | Motel
enumeration | MotionPictureTheatre
enumeration | MultiFamily
enumeration | Museum
enumeration | Office
enumeration | ParkingGarage
enumeration | Penitentiary
enumeration | PerformingArtsTheater
enumeration | PoliceStation
enumeration | PostOffice
enumeration | ReligiousBuilding
enumeration | Retail
enumeration | SchoolOrUniversity
enumeration | SingleFamily
enumeration | SportsArena
enumeration | TownHall
enumeration | Transportation
enumeration | Unknown
enumeration | Warehouse
enumeration | Workshop
annotation |
documentation
Use to specify the most predominant building use type.
source | <xsd:simpleType name="buildingTypeEnum"> <xsd:annotation> <xsd:documentation>Use to specify the most predominant building use type.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="AutomotiveFacility"/> <xsd:enumeration value="ConventionCenter"/> <xsd:enumeration value="Courthouse"/> <xsd:enumeration value="DiningBarLoungeOrLeisure"/> <xsd:enumeration value="DiningCafeteriaFastFood"/> <xsd:enumeration value="DiningFamily"/> <xsd:enumeration value="Dormitory"/> <xsd:enumeration value="ExerciseCenter"/> <xsd:enumeration value="FireStation"/> <xsd:enumeration value="Gymnasium"/> <xsd:enumeration value="HospitalOrHealthcare"/> <xsd:enumeration value="Hotel"/> <xsd:enumeration value="Library"/> <xsd:enumeration value="Manufacturing"/> <xsd:enumeration value="Motel"/> <xsd:enumeration value="MotionPictureTheatre"/> <xsd:enumeration value="MultiFamily"/> <xsd:enumeration value="Museum"/> <xsd:enumeration value="Office"/> <xsd:enumeration value="ParkingGarage"/> <xsd:enumeration value="Penitentiary"/> <xsd:enumeration value="PerformingArtsTheater"/> <xsd:enumeration value="PoliceStation"/> <xsd:enumeration value="PostOffice"/> <xsd:enumeration value="ReligiousBuilding"/> <xsd:enumeration value="Retail"/> <xsd:enumeration value="SchoolOrUniversity"/> <xsd:enumeration value="SingleFamily"/> <xsd:enumeration value="SportsArena"/> <xsd:enumeration value="TownHall"/> <xsd:enumeration value="Transportation"/> <xsd:enumeration value="Unknown"> <xsd:annotation> <xsd:documentation>Enumeration value to be used when there is no building type information available.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Warehouse"/> <xsd:enumeration value="Workshop"/> </xsd:restriction> </xsd:simpleType>

simpleType capacityTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Capacity/@capacityType
facets |
enumeration | Heating
enumeration | CoolingTotal
enumeration | CoolingSensible
enumeration | CoolingLatent
enumeration | CoolingSHR
enumeration | Volume
source | <xsd:simpleType name="capacityTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Heating"/> <xsd:enumeration value="CoolingTotal"/> <xsd:enumeration value="CoolingSensible"/> <xsd:enumeration value="CoolingLatent"/> <xsd:enumeration value="CoolingSHR"/> <xsd:enumeration value="Volume"/> </xsd:restriction> </xsd:simpleType>

simpleType capacityUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Capacity/@unit
facets |
enumeration | Tons
enumeration | kW
enumeration | BtuPerHour
enumeration | kBtuPerHour
enumeration | Gallons
enumeration | Liters
enumeration | CubicMeters
enumeration | CubicFeet
source | <xsd:simpleType name="capacityUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Tons"/> <xsd:enumeration value="kW"/> <xsd:enumeration value="BtuPerHour"/> <xsd:enumeration value="kBtuPerHour"/> <xsd:enumeration value="Gallons"/> <xsd:enumeration value="Liters"/> <xsd:enumeration value="CubicMeters"/> <xsd:enumeration value="CubicFeet"/> </xsd:restriction> </xsd:simpleType>

simpleType conditioningTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attributes | DeltaP/@conditioningType DeltaT/@conditioningType Efficiency/@operationType
facets |
enumeration | Heating
enumeration | Cooling
enumeration | HeatingAndCooling
source | <xsd:simpleType name="conditioningTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Heating"/> <xsd:enumeration value="Cooling"/> <xsd:enumeration value="HeatingAndCooling"/> </xsd:restriction> </xsd:simpleType>

simpleType conditioningUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attributes | HighValue/@unit LowValue/@unit
facets |
enumeration | kBtu
enumeration | Btu
enumeration | kW
enumeration | Tons
source | <xsd:simpleType name="conditioningUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="kBtu"/> <xsd:enumeration value="Btu"/> <xsd:enumeration value="kW"/> <xsd:enumeration value="Tons"/> </xsd:restriction> </xsd:simpleType>

simpleType conditionTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Space/@conditionType
facets |
enumeration | Heated
enumeration | Cooled
enumeration | HeatedAndCooled
enumeration | Unconditioned
enumeration | Vented
enumeration | NaturallyVentedOnly
source | <xsd:simpleType name="conditionTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Heated"/> <xsd:enumeration value="Cooled"/> <xsd:enumeration value="HeatedAndCooled"/> <xsd:enumeration value="Unconditioned"/> <xsd:enumeration value="Vented"/> <xsd:enumeration value="NaturallyVentedOnly"/> </xsd:restriction> </xsd:simpleType>

simpleType conductivityFofTUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | ConductivityFofT/@unit
facets |
enumeration | WPerMSquareK
enumeration | BtuPerHourFtSquareF
source | <xsd:simpleType name="conductivityFofTUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="WPerMSquareK"/> <xsd:enumeration value="BtuPerHourFtSquareF"/> </xsd:restriction> </xsd:simpleType>

simpleType conductivityUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attributes | Conductivity/@unit GlazeConductivity/@unit
facets |
enumeration | WPerCmC
enumeration | WPerMeterK
enumeration | BtuPerHourFtF
source | <xsd:simpleType name="conductivityUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="WPerCmC"/> <xsd:enumeration value="WPerMeterK"/> <xsd:enumeration value="BtuPerHourFtF"/> </xsd:restriction> </xsd:simpleType>

simpleType controlTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Control/@controlType
facets |
enumeration | Fan
enumeration | Pump
enumeration | Valve
source | <xsd:simpleType name="controlTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Fan"/> <xsd:enumeration value="Pump"/> <xsd:enumeration value="Valve"/> </xsd:restriction> </xsd:simpleType>

simpleType costTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Cost/@costType
facets |
enumeration | CO2
enumeration | SOx
enumeration | NOx
enumeration | EmbodiedEnergyTransportation
enumeration | EmbodiedEnergyManufacture
enumeration | EmbodiedEnergyInstallation
enumeration | EmbodiedEnergyTotal
enumeration | PurchaseCost
enumeration | DeliveryCost
enumeration | FirstCost
enumeration | MonthlyCost
enumeration | AnnualCost
enumeration | MaintenanceCost
enumeration | OverhaulCost
enumeration | InstallationCost
source | <xsd:simpleType name="costTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="CO2"/> <xsd:enumeration value="SOx"/> <xsd:enumeration value="NOx"/> <xsd:enumeration value="EmbodiedEnergyTransportation"/> <xsd:enumeration value="EmbodiedEnergyManufacture"/> <xsd:enumeration value="EmbodiedEnergyInstallation"/> <xsd:enumeration value="EmbodiedEnergyTotal"/> <xsd:enumeration value="PurchaseCost"/> <xsd:enumeration value="DeliveryCost"/> <xsd:enumeration value="FirstCost"/> <xsd:enumeration value="MonthlyCost"/> <xsd:enumeration value="AnnualCost"/> <xsd:enumeration value="MaintenanceCost"/> <xsd:enumeration value="OverhaulCost"/> <xsd:enumeration value="InstallationCost"/> </xsd:restriction> </xsd:simpleType>

simpleType currencyTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attributes | CostValue/@currency Results/@currency
facets |
enumeration | USDollars
enumeration | CanadianDollars
enumeration | Pesos
enumeration | Euros
enumeration | Yen
enumeration | IndianRupee
enumeration | Yuan
enumeration | TaiwanDollar
enumeration | EnglishPound
enumeration | Mark
enumeration | Franc
enumeration | Ruble
enumeration | Real
enumeration | NewZealandDollar
enumeration | AustralianDollar
source | <xsd:simpleType name="currencyTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="USDollars"/> <xsd:enumeration value="CanadianDollars"/> <xsd:enumeration value="Pesos"/> <xsd:enumeration value="Euros"/> <xsd:enumeration value="Yen"/> <xsd:enumeration value="IndianRupee"/> <xsd:enumeration value="Yuan"/> <xsd:enumeration value="TaiwanDollar"/> <xsd:enumeration value="EnglishPound"/> <xsd:enumeration value="Mark"/> <xsd:enumeration value="Franc"/> <xsd:enumeration value="Ruble"/> <xsd:enumeration value="Real"/> <xsd:enumeration value="NewZealandDollar"/> <xsd:enumeration value="AustralianDollar"/> </xsd:restriction> </xsd:simpleType>

simpleType dayTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Day/@dayType
facets |
enumeration | Weekday
enumeration | Weekend
enumeration | Holiday
enumeration | WeekendOrHoliday
enumeration | HeatingDesignDay
enumeration | CoolingDesignDay
enumeration | Sun
enumeration | Mon
enumeration | Tue
enumeration | Wed
enumeration | Thu
enumeration | Fri
enumeration | Sat
enumeration | All
source | <xsd:simpleType name="dayTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Weekday"/> <xsd:enumeration value="Weekend"/> <xsd:enumeration value="Holiday"/> <xsd:enumeration value="WeekendOrHoliday"/> <xsd:enumeration value="HeatingDesignDay"/> <xsd:enumeration value="CoolingDesignDay"/> <xsd:enumeration value="Sun"/> <xsd:enumeration value="Mon"/> <xsd:enumeration value="Tue"/> <xsd:enumeration value="Wed"/> <xsd:enumeration value="Thu"/> <xsd:enumeration value="Fri"/> <xsd:enumeration value="Sat"/> <xsd:enumeration value="All"/> </xsd:restriction> </xsd:simpleType>

simpleType deltaPUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | DeltaP/@unit
facets |
enumeration | PSI
enumeration | kPa
enumeration | Atmospheres
enumeration | InchesOfH2O
enumeration | CentimetersOfH2O
enumeration | InchesOfMercury
enumeration | CentimetersOfMercury
enumeration | MillimetersOfMercury
enumeration | Pascals
source | <xsd:simpleType name="deltaPUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="PSI"/> <xsd:enumeration value="kPa"/> <xsd:enumeration value="Atmospheres"/> <xsd:enumeration value="InchesOfH2O"/> <xsd:enumeration value="CentimetersOfH2O"/> <xsd:enumeration value="InchesOfMercury"/> <xsd:enumeration value="CentimetersOfMercury"/> <xsd:enumeration value="MillimetersOfMercury"/> <xsd:enumeration value="Pascals"/> </xsd:restriction> </xsd:simpleType>

simpleType densityFofTUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | DensityFofT/@unit
facets |
enumeration | LbsPerCubicFtF
enumeration | KgPerCubicMK
source | <xsd:simpleType name="densityFofTUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="LbsPerCubicFtF"/> <xsd:enumeration value="KgPerCubicMK"/> </xsd:restriction> </xsd:simpleType>

simpleType densityUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Density/@unit
facets |
enumeration | GramsPerCubicCm
enumeration | LbsPerCubicIn
enumeration | LbsPerCubicFt
enumeration | KgPerCubicM
source | <xsd:simpleType name="densityUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="GramsPerCubicCm"/> <xsd:enumeration value="LbsPerCubicIn"/> <xsd:enumeration value="LbsPerCubicFt"/> <xsd:enumeration value="KgPerCubicM"/> </xsd:restriction> </xsd:simpleType>

simpleType directionUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attributes | DDWindDirCool/@unit DDWindDirHeat/@unit
facets |
enumeration | DegreeDecimalFromNorth
source | <xsd:simpleType name="directionUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="DegreeDecimalFromNorth"/> </xsd:restriction> </xsd:simpleType>

simpleType efficiencyTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Efficiency/@efficiencyType
facets |
enumeration | COP
enumeration | EER
enumeration | SEER
enumeration | AFUE
enumeration | HSPF
enumeration | effectiveness
enumeration | EnergyFactor
enumeration | ThermalEff
enumeration | MotorEff
enumeration | FanEff
enumeration | MechanicalEff
enumeration | BoilerEff
enumeration | kWPerTon
enumeration | kWPerkW
source | <xsd:simpleType name="efficiencyTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="COP"> <xsd:annotation> <xsd:documentation>Coefficient of Performance</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="EER"> <xsd:annotation> <xsd:documentation>Energy Efficiency Ratio</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="SEER"> <xsd:annotation> <xsd:documentation>Seasonal Energy Efficiency Ratio</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="AFUE"> <xsd:annotation> <xsd:documentation>Annual Fuel Utilization Efficiency</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="HSPF"> <xsd:annotation> <xsd:documentation>Heating Seasonal Performance Factor</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="effectiveness"/> <xsd:enumeration value="EnergyFactor"/> <xsd:enumeration value="ThermalEff"> <xsd:annotation> <xsd:documentation>Thermal Efficiency</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="MotorEff"> <xsd:annotation> <xsd:documentation>Motor Efficiency</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="FanEff"> <xsd:annotation> <xsd:documentation>Fan Efficiency</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="MechanicalEff"> <xsd:annotation> <xsd:documentation>Mechanical Efficiency</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="BoilerEff"> <xsd:annotation> <xsd:documentation>Boiler Efficiency</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="kWPerTon"/> <xsd:enumeration value="kWPerkW"/> </xsd:restriction> </xsd:simpleType>

simpleType emissionUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | EmissionRate/@unit
facets |
enumeration | PoundsPerHour
enumeration | KilogramsPerHour
enumeration | GramsPerHour
source | <xsd:simpleType name="emissionUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="PoundsPerHour"/> <xsd:enumeration value="KilogramsPerHour"/> <xsd:enumeration value="GramsPerHour"/> </xsd:restriction> </xsd:simpleType>

simpleType emittanceTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Emittance/@type
facets |
enumeration | IntIR
enumeration | ExtIR
source | <xsd:simpleType name="emittanceTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="IntIR"/> <xsd:enumeration value="ExtIR"/> </xsd:restriction> </xsd:simpleType>

simpleType energyUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
element | Results
attribute | Energy/@unit
facets |
enumeration | KilowattHours
enumeration | Joules
enumeration | BTU
enumeration | Therms
source | <xsd:simpleType name="energyUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="KilowattHours"/> <xsd:enumeration value="Joules"/> <xsd:enumeration value="BTU"/> <xsd:enumeration value="Therms"/> </xsd:restriction> </xsd:simpleType>

simpleType equipmentTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | AirLoopEquipment/@equipmentType
facets |
enumeration | Fan
enumeration | HeatExchanger
enumeration | Coil
enumeration | Furnace
enumeration | Evaporative
enumeration | Radiant
enumeration | Economizer
enumeration | Duct
enumeration | Humidifier
enumeration | Dehumidifier
enumeration | UnitaryAC
enumeration | UnitaryHP
enumeration | SplitAC
enumeration | SplitHP
enumeration | TerminalUnit
enumeration | Register
enumeration | VAVBox
source | <xsd:simpleType name="equipmentTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Fan"/> <xsd:enumeration value="HeatExchanger"/> <xsd:enumeration value="Coil"/> <xsd:enumeration value="Furnace"/> <xsd:enumeration value="Evaporative"/> <xsd:enumeration value="Radiant"/> <xsd:enumeration value="Economizer"/> <xsd:enumeration value="Duct"/> <xsd:enumeration value="Humidifier"/> <xsd:enumeration value="Dehumidifier"/> <xsd:enumeration value="UnitaryAC"/> <xsd:enumeration value="UnitaryHP"/> <xsd:enumeration value="SplitAC"/> <xsd:enumeration value="SplitHP"/> <xsd:enumeration value="TerminalUnit"/> <xsd:enumeration value="Register"/> <xsd:enumeration value="VAVBox"/> </xsd:restriction> </xsd:simpleType>

simpleType extEquipTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | ExtEquip/@type
facets |
enumeration | Sprinkler
enumeration | LawnMower
enumeration | GeneralPlugload
enumeration | Fountain
enumeration | Refrigerator
enumeration | Freezer
enumeration | Pool
enumeration | HotTub
enumeration | Pump
enumeration | Sauna
enumeration | BatteryCharger
enumeration | Furnace
enumeration | IndustrialEquip
enumeration | Irrigation
enumeration | MiscEquip
enumeration | Vending
enumeration | Elevator
enumeration | Escalator
source | <xsd:simpleType name="extEquipTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Sprinkler"/> <xsd:enumeration value="LawnMower"/> <xsd:enumeration value="GeneralPlugload"/> <xsd:enumeration value="Fountain"/> <xsd:enumeration value="Refrigerator"/> <xsd:enumeration value="Freezer"/> <xsd:enumeration value="Pool"/> <xsd:enumeration value="HotTub"/> <xsd:enumeration value="Pump"/> <xsd:enumeration value="Sauna"/> <xsd:enumeration value="BatteryCharger"/> <xsd:enumeration value="Furnace"/> <xsd:enumeration value="IndustrialEquip"/> <xsd:enumeration value="Irrigation"/> <xsd:enumeration value="MiscEquip"/> <xsd:enumeration value="Vending"/> <xsd:enumeration value="Elevator"/> <xsd:enumeration value="Escalator"/> </xsd:restriction> </xsd:simpleType>

simpleType floorCategoryEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | ManualJ8Parameters/@floorCategory
facets |
enumeration | OverEnclosedCrawlSpaceOrBasement
enumeration | OverOpenCrawlSpaceOrGarage
enumeration | Basement
enumeration | SlabOnGrade
annotation |
documentation
Used with the floorCategory attribute.
source | <xsd:simpleType name="floorCategoryEnum"> <xsd:annotation> <xsd:documentation>Used with the floorCategory attribute.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="OverEnclosedCrawlSpaceOrBasement"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="OverOpenCrawlSpaceOrGarage"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Basement"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="SlabOnGrade"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType floorSlabPerimeterHeatLossCoefficientUnitTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | FloorSlabHeatLossCoefficient/@floorSlabPerimeterHeatLossCoefficientUnitTypeEnum
facets |
enumeration | btuPerHourDegreeFPerLinearFoot
enumeration | wattDegreeCPerLinearMeter
annotation |
documentation
Used with the floorSlabPerimeterHeatLossCoefficientUnitType attribute.
source | <xsd:simpleType name="floorSlabPerimeterHeatLossCoefficientUnitTypeEnum"> <xsd:annotation> <xsd:documentation>Used with the floorSlabPerimeterHeatLossCoefficientUnitType attribute.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="btuPerHourDegreeFPerLinearFoot"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="wattDegreeCPerLinearMeter"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType flowPerAreaUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attributes | FlowPerArea/@unit OAFlowPerArea/@unit
facets |
enumeration | CFMPerSquareFoot
enumeration | LPerSecPerSquareM
enumeration | CubicMPerSecPerSquareM
source | <xsd:simpleType name="flowPerAreaUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="CFMPerSquareFoot"/> <xsd:enumeration value="LPerSecPerSquareM"/> <xsd:enumeration value="CubicMPerSecPerSquareM"/> </xsd:restriction> </xsd:simpleType>

simpleType flowUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
elements | MinFlow Results
attributes | Flow/@unit FlowPerPerson/@unit OAFlowPerPerson/@unit PeakDomesticHotWaterFlow/@unit RatedFlow/@unit WaterRate/@unit
facets |
enumeration | CFM
enumeration | LPerSec
enumeration | CubicMPerHr
enumeration | GPM
enumeration | GPH
source | <xsd:simpleType name="flowUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="CFM"/> <xsd:enumeration value="LPerSec"/> <xsd:enumeration value="CubicMPerHr"/> <xsd:enumeration value="GPM"/> <xsd:enumeration value="GPH"/> </xsd:restriction> </xsd:simpleType>

simpleType fluidTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | HydronicLoop/@fluidType
facets |
enumeration | Water
enumeration | Brine
enumeration | Glycol
source | <xsd:simpleType name="fluidTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Water"/> <xsd:enumeration value="Brine"/> <xsd:enumeration value="Glycol"/> </xsd:restriction> </xsd:simpleType>

simpleType frameTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Frame/@type
facets |
enumeration | Wood
enumeration | Vinyl
enumeration | Aluminum
enumeration | AluminumWithBreak
enumeration | Insulated
source | <xsd:simpleType name="frameTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Wood"/> <xsd:enumeration value="Vinyl"/> <xsd:enumeration value="Aluminum"/> <xsd:enumeration value="AluminumWithBreak"/> <xsd:enumeration value="Insulated"/> </xsd:restriction> </xsd:simpleType>

simpleType fuelLoadUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | FuelLoad/@unit
facets |
enumeration | BtuPerHour
enumeration | kBtuPerHour
enumeration | MBtuPerHour
enumeration | Watts
enumeration | kW
source | <xsd:simpleType name="fuelLoadUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="BtuPerHour"/> <xsd:enumeration value="kBtuPerHour"/> <xsd:enumeration value="MBtuPerHour"/> <xsd:enumeration value="Watts"/> <xsd:enumeration value="kW"/> </xsd:restriction> </xsd:simpleType>

simpleType gasTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Gap/@gas
facets |
enumeration | Air
enumeration | Argon
enumeration | Krypton
enumeration | CO2
enumeration | SF6
enumeration | Custom
source | <xsd:simpleType name="gasTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Air"/> <xsd:enumeration value="Argon"/> <xsd:enumeration value="Krypton"/> <xsd:enumeration value="CO2"/> <xsd:enumeration value="SF6"/> <xsd:enumeration value="Custom"/> </xsd:restriction> </xsd:simpleType>

simpleType hOutsideUnitTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | HOutside/@hOutsideUnitTypeEnum
facets |
enumeration | BTUPerHourSquareFootDegreeF
enumeration | WattsPerSecondSquareMeterDegreeC
annotation |
documentation
Used with the hOutsideUnitType attribute.
source | <xsd:simpleType name="hOutsideUnitTypeEnum"> <xsd:annotation> <xsd:documentation>Used with the hOutsideUnitType attribute.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="BTUPerHourSquareFootDegreeF"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="WattsPerSecondSquareMeterDegreeC"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType hydronicEquipTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | HydronicLoopEquipment/@equipmentType
facets |
enumeration | Chiller
enumeration | CoolingTower
enumeration | Condenser
enumeration | Boiler
enumeration | HeatExchanger
enumeration | Pump
enumeration | RadiantPanel
enumeration | HotWaterHeater
enumeration | SolarPanels
enumeration | Earth
enumeration | Pipe
enumeration | Storage
enumeration | Coil
source | <xsd:simpleType name="hydronicEquipTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Chiller"/> <xsd:enumeration value="CoolingTower"/> <xsd:enumeration value="Condenser"/> <xsd:enumeration value="Boiler"/> <xsd:enumeration value="HeatExchanger"/> <xsd:enumeration value="Pump"/> <xsd:enumeration value="RadiantPanel"/> <xsd:enumeration value="HotWaterHeater"/> <xsd:enumeration value="SolarPanels"/> <xsd:enumeration value="Earth"/> <xsd:enumeration value="Pipe"/> <xsd:enumeration value="Storage"/> <xsd:enumeration value="Coil"/> </xsd:restriction> </xsd:simpleType>

simpleType illuminanceUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
element | Results
attribute | Illuminance/@unit
facets |
enumeration | Footcandles
source | <xsd:simpleType name="illuminanceUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Footcandles"/> </xsd:restriction> </xsd:simpleType>

simpleType infiltrationTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | InfiltrationFlow/@type
facets |
enumeration | Loose
enumeration | Average
enumeration | Tight
source | <xsd:simpleType name="infiltrationTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Loose"/> <xsd:enumeration value="Average"/> <xsd:enumeration value="Tight"/> </xsd:restriction> </xsd:simpleType>

simpleType intEquipTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | IntEquip/@type
facets |
enumeration | GeneralPlugload
enumeration | Computer
enumeration | Copier
enumeration | Refrigerator
enumeration | Stove
enumeration | Cooktop
enumeration | Fryer
enumeration | Freezer
enumeration | ClothesDryer
enumeration | ClothesWasher
enumeration | Dishwasher
enumeration | TV
enumeration | VCR
enumeration | Microwave
enumeration | Fan
enumeration | AudioEquip
enumeration | MiscEquip
enumeration | Toilet
enumeration | Urinal
enumeration | Shower
enumeration | Sink
enumeration | Pool
enumeration | HotTub
enumeration | Sauna
enumeration | BatteryCharger
enumeration | Furnace
enumeration | IndustrialEquip
enumeration | Printer
enumeration | Vending
enumeration | Elevator
enumeration | Escalator
enumeration | GeneralLaundryEquip
enumeration | GeneralKitchenEquip
enumeration | GeneralMedicalEquip
enumeration | GeneralOfficeEquip
enumeration | GeneralEntertainmentEquip
enumeration | GeneralRefrigerationEquip
enumeration | GeneralFitnessEquip
enumeration | GeneralVideoEquip
enumeration | GeneralToilet
source | <xsd:simpleType name="intEquipTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="GeneralPlugload"/> <xsd:enumeration value="Computer"/> <xsd:enumeration value="Copier"/> <xsd:enumeration value="Refrigerator"/> <xsd:enumeration value="Stove"/> <xsd:enumeration value="Cooktop"/> <xsd:enumeration value="Fryer"/> <xsd:enumeration value="Freezer"/> <xsd:enumeration value="ClothesDryer"/> <xsd:enumeration value="ClothesWasher"/> <xsd:enumeration value="Dishwasher"/> <xsd:enumeration value="TV"/> <xsd:enumeration value="VCR"/> <xsd:enumeration value="Microwave"/> <xsd:enumeration value="Fan"/> <xsd:enumeration value="AudioEquip"/> <xsd:enumeration value="MiscEquip"/> <xsd:enumeration value="Toilet"/> <xsd:enumeration value="Urinal"/> <xsd:enumeration value="Shower"/> <xsd:enumeration value="Sink"/> <xsd:enumeration value="Pool"/> <xsd:enumeration value="HotTub"/> <xsd:enumeration value="Sauna"/> <xsd:enumeration value="BatteryCharger"/> <xsd:enumeration value="Furnace"/> <xsd:enumeration value="IndustrialEquip"/> <xsd:enumeration value="Printer"/> <xsd:enumeration value="Vending"/> <xsd:enumeration value="Elevator"/> <xsd:enumeration value="Escalator"/> <xsd:enumeration value="GeneralLaundryEquip"/> <xsd:enumeration value="GeneralKitchenEquip"/> <xsd:enumeration value="GeneralMedicalEquip"/> <xsd:enumeration value="GeneralOfficeEquip"/> <xsd:enumeration value="GeneralEntertainmentEquip"/> <xsd:enumeration value="GeneralRefrigerationEquip"/> <xsd:enumeration value="GeneralFitnessEquip"/> <xsd:enumeration value="GeneralVideoEquip"/> <xsd:enumeration value="GeneralToilet"/> </xsd:restriction> </xsd:simpleType>

simpleType inverseTempUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | PrandtlNumberFofT/@unit
facets |
enumeration | PerK
enumeration | PerF
source | <xsd:simpleType name="inverseTempUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="PerK"/> <xsd:enumeration value="PerF"/> </xsd:restriction> </xsd:simpleType>

simpleType lengthUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attributes | gbXML/@lengthUnit Elevation/@unit Height/@unit Length/@unit Level/@unit PlanarGeometry/@unit RectangularGeometry/@unit Setback/@unit ShellGeometry/@unit Thickness/@unit Width/@unit
facets |
enumeration | Kilometers
enumeration | Meters
enumeration | Centimeters
enumeration | Millimeters
enumeration | Miles
enumeration | Yards
enumeration | Feet
enumeration | Inches
source | <xsd:simpleType name="lengthUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Kilometers"/> <xsd:enumeration value="Meters"/> <xsd:enumeration value="Centimeters"/> <xsd:enumeration value="Millimeters"/> <xsd:enumeration value="Miles"/> <xsd:enumeration value="Yards"/> <xsd:enumeration value="Feet"/> <xsd:enumeration value="Inches"/> </xsd:restriction> </xsd:simpleType>

simpleType lifeUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Life/@unit
facets |
enumeration | Months
enumeration | Years
enumeration | Cycles
enumeration | MillionCycles
source | <xsd:simpleType name="lifeUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Months"/> <xsd:enumeration value="Years"/> <xsd:enumeration value="Cycles"/> <xsd:enumeration value="MillionCycles"/> </xsd:restriction> </xsd:simpleType>

simpleType lightControlTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | LightingControl/@type
facets |
enumeration | Continuous
enumeration | OnOff
enumeration | Stepped2
enumeration | Stepped3
enumeration | Stepped4
enumeration | Stepped5
enumeration | Stepped6
enumeration | Stepped7
enumeration | Stepped8
enumeration | Stepped9
enumeration | Stepped10
enumeration | Stepped11
enumeration | Stepped12
enumeration | Stepped13
enumeration | Stepped14
enumeration | Stepped15
enumeration | Stepped16
enumeration | Stepped17
enumeration | Stepped18
enumeration | Stepped19
enumeration | Stepped20
enumeration | ContinuousOff
enumeration | MotionSensor
enumeration | Photocell
source | <xsd:simpleType name="lightControlTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Continuous"/> <xsd:enumeration value="OnOff"/> <xsd:enumeration value="Stepped2"/> <xsd:enumeration value="Stepped3"/> <xsd:enumeration value="Stepped4"/> <xsd:enumeration value="Stepped5"/> <xsd:enumeration value="Stepped6"/> <xsd:enumeration value="Stepped7"/> <xsd:enumeration value="Stepped8"/> <xsd:enumeration value="Stepped9"/> <xsd:enumeration value="Stepped10"/> <xsd:enumeration value="Stepped11"/> <xsd:enumeration value="Stepped12"/> <xsd:enumeration value="Stepped13"/> <xsd:enumeration value="Stepped14"/> <xsd:enumeration value="Stepped15"/> <xsd:enumeration value="Stepped16"/> <xsd:enumeration value="Stepped17"/> <xsd:enumeration value="Stepped18"/> <xsd:enumeration value="Stepped19"/> <xsd:enumeration value="Stepped20"/> <xsd:enumeration value="ContinuousOff"/> <xsd:enumeration value="MotionSensor"/> <xsd:enumeration value="Photocell"/> </xsd:restriction> </xsd:simpleType>

simpleType loadUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
element | Results
attributes | LatentLoad/@unit ZoneCoolingLoad/@unit
facets |
enumeration | BtuPerHour
enumeration | Watt
source | <xsd:simpleType name="loadUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="BtuPerHour"/> <xsd:enumeration value="Watt"/> </xsd:restriction> </xsd:simpleType>

simpleType loopTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attributes | DeltaP/@hydronicLoopType HydronicLoopId/@hydronicLoopType MinFlow/@hydronicLoopType RatedFlow/@hydronicLoopType HydronicLoop/@loopType
facets |
enumeration | PrimaryChilledWater
enumeration | SecondaryChilledWater
enumeration | HotWater
enumeration | CondenserWater
enumeration | DomesticHotWater
enumeration | WaterLoopHeatPump
enumeration | TwoPipe
enumeration | PotableWaterLoop
source | <xsd:simpleType name="loopTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="PrimaryChilledWater"/> <xsd:enumeration value="SecondaryChilledWater"/> <xsd:enumeration value="HotWater"/> <xsd:enumeration value="CondenserWater"/> <xsd:enumeration value="DomesticHotWater"/> <xsd:enumeration value="WaterLoopHeatPump"/> <xsd:enumeration value="TwoPipe"/> <xsd:enumeration value="PotableWaterLoop"/> </xsd:restriction> </xsd:simpleType>

simpleType openingTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Opening/@openingType
facets |
enumeration | FixedWindow
enumeration | OperableWindow
enumeration | FixedSkylight
enumeration | OperableSkylight
enumeration | SlidingDoor
enumeration | NonSlidingDoor
enumeration | Air
source | <xsd:simpleType name="openingTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="FixedWindow"> <xsd:annotation> <xsd:documentation>Opening in a surface with a tilt between 45° and 149.99° with a non-operable glazed opening in it. </xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="OperableWindow"> <xsd:annotation> <xsd:documentation>Opening in a surface with a tilt between 45° and 149.99° with a operable glazed opening in it. </xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="FixedSkylight"> <xsd:annotation> <xsd:documentation>Opening in a surface with a tilt between 0° and 44.99° with a non-operable glazed opening in it. </xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="OperableSkylight"> <xsd:annotation> <xsd:documentation>Opening in a surface with a tilt between 0° and 44.99° with a operable glazed opening in it. </xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="SlidingDoor"> <xsd:annotation> <xsd:documentation>Opening in a surface with a tilt between 45° and 149.99° with a sliding door in it. </xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="NonSlidingDoor"> <xsd:annotation> <xsd:documentation>Opening in a surface with a tilt between 45° and 149.99° with a non-sliding door in it. </xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Air"> <xsd:annotation> <xsd:documentation>Opening in a surface with a tilt between 0° and 180° with nothing in it. </xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType operationTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Control/@operationType
facets |
enumeration | Cycling
enumeration | Continuous
source | <xsd:simpleType name="operationTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Cycling"/> <xsd:enumeration value="Continuous"/> </xsd:restriction> </xsd:simpleType>

simpleType peopleHeatGainTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | PeopleHeatGain/@heatGainType
facets |
enumeration | Total
enumeration | Sensible
enumeration | Latent
source | <xsd:simpleType name="peopleHeatGainTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Total"/> <xsd:enumeration value="Sensible"/> <xsd:enumeration value="Latent"/> </xsd:restriction> </xsd:simpleType>

simpleType peopleHeatGainUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | PeopleHeatGain/@unit
facets |
enumeration | WattPerPerson
enumeration | BtuPerHourPerson
source | <xsd:simpleType name="peopleHeatGainUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="WattPerPerson"/> <xsd:enumeration value="BtuPerHourPerson"/> </xsd:restriction> </xsd:simpleType>

simpleType peopleNumberUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | PeopleNumber/@unit
facets |
enumeration | NumberOfPeople
enumeration | SquareFtPerPerson
enumeration | SquareMPerPerson
source | <xsd:simpleType name="peopleNumberUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="NumberOfPeople"/> <xsd:enumeration value="SquareFtPerPerson"/> <xsd:enumeration value="SquareMPerPerson"/> </xsd:restriction> </xsd:simpleType>

simpleType permUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Permeance/@unit
facets |
enumeration | PermSI
enumeration | PermIP
source | <xsd:simpleType name="permUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="PermSI"/> <xsd:enumeration value="PermIP"/> </xsd:restriction> </xsd:simpleType>

simpleType powerPerAreaUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attributes | EquipPowerPerArea/@unit HorizontalSolar/@unit LightPowerPerArea/@unit SolarOnOpening/@unit
facets |
enumeration | WattPerSquareMeter
enumeration | WattPerSquareFoot
source | <xsd:simpleType name="powerPerAreaUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="WattPerSquareMeter"/> <xsd:enumeration value="WattPerSquareFoot"/> </xsd:restriction> </xsd:simpleType>

simpleType powerTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Power/@powerType
facets |
enumeration | Electricity
enumeration | NaturalGas
enumeration | Propane
enumeration | FuelOil1
enumeration | FuelOil2
enumeration | FuelOil4
enumeration | Water
enumeration | ChilledWater
enumeration | HotWater
enumeration | Steam
source | <xsd:simpleType name="powerTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Electricity"/> <xsd:enumeration value="NaturalGas"/> <xsd:enumeration value="Propane"/> <xsd:enumeration value="FuelOil1"/> <xsd:enumeration value="FuelOil2"/> <xsd:enumeration value="FuelOil4"/> <xsd:enumeration value="Water"/> <xsd:enumeration value="ChilledWater"/> <xsd:enumeration value="HotWater"/> <xsd:enumeration value="Steam"/> </xsd:restriction> </xsd:simpleType>

simpleType powerUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
element | Results
attributes | ElecLoad/@unit InputWatts/@unit Power/@unit
facets |
enumeration | Watt
enumeration | Kilowatt
enumeration | Horsepower
enumeration | KilogramForceMeterPerSecond
enumeration | BtuPerSecond
enumeration | FootPoundForcePerSecond
enumeration | KilocaloriesPerSecond
enumeration | BtuPerHour
source | <xsd:simpleType name="powerUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Watt"/> <xsd:enumeration value="Kilowatt"/> <xsd:enumeration value="Horsepower"/> <xsd:enumeration value="KilogramForceMeterPerSecond"/> <xsd:enumeration value="BtuPerSecond"/> <xsd:enumeration value="FootPoundForcePerSecond"/> <xsd:enumeration value="KilocaloriesPerSecond"/> <xsd:enumeration value="BtuPerHour"/> </xsd:restriction> </xsd:simpleType>

simpleType powerUseTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Power/@useType
facets |
enumeration | Heating
enumeration | Cooling
enumeration | Both
enumeration | Other
source | <xsd:simpleType name="powerUseTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Heating"/> <xsd:enumeration value="Cooling"/> <xsd:enumeration value="Both"/> <xsd:enumeration value="Other"/> </xsd:restriction> </xsd:simpleType>

simpleType pressureUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attributes | DDPressureCool/@unit DDPressureHeat/@unit DesignPressure/@unit MaxPressure/@unit MinPressure/@unit
facets |
enumeration | PSI
enumeration | kPa
enumeration | Atmospheres
enumeration | InchesOfH2O
enumeration | CentimetersOfH2O
enumeration | InchesOfMercury
enumeration | CentimetersOfMercury
enumeration | MillimetersOfMercury
enumeration | Pascals
source | <xsd:simpleType name="pressureUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="PSI"/> <xsd:enumeration value="kPa"/> <xsd:enumeration value="Atmospheres"/> <xsd:enumeration value="InchesOfH2O"/> <xsd:enumeration value="CentimetersOfH2O"/> <xsd:enumeration value="InchesOfMercury"/> <xsd:enumeration value="CentimetersOfMercury"/> <xsd:enumeration value="MillimetersOfMercury"/> <xsd:enumeration value="Pascals"/> </xsd:restriction> </xsd:simpleType>

simpleType radiationWavelengthTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Transmittance/@type
facets |
enumeration | Solar
enumeration | IR
enumeration | Visible
source | <xsd:simpleType name="radiationWavelengthTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Solar"/> <xsd:enumeration value="IR"/> <xsd:enumeration value="Visible"/> </xsd:restriction> </xsd:simpleType>

simpleType reflectanceTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Reflectance/@type
facets |
enumeration | Ground
enumeration | IntSolar
enumeration | IntIR
enumeration | IntVisible
enumeration | ExtSolar
enumeration | ExtVisible
enumeration | ExtIR
source | <xsd:simpleType name="reflectanceTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Ground"/> <xsd:enumeration value="IntSolar"/> <xsd:enumeration value="IntIR"/> <xsd:enumeration value="IntVisible"/> <xsd:enumeration value="ExtSolar"/> <xsd:enumeration value="ExtVisible"/> <xsd:enumeration value="ExtIR"/> </xsd:restriction> </xsd:simpleType>

simpleType resistanceUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attributes | InsideAirFilmResistance/@unit R-value/@unit
facets |
enumeration | SquareMeterKPerW
enumeration | HrSquareFtFPerBTU
source | <xsd:simpleType name="resistanceUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="SquareMeterKPerW"/> <xsd:enumeration value="HrSquareFtFPerBTU"/> </xsd:restriction> </xsd:simpleType>

simpleType resourceTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attributes | AltEnergySource/@resourceType Energy/@resourceType Meter/@resourceType Results/@resourceType
facets |
enumeration | Electricity
enumeration | NaturalGas
enumeration | Propane
enumeration | FuelOil1
enumeration | FuelOil2
enumeration | FuelOil4
enumeration | Water
enumeration | ChilledWater
enumeration | HotWater
enumeration | Steam
source | <xsd:simpleType name="resourceTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Electricity"/> <xsd:enumeration value="NaturalGas"/> <xsd:enumeration value="Propane"/> <xsd:enumeration value="FuelOil1"/> <xsd:enumeration value="FuelOil2"/> <xsd:enumeration value="FuelOil4"/> <xsd:enumeration value="Water"/> <xsd:enumeration value="ChilledWater"/> <xsd:enumeration value="HotWater"/> <xsd:enumeration value="Steam"/> </xsd:restriction> </xsd:simpleType>

simpleType resultsExtraResourceTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
facets |
enumeration | Thermal
enumeration | Light
enumeration | Moisture
enumeration | Air
enumeration | Contaminant
source | <xsd:simpleType name="resultsExtraResourceTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Thermal"/> <xsd:enumeration value="Light"/> <xsd:enumeration value="Moisture"/> <xsd:enumeration value="Air"/> <xsd:enumeration value="Contaminant"/> </xsd:restriction> </xsd:simpleType>

simpleType resultsTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Results/@resultsType
facets |
enumeration | HeatLoad
enumeration | CoolingLoad
enumeration | CO2
enumeration | SO2
enumeration | NOx
enumeration | Energy
enumeration | Power
enumeration | Cost
enumeration | EnergyCost
enumeration | DemandCost
enumeration | CommodityCost
enumeration | TransportationCost
enumeration | DryBulbTemperature
enumeration | WetBulbTemperature
enumeration | DewPointTemperature
enumeration | FootCandles
enumeration | Humidity
enumeration | MoistureContent
enumeration | Flow
enumeration | Capacity
source | <xsd:simpleType name="resultsTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="HeatLoad"/> <xsd:enumeration value="CoolingLoad"/> <xsd:enumeration value="CO2"/> <xsd:enumeration value="SO2"/> <xsd:enumeration value="NOx"/> <xsd:enumeration value="Energy"/> <xsd:enumeration value="Power"/> <xsd:enumeration value="Cost"/> <xsd:enumeration value="EnergyCost"/> <xsd:enumeration value="DemandCost"/> <xsd:enumeration value="CommodityCost"/> <xsd:enumeration value="TransportationCost"/> <xsd:enumeration value="DryBulbTemperature"/> <xsd:enumeration value="WetBulbTemperature"/> <xsd:enumeration value="DewPointTemperature"/> <xsd:enumeration value="FootCandles"/> <xsd:enumeration value="Humidity"/> <xsd:enumeration value="MoistureContent"/> <xsd:enumeration value="Flow"/> <xsd:enumeration value="Capacity"/> </xsd:restriction> </xsd:simpleType>

simpleType roofASHRAENumberEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | CLTDParameters/@roofASHRAENumber
facets |
enumeration | 0
enumeration | 1
enumeration | 2
enumeration | 3
enumeration | 4
enumeration | 5
enumeration | 6
enumeration | 7
enumeration | 8
enumeration | 9
enumeration | 10
enumeration | 11
enumeration | 12
enumeration | 13
annotation |
documentation
Used with the roofASHRAENumber attribute. Each annotation for the values is only one example of many possible constructions for that ASHRAE roof number. The user should select the one that best matches the thermal characteristics of the roof, not necessarily the one closest to the example description.
source | <xsd:simpleType name="roofASHRAENumberEnum"> <xsd:annotation> <xsd:documentation>Used with the roofASHRAENumber attribute. Each annotation for the values is only one example of many possible constructions for that ASHRAE roof number. The user should select the one that best matches the thermal characteristics of the roof, not necessarily the one closest to the example description.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="0"> <xsd:annotation> <xsd:documentation>Undefined</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="1"> <xsd:annotation> <xsd:documentation>Steel sheet with 1 or 2 inches insulation</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="2"> <xsd:annotation> <xsd:documentation>One inch wood with 1 inch insulation</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="3"> <xsd:annotation> <xsd:documentation>Four inch light weight concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="4"> <xsd:annotation> <xsd:documentation>Two inch heavy weight concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="5"> <xsd:annotation> <xsd:documentation>One inch wood with 2 inch insulation</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="6"> <xsd:annotation> <xsd:documentation>Six inch light weight concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="7"> <xsd:annotation> <xsd:documentation>2.5 inch wood with 1 inch insulation</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="8"> <xsd:annotation> <xsd:documentation>Eight inch light weight concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="9"> <xsd:annotation> <xsd:documentation>4 inch hvy wt concrete with 1-2 inch insulation</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="10"> <xsd:annotation> <xsd:documentation>2.5 inch wood with 2 inches of insulation</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="11"> <xsd:annotation> <xsd:documentation>Roof Terrace System</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="12"> <xsd:annotation> <xsd:documentation>6 inch hvy wt concrete with 1-2 inch insulation</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="13"> <xsd:annotation> <xsd:documentation>4 inch wood with 1-2 inches of insulation</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType roofCLTDIndexEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | ManualJ8Parameters/@roofCLTDIndex
facets |
enumeration | 1
enumeration | 2
enumeration | 3
enumeration | 4
enumeration | 5
enumeration | 6
enumeration | 7
enumeration | 8
enumeration | 9
enumeration | 10
enumeration | 11
enumeration | 12
enumeration | 13
enumeration | 14
enumeration | 15
enumeration | 16
enumeration | 17
enumeration | 18
enumeration | 19
enumeration | 20
enumeration | 21
enumeration | 22
enumeration | 23
enumeration | 24
enumeration | 25
enumeration | 26
enumeration | 27
enumeration | 28
enumeration | 29
enumeration | 30
enumeration | 31
enumeration | 32
enumeration | 33
enumeration | 34
enumeration | 35
enumeration | 36
enumeration | 37
enumeration | 38
enumeration | 39
enumeration | 40
enumeration | 41
enumeration | 42
enumeration | 43
enumeration | 44
enumeration | 45
enumeration | 46
enumeration | 47
annotation |
documentation
Used with the roofCLTDIndex attribute.
source | <xsd:simpleType name="roofCLTDIndexEnum"> <xsd:annotation> <xsd:documentation>Used with the roofCLTDIndex attribute.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="1"> <xsd:annotation> <xsd:documentation>Under attic or knee wall, U-value = 0.408 - 0.018, Unvented Attic, No Radiant Barrier, Any Roofing Material, Any Roof Color</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="2"> <xsd:annotation> <xsd:documentation>Under attic or knee wall, U-value = 0.408 - 0.018, Vented Attic, No Radiant Barrier, Dark Asphalt Shingles or Dark Metal, Tar and Gravel or Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="3"> <xsd:annotation> <xsd:documentation>Under attic or knee wall, U-value = 0.408 - 0.018, Vented Attic, No Radiant Barrier, White or Light Color Shingles, Any Wood Shake Light Metal, Tar and Gravel or Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="4"> <xsd:annotation> <xsd:documentation>Under attic or knee wall, U-value = 0.408 - 0.02, Vented Attic, No Radiant Barrier, Dark Tile, Slate or Concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="5"> <xsd:annotation> <xsd:documentation>Under attic or knee wall, U-value = 0.408 - 0.02, Vented Attic, No Radiant Barrier, Light Tile, Slate or Concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="6"> <xsd:annotation> <xsd:documentation>Under attic or knee wall, U-value = 0.408 - 0.02, Vented Attic, No Radiant Barrier, White Tile, Slate or Concrete, White Metal or White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="7"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.287 - 0.134, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="8"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.118 - 0.091, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="9"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.074 - 0.063, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="10"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.054, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="11"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.048, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="12"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.043 - 0.039, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="13"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.035, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="14"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.032 - 0.027, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="15"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.287 - 0.134, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="16"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.118 - 0.091, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="17"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.074 - 0.063, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="18"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.054, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="19"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.048, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="20"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.043 - 0.039, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="21"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.035, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="22"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.032 - 0.027, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="23"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.287 - 0.134, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="24"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.118 - 0.091, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="25"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.074 - 0.063, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="26"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.054, White or Light Color Tile Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="27"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.048, White or Light Color Tile Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="28"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.043 - 0.039, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="29"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.035, White or Light Color Tile Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="30"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.032 - 0.027, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="31"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.241 - 0.109, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="32"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.09 - 0.076, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="33"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.069, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="34"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.051 - 0.047, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="35"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.034, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="36"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.029, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="37"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.241 - 0.109, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="38"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.09 - 0.076, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="39"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.069, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="40"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.051 - 0.047, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="41"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.034, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="42"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.029, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="43"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.241 - 0.109, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="44"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.09 - 0.076, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="45"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.069, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="46"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.051 - 0.034, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="47"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.029, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType roofColorEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | CLTDParameters/@roofColor
facets |
enumeration | Dark
enumeration | Light
annotation |
documentation
Used with the roofColor attribute. Only enter Light if the construction is a roof and if it's in a rural location.
source | <xsd:simpleType name="roofColorEnum"> <xsd:annotation> <xsd:documentation>Used with the roofColor attribute. Only enter Light if the construction is a roof and if it's in a rural location.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Dark"> <xsd:annotation> <xsd:documentation>Dark colored or light colored in an industrial area</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Light"> <xsd:annotation> <xsd:documentation>Permanently light colored and in a rural area</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType roofCTSTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | RTSParameters/@roofCTSType
facets |
enumeration | 1
enumeration | 2
enumeration | 3
enumeration | 4
enumeration | 5
enumeration | 6
enumeration | 7
enumeration | 8
enumeration | 9
enumeration | 10
enumeration | 11
enumeration | 12
enumeration | 13
enumeration | 14
enumeration | 15
enumeration | 16
enumeration | 17
enumeration | 18
enumeration | 19
annotation |
documentation
Used with the roofCTSType attribute. Each annotation for the values is only one example of many possible constructions for that CTS type. The user should select the one that best matches the thermal characteristics of the roof, not necessarily the one closest to the example description.
source | <xsd:simpleType name="roofCTSTypeEnum"> <xsd:annotation> <xsd:documentation>Used with the roofCTSType attribute. Each annotation for the values is only one example of many possible constructions for that CTS type. The user should select the one that best matches the thermal characteristics of the roof, not necessarily the one closest to the example description.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="1"> <xsd:annotation> <xsd:documentation>Metal Roof, R-19 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="2"> <xsd:annotation> <xsd:documentation>Metal Roof, R-19 Batt Insulation, Suspended Acoustical Ceiling </xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="3"> <xsd:annotation> <xsd:documentation>Metal Roof, R-19 Batt Insulation</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="4"> <xsd:annotation> <xsd:documentation>Asphalt Shingles, Wood Sheathing, R-19 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="5"> <xsd:annotation> <xsd:documentation>Slate or Tile, Wood Sheathing, R-19 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="6"> <xsd:annotation> <xsd:documentation>Wood Shingles, Wood Sheathing, R-19 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="7"> <xsd:annotation> <xsd:documentation>Membrane, Sheathing, R-10 Insulation Board, Wood Deck</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="8"> <xsd:annotation> <xsd:documentation>Membrane, Sheathing, R-10 Insulation Board, Wood Deck Suspended Acoustical Ceiling</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="9"> <xsd:annotation> <xsd:documentation>Membrane, Sheathing, R-10 Insulation Board, Metal Deck</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="10"> <xsd:annotation> <xsd:documentation>Membrane, Sheathing, R-10 Insulation Board, Metal Deck Suspended Acoustical Ceiling</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="11"> <xsd:annotation> <xsd:documentation>Membrane, Sheathing, R-15 Insulation Board, Metal Deck</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="12"> <xsd:annotation> <xsd:documentation>Membrane, Sheathing, R-10 plus R-15 Insulation Boards, Metal Deck</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="13"> <xsd:annotation> <xsd:documentation>2" Concrete Roof Ballast, Membrane, Sheathing, R-15 Insulation Board, Metal Deck</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="14"> <xsd:annotation> <xsd:documentation>Membrane, Sheathing, R-15 Insulation Board, 4" LW Concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="15"> <xsd:annotation> <xsd:documentation>Membrane, Sheathing, R-15 Insulation Board, 6" LW Concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="16"> <xsd:annotation> <xsd:documentation>Membrane, Sheathing, R-15 Insulation Board, 8" LW Concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="17"> <xsd:annotation> <xsd:documentation>Membrane, Sheathing, R-15 Insulation Board, 6" HW Concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="18"> <xsd:annotation> <xsd:documentation>Membrane, Sheathing, R-15 Insulation Board, 8" HW Concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="19"> <xsd:annotation> <xsd:documentation>Membrane, 6" HW Concrete, R-19 Batt Insulation, Suspended Acoustical Ceiling</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType roughnessValueEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Roughness/@value
facets |
enumeration | VeryRough
enumeration | MediumRough
enumeration | Rough
enumeration | Smooth
enumeration | MediumSmooth
enumeration | VerySmooth
source | <xsd:simpleType name="roughnessValueEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="VeryRough"/> <xsd:enumeration value="MediumRough"/> <xsd:enumeration value="Rough"/> <xsd:enumeration value="Smooth"/> <xsd:enumeration value="MediumSmooth"/> <xsd:enumeration value="VerySmooth"/> </xsd:restriction> </xsd:simpleType>

simpleType scheduleTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attributes | DaySchedule/@type Schedule/@type WeekSchedule/@type
facets |
enumeration | Temp
enumeration | Fraction
enumeration | OnOff
source | <xsd:simpleType name="scheduleTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Temp"/> <xsd:enumeration value="Fraction"/> <xsd:enumeration value="OnOff"/> </xsd:restriction> </xsd:simpleType>

simpleType shadeOperationEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attributes | Opening/@exteriorShadeType Opening/@interiorShadeType
facets |
enumeration | Fixed
enumeration | Operable
source | <xsd:simpleType name="shadeOperationEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Fixed"/> <xsd:enumeration value="Operable"/> </xsd:restriction> </xsd:simpleType>

simpleType shadeScheduleTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
facets |
enumeration | Shade
enumeration | Blind
enumeration | Operation
enumeration | Probability
enumeration | MaxSolar
source | <xsd:simpleType name="shadeScheduleTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Shade"/> <xsd:enumeration value="Blind"/> <xsd:enumeration value="Operation"/> <xsd:enumeration value="Probability"/> <xsd:enumeration value="MaxSolar"/> </xsd:restriction> </xsd:simpleType>

simpleType shadeTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | ShadeControl/@type
facets |
enumeration | InteriorInsulated
enumeration | InteriorUnInsulated
enumeration | ExternalInsulated
enumeration | ExternalUnInsulated
source | <xsd:simpleType name="shadeTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="InteriorInsulated"/> <xsd:enumeration value="InteriorUnInsulated"/> <xsd:enumeration value="ExternalInsulated"/> <xsd:enumeration value="ExternalUnInsulated"/> </xsd:restriction> </xsd:simpleType>

simpleType sinkRateUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | SinkRate/@unit
facets |
enumeration | PoundsPerHour
enumeration | KilogramsPerHour
enumeration | GramsPerHour
source | <xsd:simpleType name="sinkRateUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="PoundsPerHour"/> <xsd:enumeration value="KilogramsPerHour"/> <xsd:enumeration value="GramsPerHour"/> </xsd:restriction> </xsd:simpleType>

simpleType spaceTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Space/@spaceType
facets |
enumeration | ActiveStorage
enumeration | ActiveStorageHospitalOrHealthcare
enumeration | AirOrTrainOrBusBaggageArea
enumeration | AirportConcourse
enumeration | AtriumEachAdditionalFloor
enumeration | AtriumFirstThreeFloors
enumeration | AudienceOrSeatingAreaPenitentiary
enumeration | AudienceOrSeatingAreaExerciseCenter
enumeration | AudienceOrSeatingAreaGymnasium
enumeration | AudienceOrSeatingAreaSportsArena
enumeration | AudienceOrSeatingAreaConventionCenter
enumeration | AudienceOrSeatingAreaMotionPictureTheatre
enumeration | AudienceOrSeatingAreaPerformingArtsTheatre
enumeration | AudienceOrSeatingAreaReligious
enumeration | AudienceOrSeatingAreaPoliceOrFireStations
enumeration | AudienceOrSeatingAreaCourtHouse
enumeration | AudienceOrSeatingAreaAuditorium
enumeration | BankCustomerArea
enumeration | BankingActivityAreaOffice
enumeration | BarberAndBeautyParlor
enumeration | CardFileAndCataloguingLibrary
enumeration | ClassroomOrLectureOrTrainingPenitentiary
enumeration | ClassroomOrLectureOrTraining
enumeration | ComfinementCellsPenitentiary
enumeration | ComfinementCellsCourtHouse
enumeration | ConferenceMeetingOrMultipurpose
enumeration | CorridorOrTransition
enumeration | CorridorOrTransitionManufacturingFacility
enumeration | CorridorsWithPatientWaitingExamHospitalOrHealthcare
enumeration | CourtSportsAreaSportsArena
enumeration | CourtroomCourtHouse
enumeration | DepartmentStoreSalesAreaRetail
enumeration | DetailedManufacturingFacility
enumeration | DiningArea
enumeration | DiningAreaHotel
enumeration | DiningAreaFamilyDining
enumeration | DiningAreaLoungeOrLeisureDining
enumeration | DiningAreaMotel
enumeration | DiningAreaTransportation
enumeration | DiningAreaPenitentiary
enumeration | DiningAreaCivilServices
enumeration | DormitoryBedroom
enumeration | DormitoryStudyHall
enumeration | DressingOrLockerOrFittingRoomGymnasium
enumeration | DressingOrLockerOrFittingRoomCourtHouse
enumeration | DressingOrLockerOrFittingRoomPerformingArtsTheatre
enumeration | DressingOrLockerOrFittingRoomAuditorium
enumeration | DressingOrLockerOrFittingRoomExerciseCenter
enumeration | ElectricalOrMechanical
enumeration | ElevatorLobbies
enumeration | EmergencyHospitalOrHealthcare
enumeration | EquipmentRoomManufacturingFacility
enumeration | ExamOrTreatmentHospitalOrHealthcare
enumeration | ExcerciseAreaExerciseCenter
enumeration | ExcerciseAreaGymnasium
enumeration | ExhibitSpaceConventionCenter
enumeration | FellowshipHallReligiousBuildings
enumeration | FineMaterialWarehouse
enumeration | FineMerchandiseSalesAreaRetail
enumeration | FireStationEngineRoomPoliceOrFireStation
enumeration | FoodPreparation
enumeration | GarageServiceOrRepairAutomotiveFacility
enumeration | GeneralHighBayManufacturingFacility
enumeration | GeneralLowBayManufacturingFacility
enumeration | GeneralExhibitionMuseum
enumeration | HospitalNurseryHospitalOrHealthcare
enumeration | HospitalOrMedicalSuppliesHospitalOrHealthcare
enumeration | HospitalOrRadiologyHospitalOrHealthcare
enumeration | HotelOrConferenceCenterConferenceOrMeeting
enumeration | InactiveStorage
enumeration | JudgesChambersCourtHouse
enumeration | LaboratoryOffice
enumeration | LaundryIroningAndSorting
enumeration | LaundryWashingHospitalOrHealthcare
enumeration | LibraryAudioVisualLibraryAudioVisual
enumeration | LivingQuartersDormitory
enumeration | LivingQuartersMotel
enumeration | LivingQuartersHotel
enumeration | Lobby
enumeration | LobbyReligiousBuildings
enumeration | LobbyMotionPictureTheatre
enumeration | LobbyAuditorium
enumeration | LobbyPerformingArtsTheatre
enumeration | LobbyPostOffice
enumeration | LobbyHotel
enumeration | LoungeOrRecreation
enumeration | MallConcourseSalesAreaRetail
enumeration | MassMerchandisingSalesAreaRetail
enumeration | MediumOrBulkyMaterialWarehouse
enumeration | MerchandisingSalesAreaRetail
enumeration | MuseumAndGalleryStorage
enumeration | NurseStationHospitalOrHealthcare
enumeration | OfficeEnclosed
enumeration | OfficeOpenPlan
enumeration | OfficeCommonActivityAreasInactiveStorage
enumeration | OperatingRoomHospitalOrHealthcare
enumeration | OtherTelevisedPlayingAreaSportsArena
enumeration | ParkingAreaAttendantOnlyParkingGarage
enumeration | ParkingAreaPedestrianParkingGarage
enumeration | PatientRoomHospitalOrHealthcare
enumeration | PersonalServicesSalesAreaRetail
enumeration | PharmacyHospitalOrHealthcare
enumeration | PhysicalTherapyHospitalOrHealthcare
enumeration | PlayingAreaGymnasium
enumeration | Plenum
enumeration | PoliceStationLaboratoryPoliceOrFireStations
enumeration | PublicAndStaffLoungeHospitalOrHealthcare
enumeration | ReadingAreaLibrary
enumeration | ReceptionOrWaitingTransportation
enumeration | ReceptionOrWaitingMotel
enumeration | ReceptionOrWaitingHotel
enumeration | RecoveryHospitalOrHealthcare
enumeration | RestorationMuseum
enumeration | Restrooms
enumeration | RingSportsAreaSportsArena
enumeration | SleepingQuartersPoliceOrFireStation
enumeration | SortingAreaPostOffice
enumeration | SpecialtyStoreSalesAreaRetail
enumeration | StacksLibrary
enumeration | StairsInactive
enumeration | Stairway
enumeration | SupermarketSalesAreaRetail
enumeration | TerminalTicketCounterTransportation
enumeration | WorkshopWorkshop
enumeration | WorshipPulpitChoirReligious
source | <xsd:simpleType name="spaceTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="ActiveStorage"/> <xsd:enumeration value="ActiveStorageHospitalOrHealthcare"/> <xsd:enumeration value="AirOrTrainOrBusBaggageArea"/> <xsd:enumeration value="AirportConcourse"/> <xsd:enumeration value="AtriumEachAdditionalFloor"/> <xsd:enumeration value="AtriumFirstThreeFloors"/> <xsd:enumeration value="AudienceOrSeatingAreaPenitentiary"/> <xsd:enumeration value="AudienceOrSeatingAreaExerciseCenter"/> <xsd:enumeration value="AudienceOrSeatingAreaGymnasium"/> <xsd:enumeration value="AudienceOrSeatingAreaSportsArena"/> <xsd:enumeration value="AudienceOrSeatingAreaConventionCenter"/> <xsd:enumeration value="AudienceOrSeatingAreaMotionPictureTheatre"/> <xsd:enumeration value="AudienceOrSeatingAreaPerformingArtsTheatre"/> <xsd:enumeration value="AudienceOrSeatingAreaReligious"/> <xsd:enumeration value="AudienceOrSeatingAreaPoliceOrFireStations"/> <xsd:enumeration value="AudienceOrSeatingAreaCourtHouse"/> <xsd:enumeration value="AudienceOrSeatingAreaAuditorium"/> <xsd:enumeration value="BankCustomerArea"/> <xsd:enumeration value="BankingActivityAreaOffice"/> <xsd:enumeration value="BarberAndBeautyParlor"/> <xsd:enumeration value="CardFileAndCataloguingLibrary"/> <xsd:enumeration value="ClassroomOrLectureOrTrainingPenitentiary"/> <xsd:enumeration value="ClassroomOrLectureOrTraining"/> <xsd:enumeration value="ComfinementCellsPenitentiary"/> <xsd:enumeration value="ComfinementCellsCourtHouse"/> <xsd:enumeration value="ConferenceMeetingOrMultipurpose"/> <xsd:enumeration value="CorridorOrTransition"/> <xsd:enumeration value="CorridorOrTransitionManufacturingFacility"/> <xsd:enumeration value="CorridorsWithPatientWaitingExamHospitalOrHealthcare"/> <xsd:enumeration value="CourtSportsAreaSportsArena"/> <xsd:enumeration value="CourtroomCourtHouse"/> <xsd:enumeration value="DepartmentStoreSalesAreaRetail"/> <xsd:enumeration value="DetailedManufacturingFacility"/> <xsd:enumeration value="DiningArea"/> <xsd:enumeration value="DiningAreaHotel"/> <xsd:enumeration value="DiningAreaFamilyDining"/> <xsd:enumeration value="DiningAreaLoungeOrLeisureDining"/> <xsd:enumeration value="DiningAreaMotel"/> <xsd:enumeration value="DiningAreaTransportation"/> <xsd:enumeration value="DiningAreaPenitentiary"/> <xsd:enumeration value="DiningAreaCivilServices"/> <xsd:enumeration value="DormitoryBedroom"/> <xsd:enumeration value="DormitoryStudyHall"/> <xsd:enumeration value="DressingOrLockerOrFittingRoomGymnasium"/> <xsd:enumeration value="DressingOrLockerOrFittingRoomCourtHouse"/> <xsd:enumeration value="DressingOrLockerOrFittingRoomPerformingArtsTheatre"/> <xsd:enumeration value="DressingOrLockerOrFittingRoomAuditorium"/> <xsd:enumeration value="DressingOrLockerOrFittingRoomExerciseCenter"/> <xsd:enumeration value="ElectricalOrMechanical"/> <xsd:enumeration value="ElevatorLobbies"/> <xsd:enumeration value="EmergencyHospitalOrHealthcare"/> <xsd:enumeration value="EquipmentRoomManufacturingFacility"/> <xsd:enumeration value="ExamOrTreatmentHospitalOrHealthcare"/> <xsd:enumeration value="ExcerciseAreaExerciseCenter"/> <xsd:enumeration value="ExcerciseAreaGymnasium"/> <xsd:enumeration value="ExhibitSpaceConventionCenter"/> <xsd:enumeration value="FellowshipHallReligiousBuildings"/> <xsd:enumeration value="FineMaterialWarehouse"/> <xsd:enumeration value="FineMerchandiseSalesAreaRetail"/> <xsd:enumeration value="FireStationEngineRoomPoliceOrFireStation"/> <xsd:enumeration value="FoodPreparation"/> <xsd:enumeration value="GarageServiceOrRepairAutomotiveFacility"/> <xsd:enumeration value="GeneralHighBayManufacturingFacility"/> <xsd:enumeration value="GeneralLowBayManufacturingFacility"/> <xsd:enumeration value="GeneralExhibitionMuseum"/> <xsd:enumeration value="HospitalNurseryHospitalOrHealthcare"/> <xsd:enumeration value="HospitalOrMedicalSuppliesHospitalOrHealthcare"/> <xsd:enumeration value="HospitalOrRadiologyHospitalOrHealthcare"/> <xsd:enumeration value="HotelOrConferenceCenterConferenceOrMeeting"/> <xsd:enumeration value="InactiveStorage"/> <xsd:enumeration value="JudgesChambersCourtHouse"/> <xsd:enumeration value="LaboratoryOffice"/> <xsd:enumeration value="LaundryIroningAndSorting"/> <xsd:enumeration value="LaundryWashingHospitalOrHealthcare"/> <xsd:enumeration value="LibraryAudioVisualLibraryAudioVisual"/> <xsd:enumeration value="LivingQuartersDormitory"/> <xsd:enumeration value="LivingQuartersMotel"/> <xsd:enumeration value="LivingQuartersHotel"/> <xsd:enumeration value="Lobby"/> <xsd:enumeration value="LobbyReligiousBuildings"/> <xsd:enumeration value="LobbyMotionPictureTheatre"/> <xsd:enumeration value="LobbyAuditorium"/> <xsd:enumeration value="LobbyPerformingArtsTheatre"/> <xsd:enumeration value="LobbyPostOffice"/> <xsd:enumeration value="LobbyHotel"/> <xsd:enumeration value="LoungeOrRecreation"/> <xsd:enumeration value="MallConcourseSalesAreaRetail"/> <xsd:enumeration value="MassMerchandisingSalesAreaRetail"/> <xsd:enumeration value="MediumOrBulkyMaterialWarehouse"/> <xsd:enumeration value="MerchandisingSalesAreaRetail"/> <xsd:enumeration value="MuseumAndGalleryStorage"/> <xsd:enumeration value="NurseStationHospitalOrHealthcare"/> <xsd:enumeration value="OfficeEnclosed"/> <xsd:enumeration value="OfficeOpenPlan"/> <xsd:enumeration value="OfficeCommonActivityAreasInactiveStorage"/> <xsd:enumeration value="OperatingRoomHospitalOrHealthcare"/> <xsd:enumeration value="OtherTelevisedPlayingAreaSportsArena"/> <xsd:enumeration value="ParkingAreaAttendantOnlyParkingGarage"/> <xsd:enumeration value="ParkingAreaPedestrianParkingGarage"/> <xsd:enumeration value="PatientRoomHospitalOrHealthcare"/> <xsd:enumeration value="PersonalServicesSalesAreaRetail"/> <xsd:enumeration value="PharmacyHospitalOrHealthcare"/> <xsd:enumeration value="PhysicalTherapyHospitalOrHealthcare"/> <xsd:enumeration value="PlayingAreaGymnasium"/> <xsd:enumeration value="Plenum"/> <xsd:enumeration value="PoliceStationLaboratoryPoliceOrFireStations"/> <xsd:enumeration value="PublicAndStaffLoungeHospitalOrHealthcare"/> <xsd:enumeration value="ReadingAreaLibrary"/> <xsd:enumeration value="ReceptionOrWaitingTransportation"/> <xsd:enumeration value="ReceptionOrWaitingMotel"/> <xsd:enumeration value="ReceptionOrWaitingHotel"/> <xsd:enumeration value="RecoveryHospitalOrHealthcare"/> <xsd:enumeration value="RestorationMuseum"/> <xsd:enumeration value="Restrooms"/> <xsd:enumeration value="RingSportsAreaSportsArena"/> <xsd:enumeration value="SleepingQuartersPoliceOrFireStation"/> <xsd:enumeration value="SortingAreaPostOffice"/> <xsd:enumeration value="SpecialtyStoreSalesAreaRetail"/> <xsd:enumeration value="StacksLibrary"/> <xsd:enumeration value="StairsInactive"/> <xsd:enumeration value="Stairway"/> <xsd:enumeration value="SupermarketSalesAreaRetail"/> <xsd:enumeration value="TerminalTicketCounterTransportation"/> <xsd:enumeration value="WorkshopWorkshop"/> <xsd:enumeration value="WorshipPulpitChoirReligious"/> </xsd:restriction> </xsd:simpleType>

simpleType specificHeatUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | SpecificHeat/@unit
facets |
enumeration | JPerKgK
enumeration | BTUPerLbF
source | <xsd:simpleType name="specificHeatUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="JPerKgK"/> <xsd:enumeration value="BTUPerLbF"/> </xsd:restriction> </xsd:simpleType>

simpleType stageTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Control/@stages
facets |
enumeration | 1Stage
enumeration | 2Stage
enumeration | Variable
source | <xsd:simpleType name="stageTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="1Stage"/> <xsd:enumeration value="2Stage"/> <xsd:enumeration value="Variable"/> </xsd:restriction> </xsd:simpleType>

simpleType standardsTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Efficiency/@standardsType
facets |
enumeration | DOE
enumeration | ARI
enumeration | ANSI
enumeration | NEMA
source | <xsd:simpleType name="standardsTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="DOE"> <xsd:annotation> <xsd:documentation>Department of Energy</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="ARI"> <xsd:annotation> <xsd:documentation>Air-Conditioning and Refrigeration Institute</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="ANSI"> <xsd:annotation> <xsd:documentation>American National Standards Institute</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="NEMA"> <xsd:annotation> <xsd:documentation>National Electrical Manufacturers Association</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType stationIdTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | StationId/@IDType
facets |
enumeration | WMO
enumeration | WBAN
enumeration | ICAO
enumeration | NWSLI
enumeration | FAACallSign
enumeration | COOP
source | <xsd:simpleType name="stationIdTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="WMO"> <xsd:annotation> <xsd:documentation>A five-digit station identifier assigned by the World Meteorological Organization (WMO), used for international weather data exchange and station documentation.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="WBAN"> <xsd:annotation> <xsd:documentation>Weather-Bureau-Army-Navy station id. A five-digit station identifier used at National Climatic Data Center (NCDC) for digital data storage and general station identification purposes.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="ICAO"> <xsd:annotation> <xsd:documentation>A 4-letter indicator for geographical locations throughout the world, managed by the International Civil Aviation Organization (ICAO).</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="NWSLI"> <xsd:annotation> <xsd:documentation>A 3- to 5-character alpha-numeric identifier assigned by the US National Weather Service (NWS), used for site identification in the NWS communications systems (e.g. AFOS, ROSA, SHEF, etc.).</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="FAACallSign"> <xsd:annotation> <xsd:documentation>An alpha-numeric identifier of up to 4-characters managed by the USDT Federal Aviation Administration (FAA), used for site identification of airports, weather stations and other sites vital to navigation.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="COOP"> <xsd:annotation> <xsd:documentation>A 6-digit number identifying a station in the NWS Cooperative Network.</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType surfaceTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attributes | AdjacentSpaceId/@surfaceType Surface/@surfaceType
facets |
enumeration | InteriorWall
enumeration | ExteriorWall
enumeration | Roof
enumeration | InteriorFloor
enumeration | Shade
enumeration | UndergroundWall
enumeration | UndergroundSlab
enumeration | Ceiling
enumeration | Air
enumeration | UndergroundCeiling
enumeration | RaisedFloor
enumeration | SlabOnGrade
enumeration | FreestandingColumn
enumeration | EmbeddedColumn
source | <xsd:simpleType name="surfaceTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="InteriorWall"> <xsd:annotation> <xsd:documentation>Surface adjacent to two conditioned or unconditioned spaces with a tilt between 45° and 149.99°.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="ExteriorWall"> <xsd:annotation> <xsd:documentation>Surface adjacent to one conditioned or unconditioned space and the outside with a tilt between 45° and 149.99°.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Roof"> <xsd:annotation> <xsd:documentation>Surface adjacent to one conditioned or unconditioned space and the outside with a tilt between 0° and 44.99°.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="InteriorFloor"> <xsd:annotation> <xsd:documentation>Surface adjacent to two conditioned or unconditioned spaces with a tilt between 150° and 180°.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Shade"> <xsd:annotation> <xsd:documentation>Surface not adjacent to any spaces with tilt between 0° and 180°.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="UndergroundWall"> <xsd:annotation> <xsd:documentation>Surface adjacent to one conditioned or unconditioned space and earth (soil) with a tilt between 45° and 149.99°.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="UndergroundSlab"> <xsd:annotation> <xsd:documentation>Surface adjacent to one conditioned or unconditioned space and earth (soil) below grade with a tilt between 150° and 180°.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Ceiling"> <xsd:annotation> <xsd:documentation>Surface adjacent to two conditioned or unconditioned spaces with a tilt between 0° and 44.99°.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Air"> <xsd:annotation> <xsd:documentation>Air membrane between two conditioned or unconditioned spaces with a tilt between 0° and 180°. </xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="UndergroundCeiling"> <xsd:annotation> <xsd:documentation>Surface adjacent to one conditioned or unconditioned space and earth (soil) with a tilt between 0° and 44.99°.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="RaisedFloor"> <xsd:annotation> <xsd:documentation>Surface adjacent to one conditioned or unconditioned space and the outside with a tilt between 150° and 180°.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="SlabOnGrade"> <xsd:annotation> <xsd:documentation>Surface adjacent to one conditioned or unconditioned space and earth (soil) at grade with a tilt between 150° and 180°.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="FreestandingColumn"> <xsd:annotation> <xsd:documentation>Freestanding column in space specified by its top surface having the same ifcGUID.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="EmbeddedColumn"> <xsd:annotation> <xsd:documentation>Embedded column in wall specified by a surface which is coplanar with (one of) the embedding wall(s).</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType systemTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | AirLoop/@systemType
facets |
enumeration | SingleZoneReheat
enumeration | PackagedSingleZone
enumeration | SingleZoneCeilingInduction
enumeration | ReheatFan
enumeration | VariableAirVolume
enumeration | PoweredInductionUnit
enumeration | PackagedVariableAirVolume
enumeration | PackagedVariableVolumeVariableTemperature
enumeration | CeilingBypassVariableAirVolume
enumeration | EvaporativeCooling
enumeration | MultiZone
enumeration | PackagedMultiZone
enumeration | DualDuct
enumeration | FanCoil
enumeration | InductionUnit
enumeration | PackagedTerminalAirConditioner
enumeration | WaterLoopHeatPump
enumeration | ResidentialCyclingFurnaceCyclingAC
enumeration | ResidentialVariableAirVolumeVariableTemperature
enumeration | FloorPanelHeating
enumeration | HeatingAndVentilating
enumeration | UnitHeater
enumeration | UnitVentilator
source | <xsd:simpleType name="systemTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="SingleZoneReheat"> <xsd:annotation> <xsd:documentation>Variable Temperature</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="PackagedSingleZone"> <xsd:annotation> <xsd:documentation>Packaged Single-zone</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="SingleZoneCeilingInduction"> <xsd:annotation> <xsd:documentation>Ceiling Induction</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="ReheatFan"> <xsd:annotation> <xsd:documentation>Constant-volume Reheat Fan</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="VariableAirVolume"> <xsd:annotation> <xsd:documentation>Variable-volume Fan</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="PoweredInductionUnit"> <xsd:annotation> <xsd:documentation>Powered Induction Unit</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="PackagedVariableAirVolume"> <xsd:annotation> <xsd:documentation>Packaged Variable Air Volume</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="PackagedVariableVolumeVariableTemperature"> <xsd:annotation> <xsd:documentation>Packaged Variable-Volume Variable-Temperature</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="CeilingBypassVariableAirVolume"> <xsd:annotation> <xsd:documentation>Ceiling Bypass</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="EvaporativeCooling"> <xsd:annotation> <xsd:documentation>Evaporative Cooling</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="MultiZone"> <xsd:annotation> <xsd:documentation>Multizone Fan</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="PackagedMultiZone"> <xsd:annotation> <xsd:documentation>Packaged Multizone</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="DualDuct"> <xsd:annotation> <xsd:documentation>Dual-duct Fan</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="FanCoil"> <xsd:annotation> <xsd:documentation>Fan Coil</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="InductionUnit"> <xsd:annotation> <xsd:documentation>Induction Unit</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="PackagedTerminalAirConditioner"> <xsd:annotation> <xsd:documentation>Packaged Terminal Air Conditioner</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="WaterLoopHeatPump"> <xsd:annotation> <xsd:documentation>Water Loop Heat Pump</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="ResidentialCyclingFurnaceCyclingAC"> <xsd:annotation> <xsd:documentation>Residential with cycling furnace and cycling air-conditioner</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="ResidentialVariableAirVolumeVariableTemperature"> <xsd:annotation> <xsd:documentation>Residential Variable-Volume Variable-Temperature</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="FloorPanelHeating"> <xsd:annotation> <xsd:documentation>Floor Panel Heating</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="HeatingAndVentilating"> <xsd:annotation> <xsd:documentation>Heating and Ventilating</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="UnitHeater"> <xsd:annotation> <xsd:documentation>Unit Heater</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="UnitVentilator"> <xsd:annotation> <xsd:documentation>Unit Ventilator</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType temperatureUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
element | Results
attributes | gbXML/@temperatureUnit Temperature/@unit Temp/@unit NaturalVentLoTemp/@unit NaturalVentHiTemp/@unit GroundTemp/@unit DesignHeatT/@unit DesignCoolT/@unit DeltaT/@unit DDWBHeat/@unit DDWBCool/@unit DDGroundTHeat/@unit DDGroundTCool/@unit DDDBRangeHeat/@unit DDDBRangeCool/@unit DDDBHeat/@unit DDDBCool/@unit AirTemperature/@unit
facets |
enumeration | F
enumeration | C
enumeration | K
enumeration | R
source | <xsd:simpleType name="temperatureUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="F"/> <xsd:enumeration value="C"/> <xsd:enumeration value="K"/> <xsd:enumeration value="R"/> </xsd:restriction> </xsd:simpleType>

simpleType tempTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Temp/@tempType
facets |
enumeration | Max
enumeration | Min
enumeration | Design
enumeration | CoolDesign
enumeration | HeatDesign
enumeration | Throttle
enumeration | Range
enumeration | Approach
enumeration | EnteringWetBulb
enumeration | LeavingDryBulb
enumeration | EnteringDryBulb
enumeration | LeavingWetBulb
enumeration | ChilledWaterSupply
enumeration | CondenserWaterSupply
enumeration | LeavingChilledWater
enumeration | LeavingCondenserWater
source | <xsd:simpleType name="tempTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Max"/> <xsd:enumeration value="Min"/> <xsd:enumeration value="Design"/> <xsd:enumeration value="CoolDesign"/> <xsd:enumeration value="HeatDesign"/> <xsd:enumeration value="Throttle"/> <xsd:enumeration value="Range"/> <xsd:enumeration value="Approach"/> <xsd:enumeration value="EnteringWetBulb"/> <xsd:enumeration value="LeavingDryBulb"/> <xsd:enumeration value="EnteringDryBulb"/> <xsd:enumeration value="LeavingWetBulb"/> <xsd:enumeration value="ChilledWaterSupply"/> <xsd:enumeration value="CondenserWaterSupply"/> <xsd:enumeration value="LeavingChilledWater"/> <xsd:enumeration value="LeavingCondenserWater"/> </xsd:restriction> </xsd:simpleType>

simpleType timePeriodEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Energy/@timePeriod
facets |
enumeration | Annual
enumeration | Jan
enumeration | Feb
enumeration | Mar
enumeration | Apr
enumeration | May
enumeration | Jun
enumeration | Jul
enumeration | Aug
enumeration | Sep
enumeration | Oct
enumeration | Nov
enumeration | Dec
source | <xsd:simpleType name="timePeriodEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Annual"/> <xsd:enumeration value="Jan"/> <xsd:enumeration value="Feb"/> <xsd:enumeration value="Mar"/> <xsd:enumeration value="Apr"/> <xsd:enumeration value="May"/> <xsd:enumeration value="Jun"/> <xsd:enumeration value="Jul"/> <xsd:enumeration value="Aug"/> <xsd:enumeration value="Sep"/> <xsd:enumeration value="Oct"/> <xsd:enumeration value="Nov"/> <xsd:enumeration value="Dec"/> </xsd:restriction> </xsd:simpleType>

simpleType timeUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | TimeIncrement/@timeUnit
facets |
enumeration | Year
enumeration | Month
enumeration | Week
enumeration | Day
enumeration | Hour
enumeration | Minute
source | <xsd:simpleType name="timeUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Year"/> <xsd:enumeration value="Month"/> <xsd:enumeration value="Week"/> <xsd:enumeration value="Day"/> <xsd:enumeration value="Hour"/> <xsd:enumeration value="Minute"/> </xsd:restriction> </xsd:simpleType>

simpleType transportationTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Transportation/@transportationType
facets |
enumeration | Bus
enumeration | Train
enumeration | Car
enumeration | LightRail
enumeration | Ferry
enumeration | Airplane
enumeration | Monorail
enumeration | Bike
source | <xsd:simpleType name="transportationTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Bus"/> <xsd:enumeration value="Train"/> <xsd:enumeration value="Car"/> <xsd:enumeration value="LightRail"/> <xsd:enumeration value="Ferry"/> <xsd:enumeration value="Airplane"/> <xsd:enumeration value="Monorail"/> <xsd:enumeration value="Bike"/> </xsd:restriction> </xsd:simpleType>

simpleType unitlessSmallUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
element | Results
attribute | HighLimit/@unit
facets |
enumeration | Percent
enumeration | PartPerMillionByVolume
enumeration | milliGramsPerCubicMeter
source | <xsd:simpleType name="unitlessSmallUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Percent"/> <xsd:enumeration value="PartPerMillionByVolume"/> <xsd:enumeration value="milliGramsPerCubicMeter"/> </xsd:restriction> </xsd:simpleType>

simpleType unitlessUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
elements | MinFlow Results
attributes | WaterLoss/@unit WasteWaterHREff/@unit Transmittance/@unit SolarHeatGainCoeff/@unit ShadingCoeff/@unit Reflectance/@unit RecycledContent/@unit Porosity/@unit PercentExisting/@unit PercentAreaDaylitControled/@unit MinRelativeHumidity/@unit MaxRelativeHumidity/@unit Glare/@unit Emittance/@unit DDSkyClearnessHeat/@unit DDSkyClearnessCool/@unit Albedo/@unit Absorptance/@unit
facets |
enumeration | Percent
enumeration | Fraction
source | <xsd:simpleType name="unitlessUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Percent"/> <xsd:enumeration value="Fraction"/> </xsd:restriction> </xsd:simpleType>

simpleType uValueUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | U-value/@unit
facets |
enumeration | WPerSquareMeterK
enumeration | BtuPerHourSquareFtF
source | <xsd:simpleType name="uValueUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="WPerSquareMeterK"/> <xsd:enumeration value="BtuPerHourSquareFtF"/> </xsd:restriction> </xsd:simpleType>

simpleType valueTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attributes | Energy/@valueType Results/@valueType
facets |
enumeration | Historical
enumeration | Simulated
enumeration | Rated
enumeration | Measured
source | <xsd:simpleType name="valueTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Historical"/> <xsd:enumeration value="Simulated"/> <xsd:enumeration value="Rated"/> <xsd:enumeration value="Measured"/> </xsd:restriction> </xsd:simpleType>

simpleType vegetationTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Vegetation/@vegetationType
facets |
enumeration | Trees
enumeration | Bushes
enumeration | Plants
enumeration | Grass
enumeration | Moss
enumeration | EvergreenTrees
enumeration | EvergreenShrubs
enumeration | DeciduousTrees
enumeration | DeciduousShrubs
source | <xsd:simpleType name="vegetationTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Trees"/> <xsd:enumeration value="Bushes"/> <xsd:enumeration value="Plants"/> <xsd:enumeration value="Grass"/> <xsd:enumeration value="Moss"/> <xsd:enumeration value="EvergreenTrees"/> <xsd:enumeration value="EvergreenShrubs"/> <xsd:enumeration value="DeciduousTrees"/> <xsd:enumeration value="DeciduousShrubs"/> </xsd:restriction> </xsd:simpleType>

simpleType velocityUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attributes | DDWindSpeedCool/@unit DDWindSpeedHeat/@unit
facets |
enumeration | MetersPerSecond
enumeration | MilesPerHour
enumeration | Knots
source | <xsd:simpleType name="velocityUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="MetersPerSecond"/> <xsd:enumeration value="MilesPerHour"/> <xsd:enumeration value="Knots"/> </xsd:restriction> </xsd:simpleType>

simpleType viscosityFofTUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | ViscosityFofT/@unit
facets |
enumeration | KgPerMSecK
enumeration | PoundPerFootSecF
source | <xsd:simpleType name="viscosityFofTUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="KgPerMSecK"/> <xsd:enumeration value="PoundPerFootSecF"/> </xsd:restriction> </xsd:simpleType>

simpleType viscosityUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Viscosity/@unit
facets |
enumeration | KgPerMSec
enumeration | PoundPerFootSec
source | <xsd:simpleType name="viscosityUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="KgPerMSec"/> <xsd:enumeration value="PoundPerFootSec"/> </xsd:restriction> </xsd:simpleType>

simpleType volumeUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attributes | Volume/@unit gbXML/@volumeUnit
facets |
enumeration | CubicKilometers
enumeration | CubicMeters
enumeration | CubicCentimeters
enumeration | CubicMillimeters
enumeration | CubicMiles
enumeration | CubicYards
enumeration | CubicFeet
enumeration | CubicInches
source | <xsd:simpleType name="volumeUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="CubicKilometers"/> <xsd:enumeration value="CubicMeters"/> <xsd:enumeration value="CubicCentimeters"/> <xsd:enumeration value="CubicMillimeters"/> <xsd:enumeration value="CubicMiles"/> <xsd:enumeration value="CubicYards"/> <xsd:enumeration value="CubicFeet"/> <xsd:enumeration value="CubicInches"/> </xsd:restriction> </xsd:simpleType>

simpleType wallASHRAEGroupEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | CLTDParameters/@wallASHRAEGroup
facets |
enumeration | A
enumeration | B
enumeration | C
enumeration | D
enumeration | E
enumeration | F
enumeration | G
annotation |
documentation
Used with the wallASHRAEGroup attribute. Each annotation for the values is only one example of many possible constructions for that ASHRAE wall group. The user should select the one that best matches the thermal characteristics of the wall, not necessarily the one closest to the example description.
source | <xsd:simpleType name="wallASHRAEGroupEnum"> <xsd:annotation> <xsd:documentation>Used with the wallASHRAEGroup attribute. Each annotation for the values is only one example of many possible constructions for that ASHRAE wall group. The user should select the one that best matches the thermal characteristics of the wall, not necessarily the one closest to the example description.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="A"> <xsd:annotation> <xsd:documentation>4-in. face brick, insulation + 8-in. com. brick</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="B"> <xsd:annotation> <xsd:documentation>4-in. face brick, 2-in. insul., 4-in. com. brick</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="C"> <xsd:annotation> <xsd:documentation>4-in. face brick, air space + 4-in. face brick</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="D"> <xsd:annotation> <xsd:documentation>4-in. face brick + 4-in. common brick</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="E"> <xsd:annotation> <xsd:documentation>4-in. face brick + 4-in. block</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="F"> <xsd:annotation> <xsd:documentation>4-in. block + air space or insulation</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="G"> <xsd:annotation> <xsd:documentation>Metal curtain wall + 1 to 3-in. insulation</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType wallColorEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | CLTDParameters/@wallColor
facets |
enumeration | Dark
enumeration | Medium
enumeration | Light
annotation |
documentation
Used with the wallColor attribute. Only enter Light or Medium if the construction is a wall and if it's in a rural location.
source | <xsd:simpleType name="wallColorEnum"> <xsd:annotation> <xsd:documentation>Used with the wallColor attribute. Only enter Light or Medium if the construction is a wall and if it's in a rural location.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Dark"> <xsd:annotation> <xsd:documentation>Dark colored or light colored in an industrial area</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Medium"> <xsd:annotation> <xsd:documentation>Permanently medium colored and in a rural area</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Light"> <xsd:annotation> <xsd:documentation>Permanently light colored and in a rural area</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType wallCTSTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | RTSParameters/@wallCTSType
facets |
enumeration | 1
enumeration | 2
enumeration | 3
enumeration | 4
enumeration | 5
enumeration | 6
enumeration | 7
enumeration | 8
enumeration | 9
enumeration | 10
enumeration | 11
enumeration | 12
enumeration | 13
enumeration | 14
enumeration | 15
enumeration | 16
enumeration | 17
enumeration | 18
enumeration | 19
enumeration | 20
enumeration | 21
enumeration | 22
enumeration | 23
enumeration | 24
enumeration | 25
enumeration | 26
enumeration | 27
enumeration | 28
enumeration | 29
enumeration | 30
enumeration | 31
enumeration | 32
enumeration | 33
enumeration | 34
enumeration | 35
annotation |
documentation
Used with the wallCTSType attribute. Each annotation for the values is only one example of many possible constructions for that CTS type. The user should select the one that best matches the thermal characteristics of the wall, not necessarily the one closest to the example description.
source | <xsd:simpleType name="wallCTSTypeEnum"> <xsd:annotation> <xsd:documentation>Used with the wallCTSType attribute. Each annotation for the values is only one example of many possible constructions for that CTS type. The user should select the one that best matches the thermal characteristics of the wall, not necessarily the one closest to the example description.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="1"> <xsd:annotation> <xsd:documentation>Spandrel Glass, R-10 Insulation Board, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="2"> <xsd:annotation> <xsd:documentation>Metal Wall Panel, R-10 Insulation Board, Gyp Board </xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="3"> <xsd:annotation> <xsd:documentation>1" Stone, R-10 Insulation Board, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="4"> <xsd:annotation> <xsd:documentation>Metal Wall Panel, Sheathing, R-11 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="5"> <xsd:annotation> <xsd:documentation>1" Stone, Sheathing, R-11 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="6"> <xsd:annotation> <xsd:documentation>Wood Siding, Sheathing, R-11 Batt Insulation, 1/2" Wood</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="7"> <xsd:annotation> <xsd:documentation>1" Stucco, Sheathing, R-11 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="8"> <xsd:annotation> <xsd:documentation>EIFS Finish, R-5 Insulation Board, Sheathing, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="9"> <xsd:annotation> <xsd:documentation>EIFS Finish, R-5 Insulation Board, Sheathing, R-11 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="10"> <xsd:annotation> <xsd:documentation>EIFS Finish, R-5 Insulation Board, Sheathing, 8" LW CMU, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="11"> <xsd:annotation> <xsd:documentation>Brick, R-5 Insulation Board, Sheathing, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="12"> <xsd:annotation> <xsd:documentation>Brick, Sheathing, R-11 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="13"> <xsd:annotation> <xsd:documentation>Brick, R-5 Insulation Board, Sheathing, R-11 Batt Insulation Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="14"> <xsd:annotation> <xsd:documentation>Brick, R-5 Insulation Board, 8" LW CMU</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="15"> <xsd:annotation> <xsd:documentation>Brick, 8" LW CMU, R-11 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="16"> <xsd:annotation> <xsd:documentation>Brick, R-5 Insulation Board, 8" HW CMU, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="17"> <xsd:annotation> <xsd:documentation>Brick, R-5 Insulation Board, Brick</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="18"> <xsd:annotation> <xsd:documentation>Brick, R-5 Insulation Board, 8" LW Concrete, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="19"> <xsd:annotation> <xsd:documentation>Brick, R-5 Insulation Board, 12" HW Concrete, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="20"> <xsd:annotation> <xsd:documentation>Brick, 8" HW Concrete, R-11 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="21"> <xsd:annotation> <xsd:documentation>8" LW CMU, R-11 Batt Insulation, Gyp Board </xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="22"> <xsd:annotation> <xsd:documentation>8" LW CMU w Fill Insulation, R-11 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="23"> <xsd:annotation> <xsd:documentation>1" Stucco, 8" HW CMU, R-11 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="24"> <xsd:annotation> <xsd:documentation>8" LW CMU w Fill Insulation</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="25"> <xsd:annotation> <xsd:documentation>8" LW CMU w Fill Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="26"> <xsd:annotation> <xsd:documentation>12" LW CMU w Fill Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="27"> <xsd:annotation> <xsd:documentation>4" LW Concrete. R-5 Board Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="28"> <xsd:annotation> <xsd:documentation>4" LW Concrete. R-11 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="29"> <xsd:annotation> <xsd:documentation>4" LW Concrete. R-10 Board Insulation, 4" LW Concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="30"> <xsd:annotation> <xsd:documentation>EIFS Finish, R-5 Insulation Board, 8" LW Concrete, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="31"> <xsd:annotation> <xsd:documentation>8" LW Concrete. R-11 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="32"> <xsd:annotation> <xsd:documentation>EIFS Finish, R-10 Insulation Board, 8" HW Concrete, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="33"> <xsd:annotation> <xsd:documentation>8" HW Concrete. R-11 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="34"> <xsd:annotation> <xsd:documentation>12" HW Concrete. R-19 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="35"> <xsd:annotation> <xsd:documentation>12" HW Concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType wallGroupManualJEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | ManualJ8Parameters/@wallGroupManualJ
facets |
enumeration | A
enumeration | B
enumeration | C
enumeration | D
enumeration | E
enumeration | F
enumeration | G
enumeration | H
enumeration | I
enumeration | J
enumeration | K
annotation |
documentation
Used with the wallGroupManualJ attribute.
source | <xsd:simpleType name="wallGroupManualJEnum"> <xsd:annotation> <xsd:documentation>Used with the wallGroupManualJ attribute.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="A"> <xsd:annotation> <xsd:documentation>Fastest heat transfer</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="B"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="C"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="D"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="E"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="F"> <xsd:annotation> <xsd:documentation>Medium heat transfer</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="G"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="H"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="I"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="J"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="K"> <xsd:annotation> <xsd:documentation>Slowest heat transfer</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType waterUseUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | WaterUsePerCycle/@unit
facets |
enumeration | CubicMeters
enumeration | Gallons
enumeration | Tons
enumeration | Kilograms
enumeration | Liters
source | <xsd:simpleType name="waterUseUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="CubicMeters"/> <xsd:enumeration value="Gallons"/> <xsd:enumeration value="Tons"/> <xsd:enumeration value="Kilograms"/> <xsd:enumeration value="Liters"/> </xsd:restriction> </xsd:simpleType>

simpleType weightUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
used by |
attribute | Weight/@unit
facets |
enumeration | Pounds
enumeration | Kilograms
enumeration | Tons
source | <xsd:simpleType name="weightUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Pounds"/> <xsd:enumeration value="Kilograms"/> <xsd:enumeration value="Tons"/> </xsd:restriction> </xsd:simpleType>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy