Schema GreenBuildingXML_Ver8.01.xsd

schema location: | E:\Data\Carmel\gbXML\Schemas_Archived\GreenBuildingXML_Ver8.01.xsd
attributeFormDefault: | unqualified
elementFormDefault: | unqualified
targetNamespace: | http://www.gbxml.org/schema

Elements | Complex types | Simple types
Absorptance | CustomProbabilityModelType | absorptanceUnitEnum
Accommodating | eqConstantValueType | airTemperatureTypeEnum
Actions | eqGaussianNormal1DType | areaUnitEnum
Activity | eqLinear1DType | baseboardHeatingTypeEnum
ActivityDuration | eqLinear2DType | blowerDoorUnitEnum
ActivityOccurModel | eqLinear3DType | buildingSystemTypeEnum
Address1 | eqLogit1DLinearType | buildingTypeEnum
Address2 | eqLogit1DQuadraticType | capacityTypeEnum
AdjacentSpaceId | eqLogit2DLinearType | capacityUnitEnum
aecXML | eqLogit3DLinearType | chillerTypeEnum
Age | eqQuadratic1DType | ClimateZoneType
AirChangesPerHour | eqWeibull1D3P | coilTypeEnum
AirLoop | MarkovChainModelType | CommuteModeType
AirLoopEquipment | MeetingDurationProbabilityType | conditioningTypeEnum
AirLoopEquipmentId | NormalDurationModelType | conditioningUnitEnum
AirLoopId | NormalProbabilityModelType | conditionTypeEnum
AirStreamFraction | OperationRange | conductivityFofTUnitEnum
AirSystem | SpaceOccupancyType | conductivityUnitEnum
AirSystemId |  | controlTypeEnum
AirTemperature |  | coolingCoilSetpointResetTypeEnum
Albedo |  | coolingCoilTypeEnum
AltEnergySource |  | costTypeEnum
AnalysisParameter |  | currencyTypeEnum
Area |  | damperHeatingActionEnum
ASHRAEComfortEnvelope |  | dayTypeEnum
ASHRAEComfortTemperatures |  | defrostControlEnum
ASHRAECoolingAdaptiveComfort |  | defrostStrategyEnum
AverageNumberOfFloors |  | deltaPUnitEnum
Azimuth |  | densityFofTUnitEnum
Ballast |  | densityUnitEnum
BaseboardHeatingCapacity |  | directionUnitEnum
BaseboardHeatingType |  | economizerLockoutEnum
BeginDate |  | EducationType
Behavior |  | efficiencyTypeEnum
BehaviorID |  | emissionUnitEnum
Behaviors |  | emittanceTypeEnum
BiomassDensity |  | EmploymentType
Blind |  | energyUnitEnum
BlowerDoorValue |  | enthalpyTypeEnum
Building |  | enthalpyUnitEnum
BuildingStorey |  | entityTypeEnum
BuildingSystems |  | equipmentTypeEnum
CADMaterialId |  | extEquipTypeEnum
CADModelAzimuth |  | fanTypeEnum
CADModelId |  | floorCategoryEnum
CADObjectId |  | floorSlabPerimeterHeatLossCoefficientUnitTypeEnum
Campus |  | flowPerAreaUnitEnum
Capacity |  | flowTypeEnum
CartesianPoint |  | flowUnitEnum
CDD |  | fluidTypeEnum
CDDValue |  | frameTypeEnum
City |  | fuelLoadUnitEnum
ClimateZone |  | gasTypeEnum
ClosedShell |  | GenderType
CLTDParameters |  | GroupPriority
CoefficientA |  | heatExchangerTypeEnum
CoefficientB |  | heatingCoilSetpointResetTypeEnum
CoefficientC |  | heatingCoilTypeEnum
CoefficientD |  | heatRecoveryTypeEnum
CoefficientOfUtilization |  | hOutsideUnitTypeEnum
CommuteMode |  | HVACTypeEnum
CompanyName |  | hydronicEquipTypeEnum
Conductivity |  | illuminanceUnitEnum
ConductivityFofT |  | IncomeGroupType
ConstantValue |  | infiltrationTypeEnum
Construction |  | InfrastructureType
Control |  | intEquipTypeEnum
ControlValue |  | interactionType
ConvergenceLimits |  | inverseTempUnitEnum
CoolingCoilSetpointResetType |  | JobType
CoolingCoilType |  | lengthUnitEnum
CoolingSizingFactor |  | LifeStyleType
CoolingTemperature |  | lifeUnitEnum
Coordinate |  | lightControlTypeEnum
Cost |  | lightTypeEnum
CostConscious |  | loadUnitEnum
CostValue |  | loopTypeEnum
Country |  | MaritalStatusType
CreatedBy |  | minimumOutdoorAirControlTypeEnum
CustomProbabilityModel |  | nightCycleControlEnum
CyclesPerWeek |  | openingTypeEnum
CyclingRateMax |  | operationTypeEnum
DamperHeatingAction |  | OtherConstraintType
Data |  | parameterType
Day |  | peopleHeatGainTypeEnum
DaylightSavings |  | peopleHeatGainUnitEnum
DayofWeek |  | peopleNumberUnitEnum
DaySchedule |  | permUnitEnum
DDDayCool |  | plugLoadTypeEnum
DDDayHeat |  | PolicyType
DDDaylightCool |  | powerPerAreaUnitEnum
DDDaylightHeat |  | powerTypeEnum
DDDBCool |  | powerUnitEnum
DDDBHeat |  | powerUseTypeEnum
DDDBRangeCool |  | preheatCoilTypeEnum
DDDBRangeHeat |  | pressureUnitEnum
DDGroundTCool |  | radiationWavelengthTypeEnum
DDGroundTHeat |  | reflectanceTypeEnum
DDHiHrCool |  | resetTemperatureTypeEnum
DDHiHrHeat |  | resistanceUnitEnum
DDLoHrCool |  | resourceTypeEnum
DDLoHrHeat |  | resultsExtraResourceTypeEnum
DDMonthCool |  | resultsTypeEnum
DDMonthHeat |  | roofASHRAENumberEnum
DDPressureCool |  | roofCLTDIndexEnum
DDPressureHeat |  | roofColorEnum
DDRainCool |  | roofCTSTypeEnum
DDRainHeat |  | RoomEventType
DDSkyClearnessCool |  | roughnessValueEnum
DDSkyClearnessHeat |  | scheduleTypeEnum
DDSnowCool |  | scheduleTypeLimitsEnum
DDSnowHeat |  | SeasonType
DDWBCool |  | shadeAndBlindTypeEnum
DDWBHeat |  | shadeOperationEnum
DDWindDirCool |  | shadeScheduleTypeEnum
DDWindDirHeat |  | shadeTypeEnum
DDWindSpeedCool |  | sinkRateUnitEnum
DDWindSpeedHeat |  | SpaceCategory
DeltaP |  | spaceTypeEnum
DeltaT |  | specificHeatUnitEnum
Density |  | stageTypeEnum
DensityFofT |  | standardsTypeEnum
DependentValue |  | stationIdTypeEnum
DependentVariable |  | statusTransitionEventType
Description |  | subjectiveValueType
DesignCoolRH |  | supplementalHeatingCoilTypeEnum
DesignCoolT |  | surfaceDescriptionEnum
DesignFlow |  | surfaceReferenceLocationEnum
DesignHeatRH |  | surfaceTypeEnum
DesignHeatT |  | systemTypeEnum
DesignPressure |  | temperatureUnitEnum
DesignTemp |  | tempTypeEnum
Dimensions |  | thermostatTypeEnum
DocumentHistory |  | TimeofDayType
Drivers |  | timePeriodEnum
EconomizerLockout |  | timeUnitEnum
Education |  | transportationTypeEnum
Efficiency |  | TypesDataCollectedList
ElecLoad |  | unitlessSmallUnitEnum
Elevation |  | unitlessUnitEnum
Email1Address |  | uValueUnitEnum
EmissionRate |  | valueTypeEnum
Emittance |  | vegetationTypeEnum
Employment |  | velocityUnitEnum
EndDate |  | versionEnum
EndDay |  | viscosityFofTUnitEnum
EndHour |  | viscosityUnitEnum
EndMinute |  | volumeUnitEnum
EndMonth |  | wallASHRAEGroupEnum
Energy |  | wallColorEnum
Enthalpy |  | wallCTSTypeEnum
Environment |  | wallGroupManualJEnum
EnvironmentAwareness |  | waterUseUnitEnum
Equation |  | weightUnitEnum
EquipPowerPerArea |  | windowTypeEnum
EventDuration |  | windSpeedEnum
EventOccurModel |  | zoneHVACEquipmentTypeEnum
Expression |  |
ExtEquip |  |
ExtEquipId |  |
FamilyName |  |
Fan |  |
FileName |  |
Fire |  |
FireFace |  |
FirstName |  |
FloorSlabHeatLossCoefficient |  |
Flow |  |
FlowControl |  |
FlowPerArea |  |
FlowPerPerson |  |
FlowType |  |
Formula |  |
FractionOnCyclePowerUse |  |
Frame |  |
FuelLoad |  |
Gap |  |
GapId |  |
GasPreheatCoilEfficiency |  |
GasPreheatCoilParasiticElectricLoad |  |
gbXML |  |
Gender |  |
GeneralGeometry |  |
GeographicLocation |  |
Glare |  |
Glaze |  |
GlazeConductivity |  |
GlazeId |  |
GroundTemp |  |
GroundTempValue |  |
GroupPriority |  |
GUID |  |
HDD |  |
HDDValue |  |
HeatExchanger |  |
HeatingCoilSetpointResetType |  |
HeatingSizingFactor |  |
HeatingTemperature |  |
HeatPumpDefrostControl |  |
HeatPumpDefrostStrategy |  |
HeatPumpFanDelayTime |  |
HeatPumpTimeConstant |  |
HeatRecoveryType |  |
HeatRejectedtoSpace |  |
Height |  |
HighLimit |  |
HighValue |  |
HolidayDate |  |
HolidaysModeled |  |
HorizontalSolar |  |
HOutside |  |
HVAC |  |
HVACType |  |
HydronicLoop |  |
HydronicLoopEquipment |  |
HydronicLoopEquipmentId |  |
HydronicLoopId |  |
IAQ |  |
Illuminance |  |
ImageTexture |  |
IncomeGroup |  |
IndependentValue |  |
IndependentVariable |  |
IndoorAirQuality |  |
InfiltrationFlow |  |
Infrastructure |  |
InputWatts |  |
InsideAirFilmResistance |  |
IntEquip |  |
IntEquipId |  |
Interaction |  |
InteractionType |  |
IsSpecialBehavior |  |
JobType |  |
Lamp |  |
LastName |  |
LatentHeatRecoveryEffectiveness |  |
LatentLoad |  |
Latitude |  |
Layer |  |
LayerId |  |
Length |  |
Level |  |
Life |  |
LifeStyle |  |
LightControlId |  |
LightId |  |
Lighting |  |
LightingControl |  |
LightingSystem |  |
LightPowerPerArea |  |
Lights |  |
LightType |  |
Linear1D |  |
Linear2D |  |
Linear3D |  |
LoadCalcInputParameters |  |
Location |  |
Logit1D |  |
Logit1DQuadratic |  |
Logit2D |  |
Logit3D |  |
Longitude |  |
LowerBound |  |
LowerLimitValue |  |
LowValue |  |
LumensPerLamp |  |
Luminaire |  |
ManualJ8Parameters |  |
Manufacturer |  |
MaritalStatus |  |
MarkovChainModel |  |
Material |  |
MaterialId |  |
MaximumFlow |  |
MaximumFlowFractionDuringReheat |  |
MaxNumberOfMeetingsPerDay |  |
MaxNumOccupantsPerMeeting |  |
MaxOAFlowPerZone |  |
MaxPressure |  |
MaxRelativeHumidity |  |
MaxTemp |  |
Mean |  |
MeetingDuration |  |
MeetingDurationProbability |  |
MeetingEvent |  |
Meter |  |
MeterId |  |
MiddleName |  |
MinFlow |  |
MinimumFlow |  |
MinimumOutdoorAirControlType |  |
MinLightFrac |  |
MinNumberOfMeetingsPerDay |  |
MinNumOccupantsPerMeeting |  |
MinOAFlowPerZone |  |
MinPowerFrac |  |
MinPressure |  |
MinRelativeHumidity |  |
MinTemp |  |
Model |  |
ModifiedBy |  |
MotorInAirstream |  |
MovementBehavior |  |
MovementBehaviorID |  |
Name |  |
NaturalVentHiTemp |  |
NaturalVentLoTemp |  |
NaturalVentOccDep |  |
Needs |  |
NightCycleControl |  |
NormalDurationModel |  |
NormalProbabilityModel |  |
NumberOfLamps |  |
OAFlowPerArea |  |
OAFlowPerPerson |  |
OAFlowPerZone |  |
ObjectId |  |
Occupant |  |
OccupantBehavior |  |
Occupants |  |
Opening |  |
OperationSchedule |  |
OtherConstraint |  |
ParallelFanOnFlowFraction |  |
Parameter |  |
Parameter1ID |  |
Parameter2ID |  |
Parameter3ID |  |
ParameterRange |  |
ParameterType |  |
ParameterValue |  |
PastExperience |  |
PeakDomesticHotWaterFlow |  |
PeopleHeatGain |  |
PeopleNumber |  |
PercentAreaDaylitControlled |  |
PercentExisting |  |
Performance |  |
Permeance |  |
PersonInfo |  |
PhoneNumber |  |
Photometry |  |
PhotometryOrientation |  |
Physical |  |
PlanarGeometry |  |
Platform |  |
PlugLoad |  |
PlugLoadType |  |
PointData |  |
Policy |  |
PolyLoop |  |
Porosity |  |
Power |  |
PrandtlNumber |  |
PrandtlNumberFofT |  |
PreheatCoilType |  |
PressureControl |  |
Priority |  |
Probability |  |
ProductName |  |
ProgramInfo |  |
ProjectEntity |  |
Quadratic1D |  |
R-value |  |
RandomMovementEvent |  |
RatedFlow |  |
RecircFlow |  |
RectangularGeometry |  |
RecycledContent |  |
Reference |  |
Reflectance |  |
RefrigerantType |  |
ResetTemperature |  |
Results |  |
RoomEventType |  |
Roughness |  |
RTSParameters |  |
Schedule |  |
ScheduleTypeLimits |  |
ScheduleValue |  |
Seasons |  |
SeasonType |  |
SecondaryFlow |  |
SensibleHeatRecoveryEffectiveness |  |
Setback |  |
ShadeAndBlindType |  |
ShadeControl |  |
ShadesAndBlinds |  |
ShadeSchedule |  |
ShadingCoeff |  |
ShellGeometry |  |
SimulationParameters |  |
SinkRate |  |
SocialInfluence |  |
SocioEconomic |  |
SolarHeatGainCoeff |  |
SolarOnOpening |  |
Space |  |
SpaceBoundary |  |
SpaceOccupancy |  |
SpecificHeat |  |
StartDay |  |
StartHour |  |
StartMinute |  |
StartMonth |  |
State |  |
StateOrProvince |  |
StationId |  |
StatusOfActivity |  |
StatusTransitionEvent |  |
StatusTransitionEventType |  |
StatusTransitionProbability |  |
StDev |  |
StreetAddress |  |
SubjectiveValues |  |
SupplementalGasHeatingCoilEfficiency |  |
SupplementalGasHeatingCoilParasiticElectricLoad |  |
SupplementalHeatingCoilCapacity |  |
SupplementalHeatingCoilType |  |
Surface |  |
TechnologyOriented |  |
Temp |  |
Temperature |  |
TemperatureControl |  |
TemperatureProbabilityModel |  |
Thermal |  |
Thermostats |  |
ThermostatType |  |
Thickness |  |
Tilt |  |
Time |  |
TimeFrequencyType |  |
TimeIncrement |  |
TimeofDay |  |
TimeofDays |  |
Transmittance |  |
Transportation |  |
TypeCode |  |
U-value |  |
UpperBound |  |
UpperLimitValue |  |
URI |  |
UtilityRate |  |
Value |  |
Vegetation |  |
Version |  |
Viscosity |  |
ViscosityFofT |  |
Visual |  |
Volume |  |
WasteWaterHREff |  |
WaterLoss |  |
WaterRate |  |
WaterUsePerCycle |  |
Weather |  |
WebPage |  |
WeekSchedule |  |
WeekScheduleId |  |
Weibull1D |  |
Weight |  |
WFTDPressure |  |
WFTDRelHumidity |  |
WFTDTemp |  |
WFTDWindDir |  |
WFTDWindSpeed |  |
Width |  |
Windows |  |
WindowType |  |
WindowTypeSimple |  |
WindSpeed |  |
XAxis |  |
YAxis |  |
YearModeled |  |
YearSchedule |  |
ZipCode |  |
ZipcodeOrPostalCode |  |
Zone |  |
ZoneCoolingLoad |  |
ZoneHVACEquipment |  |
ZoneHVACEquipmentId |  |

element Absorptance

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Construction FireFace Material
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | unitlessUnitEnum | required |  |  |
type | absorptanceUnitEnum | required |  |  |
annotation |
documentation
Absorptance of the outside surface
source | <xsd:element name="Absorptance"> <xsd:annotation> <xsd:documentation>Absorptance of the outside surface</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> <xsd:attribute name="type" type="absorptanceUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Absorptance/@unit

type | unitlessUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Percent |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

attribute Absorptance/@type

type | absorptanceUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | IntIR |
enumeration | IntSolar |
enumeration | IntVisible |
enumeration | IntTotal |
enumeration | ExtIR |
enumeration | ExtSolar |
enumeration | ExtVisible |
enumeration | ExtTotal |
source | <xsd:attribute name="type" type="absorptanceUnitEnum" use="required"/>

element Accommodating

diagram |
namespace | http://www.gbxml.org/schema
type | subjectiveValueType
properties |
content | simple
used by |
element | SubjectiveValues
facets |
Kind | Value | Annotation
enumeration | High |
enumeration | Medium |
enumeration | Low |
source | <xsd:element name="Accommodating" type="subjectiveValueType"/>

element Actions

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Interaction
used by |
element | Behavior
annotation |
documentation
Occupants can conduct an action in order to satisfy their needs. The action may be an interaction with a system or movement to another location.
source | <xsd:element name="Actions"> <xsd:annotation> <xsd:documentation>Occupants can conduct an action in order to satisfy their needs. The action may be an interaction with a system or movement to another location. </xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice> <xsd:element ref="Interaction" minOccurs="0"/> </xsd:choice> </xsd:complexType> </xsd:element>

element Activity

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description StatusOfActivity
used by |
element | Behaviors
attributes |
Name | Type | Use | Default | Fixed | Annotation
ID | xsd:ID | required |  |  |
Name | xsd:string | optional |  |  |
IfcGuid | xsd:string | optional |  |  |
annotation |
documentation
Regarding the types of activities of an occupant
source | <xsd:element name="Activity"> <xsd:annotation> <xsd:documentation>Regarding the types of activities of an occupant </xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:sequence> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="StatusOfActivity" maxOccurs="unbounded"/> </xsd:sequence> <xsd:attribute name="ID" type="xsd:ID" use="required"/> <xsd:attribute name="Name" type="xsd:string" use="optional"/> <xsd:attribute name="IfcGuid" type="xsd:string" use="optional"/> </xsd:complexType> </xsd:element>

attribute Activity/@ID

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="ID" type="xsd:ID" use="required"/>

attribute Activity/@Name

type | xsd:string
properties |
use | optional
source | <xsd:attribute name="Name" type="xsd:string" use="optional"/>

attribute Activity/@IfcGuid

type | xsd:string
properties |
use | optional
source | <xsd:attribute name="IfcGuid" type="xsd:string" use="optional"/>

element ActivityDuration

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | NormalDurationModel
used by |
element | StatusOfActivity
annotation |
documentation
Duration properties of an activity. If specify, the event will end after the duration.
source | <xsd:element name="ActivityDuration"> <xsd:annotation> <xsd:documentation>Duration properties of an activity. If specify, the event will end after the duration.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:sequence> <xsd:element ref="NormalDurationModel"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element ActivityOccurModel

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | CustomProbabilityModel NormalProbabilityModel
used by |
element | StatusOfActivity
annotation |
documentation
The event occur model
source | <xsd:element name="ActivityOccurModel"> <xsd:annotation> <xsd:documentation>The event occur model</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice> <xsd:element ref="CustomProbabilityModel"/> <xsd:element ref="NormalProbabilityModel"/> </xsd:choice> </xsd:complexType> </xsd:element>

element Address1

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | PersonInfo
source | <xsd:element name="Address1" type="xsd:string"/>

element Address2

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | PersonInfo
source | <xsd:element name="Address2" type="xsd:string"/>

element AdjacentSpaceId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | Surface
attributes |
Name | Type | Use | Default | Fixed | Annotation
spaceIdRef | xsd:IDREF | required |  |  |
documentation
References the ID of a Space that is bounded by this surface. First AdjacentSpaceId entered will determine how the referenced construction layers are ordered with the first construction layer being in contact with the outside or 2nd space listed and the last layer in contact with the first space listed. The outward normal of the surface, as defined by the right hand rule of the coordinates in the planar geometry element, is always pointing away from the first AdjacentSpaceID listed.
surfaceType | surfaceTypeEnum | optional |  |  |
documentation
With interior horizontal surfaces, this attribute can distinguish between ceiling and floor surfaces to avoid double-counting of floor areas, etc. If not present, the surface type can be assumed based on the description of the surface type enums. When the surfaceTypeEnum is provided and the surface attributes (i.e. adjacency, tilt angle) do not match the enumeration's description, the enumeration should have precedence.
source | <xsd:element name="AdjacentSpaceId"> <xsd:complexType> <xsd:attribute name="spaceIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>References the ID of a Space that is bounded by this surface. First AdjacentSpaceId entered will determine how the referenced construction layers are ordered with the first construction layer being in contact with the outside or 2nd space listed and the last layer in contact with the first space listed. The outward normal of the surface, as defined by the right hand rule of the coordinates in the planar geometry element, is always pointing away from the first AdjacentSpaceID listed.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="surfaceType" type="surfaceTypeEnum" use="optional"> <xsd:annotation> <xsd:documentation>With interior horizontal surfaces, this attribute can distinguish between ceiling and floor surfaces to avoid double-counting of floor areas, etc. If not present, the surface type can be assumed based on the description of the surface type enums. When the surfaceTypeEnum is provided and the surface attributes (i.e. adjacency, tilt angle) do not match the enumeration's description, the enumeration should have precedence.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute AdjacentSpaceId/@spaceIdRef

type | xsd:IDREF
properties |
use | required
annotation |
documentation
References the ID of a Space that is bounded by this surface. First AdjacentSpaceId entered will determine how the referenced construction layers are ordered with the first construction layer being in contact with the outside or 2nd space listed and the last layer in contact with the first space listed. The outward normal of the surface, as defined by the right hand rule of the coordinates in the planar geometry element, is always pointing away from the first AdjacentSpaceID listed.
source | <xsd:attribute name="spaceIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>References the ID of a Space that is bounded by this surface. First AdjacentSpaceId entered will determine how the referenced construction layers are ordered with the first construction layer being in contact with the outside or 2nd space listed and the last layer in contact with the first space listed. The outward normal of the surface, as defined by the right hand rule of the coordinates in the planar geometry element, is always pointing away from the first AdjacentSpaceID listed.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute AdjacentSpaceId/@surfaceType

type | surfaceTypeEnum
properties |
use | optional
facets |
Kind | Value | Annotation
enumeration | InteriorWall |
documentation
The portion of the building envelope, including opaque area and fenestration, that is adjacent to two conditioned or unconditioned spaces and that is vertical or tilted at an angle of 60° from horizontal or greater.
enumeration | ExteriorWall |
documentation
The portion of the building envelope, including opaque area and fenestration, that is adjacent to one conditioned or unconditioned space and that is vertical or tilted at an angle of 60° from horizontal or greater.
enumeration | Roof |
documentation
The upper portion of the building envelope, including opaque areas and fenestration, that is adjacent to one conditioned or unconditioned space and that is horizontal or tilted at an angle of less than 60° from horizontal.
enumeration | InteriorFloor |
documentation
The lower portion of the building envelope, including opaque area and fenestration, that has conditioned or semiheated space above and is horizontal or tilted at an angle of less than 60 degrees from horizontal but excluding slab-on-grade floors.
enumeration | ExposedFloor |
documentation
The floor area exposed to non-conditioned space or outside.
enumeration | Shade |
documentation
Surface not adjacent to any spaces with tilt between 0° and 180°.
enumeration | UndergroundWall |
documentation
The portion of the building envelope, including opaque area and fenestration, that is adjacent to one conditioned or unconditioned space and earth (soil) and that is vertical or tilted at an angle of 60° from horizontal or greater.
enumeration | UndergroundSlab |
documentation
Surface adjacent to one conditioned or unconditioned space and earth (soil) below grade with a tilt between 150° and 180°.
enumeration | Ceiling |
documentation
The upper portion of the building envelope that is adjacent to two conditioned or unconditioned spaces and that is horizontal or tilted at an angle of less than 60° from horizontal.
enumeration | Air |
documentation
Air membrane between two conditioned or unconditioned spaces with a tilt between 0° and 180°.
enumeration | UndergroundCeiling |
documentation
The portion of the building envelope, including opaque area and fenestration, that is adjacent to one conditioned or unconditioned space and earth (soil) and that is horizontal or tilted at an angle of less than 60° from horizontal.
enumeration | RaisedFloor |
documentation
The lower portion of the building envelope, including opaque area and fenestration, that is adjacent to one conditioned or unconditioned space and the outside and is horizontal or tilted at an angle between 150° and 180°.
enumeration | SlabOnGrade |
documentation
The lower portion of the building envelope, including opaque area and fenestration, that is adjacent to one conditioned or unconditioned space and earth (soil) at grade with a tilt between 150° and 180°.
enumeration | FreestandingColumn |
documentation
Freestanding column in space specified by its top surface having the same ifcGUID.
enumeration | EmbeddedColumn |
documentation
Embedded column in wall specified by a surface which is coplanar with (one of) the embedding wall(s).
annotation |
documentation
With interior horizontal surfaces, this attribute can distinguish between ceiling and floor surfaces to avoid double-counting of floor areas, etc. If not present, the surface type can be assumed based on the description of the surface type enums. When the surfaceTypeEnum is provided and the surface attributes (i.e. adjacency, tilt angle) do not match the enumeration's description, the enumeration should have precedence.
source | <xsd:attribute name="surfaceType" type="surfaceTypeEnum" use="optional"> <xsd:annotation> <xsd:documentation>With interior horizontal surfaces, this attribute can distinguish between ceiling and floor surfaces to avoid double-counting of floor areas, etc. If not present, the surface type can be assumed based on the description of the surface type enums. When the surfaceTypeEnum is provided and the surface attributes (i.e. adjacency, tilt angle) do not match the enumeration's description, the enumeration should have precedence.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element aecXML

diagram |
namespace | http://www.gbxml.org/schema
used by |
element | gbXML
source | <xsd:element name="aecXML"/>

element Age

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:string
properties |
content | complex
used by |
elements | ExtEquip HydronicLoopEquipment IntEquip SocioEconomic
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | derived by: xsd:NMTOKEN | required |  |  |
source | <xsd:element name="Age"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:string"> <xsd:attribute name="unit" use="required"> <xsd:simpleType> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Years"/> </xsd:restriction> </xsd:simpleType> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Age/@unit

type | restriction of xsd:NMTOKEN
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Years |
source | <xsd:attribute name="unit" use="required"> <xsd:simpleType> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Years"/> </xsd:restriction> </xsd:simpleType> </xsd:attribute>

element AirChangesPerHour

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
elements | Space Zone
source | <xsd:element name="AirChangesPerHour" type="xsd:decimal"/>

element AirLoop

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Reference AirLoopEquipment TemperatureControl PressureControl
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
controlZoneIdRef | xsd:IDREF |  |  |  |
systemType | systemTypeEnum |  |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
annotation |
documentation
The AirLoop element represents the equipment serving one path of air
source | <xsd:element name="AirLoop"> <xsd:annotation> <xsd:documentation>The AirLoop element represents the equipment serving one path of air</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Reference" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="AirLoopEquipment" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="TemperatureControl" minOccurs="0"/> <xsd:element ref="PressureControl" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="controlZoneIdRef" type="xsd:IDREF"/> <xsd:attribute name="systemType" type="systemTypeEnum"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute AirLoop/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute AirLoop/@controlZoneIdRef

type | xsd:IDREF
source | <xsd:attribute name="controlZoneIdRef" type="xsd:IDREF"/>

attribute AirLoop/@systemType

type | systemTypeEnum
facets |
Kind | Value | Annotation
enumeration | SingleZoneReheat |
documentation
Variable Temperature
enumeration | PackagedSingleZone |
documentation
Packaged Single-zone
enumeration | SingleZoneCeilingInduction |
documentation
Ceiling Induction
enumeration | ReheatFan |
documentation
Constant-volume Reheat Fan
enumeration | VariableAirVolume |
documentation
Variable-volume Fan
enumeration | PoweredInductionUnit |
documentation
Powered Induction Unit
enumeration | PackagedVariableAirVolume |
documentation
Packaged Variable Air Volume
enumeration | PackagedVariableVolumeVariableTemperature |
documentation
Packaged Variable-Volume Variable-Temperature
enumeration | CeilingBypassVariableAirVolume |
documentation
Ceiling Bypass
enumeration | EvaporativeCooling |
documentation
Evaporative Cooling
enumeration | MultiZone |
documentation
Multizone Fan
enumeration | PackagedMultiZone |
documentation
Packaged Multizone
enumeration | DualDuct |
documentation
Dual-duct Fan
enumeration | FanCoil |
documentation
Fan Coil
enumeration | InductionUnit |
documentation
Induction Unit
enumeration | PackagedTerminalAirConditioner |
documentation
Packaged Terminal Air Conditioner
enumeration | WaterLoopHeatPump |
documentation
Water Loop Heat Pump
enumeration | ResidentialCyclingFurnaceCyclingAC |
documentation
Residential with cycling furnace and cycling air-conditioner
enumeration | ResidentialVariableAirVolumeVariableTemperature |
documentation
Residential Variable-Volume Variable-Temperature
enumeration | FloorPanelHeating |
documentation
Floor Panel Heating
enumeration | HeatingAndVentilating |
documentation
Heating and Ventilating
enumeration | UnitHeater |
documentation
Unit Heater
enumeration | UnitVentilator |
documentation
Unit Ventilator
enumeration | CentralHeatingRadiators |
documentation
Central Heating Radiators
enumeration | CentralHeatingConvectors |
documentation
Central Heating Convectors
enumeration | CentralHeatingRadiantFloor |
documentation
Central Heating Radiant Floor
enumeration | CentralHeatingHotAir |
documentation
Central Heating Hot Air
enumeration | OtherRoomHeater |
documentation
Other Room Heater
enumeration | RadiantHeaterNoFlue |
documentation
Radiant Heater No Flue
enumeration | RadiantHeaterFlue |
documentation
Radiant Heater Flue
enumeration | RadiantHeaterMultiburner |
documentation
Radiant Heater Multiburner
enumeration | ForcedConvectionHeaterFlue |
documentation
Forced Convection Heater Flue
enumeration | ForcedConvectionHeaterNoFlue |
documentation
Forced Convection Heater No Flue
enumeration | VAVSingleDuct |
documentation
VAV Single Duct
enumeration | VAVDualDuct |
documentation
VAV Dual Duct
enumeration | VAVReheatFan |
documentation
VAV Reheat Fan
enumeration | VAVIndoorPackagedCabinet |
documentation
VAV Indoor Packaged Cabinet
enumeration | ConstantVolumeFixedOA |
documentation
Constant Volume Fixed OA
enumeration | ConstantVolumeVariableOA |
documentation
Constant Volume Variable OA
enumeration | ConstantVolumeTerminalReheat |
documentation
Constant Volume Terminal Reheat
enumeration | MultizoneHotDeckColdDeck |
documentation
Multizone Hot Deck Cold Deck
enumeration | ConstantVolumeDualDuct |
documentation
Constant Volume Dual Duct
enumeration | RadiantCooledCeilings |
documentation
Radiant Cooled Ceilings
enumeration | ActiveChilledBeams |
documentation
Active Chilled Beams
enumeration | VariableRefrigerantFlow |
documentation
Variable Refrigerant Flow
enumeration | SplitSystemsWithNaturalVentilation |
documentation
Split Systems With Natural Ventilation
enumeration | SplitSystemsWithMechanicalVentilation |
documentation
Split Systems With Mechanical Ventilation
enumeration | SplitSystemsWithMechanicalVentilationWithCooling |
documentation
Split Systems With Mechanical Ventilation With Cooling
enumeration | Exhaust |
documentation
Exhaust Air Systems
source | <xsd:attribute name="systemType" type="systemTypeEnum"/>

attribute AirLoop/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element AirLoopEquipment

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Model Manufacturer RatedFlow MinFlow MaximumFlow MaximumFlowFractionDuringReheat OperationSchedule MotorInAirstream Temp Enthalpy EconomizerLockout ResetTemperature DeltaP DeltaT MinRelativeHumidity MaxRelativeHumidity Power Capacity Control Efficiency AirStreamFraction Performance Cost Weight Life WaterLoss Energy HydronicLoopId Reference RefrigerantType CADObjectId GeneralGeometry ShellGeometry FlowType ParallelFanOnFlowFraction NightCycleControl HeatRecoveryType SensibleHeatRecoveryEffectiveness LatentHeatRecoveryEffectiveness CoolingCoilSetpointResetType HeatingCoilSetpointResetType DamperHeatingAction HeatPumpDefrostControl HeatPumpDefrostStrategy SupplementalHeatingCoilType SupplementalHeatingCoilCapacity SupplementalGasHeatingCoilEfficiency SupplementalGasHeatingCoilParasiticElectricLoad CyclingRateMax HeatPumpTimeConstant FractionOnCyclePowerUse HeatPumpFanDelayTime CoolingCoilType PreheatCoilType GasPreheatCoilEfficiency GasPreheatCoilParasiticElectricLoad
used by |
element | AirLoop
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
equipmentType | equipmentTypeEnum | required |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
annotation |
documentation
A piece of equipment serving an air-loop. This is generalized to be able to contain any type of air loop equipment. The air loop equipment are ordered as they exist on the airloop. A blow-through system should have fan listed before the coils. A draw-through system should have the fan listed after the coils.
source | <xsd:element name="AirLoopEquipment"> <xsd:annotation> <xsd:documentation>A piece of equipment serving an air-loop. This is generalized to be able to contain any type of air loop equipment. The air loop equipment are ordered as they exist on the airloop. A blow-through system should have fan listed before the coils. A draw-through system should have the fan listed after the coils.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Model" minOccurs="0"/> <xsd:element ref="Manufacturer" minOccurs="0"/> <xsd:element ref="RatedFlow" minOccurs="0"/> <xsd:element ref="MinFlow" minOccurs="0"/> <xsd:element ref="MaximumFlow" minOccurs="0"> <xsd:annotation> <xsd:documentation>Maximum flow per zone floor area during reheat</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="MaximumFlowFractionDuringReheat" minOccurs="0"> <xsd:annotation> <xsd:documentation>Maximum flow flow fraction during reheat</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="OperationSchedule" minOccurs="0"/> <xsd:element ref="MotorInAirstream" minOccurs="0"/> <xsd:element ref="Temp" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Enthalpy" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="EconomizerLockout" minOccurs="0"/> <xsd:element ref="ResetTemperature" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="DeltaP" minOccurs="0"/> <xsd:element ref="DeltaT" minOccurs="0"/> <xsd:element ref="MinRelativeHumidity" minOccurs="0"/> <xsd:element ref="MaxRelativeHumidity" minOccurs="0"/> <xsd:element ref="Power" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Capacity" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Control" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Efficiency" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="AirStreamFraction" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Performance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Cost" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Weight" minOccurs="0"/> <xsd:element ref="Life" minOccurs="0"/> <xsd:element ref="WaterLoss" minOccurs="0"/> <xsd:element ref="Energy" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="HydronicLoopId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Reference" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="RefrigerantType" minOccurs="0"/> <xsd:element ref="CADObjectId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="GeneralGeometry" minOccurs="0"/> <xsd:element ref="ShellGeometry" minOccurs="0"/> <xsd:element ref="FlowType" minOccurs="0"/> <xsd:element ref="ParallelFanOnFlowFraction" minOccurs="0"/> <xsd:element ref="NightCycleControl" minOccurs="0"/> <xsd:element ref="HeatRecoveryType" minOccurs="0"/> <xsd:element ref="SensibleHeatRecoveryEffectiveness" minOccurs="0"/> <xsd:element ref="LatentHeatRecoveryEffectiveness" minOccurs="0"/> <xsd:element ref="CoolingCoilSetpointResetType" minOccurs="0"/> <xsd:element ref="HeatingCoilSetpointResetType" minOccurs="0"/> <xsd:element ref="DamperHeatingAction" minOccurs="0"/> <xsd:element ref="HeatPumpDefrostControl" minOccurs="0"/> <xsd:element ref="HeatPumpDefrostStrategy" minOccurs="0"/> <xsd:element ref="SupplementalHeatingCoilType" minOccurs="0"/> <xsd:element ref="SupplementalHeatingCoilCapacity" minOccurs="0"/> <xsd:element ref="SupplementalGasHeatingCoilEfficiency" minOccurs="0"/> <xsd:element ref="SupplementalGasHeatingCoilParasiticElectricLoad" minOccurs="0"/> <xsd:element ref="CyclingRateMax" minOccurs="0"/> <xsd:element ref="HeatPumpTimeConstant" minOccurs="0"/> <xsd:element ref="FractionOnCyclePowerUse" minOccurs="0"/> <xsd:element ref="HeatPumpFanDelayTime" minOccurs="0"/> <xsd:element ref="CoolingCoilType" minOccurs="0"/> <xsd:element ref="PreheatCoilType" minOccurs="0"/> <xsd:element ref="GasPreheatCoilEfficiency" minOccurs="0"/> <xsd:element ref="GasPreheatCoilParasiticElectricLoad" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="equipmentType" type="equipmentTypeEnum" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute AirLoopEquipment/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute AirLoopEquipment/@equipmentType

type | equipmentTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Fan |
enumeration | HeatExchanger |
enumeration | Coil |
enumeration | Furnace |
enumeration | Evaporative |
enumeration | Radiant |
enumeration | Economizer |
enumeration | Duct |
enumeration | Humidifier |
enumeration | Dehumidifier |
enumeration | UnitaryAC |
enumeration | UnitaryHP |
enumeration | SplitAC |
enumeration | SplitHP |
enumeration | TerminalUnit |
enumeration | Register |
enumeration | VAVBox |
enumeration | EvaporativePreCooler |
enumeration | PreheatCoil |
source | <xsd:attribute name="equipmentType" type="equipmentTypeEnum" use="required"/>

attribute AirLoopEquipment/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element AirLoopEquipmentId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | Space
attributes |
Name | Type | Use | Default | Fixed | Annotation
airLoopEquipIdRef | xsd:IDREF | required |  |  |
documentation
ID pointing at an air loop equipment object
source | <xsd:element name="AirLoopEquipmentId"> <xsd:complexType> <xsd:attribute name="airLoopEquipIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID pointing at an air loop equipment object</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute AirLoopEquipmentId/@airLoopEquipIdRef

type | xsd:IDREF
properties |
use | required
annotation |
documentation
ID pointing at an air loop equipment object
source | <xsd:attribute name="airLoopEquipIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID pointing at an air loop equipment object</xsd:documentation> </xsd:annotation> </xsd:attribute>

element AirLoopId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
elements | Space Zone
attributes |
Name | Type | Use | Default | Fixed | Annotation
airLoopIdRef | xsd:IDREF | required |  |  |
documentation
ID pointing to an air loop
source | <xsd:element name="AirLoopId"> <xsd:complexType> <xsd:attribute name="airLoopIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID pointing to an air loop</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute AirLoopId/@airLoopIdRef

type | xsd:IDREF
properties |
use | required
annotation |
documentation
ID pointing to an air loop
source | <xsd:attribute name="airLoopIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID pointing to an air loop</xsd:documentation> </xsd:annotation> </xsd:attribute>

element AirStreamFraction

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | AirLoopEquipment
annotation |
documentation
Fraction of motor in air stream
source | <xsd:element name="AirStreamFraction"> <xsd:annotation> <xsd:documentation>Fraction of motor in air stream</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"/> </xsd:simpleContent> </xsd:complexType> </xsd:element>

element AirSystem

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description CADObjectId HeatExchanger Fan HydronicLoopId AnalysisParameter
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | Annotation
preheatCoilType | heatingCoilTypeEnum | optional |  |  |
heatingCoilType | heatingCoilTypeEnum | required |  |  |
coolingCoilType | coolingCoilTypeEnum | required |  |  |
id | xsd:ID | required |  |  |
annotation |
documentation
This represents an alternative to the original DOE-2 based AirLoop element. This AirSystem element is geared toward an EnergyPlus and Open Studio workflow.
source | <xsd:element name="AirSystem"> <xsd:annotation> <xsd:documentation>This represents an alternative to the original DOE-2 based AirLoop element. This AirSystem element is geared toward an EnergyPlus and Open Studio workflow.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="CADObjectId" minOccurs="0"/> <xsd:element ref="HeatExchanger" minOccurs="0"/> <xsd:element ref="Fan" minOccurs="0"/> <xsd:element ref="HydronicLoopId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="AnalysisParameter" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="preheatCoilType" type="heatingCoilTypeEnum" use="optional"/> <xsd:attribute name="heatingCoilType" type="heatingCoilTypeEnum" use="required"/> <xsd:attribute name="coolingCoilType" type="coolingCoilTypeEnum" use="required"/> <xsd:attribute name="id" type="xsd:ID" use="required"/> </xsd:complexType> </xsd:element>

attribute AirSystem/@preheatCoilType

type | heatingCoilTypeEnum
properties |
use | optional
facets |
Kind | Value | Annotation
enumeration | ElectricResistance |
enumeration | Furnace |
enumeration | HotWater |
source | <xsd:attribute name="preheatCoilType" type="heatingCoilTypeEnum" use="optional"/>

attribute AirSystem/@heatingCoilType

type | heatingCoilTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | ElectricResistance |
enumeration | Furnace |
enumeration | HotWater |
source | <xsd:attribute name="heatingCoilType" type="heatingCoilTypeEnum" use="required"/>

attribute AirSystem/@coolingCoilType

type | coolingCoilTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | ChilledWater |
enumeration | ChilledWaterDetailedFlatModel |
enumeration | DirectExpansion |
source | <xsd:attribute name="coolingCoilType" type="coolingCoilTypeEnum" use="required"/>

attribute AirSystem/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

element AirSystemId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | ZoneHVACEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
airSystemIdRef | xsd:IDREF | required |  |  |
documentation
An unique identifier pointing to an air system.
source | <xsd:element name="AirSystemId"> <xsd:complexType> <xsd:attribute name="airSystemIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>An unique identifier pointing to an air system.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute AirSystemId/@airSystemIdRef

type | xsd:IDREF
properties |
use | required
annotation |
documentation
An unique identifier pointing to an air system.
source | <xsd:attribute name="airSystemIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>An unique identifier pointing to an air system.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element AirTemperature

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | ShadeControl
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | temperatureUnitEnum | required |  |  |
type | airTemperatureTypeEnum | required |  |  |
annotation |
documentation
Minimum air temperature before shades are closed.
source | <xsd:element name="AirTemperature"> <xsd:annotation> <xsd:documentation>Minimum air temperature before shades are closed.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum" use="required"/> <xsd:attribute name="type" type="airTemperatureTypeEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute AirTemperature/@unit

type | temperatureUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | F |
enumeration | C |
enumeration | K |
enumeration | R |
source | <xsd:attribute name="unit" type="temperatureUnitEnum" use="required"/>

attribute AirTemperature/@type

type | airTemperatureTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Outside |
enumeration | Zone |
source | <xsd:attribute name="type" type="airTemperatureTypeEnum" use="required"/>

element Albedo

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Construction Material
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | unitlessUnitEnum | required |  |  |
annotation |
documentation
Reflectance of solar radiation
source | <xsd:element name="Albedo"> <xsd:annotation> <xsd:documentation>Reflectance of solar radiation</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Albedo/@unit

type | unitlessUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Percent |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element AltEnergySource

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | MeterId
used by |
element | Campus
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
altEnergyType | derived by: xsd:NMTOKEN | required |  |  |
resourceType | resourceTypeEnum | required |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
annotation |
documentation
Alternative energy source
source | <xsd:element name="AltEnergySource"> <xsd:annotation> <xsd:documentation>Alternative energy source</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="MeterId" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="altEnergyType" use="required"> <xsd:simpleType> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Solar"/> <xsd:enumeration value="Wind"/> <xsd:enumeration value="Geothermal"/> <xsd:enumeration value="HeatRecovery"/> <xsd:enumeration value="NaturalGas"/> <xsd:enumeration value="Electrical"/> </xsd:restriction> </xsd:simpleType> </xsd:attribute> <xsd:attribute name="resourceType" type="resourceTypeEnum" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute AltEnergySource/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute AltEnergySource/@altEnergyType

type | restriction of xsd:NMTOKEN
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Solar |
enumeration | Wind |
enumeration | Geothermal |
enumeration | HeatRecovery |
enumeration | NaturalGas |
enumeration | Electrical |
source | <xsd:attribute name="altEnergyType" use="required"> <xsd:simpleType> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Solar"/> <xsd:enumeration value="Wind"/> <xsd:enumeration value="Geothermal"/> <xsd:enumeration value="HeatRecovery"/> <xsd:enumeration value="NaturalGas"/> <xsd:enumeration value="Electrical"/> </xsd:restriction> </xsd:simpleType> </xsd:attribute>

attribute AltEnergySource/@resourceType

type | resourceTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Electricity |
enumeration | NaturalGas |
enumeration | Propane |
enumeration | FuelOil1 |
enumeration | FuelOil2 |
enumeration | FuelOil4 |
enumeration | Water |
enumeration | ChilledWater |
enumeration | HotWater |
enumeration | Steam |
source | <xsd:attribute name="resourceType" type="resourceTypeEnum" use="required"/>

attribute AltEnergySource/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element AnalysisParameter

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description ParameterValue
used by |
elements | AirSystem Building HydronicLoop Space ZoneHVACEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
parameterType | xsd:string | required |  |  |
unit | xsd:string |  |  |  |
source | <xsd:element name="AnalysisParameter"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="ParameterValue" minOccurs="0"/> </xsd:choice> <xsd:attribute name="parameterType" type="xsd:string" use="required"/> <xsd:attribute name="unit" type="xsd:string"/> </xsd:complexType> </xsd:element>

attribute AnalysisParameter/@parameterType

type | xsd:string
properties |
use | required
source | <xsd:attribute name="parameterType" type="xsd:string" use="required"/>

attribute AnalysisParameter/@unit

type | xsd:string
source | <xsd:attribute name="unit" type="xsd:string"/>

element Area

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Building Space
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | areaUnitEnum |  |  |  |
annotation |
documentation
Specifies the area of the space or building. This value should be equal to the area enclosed by the physical boundaries of the space, as defined by the intersection of the horizontal plane at the highest floor height and the volumetric model's vertical interior surface planes. Building area should be the sum of space areas whose PeopleNumber element values are greater than zero.
source | <xsd:element name="Area"> <xsd:annotation> <xsd:documentation>Specifies the area of the space or building. This value should be equal to the area enclosed by the physical boundaries of the space, as defined by the intersection of the horizontal plane at the highest floor height and the volumetric model's vertical interior surface planes. Building area should be the sum of space areas whose PeopleNumber element values are greater than zero.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="areaUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Area/@unit

type | areaUnitEnum
facets |
Kind | Value | Annotation
enumeration | SquareKilometers |
enumeration | SquareMeters |
enumeration | SquareCentimeters |
enumeration | SquareMillimeters |
enumeration | SquareMiles |
enumeration | SquareYards |
enumeration | SquareFeet |
enumeration | SquareInches |
source | <xsd:attribute name="unit" type="areaUnitEnum"/>

element ASHRAEComfortEnvelope

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | ParameterRange
used by |
element | Thermal
annotation |
documentation
Range of indoor air temperatures can be given where occupants do not feel thermal discomfort and therefore, they don't carry out any actions.
source | <xsd:element name="ASHRAEComfortEnvelope"> <xsd:annotation> <xsd:documentation>Range of indoor air temperatures can be given where occupants do not feel thermal discomfort and therefore, they don't carry out any actions. </xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:sequence> <xsd:element ref="ParameterRange" maxOccurs="unbounded"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element ASHRAEComfortTemperatures

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | CoolingTemperature HeatingTemperature
used by |
element | Thermal
annotation |
documentation
A distribution of comfort cooling and heating temperatures can be given where occupants and therefore, they don't carry out any actions.
source | <xsd:element name="ASHRAEComfortTemperatures"> <xsd:annotation> <xsd:documentation>A distribution of comfort cooling and heating temperatures can be given where occupants and therefore, they don't carry out any actions. </xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:all> <xsd:element ref="CoolingTemperature" minOccurs="0"/> <xsd:element ref="HeatingTemperature" minOccurs="0"/> </xsd:all> </xsd:complexType> </xsd:element>

element ASHRAECoolingAdaptiveComfort

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | ParameterRange
used by |
element | Thermal
annotation |
documentation
Range of indoor air temperatures can be given where occupants do not feel thermal discomfort and therefore, they don't carry out any actions.
source | <xsd:element name="ASHRAECoolingAdaptiveComfort"> <xsd:annotation> <xsd:documentation>Range of indoor air temperatures can be given where occupants do not feel thermal discomfort and therefore, they don't carry out any actions. </xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:sequence> <xsd:element ref="ParameterRange" maxOccurs="unbounded"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element AverageNumberOfFloors

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Building
source | <xsd:element name="AverageNumberOfFloors" type="xsd:decimal"/>

element Azimuth

diagram |
namespace | http://www.gbxml.org/schema
type | restriction of xsd:double
properties |
content | simple
used by |
element | RectangularGeometry
facets |
Kind | Value | Annotation
minInclusive | 0 |
maxInclusive | 360 |
annotation |
documentation
Polygon azimuth. The direction of the outward normal for the polygon (surface or opening) defined in RectangularGeometry element. Azimuth is measured in degrees clockwise from North, where North = 0 degrees. Examples: East = 90 deg, South = 180 deg, West = 270 deg. If CADModelAzimuth is defined, the Azimuth value is relative to the CADModelAzimuth value rather then North.
source | <xsd:element name="Azimuth"> <xsd:annotation> <xsd:documentation>Polygon azimuth. The direction of the outward normal for the polygon (surface or opening) defined in RectangularGeometry element. Azimuth is measured in degrees clockwise from North, where North = 0 degrees. Examples: East = 90 deg, South = 180 deg, West = 270 deg. If CADModelAzimuth is defined, the Azimuth value is relative to the CADModelAzimuth value rather then North.</xsd:documentation> </xsd:annotation> <xsd:simpleType> <xsd:restriction base="xsd:double"> <xsd:minInclusive value="0"/> <xsd:maxInclusive value="360"/> </xsd:restriction> </xsd:simpleType> </xsd:element>

element Ballast

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | LightingSystem
annotation |
documentation
Type of ballast used
source | <xsd:element name="Ballast" type="xsd:string"> <xsd:annotation> <xsd:documentation>Type of ballast used</xsd:documentation> </xsd:annotation> </xsd:element>

element BaseboardHeatingCapacity

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Zone
annotation |
documentation
Baseboard heating capacity
source | <xsd:element name="BaseboardHeatingCapacity" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Baseboard heating capacity</xsd:documentation> </xsd:annotation> </xsd:element>

element BaseboardHeatingType

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | Zone
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | baseboardHeatingTypeEnum |  |  |  |
source | <xsd:element name="BaseboardHeatingType"> <xsd:complexType> <xsd:attribute name="unit" type="baseboardHeatingTypeEnum"/> </xsd:complexType> </xsd:element>

attribute BaseboardHeatingType/@unit

type | baseboardHeatingTypeEnum
facets |
Kind | Value | Annotation
enumeration | ACH |
enumeration | HotWater |
enumeration | Electric |
source | <xsd:attribute name="unit" type="baseboardHeatingTypeEnum"/>

element BeginDate

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:date
properties |
content | simple
used by |
elements | YearModeled YearSchedule
annotation |
documentation
Month and day year schedule begins
source | <xsd:element name="BeginDate" type="xsd:date"> <xsd:annotation> <xsd:documentation>Month and day year schedule begins</xsd:documentation> </xsd:annotation> </xsd:element>

element Behavior

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Description Drivers Needs Actions BuildingSystems IsSpecialBehavior
used by |
element | Behaviors
attributes |
Name | Type | Use | Default | Fixed | Annotation
ID | xsd:ID | required |  |  |
documentation
Identification of the specific behavior defined in this branch can be given.
Name | xsd:string | optional |  |  |
IfcGuid | xsd:string | optional |  |  |
AppliedBuildingType | buildingTypeEnum | optional |  |  |
BuildingTypeComment | xsd:string | optional |  |  |
ActionType | interactionType | optional |  |  |
SystemType | buildingSystemTypeEnum | optional |  |  |
PaperAuthors | xsd:string | optional |  |  |
PaperYear | xsd:string | optional |  |  |
PaperTitle | xsd:string | optional |  |  |
PaperDOI | xsd:string | optional |  |  |
DataCollectionRegion | xsd:string | optional |  |  |
TypesDataCollected1 | TypesDataCollectedList | optional |  |  |
TypesDataCollected2 | TypesDataCollectedList | optional |  |  |
TypesDataCollected3 | TypesDataCollectedList | optional |  |  |
TypesDataCollectedOther | xsd:string | optional |  |  |
SampleSize | xsd:string | optional |  |  |
annotation |
documentation
Behavior related to the interaction with buildings
source | <xsd:element name="Behavior"> <xsd:annotation> <xsd:documentation>Behavior related to the interaction with buildings</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:sequence> <xsd:element ref="Description" minOccurs="0"> <xsd:annotation> <xsd:documentation>Description of the specific behavior defined in this branch can be given.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="Drivers" minOccurs="0"> <xsd:annotation> <xsd:documentation>Drivers represent the environmental factors from the outside world that stimulate occupants in their inside world to fulfill a physical, physiological or psychological need.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="Needs" minOccurs="0"> <xsd:annotation> <xsd:documentation>Needs represent the physical and non-physical requirements of the occupant's inside world that must be met in order to ensure the satisfaction of the occupant with their environment.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="Actions"> <xsd:annotation> <xsd:documentation>Actions are the interactions with systems or activities that an occupant can conduct to achieve environmental comfort. Actions connect occupants' inside-world needs with the environmental outside world.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="BuildingSystems" minOccurs="0"> <xsd:annotation> <xsd:documentation>Systems refer to the equipment or mechanisms within the building outside world with which an occupant may interact to restore or maintain environmental comfort. Systems are not described in a detailed way, only control types (other parameters of a system can be mapped to building information models).</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="IsSpecialBehavior" minOccurs="0"/> </xsd:sequence> <xsd:attribute name="ID" type="xsd:ID" use="required"> <xsd:annotation> <xsd:documentation>Identification of the specific behavior defined in this branch can be given.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="Name" type="xsd:string" use="optional"/> <xsd:attribute name="IfcGuid" type="xsd:string" use="optional"/> <xsd:attribute name="AppliedBuildingType" type="buildingTypeEnum" use="optional"/> <xsd:attribute name="BuildingTypeComment" type="xsd:string" use="optional"/> <xsd:attribute name="ActionType" type="interactionType" use="optional"/> <xsd:attribute name="SystemType" type="buildingSystemTypeEnum" use="optional"/> <xsd:attribute name="PaperAuthors" type="xsd:string" use="optional"/> <xsd:attribute name="PaperYear" type="xsd:string" use="optional"/> <xsd:attribute name="PaperTitle" type="xsd:string" use="optional"/> <xsd:attribute name="PaperDOI" type="xsd:string" use="optional"/> <xsd:attribute name="DataCollectionRegion" type="xsd:string" use="optional"/> <xsd:attribute name="TypesDataCollected1" type="TypesDataCollectedList" use="optional"/> <xsd:attribute name="TypesDataCollected2" type="TypesDataCollectedList" use="optional"/> <xsd:attribute name="TypesDataCollected3" type="TypesDataCollectedList" use="optional"/> <xsd:attribute name="TypesDataCollectedOther" type="xsd:string" use="optional"/> <xsd:attribute name="SampleSize" type="xsd:string" use="optional"/> </xsd:complexType> </xsd:element>

attribute Behavior/@ID

type | xsd:ID
properties |
use | required
annotation |
documentation
Identification of the specific behavior defined in this branch can be given.
source | <xsd:attribute name="ID" type="xsd:ID" use="required"> <xsd:annotation> <xsd:documentation>Identification of the specific behavior defined in this branch can be given.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Behavior/@Name

type | xsd:string
properties |
use | optional
source | <xsd:attribute name="Name" type="xsd:string" use="optional"/>

attribute Behavior/@IfcGuid

type | xsd:string
properties |
use | optional
source | <xsd:attribute name="IfcGuid" type="xsd:string" use="optional"/>

attribute Behavior/@AppliedBuildingType

type | buildingTypeEnum
properties |
use | optional
facets |
Kind | Value | Annotation
enumeration | AutomotiveFacility |
enumeration | ConventionCenter |
enumeration | Courthouse |
enumeration | DataCenter |
enumeration | DiningBarLoungeOrLeisure |
enumeration | DiningCafeteriaFastFood |
enumeration | DiningFamily |
enumeration | Dormitory |
enumeration | ExerciseCenter |
enumeration | FireStation |
enumeration | Gymnasium |
enumeration | HospitalOrHealthcare |
enumeration | Hotel |
enumeration | Library |
enumeration | Manufacturing |
enumeration | Motel |
enumeration | MotionPictureTheatre |
enumeration | MultiFamily |
enumeration | Museum |
enumeration | Office |
enumeration | ParkingGarage |
enumeration | Penitentiary |
enumeration | PerformingArtsTheater |
enumeration | PoliceStation |
enumeration | PostOffice |
enumeration | ReligiousBuilding |
enumeration | Retail |
enumeration | SchoolOrUniversity |
enumeration | SingleFamily |
enumeration | SportsArena |
enumeration | TownHall |
enumeration | Transportation |
enumeration | Unknown |
documentation
Enumeration value to be used when there is no building type information available.
enumeration | Warehouse |
enumeration | Workshop |
source | <xsd:attribute name="AppliedBuildingType" type="buildingTypeEnum" use="optional"/>

attribute Behavior/@BuildingTypeComment

type | xsd:string
properties |
use | optional
source | <xsd:attribute name="BuildingTypeComment" type="xsd:string" use="optional"/>

attribute Behavior/@ActionType

type | interactionType
properties |
use | optional
facets |
Kind | Value | Annotation
enumeration | TurnOn |
documentation
Set the value of a parameter to 1.
enumeration | TurnOff |
documentation
Set the value of a parameter to 0.
enumeration | SetToControlValue |
documentation
Set the value of a parameter to a desired value when event occurs.
source | <xsd:attribute name="ActionType" type="interactionType" use="optional"/>

attribute Behavior/@SystemType

type | buildingSystemTypeEnum
properties |
use | optional
facets |
Kind | Value | Annotation
enumeration | HVAC |
enumeration | Lights |
enumeration | Windows |
enumeration | PlugLoad |
enumeration | Thermostats |
enumeration | ShadesAndBlinds |
source | <xsd:attribute name="SystemType" type="buildingSystemTypeEnum" use="optional"/>

attribute Behavior/@PaperAuthors

type | xsd:string
properties |
use | optional
source | <xsd:attribute name="PaperAuthors" type="xsd:string" use="optional"/>

attribute Behavior/@PaperYear

type | xsd:string
properties |
use | optional
source | <xsd:attribute name="PaperYear" type="xsd:string" use="optional"/>

attribute Behavior/@PaperTitle

type | xsd:string
properties |
use | optional
source | <xsd:attribute name="PaperTitle" type="xsd:string" use="optional"/>

attribute Behavior/@PaperDOI

type | xsd:string
properties |
use | optional
source | <xsd:attribute name="PaperDOI" type="xsd:string" use="optional"/>

attribute Behavior/@DataCollectionRegion

type | xsd:string
properties |
use | optional
source | <xsd:attribute name="DataCollectionRegion" type="xsd:string" use="optional"/>

attribute Behavior/@TypesDataCollected1

type | TypesDataCollectedList
properties |
use | optional
facets |
Kind | Value | Annotation
enumeration | CrossSectionSurvey |
enumeration | LongitudinalSurvey |
enumeration | IEQmeasurements |
source | <xsd:attribute name="TypesDataCollected1" type="TypesDataCollectedList" use="optional"/>

attribute Behavior/@TypesDataCollected2

type | TypesDataCollectedList
properties |
use | optional
facets |
Kind | Value | Annotation
enumeration | CrossSectionSurvey |
enumeration | LongitudinalSurvey |
enumeration | IEQmeasurements |
source | <xsd:attribute name="TypesDataCollected2" type="TypesDataCollectedList" use="optional"/>

attribute Behavior/@TypesDataCollected3

type | TypesDataCollectedList
properties |
use | optional
facets |
Kind | Value | Annotation
enumeration | CrossSectionSurvey |
enumeration | LongitudinalSurvey |
enumeration | IEQmeasurements |
source | <xsd:attribute name="TypesDataCollected3" type="TypesDataCollectedList" use="optional"/>

attribute Behavior/@TypesDataCollectedOther

type | xsd:string
properties |
use | optional
source | <xsd:attribute name="TypesDataCollectedOther" type="xsd:string" use="optional"/>

attribute Behavior/@SampleSize

type | xsd:string
properties |
use | optional
source | <xsd:attribute name="SampleSize" type="xsd:string" use="optional"/>

element BehaviorID

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:IDREF
properties |
content | simple
used by |
element | Occupant
annotation |
documentation
A specific behavior can be assigned to each occupant.
source | <xsd:element name="BehaviorID" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>A specific behavior can be assigned to each occupant.</xsd:documentation> </xsd:annotation> </xsd:element>

element Behaviors

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | MovementBehavior Behavior Activity
used by |
elements | gbXML OccupantBehavior
source | <xsd:element name="Behaviors"> <xsd:complexType> <xsd:sequence> <xsd:element ref="MovementBehavior" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Behavior" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Activity" minOccurs="0" maxOccurs="unbounded"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element BiomassDensity

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Vegetation
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | densityUnitEnum | required |  |  |
annotation |
documentation
Biomass of vegetation
source | <xsd:element name="BiomassDensity"> <xsd:annotation> <xsd:documentation>Biomass of vegetation</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="densityUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute BiomassDensity/@unit

type | densityUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | GramsPerCubicCm |
enumeration | LbsPerCubicIn |
enumeration | LbsPerCubicFt |
enumeration | KgPerCubicM |
source | <xsd:attribute name="unit" type="densityUnitEnum" use="required"/>

element Blind

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Transmittance Reflectance Emittance Thickness Conductivity
used by |
element | WindowType
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
source | <xsd:element name="Blind"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Transmittance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Reflectance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Emittance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Thickness" minOccurs="0"/> <xsd:element ref="Conductivity" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> </xsd:complexType> </xsd:element>

attribute Blind/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

element BlowerDoorValue

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | InfiltrationFlow
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | blowerDoorUnitEnum | required |  |  |
annotation |
documentation
Leakage value obtained from blower door test.
source | <xsd:element name="BlowerDoorValue"> <xsd:annotation> <xsd:documentation>Leakage value obtained from blower door test.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="blowerDoorUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute BlowerDoorValue/@unit

type | blowerDoorUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | ACH |
enumeration | AirChangesPerHour |
enumeration | SquareFeet |
enumeration | SquareMeter |
source | <xsd:attribute name="unit" type="blowerDoorUnitEnum" use="required"/>

element Building

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description StreetAddress Area Space AverageNumberOfFloors InfiltrationFlow AnalysisParameter ShellGeometry SpaceBoundary Lighting IntEquipId MeterId PeakDomesticHotWaterFlow BuildingStorey
used by |
elements | Campus OccupantBehavior
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
buildingType | buildingTypeEnum | required |  |  |
ifcGUID | xsd:string | optional |  |  |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
source | <xsd:element name="Building"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="StreetAddress" minOccurs="0"/> <xsd:element ref="Area"/> <xsd:element ref="Space" maxOccurs="unbounded"/> <xsd:element ref="AverageNumberOfFloors" minOccurs="0"/> <xsd:element ref="InfiltrationFlow" minOccurs="0"/> <xsd:element ref="AnalysisParameter" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="ShellGeometry" minOccurs="0"> <xsd:annotation> <xsd:documentation>Use this element to define the shell of the building.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="SpaceBoundary" minOccurs="0"> <xsd:annotation> <xsd:documentation>This element establishes the logical relation of a given part of the building envelope such that its PlanarGeometry is part of an exterior surface of the building.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="Lighting" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="IntEquipId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="MeterId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="PeakDomesticHotWaterFlow" minOccurs="0"/> <xsd:element ref="BuildingStorey" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="buildingType" type="buildingTypeEnum" use="required"/> <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Building/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Building/@buildingType

type | buildingTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | AutomotiveFacility |
enumeration | ConventionCenter |
enumeration | Courthouse |
enumeration | DataCenter |
enumeration | DiningBarLoungeOrLeisure |
enumeration | DiningCafeteriaFastFood |
enumeration | DiningFamily |
enumeration | Dormitory |
enumeration | ExerciseCenter |
enumeration | FireStation |
enumeration | Gymnasium |
enumeration | HospitalOrHealthcare |
enumeration | Hotel |
enumeration | Library |
enumeration | Manufacturing |
enumeration | Motel |
enumeration | MotionPictureTheatre |
enumeration | MultiFamily |
enumeration | Museum |
enumeration | Office |
enumeration | ParkingGarage |
enumeration | Penitentiary |
enumeration | PerformingArtsTheater |
enumeration | PoliceStation |
enumeration | PostOffice |
enumeration | ReligiousBuilding |
enumeration | Retail |
enumeration | SchoolOrUniversity |
enumeration | SingleFamily |
enumeration | SportsArena |
enumeration | TownHall |
enumeration | Transportation |
enumeration | Unknown |
documentation
Enumeration value to be used when there is no building type information available.
enumeration | Warehouse |
enumeration | Workshop |
source | <xsd:attribute name="buildingType" type="buildingTypeEnum" use="required"/>

attribute Building/@ifcGUID

type | xsd:string
properties |
use | optional
annotation |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
source | <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element BuildingStorey

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Level PlanarGeometry
used by |
element | Building
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
ifcGUID | xsd:string | optional |  |  |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
annotation |
documentation
Captures Building Storey Structure
source | <xsd:element name="BuildingStorey"> <xsd:annotation> <xsd:documentation>Captures Building Storey Structure</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Level"/> <xsd:element ref="PlanarGeometry" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute BuildingStorey/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute BuildingStorey/@ifcGUID

type | xsd:string
properties |
use | optional
annotation |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
source | <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element BuildingSystems

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | HVAC Lights Windows PlugLoad Thermostats ShadesAndBlinds
used by |
elements | Behavior Space
source | <xsd:element name="BuildingSystems"> <xsd:complexType> <xsd:choice> <xsd:element ref="HVAC"/> <xsd:element ref="Lights"/> <xsd:element ref="Windows"/> <xsd:element ref="PlugLoad"/> <xsd:element ref="Thermostats"/> <xsd:element ref="ShadesAndBlinds"/> </xsd:choice> </xsd:complexType> </xsd:element>

element CADMaterialId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | Material
attributes |
Name | Type | Use | Default | Fixed | Annotation
CADMaterialIdRef | xsd:string | required |  |  |
documentation
ID used by a CAD/BIM program to reference its internal materials library
source | <xsd:element name="CADMaterialId"> <xsd:complexType> <xsd:attribute name="CADMaterialIdRef" type="xsd:string" use="required"> <xsd:annotation> <xsd:documentation>ID used by a CAD/BIM program to reference its internal materials library</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute CADMaterialId/@CADMaterialIdRef

type | xsd:string
properties |
use | required
annotation |
documentation
ID used by a CAD/BIM program to reference its internal materials library
source | <xsd:attribute name="CADMaterialIdRef" type="xsd:string" use="required"> <xsd:annotation> <xsd:documentation>ID used by a CAD/BIM program to reference its internal materials library</xsd:documentation> </xsd:annotation> </xsd:attribute>

element CADModelAzimuth

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:double
properties |
content | simple
used by |
element | Location
annotation |
documentation
The number of degrees (0 to 360) of the angle of positive Y axis from north. (Value of the of Azimuth of Model's North relative to Cardinal North)
source | <xsd:element name="CADModelAzimuth" type="xsd:double"> <xsd:annotation> <xsd:documentation>The number of degrees (0 to 360) of the angle of positive Y axis from north. (Value of the of Azimuth of Model's North relative to Cardinal North)</xsd:documentation> </xsd:annotation> </xsd:element>

element CADModelId

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:string
properties |
content | complex
used by |
element | CreatedBy
attributes |
Name | Type | Use | Default | Fixed | Annotation
programIdRef | xsd:IDREF |  |  |  |
documentation
ID reference to unique CAD/BIM program defined in DocumentHistory/ProgramInfo element.
annotation |
documentation
The CADModelId Element is used to map a CAD model or BIM to its corresponding gbXML file. Allows the CAD/BIM tool referenced by the programIdRef to correlate the gbXML file to its CAD/BIM model.
source | <xsd:element name="CADModelId"> <xsd:annotation> <xsd:documentation>The CADModelId Element is used to map a CAD model or BIM to its corresponding gbXML file. Allows the CAD/BIM tool referenced by the programIdRef to correlate the gbXML file to its CAD/BIM model.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:string"> <xsd:attribute name="programIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID reference to unique CAD/BIM program defined in DocumentHistory/ProgramInfo element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute CADModelId/@programIdRef

type | xsd:IDREF
annotation |
documentation
ID reference to unique CAD/BIM program defined in DocumentHistory/ProgramInfo element.
source | <xsd:attribute name="programIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID reference to unique CAD/BIM program defined in DocumentHistory/ProgramInfo element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element CADObjectId

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:string
properties |
content | complex
used by |
elements | AirLoopEquipment AirSystem ExtEquip HydronicLoop HydronicLoopEquipment IntEquip Opening Results Space Surface Zone ZoneHVACEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
programIdRef | xsd:IDREF |  |  |  |
documentation
ID reference to unique CAD/BIM program defined in DocumentHistory/ProgramInfo element.
annotation |
documentation
The CADObjectId Element is used to map unique CAD object identifiers to gbXML elements. Allows CAD/BIM tools to read results from a gbXML file and map them to their CAD objects.
source | <xsd:element name="CADObjectId"> <xsd:annotation> <xsd:documentation>The CADObjectId Element is used to map unique CAD object identifiers to gbXML elements. Allows CAD/BIM tools to read results from a gbXML file and map them to their CAD objects.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:string"> <xsd:attribute name="programIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID reference to unique CAD/BIM program defined in DocumentHistory/ProgramInfo element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute CADObjectId/@programIdRef

type | xsd:IDREF
annotation |
documentation
ID reference to unique CAD/BIM program defined in DocumentHistory/ProgramInfo element.
source | <xsd:attribute name="programIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID reference to unique CAD/BIM program defined in DocumentHistory/ProgramInfo element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Campus

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Location Building Surface YearModeled DaylightSavings Life AltEnergySource ShellGeometry Vegetation Transportation MeterId ExtEquipId Lighting LightControlId
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
designHeatWeathIdRef | xsd:IDREF |  |  |  |
documentation
ID for the weather data used for a heating design day
designCoolWeathIdRef | xsd:IDREF |  |  |  |
documentation
ID for the weather data used for a cooling design day
ifcGUID | xsd:string | optional |  |  |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
annotation |
documentation
The Campus element should be used as the base for all physical objects. On a campus, place one or more buildings.
source | <xsd:element name="Campus"> <xsd:annotation> <xsd:documentation>The Campus element should be used as the base for all physical objects. On a campus, place one or more buildings.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Location"/> <xsd:element ref="Building" maxOccurs="unbounded"/> <xsd:element ref="Surface" minOccurs="4" maxOccurs="unbounded"/> <xsd:element ref="YearModeled" minOccurs="0"/> <xsd:element ref="DaylightSavings" minOccurs="0"/> <xsd:element ref="Life" minOccurs="0"/> <xsd:element ref="AltEnergySource" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="ShellGeometry" minOccurs="0"/> <xsd:element ref="Vegetation" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Transportation" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="MeterId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="ExtEquipId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Lighting" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="LightControlId" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="designHeatWeathIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the weather data used for a heating design day</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="designCoolWeathIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the weather data used for a cooling design day</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Campus/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Campus/@designHeatWeathIdRef

type | xsd:IDREF
annotation |
documentation
ID for the weather data used for a heating design day
source | <xsd:attribute name="designHeatWeathIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the weather data used for a heating design day</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Campus/@designCoolWeathIdRef

type | xsd:IDREF
annotation |
documentation
ID for the weather data used for a cooling design day
source | <xsd:attribute name="designCoolWeathIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the weather data used for a cooling design day</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Campus/@ifcGUID

type | xsd:string
properties |
use | optional
annotation |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
source | <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Capacity

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | AirLoopEquipment HydronicLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | capacityUnitEnum | required |  |  |
capacityType | capacityTypeEnum | required |  |  |
source | <xsd:element name="Capacity"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="capacityUnitEnum" use="required"/> <xsd:attribute name="capacityType" type="capacityTypeEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Capacity/@unit

type | capacityUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Tons |
enumeration | kW |
enumeration | BtuPerHour |
enumeration | kBtuPerHour |
enumeration | Gallons |
enumeration | Liters |
enumeration | CubicMeters |
enumeration | CubicFeet |
source | <xsd:attribute name="unit" type="capacityUnitEnum" use="required"/>

attribute Capacity/@capacityType

type | capacityTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Heating |
enumeration | CoolingTotal |
enumeration | CoolingSensible |
enumeration | CoolingLatent |
enumeration | CoolingSHR |
enumeration | Volume |
source | <xsd:attribute name="capacityType" type="capacityTypeEnum" use="required"/>

element CartesianPoint

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Coordinate
used by |
elements | LightingControl PhotometryOrientation PolyLoop RectangularGeometry Results
annotation |
documentation
This is the x, y, and z distances from the origin. This element must have three Coordinate elements when representing 3-d space, which represent x, y and z in order. This element must have two Coordinate elements when representing 2-d space.
appinfo
<xhtml:a href="http://cig.bre.co.uk/iai_uk/documentation/IfcR2x_Final/ifcgeometryresource/lexical/ifccartesianpoint.html">IfcCartesianPoint</xhtml:a>
source | <xsd:element name="CartesianPoint"> <xsd:annotation> <xsd:documentation>This is the x, y, and z distances from the origin. This element must have three Coordinate elements when representing 3-d space, which represent x, y and z in order. This element must have two Coordinate elements when representing 2-d space.</xsd:documentation> <xsd:appinfo> <xhtml:a href="http://cig.bre.co.uk/iai_uk/documentation/IfcR2x_Final/ifcgeometryresource/lexical/ifccartesianpoint.html">IfcCartesianPoint</xhtml:a> </xsd:appinfo> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Coordinate" minOccurs="2" maxOccurs="3"/> </xsd:choice> </xsd:complexType> </xsd:element>

element CDD

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Temperature CDDValue
used by |
element | Weather
annotation |
documentation
Cooling degree days. CDD is calculated as the number of degrees a mean daily temperature is above a value (specified as the Temperature element), for each day. For example, if the mean temperature in a region rises to 77 degrees for three days during a year, the rest of the time staying below 75, and the Temperature element is set at 75, then CDD = 6.
source | <xsd:element name="CDD"> <xsd:annotation> <xsd:documentation>Cooling degree days. CDD is calculated as the number of degrees a mean daily temperature is above a value (specified as the Temperature element), for each day. For example, if the mean temperature in a region rises to 77 degrees for three days during a year, the rest of the time staying below 75, and the Temperature element is set at 75, then CDD = 6.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Temperature"/> <xsd:element ref="CDDValue"/> </xsd:choice> </xsd:complexType> </xsd:element>

element CDDValue

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | CDD
annotation |
documentation
Cooling degree day value
source | <xsd:element name="CDDValue" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Cooling degree day value</xsd:documentation> </xsd:annotation> </xsd:element>

element City

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
elements | PersonInfo Weather
source | <xsd:element name="City" type="xsd:string"/>

element ClimateZone

diagram |
namespace | http://www.gbxml.org/schema
type | ClimateZoneType
properties |
content | simple
used by |
element | GeographicLocation
facets |
Kind | Value | Annotation
enumeration | 1 |
enumeration | 2 |
enumeration | 3 |
enumeration | 4 |
enumeration | 5 |
enumeration | 6 |
enumeration | 7 |
source | <xsd:element name="ClimateZone" type="ClimateZoneType"/>

element ClosedShell

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | PolyLoop
used by |
element | ShellGeometry
annotation |
documentation
This is an element from ifcXML that describes a collection of faces that make up a closed shell.
appinfo
<xhtml:a href="http://cig.bre.co.uk/iai_uk/documentation/IfcR2x_Final/IFCTOPOLOGYRESOURCE/lexical/ifcclosedshell">IfcClosedShell</xhtml:a>
source | <xsd:element name="ClosedShell"> <xsd:annotation> <xsd:documentation>This is an element from ifcXML that describes a collection of faces that make up a closed shell.</xsd:documentation> <xsd:appinfo> <xhtml:a href="http://cig.bre.co.uk/iai_uk/documentation/IfcR2x_Final/IFCTOPOLOGYRESOURCE/lexical/ifcclosedshell">IfcClosedShell</xhtml:a> </xsd:appinfo> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="PolyLoop" minOccurs="4" maxOccurs="unbounded"/> </xsd:choice> </xsd:complexType> </xsd:element>

element CLTDParameters

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | LoadCalcInputParameters
attributes |
Name | Type | Use | Default | Fixed | Annotation
roofASHRAENumber | roofASHRAENumberEnum |  |  |  |
documentation
Specifies the number 1 to 13 to use for a roof. See Table 29 page 26.34, 1989 ASHRAE Handbook, Fundamentals volume.
wallASHRAEGroup | wallASHRAEGroupEnum |  |  |  |
documentation
Specifies the wall group code A to G to use for a wall. See Table 31, page 26.36, 1989 ASHRAE Handbook, Fundamentals volume.
roofColor | roofColorEnum |  |  |  |
documentation
Specifies the effective roof color, which depends on the actual color and whether the location is industrial or rural. See page 26.34, 1989 ASHRAE Handbook, Fundamentals volume.
roofHasSuspendedCeiling | xsd:boolean |  |  |  |
documentation
Specifies whether or not a roof has a suspended ceiling under it. See table 29, page 26.34, 1989 ASHRAE Handbook, Fundamentals volume.
wallColor | wallColorEnum |  |  |  |
documentation
Specifies the effective wall color, which depends on the actual color and whether the location is industrial or rural. See page 26.36, 1989 ASHRAE Handbook, Fundamentals volume.
annotation |
documentation
Parameters required by CLTD load calculation method, as described in the 1989 ASHRAE Handbook, Fundamentals volume, pages 26.32 and following. Ignore this element and all elements under it if you are not planning to use that method.
source | <xsd:element name="CLTDParameters"> <xsd:annotation> <xsd:documentation>Parameters required by CLTD load calculation method, as described in the 1989 ASHRAE Handbook, Fundamentals volume, pages 26.32 and following. Ignore this element and all elements under it if you are not planning to use that method.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:attribute name="roofASHRAENumber" type="roofASHRAENumberEnum"> <xsd:annotation> <xsd:documentation>Specifies the number 1 to 13 to use for a roof. See Table 29 page 26.34, 1989 ASHRAE Handbook, Fundamentals volume.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="wallASHRAEGroup" type="wallASHRAEGroupEnum"> <xsd:annotation> <xsd:documentation>Specifies the wall group code A to G to use for a wall. See Table 31, page 26.36, 1989 ASHRAE Handbook, Fundamentals volume.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="roofColor" type="roofColorEnum"> <xsd:annotation> <xsd:documentation>Specifies the effective roof color, which depends on the actual color and whether the location is industrial or rural. See page 26.34, 1989 ASHRAE Handbook, Fundamentals volume.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="roofHasSuspendedCeiling" type="xsd:boolean"> <xsd:annotation> <xsd:documentation>Specifies whether or not a roof has a suspended ceiling under it. See table 29, page 26.34, 1989 ASHRAE Handbook, Fundamentals volume.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="wallColor" type="wallColorEnum"> <xsd:annotation> <xsd:documentation>Specifies the effective wall color, which depends on the actual color and whether the location is industrial or rural. See page 26.36, 1989 ASHRAE Handbook, Fundamentals volume.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute CLTDParameters/@roofASHRAENumber

type | roofASHRAENumberEnum
facets |
Kind | Value | Annotation
enumeration | 0 |
documentation
Undefined
enumeration | 1 |
documentation
Steel sheet with 1 or 2 inches insulation
enumeration | 2 |
documentation
One inch wood with 1 inch insulation
enumeration | 3 |
documentation
Four inch light weight concrete
enumeration | 4 |
documentation
Two inch heavy weight concrete
enumeration | 5 |
documentation
One inch wood with 2 inch insulation
enumeration | 6 |
documentation
Six inch light weight concrete
enumeration | 7 |
documentation
2.5 inch wood with 1 inch insulation
enumeration | 8 |
documentation
Eight inch light weight concrete
enumeration | 9 |
documentation
4 inch hvy wt concrete with 1-2 inch insulation
enumeration | 10 |
documentation
2.5 inch wood with 2 inches of insulation
enumeration | 11 |
documentation
Roof Terrace System
enumeration | 12 |
documentation
6 inch hvy wt concrete with 1-2 inch insulation
enumeration | 13 |
documentation
4 inch wood with 1-2 inches of insulation
annotation |
documentation
Specifies the number 1 to 13 to use for a roof. See Table 29 page 26.34, 1989 ASHRAE Handbook, Fundamentals volume.
source | <xsd:attribute name="roofASHRAENumber" type="roofASHRAENumberEnum"> <xsd:annotation> <xsd:documentation>Specifies the number 1 to 13 to use for a roof. See Table 29 page 26.34, 1989 ASHRAE Handbook, Fundamentals volume.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute CLTDParameters/@wallASHRAEGroup

type | wallASHRAEGroupEnum
facets |
Kind | Value | Annotation
enumeration | A |
documentation
4-in. face brick, insulation + 8-in. com. brick
enumeration | B |
documentation
4-in. face brick, 2-in. insul., 4-in. com. brick
enumeration | C |
documentation
4-in. face brick, air space + 4-in. face brick
enumeration | D |
documentation
4-in. face brick + 4-in. common brick
enumeration | E |
documentation
4-in. face brick + 4-in. block
enumeration | F |
documentation
4-in. block + air space or insulation
enumeration | G |
documentation
Metal curtain wall + 1 to 3-in. insulation
annotation |
documentation
Specifies the wall group code A to G to use for a wall. See Table 31, page 26.36, 1989 ASHRAE Handbook, Fundamentals volume.
source | <xsd:attribute name="wallASHRAEGroup" type="wallASHRAEGroupEnum"> <xsd:annotation> <xsd:documentation>Specifies the wall group code A to G to use for a wall. See Table 31, page 26.36, 1989 ASHRAE Handbook, Fundamentals volume.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute CLTDParameters/@roofColor

type | roofColorEnum
facets |
Kind | Value | Annotation
enumeration | Dark |
documentation
Dark colored or light colored in an industrial area
enumeration | Light |
documentation
Permanently light colored and in a rural area
annotation |
documentation
Specifies the effective roof color, which depends on the actual color and whether the location is industrial or rural. See page 26.34, 1989 ASHRAE Handbook, Fundamentals volume.
source | <xsd:attribute name="roofColor" type="roofColorEnum"> <xsd:annotation> <xsd:documentation>Specifies the effective roof color, which depends on the actual color and whether the location is industrial or rural. See page 26.34, 1989 ASHRAE Handbook, Fundamentals volume.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute CLTDParameters/@roofHasSuspendedCeiling

type | xsd:boolean
annotation |
documentation
Specifies whether or not a roof has a suspended ceiling under it. See table 29, page 26.34, 1989 ASHRAE Handbook, Fundamentals volume.
source | <xsd:attribute name="roofHasSuspendedCeiling" type="xsd:boolean"> <xsd:annotation> <xsd:documentation>Specifies whether or not a roof has a suspended ceiling under it. See table 29, page 26.34, 1989 ASHRAE Handbook, Fundamentals volume.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute CLTDParameters/@wallColor

type | wallColorEnum
facets |
Kind | Value | Annotation
enumeration | Dark |
documentation
Dark colored or light colored in an industrial area
enumeration | Medium |
documentation
Permanently medium colored and in a rural area
enumeration | Light |
documentation
Permanently light colored and in a rural area
annotation |
documentation
Specifies the effective wall color, which depends on the actual color and whether the location is industrial or rural. See page 26.36, 1989 ASHRAE Handbook, Fundamentals volume.
source | <xsd:attribute name="wallColor" type="wallColorEnum"> <xsd:annotation> <xsd:documentation>Specifies the effective wall color, which depends on the actual color and whether the location is industrial or rural. See page 26.36, 1989 ASHRAE Handbook, Fundamentals volume.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element CoefficientA

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
complexTypes | eqConstantValueType eqLinear1DType eqLinear2DType eqLinear3DType eqLogit1DLinearType eqLogit1DQuadraticType eqLogit2DLinearType eqLogit3DLinearType eqQuadratic1DType eqWeibull1D3P
source | <xsd:element name="CoefficientA" type="xsd:decimal"/>

element CoefficientB

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
complexTypes | eqLinear1DType eqLinear2DType eqLinear3DType eqLogit1DLinearType eqLogit1DQuadraticType eqLogit2DLinearType eqLogit3DLinearType eqQuadratic1DType eqWeibull1D3P
source | <xsd:element name="CoefficientB" type="xsd:decimal"/>

element CoefficientC

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
complexTypes | eqLinear2DType eqLinear3DType eqLogit1DQuadraticType eqLogit2DLinearType eqLogit3DLinearType eqQuadratic1DType eqWeibull1D3P
source | <xsd:element name="CoefficientC" type="xsd:decimal"/>

element CoefficientD

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
complexTypes | eqLinear3DType eqLogit3DLinearType
source | <xsd:element name="CoefficientD" type="xsd:decimal"/>

element CoefficientOfUtilization

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Lighting LightingSystem
attributes |
Name | Type | Use | Default | Fixed | Annotation
wallReflectance | xsd:decimal |  |  |  |
ceilingCavityReflectance | xsd:decimal |  |  |  |
floorReflectance | xsd:decimal |  |  |  |
roomCavityRatio | xsd:decimal |  |  |  |
documentation
Room cavity ratio is a measure of the room cavity proportions.
annotation |
documentation
The coefficient of utilization is the ratio of luminous flux on a work plane to the luminous flux emitted by the lamps alone.
source | <xsd:element name="CoefficientOfUtilization"> <xsd:annotation> <xsd:documentation>The coefficient of utilization is the ratio of luminous flux on a work plane to the luminous flux emitted by the lamps alone. </xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="wallReflectance" type="xsd:decimal"/> <xsd:attribute name="ceilingCavityReflectance" type="xsd:decimal"/> <xsd:attribute name="floorReflectance" type="xsd:decimal"/> <xsd:attribute name="roomCavityRatio" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Room cavity ratio is a measure of the room cavity proportions.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute CoefficientOfUtilization/@wallReflectance

type | xsd:decimal
source | <xsd:attribute name="wallReflectance" type="xsd:decimal"/>

attribute CoefficientOfUtilization/@ceilingCavityReflectance

type | xsd:decimal
source | <xsd:attribute name="ceilingCavityReflectance" type="xsd:decimal"/>

attribute CoefficientOfUtilization/@floorReflectance

type | xsd:decimal
source | <xsd:attribute name="floorReflectance" type="xsd:decimal"/>

attribute CoefficientOfUtilization/@roomCavityRatio

type | xsd:decimal
annotation |
documentation
Room cavity ratio is a measure of the room cavity proportions.
source | <xsd:attribute name="roomCavityRatio" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Room cavity ratio is a measure of the room cavity proportions.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element CommuteMode

diagram |
namespace | http://www.gbxml.org/schema
type | CommuteModeType
properties |
content | simple
used by |
element | GeographicLocation
facets |
Kind | Value | Annotation
enumeration | Walk |
enumeration | Cycle |
enumeration | Car |
enumeration | Transit |
source | <xsd:element name="CommuteMode" type="CommuteModeType"/>

element CompanyName

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
elements | PersonInfo ProgramInfo
source | <xsd:element name="CompanyName" type="xsd:string"/>

element Conductivity

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Blind Fire Gap Glaze Material
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | conductivityUnitEnum | required |  |  |
source | <xsd:element name="Conductivity"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="conductivityUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Conductivity/@unit

type | conductivityUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | WPerCmC |
enumeration | WPerMeterK |
enumeration | BtuPerHourFtF |
source | <xsd:attribute name="unit" type="conductivityUnitEnum" use="required"/>

element ConductivityFofT

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Gap
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | conductivityFofTUnitEnum | required |  |  |
annotation |
documentation
Conductivity as a function of temperature
source | <xsd:element name="ConductivityFofT"> <xsd:annotation> <xsd:documentation>Conductivity as a function of temperature</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="conductivityFofTUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute ConductivityFofT/@unit

type | conductivityFofTUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | WPerMSquareK |
enumeration | BtuPerHourFtSquareF |
source | <xsd:attribute name="unit" type="conductivityFofTUnitEnum" use="required"/>

element ConstantValue

diagram |
namespace | http://www.gbxml.org/schema
type | eqConstantValueType
properties |
content | complex
children | Description CoefficientA
used by |
element | Formula
source | <xsd:element name="ConstantValue" type="eqConstantValueType"/>

element Construction

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description U-value Absorptance Roughness Albedo Reflectance Transmittance Emittance Cost PercentExisting FireFace LayerId ExtEquipId LoadCalcInputParameters
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
DOELibIdRef | xsd:string |  |  |  |
documentation
Use this attribute to reference objects in the DOE2 library
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
constructionIsSchematic | xsd:boolean | optional |  |  |
annotation |
documentation
A Construction is a combination of layers, such as a wall or a roof
source | <xsd:element name="Construction"> <xsd:annotation> <xsd:documentation>A Construction is a combination of layers, such as a wall or a roof</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="U-value" minOccurs="0"/> <xsd:element ref="Absorptance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Roughness" minOccurs="0"/> <xsd:element ref="Albedo" minOccurs="0"/> <xsd:element ref="Reflectance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Transmittance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Emittance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Cost" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="PercentExisting" minOccurs="0"/> <xsd:element ref="FireFace" minOccurs="0" maxOccurs="2"/> <xsd:element ref="LayerId" minOccurs="0" maxOccurs="unbounded"> <xsd:annotation> <xsd:documentation>Reference to layers that comprise this construction. Multiple LayerId's order is important and specifies the layering of the layer's referenced materials. The first Surface/AdjacentSpaceId entered will determine how the referenced construction layers are ordered with the first construction layer being in contact with the outside or 2nd Surface/AdjacentSpaceId listed and the last layer in contact with the first Surface/AdjacentSpaceId listed.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="ExtEquipId" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This element is for purposes of modeling BIPV (building integrated photovoltaics).</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="LoadCalcInputParameters" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="constructionIsSchematic" type="xsd:boolean" use="optional"/> </xsd:complexType> </xsd:element>

attribute Construction/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Construction/@DOELibIdRef

type | xsd:string
annotation |
documentation
Use this attribute to reference objects in the DOE2 library
source | <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Construction/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Construction/@constructionIsSchematic

type | xsd:boolean
properties |
use | optional
source | <xsd:attribute name="constructionIsSchematic" type="xsd:boolean" use="optional"/>

element Control

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
elements | AirLoopEquipment HydronicLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
controlType | controlTypeEnum |  |  |  |
stages | stageTypeEnum | optional |  |  |
minPowerRatio | xsd:float |  |  |  |
operationType | operationTypeEnum |  |  |  |
performanceIdRef | xsd:IDREF |  |  |  |
annotation |
documentation
The Control element should be used for describing how this equipment is controlled.
source | <xsd:element name="Control"> <xsd:annotation> <xsd:documentation>The Control element should be used for describing how this equipment is controlled.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:attribute name="controlType" type="controlTypeEnum"/> <xsd:attribute name="stages" type="stageTypeEnum" use="optional"/> <xsd:attribute name="minPowerRatio" type="xsd:float"/> <xsd:attribute name="operationType" type="operationTypeEnum"/> <xsd:attribute name="performanceIdRef" type="xsd:IDREF"/> </xsd:complexType> </xsd:element>

attribute Control/@controlType

type | controlTypeEnum
facets |
Kind | Value | Annotation
enumeration | Boiler |
enumeration | Chiller |
enumeration | Damper |
enumeration | Fan |
enumeration | Pump |
enumeration | Valve |
source | <xsd:attribute name="controlType" type="controlTypeEnum"/>

attribute Control/@stages

type | stageTypeEnum
properties |
use | optional
facets |
Kind | Value | Annotation
enumeration | 1Stage |
enumeration | 2Stage |
enumeration | Variable |
source | <xsd:attribute name="stages" type="stageTypeEnum" use="optional"/>

attribute Control/@minPowerRatio

type | xsd:float
source | <xsd:attribute name="minPowerRatio" type="xsd:float"/>

attribute Control/@operationType

type | operationTypeEnum
facets |
Kind | Value | Annotation
enumeration | Cycling |
enumeration | Continuous |
source | <xsd:attribute name="operationType" type="operationTypeEnum"/>

attribute Control/@performanceIdRef

type | xsd:IDREF
source | <xsd:attribute name="performanceIdRef" type="xsd:IDREF"/>

element ControlValue

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:double
properties |
content | simple
used by |
element | Interaction
source | <xsd:element name="ControlValue" type="xsd:double"/>

element ConvergenceLimits

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:string
properties |
content | complex
used by |
element | SimulationParameters
attributes |
Name | Type | Use | Default | Fixed | Annotation
minimumSystemTimeStep | xsd:integer |  |  |  |
maximumHVACIterations | xsd:integer |  |  |  |
minimumPlantIterations | xsd:integer |  |  |  |
maximumPlantIterations | xsd:integer |  |  |  |
annotation |
documentation
ConvergenceLimits is an optional element that can be used to specify timesteps on individual simulation loops. It is generally reserved for EnergyPlus simulations, and is recommended for advanced users wishing to speed up calculations. This may be a valid location to store this information if the gbXML file is used as a simulation archive.
source | <xsd:element name="ConvergenceLimits"> <xsd:annotation> <xsd:documentation>ConvergenceLimits is an optional element that can be used to specify timesteps on individual simulation loops. It is generally reserved for EnergyPlus simulations, and is recommended for advanced users wishing to speed up calculations. This may be a valid location to store this information if the gbXML file is used as a simulation archive.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:string"> <xsd:attribute name="minimumSystemTimeStep" type="xsd:integer"/> <xsd:attribute name="maximumHVACIterations" type="xsd:integer"/> <xsd:attribute name="minimumPlantIterations" type="xsd:integer"/> <xsd:attribute name="maximumPlantIterations" type="xsd:integer"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute ConvergenceLimits/@minimumSystemTimeStep

type | xsd:integer
source | <xsd:attribute name="minimumSystemTimeStep" type="xsd:integer"/>

attribute ConvergenceLimits/@maximumHVACIterations

type | xsd:integer
source | <xsd:attribute name="maximumHVACIterations" type="xsd:integer"/>

attribute ConvergenceLimits/@minimumPlantIterations

type | xsd:integer
source | <xsd:attribute name="minimumPlantIterations" type="xsd:integer"/>

attribute ConvergenceLimits/@maximumPlantIterations

type | xsd:integer
source | <xsd:attribute name="maximumPlantIterations" type="xsd:integer"/>

element CoolingCoilSetpointResetType

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | AirLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | coolingCoilSetpointResetTypeEnum |  |  |  |
source | <xsd:element name="CoolingCoilSetpointResetType"> <xsd:complexType> <xsd:attribute name="unit" type="coolingCoilSetpointResetTypeEnum"/> </xsd:complexType> </xsd:element>

attribute CoolingCoilSetpointResetType/@unit

type | coolingCoilSetpointResetTypeEnum
facets |
Kind | Value | Annotation
enumeration | None |
enumeration | Warmest |
enumeration | OutdoorAirTemperatureReset |
enumeration | WarmestTemperatureFirst |
source | <xsd:attribute name="unit" type="coolingCoilSetpointResetTypeEnum"/>

element CoolingCoilType

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | AirLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | coolingCoilTypeEnum |  |  |  |
source | <xsd:element name="CoolingCoilType"> <xsd:complexType> <xsd:attribute name="unit" type="coolingCoilTypeEnum"/> </xsd:complexType> </xsd:element>

attribute CoolingCoilType/@unit

type | coolingCoilTypeEnum
facets |
Kind | Value | Annotation
enumeration | ChilledWater |
enumeration | ChilledWaterDetailedFlatModel |
enumeration | DirectExpansion |
source | <xsd:attribute name="unit" type="coolingCoilTypeEnum"/>

element CoolingSizingFactor

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Zone
source | <xsd:element name="CoolingSizingFactor" type="xsd:decimal"/>

element CoolingTemperature

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | TemperatureProbabilityModel
used by |
element | ASHRAEComfortTemperatures
annotation |
documentation
A distribution of comfort cooling temperature can be given where occupants and therefore, they don't carry out any actions.
source | <xsd:element name="CoolingTemperature"> <xsd:annotation> <xsd:documentation>A distribution of comfort cooling temperature can be given where occupants and therefore, they don't carry out any actions. </xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice> <xsd:element ref="TemperatureProbabilityModel" minOccurs="0"/> </xsd:choice> </xsd:complexType> </xsd:element>

element Coordinate

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | CartesianPoint
annotation |
documentation
This is the an x, y, or z length measurement from the origin.
appinfo
<xhtml:a href="http://cig.bre.co.uk/iai_uk/documentation/IfcR2x_Final/ifcmeasureresource/lexical/ifclengthmeasure.html">IfcLengthMeasure</xhtml:a>
source | <xsd:element name="Coordinate"> <xsd:annotation> <xsd:documentation>This is the an x, y, or z length measurement from the origin.</xsd:documentation> <xsd:appinfo> <xhtml:a href="http://cig.bre.co.uk/iai_uk/documentation/IfcR2x_Final/ifcmeasureresource/lexical/ifclengthmeasure.html">IfcLengthMeasure</xhtml:a> </xsd:appinfo> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"/> </xsd:simpleContent> </xsd:complexType> </xsd:element>

element Cost

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | CostValue Reference
used by |
elements | AirLoopEquipment Construction ExtEquip GeographicLocation HydronicLoop HydronicLoopEquipment IntEquip Layer LightingSystem Material Transportation Vegetation WindowType
attributes |
Name | Type | Use | Default | Fixed | Annotation
costType | costTypeEnum | required |  |  |
source | <xsd:element name="Cost"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="CostValue"/> <xsd:element ref="Reference" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="costType" type="costTypeEnum" use="required"/> </xsd:complexType> </xsd:element>

attribute Cost/@costType

type | costTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | CO2 |
enumeration | SOx |
enumeration | NOx |
enumeration | EmbodiedEnergyTransportation |
enumeration | EmbodiedEnergyManufacture |
enumeration | EmbodiedEnergyInstallation |
enumeration | EmbodiedEnergyTotal |
enumeration | PurchaseCost |
enumeration | DeliveryCost |
enumeration | FirstCost |
enumeration | MonthlyCost |
enumeration | AnnualCost |
enumeration | MaintenanceCost |
enumeration | OverhaulCost |
enumeration | InstallationCost |
enumeration | ServiceFees |
source | <xsd:attribute name="costType" type="costTypeEnum" use="required"/>

element CostConscious

diagram |
namespace | http://www.gbxml.org/schema
type | subjectiveValueType
properties |
content | simple
used by |
element | SubjectiveValues
facets |
Kind | Value | Annotation
enumeration | High |
enumeration | Medium |
enumeration | Low |
source | <xsd:element name="CostConscious" type="subjectiveValueType"/>

element CostValue

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Cost
attributes |
Name | Type | Use | Default | Fixed | Annotation
currency | currencyTypeEnum |  |  |  |
unit | xsd:string | optional |  |  |
source | <xsd:element name="CostValue"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="currency" type="currencyTypeEnum"/> <xsd:attribute name="unit" type="xsd:string" use="optional"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute CostValue/@currency

type | currencyTypeEnum
facets |
Kind | Value | Annotation
enumeration | USDollars |
enumeration | CanadianDollars |
enumeration | Pesos |
enumeration | Euros |
enumeration | Yen |
enumeration | IndianRupee |
enumeration | Yuan |
enumeration | TaiwanDollar |
enumeration | EnglishPound |
enumeration | Mark |
enumeration | Franc |
enumeration | Ruble |
enumeration | Real |
enumeration | NewZealandDollar |
enumeration | AustralianDollar |
source | <xsd:attribute name="currency" type="currencyTypeEnum"/>

attribute CostValue/@unit

type | xsd:string
properties |
use | optional
source | <xsd:attribute name="unit" type="xsd:string" use="optional"/>

element Country

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
elements | GeographicLocation PersonInfo Weather
source | <xsd:element name="Country" type="xsd:string"/>

element CreatedBy

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | CADModelId
used by |
element | DocumentHistory
attributes |
Name | Type | Use | Default | Fixed | Annotation
personId | xsd:IDREF | required |  |  |
programId | xsd:IDREF | required |  |  |
date | xsd:dateTime | required |  |  |
annotation |
documentation
Denotes the time this file has been created, as well as the person and program used to create this file.
source | <xsd:element name="CreatedBy"> <xsd:annotation> <xsd:documentation>Denotes the time this file has been created, as well as the person and program used to create this file.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="CADModelId" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="personId" type="xsd:IDREF" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="required"/> <xsd:attribute name="date" type="xsd:dateTime" use="required"/> </xsd:complexType> </xsd:element>

attribute CreatedBy/@personId

type | xsd:IDREF
properties |
use | required
source | <xsd:attribute name="personId" type="xsd:IDREF" use="required"/>

attribute CreatedBy/@programId

type | xsd:IDREF
properties |
use | required
source | <xsd:attribute name="programId" type="xsd:IDREF" use="required"/>

attribute CreatedBy/@date

type | xsd:dateTime
properties |
use | required
source | <xsd:attribute name="date" type="xsd:dateTime" use="required"/>

element CustomProbabilityModel

diagram |
namespace | http://www.gbxml.org/schema
type | CustomProbabilityModelType
properties |
content | complex
children | StatusTransitionProbability
used by |
elements | ActivityOccurModel EventOccurModel
source | <xsd:element name="CustomProbabilityModel" type="CustomProbabilityModelType"/>

element CyclesPerWeek

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
elements | ExtEquip IntEquip
annotation |
documentation
Number of operation cycles per week.
source | <xsd:element name="CyclesPerWeek" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Number of operation cycles per week.</xsd:documentation> </xsd:annotation> </xsd:element>

element CyclingRateMax

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | AirLoopEquipment
annotation |
documentation
Maximum cycling rate (cycles/hr)
source | <xsd:element name="CyclingRateMax" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Maximum cycling rate (cycles/hr)</xsd:documentation> </xsd:annotation> </xsd:element>

element DamperHeatingAction

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | AirLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | damperHeatingActionEnum |  |  |  |
source | <xsd:element name="DamperHeatingAction"> <xsd:complexType> <xsd:attribute name="unit" type="damperHeatingActionEnum"/> </xsd:complexType> </xsd:element>

attribute DamperHeatingAction/@unit

type | damperHeatingActionEnum
facets |
Kind | Value | Annotation
enumeration | Normal |
enumeration | Reverse |
source | <xsd:attribute name="unit" type="damperHeatingActionEnum"/>

element Data

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | IndependentValue DependentValue
used by |
element | PointData
source | <xsd:element name="Data"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="IndependentValue" maxOccurs="2"/> <xsd:element ref="DependentValue" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> </xsd:complexType> </xsd:element>

element Day

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:string
properties |
content | complex
used by |
element | WeekSchedule
attributes |
Name | Type | Use | Default | Fixed | Annotation
dayScheduleIdRef | xsd:IDREF | required |  |  |
documentation
ID for operation schedules
dayType | dayTypeEnum | required |  |  |
source | <xsd:element name="Day"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:string"> <xsd:attribute name="dayScheduleIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID for operation schedules</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="dayType" type="dayTypeEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Day/@dayScheduleIdRef

type | xsd:IDREF
properties |
use | required
annotation |
documentation
ID for operation schedules
source | <xsd:attribute name="dayScheduleIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID for operation schedules</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Day/@dayType

type | dayTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Weekday |
enumeration | Weekend |
enumeration | Holiday |
enumeration | WeekendOrHoliday |
enumeration | HeatingDesignDay |
enumeration | CoolingDesignDay |
enumeration | Sun |
enumeration | Mon |
enumeration | Tue |
enumeration | Wed |
enumeration | Thu |
enumeration | Fri |
enumeration | Sat |
enumeration | Custom |
enumeration | All |
source | <xsd:attribute name="dayType" type="dayTypeEnum" use="required"/>

element DaylightSavings

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:boolean
properties |
content | simple
used by |
element | Campus
annotation |
documentation
Allows for including daylight savings time
source | <xsd:element name="DaylightSavings" type="xsd:boolean"> <xsd:annotation> <xsd:documentation>Allows for including daylight savings time</xsd:documentation> </xsd:annotation> </xsd:element>

element DayofWeek

diagram |
namespace | http://www.gbxml.org/schema
type | dayTypeEnum
properties |
content | simple
used by |
elements | MeetingEvent MovementBehavior Time
facets |
Kind | Value | Annotation
enumeration | Weekday |
enumeration | Weekend |
enumeration | Holiday |
enumeration | WeekendOrHoliday |
enumeration | HeatingDesignDay |
enumeration | CoolingDesignDay |
enumeration | Sun |
enumeration | Mon |
enumeration | Tue |
enumeration | Wed |
enumeration | Thu |
enumeration | Fri |
enumeration | Sat |
enumeration | Custom |
enumeration | All |
source | <xsd:element name="DayofWeek" type="dayTypeEnum"/>

element DaySchedule

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description ScheduleValue
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
scheduleType | scheduleTypeEnum | required |  |  |
scheduleTypeLimitsId | xsd:string |  |  |  |
annotation |
documentation
Set of values that define the profile of one 24 hour period divided equally to the number of values entered.
source | <xsd:element name="DaySchedule"> <xsd:annotation> <xsd:documentation>Set of values that define the profile of one 24 hour period divided equally to the number of values entered.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="ScheduleValue" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="scheduleType" type="scheduleTypeEnum" use="required"/> <xsd:attribute name="scheduleTypeLimitsId" type="xsd:string"/> </xsd:complexType> </xsd:element>

attribute DaySchedule/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute DaySchedule/@scheduleType

type | scheduleTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Temp |
enumeration | Fraction |
enumeration | OnOff |
enumeration | ResetTemp |
enumeration | ActivityLevel |
source | <xsd:attribute name="scheduleType" type="scheduleTypeEnum" use="required"/>

attribute DaySchedule/@scheduleTypeLimitsId

type | xsd:string
source | <xsd:attribute name="scheduleTypeLimitsId" type="xsd:string"/>

element DDDayCool

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Day of the month that the cooling design day occurs on
source | <xsd:element name="DDDayCool" type="xsd:integer"> <xsd:annotation> <xsd:documentation>Day of the month that the cooling design day occurs on</xsd:documentation> </xsd:annotation> </xsd:element>

element DDDayHeat

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Day of the month that the heating design day occurs on
source | <xsd:element name="DDDayHeat" type="xsd:integer"> <xsd:annotation> <xsd:documentation>Day of the month that the heating design day occurs on</xsd:documentation> </xsd:annotation> </xsd:element>

element DDDaylightCool

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Flag for daylight savings on the cooling design day
source | <xsd:element name="DDDaylightCool" type="xsd:integer"> <xsd:annotation> <xsd:documentation>Flag for daylight savings on the cooling design day</xsd:documentation> </xsd:annotation> </xsd:element>

element DDDaylightHeat

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Flag for daylight savings for the heating design day
source | <xsd:element name="DDDaylightHeat" type="xsd:integer"> <xsd:annotation> <xsd:documentation>Flag for daylight savings for the heating design day</xsd:documentation> </xsd:annotation> </xsd:element>

element DDDBCool

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | temperatureUnitEnum |  |  |  |
annotation |
documentation
Cooling design day dry bulb temperature
source | <xsd:element name="DDDBCool"> <xsd:annotation> <xsd:documentation>Cooling design day dry bulb temperature</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDDBCool/@unit

type | temperatureUnitEnum
facets |
Kind | Value | Annotation
enumeration | F |
enumeration | C |
enumeration | K |
enumeration | R |
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element DDDBHeat

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | temperatureUnitEnum |  |  |  |
annotation |
documentation
Heating design day dry bulb temperature
source | <xsd:element name="DDDBHeat"> <xsd:annotation> <xsd:documentation>Heating design day dry bulb temperature</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDDBHeat/@unit

type | temperatureUnitEnum
facets |
Kind | Value | Annotation
enumeration | F |
enumeration | C |
enumeration | K |
enumeration | R |
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element DDDBRangeCool

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | temperatureUnitEnum |  |  |  |
annotation |
documentation
Cooling design day dry bulb temperature range
source | <xsd:element name="DDDBRangeCool"> <xsd:annotation> <xsd:documentation>Cooling design day dry bulb temperature range</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDDBRangeCool/@unit

type | temperatureUnitEnum
facets |
Kind | Value | Annotation
enumeration | F |
enumeration | C |
enumeration | K |
enumeration | R |
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element DDDBRangeHeat

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | temperatureUnitEnum |  |  |  |
annotation |
documentation
Heating design day dry bulb temperature range
source | <xsd:element name="DDDBRangeHeat"> <xsd:annotation> <xsd:documentation>Heating design day dry bulb temperature range</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDDBRangeHeat/@unit

type | temperatureUnitEnum
facets |
Kind | Value | Annotation
enumeration | F |
enumeration | C |
enumeration | K |
enumeration | R |
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element DDGroundTCool

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | temperatureUnitEnum |  |  |  |
annotation |
documentation
Ground temperature on the cooling design day
source | <xsd:element name="DDGroundTCool"> <xsd:annotation> <xsd:documentation>Ground temperature on the cooling design day</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDGroundTCool/@unit

type | temperatureUnitEnum
facets |
Kind | Value | Annotation
enumeration | F |
enumeration | C |
enumeration | K |
enumeration | R |
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element DDGroundTHeat

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | temperatureUnitEnum |  |  |  |
annotation |
documentation
Ground temperature for the heating design day
source | <xsd:element name="DDGroundTHeat"> <xsd:annotation> <xsd:documentation>Ground temperature for the heating design day</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDGroundTHeat/@unit

type | temperatureUnitEnum
facets |
Kind | Value | Annotation
enumeration | F |
enumeration | C |
enumeration | K |
enumeration | R |
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element DDHiHrCool

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Cooling design day hour of high temperature
source | <xsd:element name="DDHiHrCool" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Cooling design day hour of high temperature</xsd:documentation> </xsd:annotation> </xsd:element>

element DDHiHrHeat

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Heating design day hour of high temperature
source | <xsd:element name="DDHiHrHeat" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Heating design day hour of high temperature</xsd:documentation> </xsd:annotation> </xsd:element>

element DDLoHrCool

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Cooling design day hour of low temperature
source | <xsd:element name="DDLoHrCool" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Cooling design day hour of low temperature</xsd:documentation> </xsd:annotation> </xsd:element>

element DDLoHrHeat

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Heating design day hour of low temperature
source | <xsd:element name="DDLoHrHeat" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Heating design day hour of low temperature</xsd:documentation> </xsd:annotation> </xsd:element>

element DDMonthCool

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Month the cooling design day lands on. 1=Jan 12=Dec
source | <xsd:element name="DDMonthCool" type="xsd:integer"> <xsd:annotation> <xsd:documentation>Month the cooling design day lands on. 1=Jan 12=Dec</xsd:documentation> </xsd:annotation> </xsd:element>

element DDMonthHeat

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Month that the heating design day occurs on. 1=Jan 12=Dec
source | <xsd:element name="DDMonthHeat" type="xsd:integer"> <xsd:annotation> <xsd:documentation>Month that the heating design day occurs on. 1=Jan 12=Dec</xsd:documentation> </xsd:annotation> </xsd:element>

element DDPressureCool

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | pressureUnitEnum |  |  |  |
annotation |
documentation
Cooling design day atmospheric pressure
source | <xsd:element name="DDPressureCool"> <xsd:annotation> <xsd:documentation>Cooling design day atmospheric pressure</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="pressureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDPressureCool/@unit

type | pressureUnitEnum
facets |
Kind | Value | Annotation
enumeration | PSI |
enumeration | kPa |
enumeration | Atmospheres |
enumeration | InchesOfH2O |
enumeration | CentimetersOfH2O |
enumeration | InchesOfMercury |
enumeration | CentimetersOfMercury |
enumeration | MillimetersOfMercury |
enumeration | Pascals |
source | <xsd:attribute name="unit" type="pressureUnitEnum"/>

element DDPressureHeat

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | pressureUnitEnum |  |  |  |
annotation |
documentation
Heating design day atmospheric pressure
source | <xsd:element name="DDPressureHeat"> <xsd:annotation> <xsd:documentation>Heating design day atmospheric pressure</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="pressureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDPressureHeat/@unit

type | pressureUnitEnum
facets |
Kind | Value | Annotation
enumeration | PSI |
enumeration | kPa |
enumeration | Atmospheres |
enumeration | InchesOfH2O |
enumeration | CentimetersOfH2O |
enumeration | InchesOfMercury |
enumeration | CentimetersOfMercury |
enumeration | MillimetersOfMercury |
enumeration | Pascals |
source | <xsd:attribute name="unit" type="pressureUnitEnum"/>

element DDRainCool

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Flag for rain on the cooling design day. 0=no rain 1=rain
source | <xsd:element name="DDRainCool" type="xsd:integer"> <xsd:annotation> <xsd:documentation>Flag for rain on the cooling design day. 0=no rain 1=rain</xsd:documentation> </xsd:annotation> </xsd:element>

element DDRainHeat

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Heating design day rain flag. 0=no rain, 1=rain
source | <xsd:element name="DDRainHeat" type="xsd:integer"> <xsd:annotation> <xsd:documentation>Heating design day rain flag. 0=no rain, 1=rain</xsd:documentation> </xsd:annotation> </xsd:element>

element DDSkyClearnessCool

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | unitlessUnitEnum | required |  |  |
annotation |
documentation
Cooling design day sky clearness
source | <xsd:element name="DDSkyClearnessCool"> <xsd:annotation> <xsd:documentation>Cooling design day sky clearness</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDSkyClearnessCool/@unit

type | unitlessUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Percent |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element DDSkyClearnessHeat

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | unitlessUnitEnum | required |  |  |
annotation |
documentation
Heating design day sky clearness
source | <xsd:element name="DDSkyClearnessHeat"> <xsd:annotation> <xsd:documentation>Heating design day sky clearness</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDSkyClearnessHeat/@unit

type | unitlessUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Percent |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element DDSnowCool

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Flag for snow on the cooling design day. 0=not snowing 1=snowing
source | <xsd:element name="DDSnowCool" type="xsd:integer"> <xsd:annotation> <xsd:documentation>Flag for snow on the cooling design day. 0=not snowing 1=snowing</xsd:documentation> </xsd:annotation> </xsd:element>

element DDSnowHeat

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Weather
annotation |
documentation
Heating design day snow flag. 0=not snowing 1=snowing
source | <xsd:element name="DDSnowHeat" type="xsd:integer"> <xsd:annotation> <xsd:documentation>Heating design day snow flag. 0=not snowing 1=snowing</xsd:documentation> </xsd:annotation> </xsd:element>

element DDWBCool

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | temperatureUnitEnum |  |  |  |
annotation |
documentation
Cooling design day wet bulb temperature
source | <xsd:element name="DDWBCool"> <xsd:annotation> <xsd:documentation>Cooling design day wet bulb temperature</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDWBCool/@unit

type | temperatureUnitEnum
facets |
Kind | Value | Annotation
enumeration | F |
enumeration | C |
enumeration | K |
enumeration | R |
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element DDWBHeat

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | temperatureUnitEnum |  |  |  |
annotation |
documentation
Heating design day wet bulb temperature
source | <xsd:element name="DDWBHeat"> <xsd:annotation> <xsd:documentation>Heating design day wet bulb temperature</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDWBHeat/@unit

type | temperatureUnitEnum
facets |
Kind | Value | Annotation
enumeration | F |
enumeration | C |
enumeration | K |
enumeration | R |
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element DDWindDirCool

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | directionUnitEnum | required |  |  |
annotation |
documentation
Cooing design day wind direction
source | <xsd:element name="DDWindDirCool"> <xsd:annotation> <xsd:documentation>Cooing design day wind direction</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="directionUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDWindDirCool/@unit

type | directionUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | DegreeDecimalFromNorth |
source | <xsd:attribute name="unit" type="directionUnitEnum" use="required"/>

element DDWindDirHeat

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | directionUnitEnum | required |  |  |
annotation |
documentation
Heating design day wind direction
source | <xsd:element name="DDWindDirHeat"> <xsd:annotation> <xsd:documentation>Heating design day wind direction</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="directionUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDWindDirHeat/@unit

type | directionUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | DegreeDecimalFromNorth |
source | <xsd:attribute name="unit" type="directionUnitEnum" use="required"/>

element DDWindSpeedCool

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | velocityUnitEnum | required |  |  |
annotation |
documentation
Cooling design day wind speed
source | <xsd:element name="DDWindSpeedCool"> <xsd:annotation> <xsd:documentation>Cooling design day wind speed</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="velocityUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDWindSpeedCool/@unit

type | velocityUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | MetersPerSecond |
enumeration | MilesPerHour |
enumeration | Knots |
source | <xsd:attribute name="unit" type="velocityUnitEnum" use="required"/>

element DDWindSpeedHeat

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | velocityUnitEnum | required |  |  |
annotation |
documentation
Heating design day wind speed
source | <xsd:element name="DDWindSpeedHeat"> <xsd:annotation> <xsd:documentation>Heating design day wind speed</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="velocityUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DDWindSpeedHeat/@unit

type | velocityUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | MetersPerSecond |
enumeration | MilesPerHour |
enumeration | Knots |
source | <xsd:attribute name="unit" type="velocityUnitEnum" use="required"/>

element DeltaP

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | AirLoopEquipment HydronicLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | deltaPUnitEnum | required |  |  |
hydronicLoopType | loopTypeEnum |  |  |  |
hydronicLoopIdRef | xsd:IDREF |  |  |  |
conditioningType | conditioningTypeEnum |  |  |  |
documentation
Use this attribute for conditioning units with both heating and cooling.
performanceId | xsd:IDREF |  |  |  |
documentation
Use this attribute to point to a performance curve if one is provided
annotation |
documentation
Difference in pressure
source | <xsd:element name="DeltaP"> <xsd:annotation> <xsd:documentation>Difference in pressure</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="deltaPUnitEnum" use="required"/> <xsd:attribute name="hydronicLoopType" type="loopTypeEnum"/> <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF"/> <xsd:attribute name="conditioningType" type="conditioningTypeEnum"> <xsd:annotation> <xsd:documentation>Use this attribute for conditioning units with both heating and cooling.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="performanceId" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Use this attribute to point to a performance curve if one is provided</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DeltaP/@unit

type | deltaPUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | PSI |
enumeration | kPa |
enumeration | Atmospheres |
enumeration | InchesOfH2O |
enumeration | CentimetersOfH2O |
enumeration | InchesOfMercury |
enumeration | CentimetersOfMercury |
enumeration | MillimetersOfMercury |
enumeration | Pascals |
source | <xsd:attribute name="unit" type="deltaPUnitEnum" use="required"/>

attribute DeltaP/@hydronicLoopType

type | loopTypeEnum
facets |
Kind | Value | Annotation
enumeration | PrimaryChilledWater |
enumeration | SecondaryChilledWater |
enumeration | HotWater |
enumeration | CondenserWater |
enumeration | DomesticHotWater |
enumeration | WaterLoopHeatPump |
enumeration | TwoPipe |
enumeration | PotableWaterLoop |
enumeration | VRFLoop |
source | <xsd:attribute name="hydronicLoopType" type="loopTypeEnum"/>

attribute DeltaP/@hydronicLoopIdRef

type | xsd:IDREF
source | <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF"/>

attribute DeltaP/@conditioningType

type | conditioningTypeEnum
facets |
Kind | Value | Annotation
enumeration | Heating |
enumeration | Cooling |
enumeration | HeatingAndCooling |
annotation |
documentation
Use this attribute for conditioning units with both heating and cooling.
source | <xsd:attribute name="conditioningType" type="conditioningTypeEnum"> <xsd:annotation> <xsd:documentation>Use this attribute for conditioning units with both heating and cooling.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute DeltaP/@performanceId

type | xsd:IDREF
annotation |
documentation
Use this attribute to point to a performance curve if one is provided
source | <xsd:attribute name="performanceId" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Use this attribute to point to a performance curve if one is provided</xsd:documentation> </xsd:annotation> </xsd:attribute>

element DeltaT

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | AirLoopEquipment HydronicLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | temperatureUnitEnum |  |  |  |
conditioningType | conditioningTypeEnum |  |  |  |
documentation
Use this attribute for conditioning units with both heating and cooling.
annotation |
documentation
Difference in temperature
source | <xsd:element name="DeltaT"> <xsd:annotation> <xsd:documentation>Difference in temperature</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> <xsd:attribute name="conditioningType" type="conditioningTypeEnum"> <xsd:annotation> <xsd:documentation>Use this attribute for conditioning units with both heating and cooling.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DeltaT/@unit

type | temperatureUnitEnum
facets |
Kind | Value | Annotation
enumeration | F |
enumeration | C |
enumeration | K |
enumeration | R |
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

attribute DeltaT/@conditioningType

type | conditioningTypeEnum
facets |
Kind | Value | Annotation
enumeration | Heating |
enumeration | Cooling |
enumeration | HeatingAndCooling |
annotation |
documentation
Use this attribute for conditioning units with both heating and cooling.
source | <xsd:attribute name="conditioningType" type="conditioningTypeEnum"> <xsd:annotation> <xsd:documentation>Use this attribute for conditioning units with both heating and cooling.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Density

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Fire Gap Material
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | densityUnitEnum | required |  |  |
source | <xsd:element name="Density"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="densityUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Density/@unit

type | densityUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | GramsPerCubicCm |
enumeration | LbsPerCubicIn |
enumeration | LbsPerCubicFt |
enumeration | KgPerCubicM |
source | <xsd:attribute name="unit" type="densityUnitEnum" use="required"/>

element DensityFofT

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Gap
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | densityFofTUnitEnum | required |  |  |
annotation |
documentation
Density as a function of temperature
source | <xsd:element name="DensityFofT"> <xsd:annotation> <xsd:documentation>Density as a function of temperature</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="densityFofTUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DensityFofT/@unit

type | densityFofTUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | LbsPerCubicFtF |
enumeration | KgPerCubicMK |
source | <xsd:attribute name="unit" type="densityFofTUnitEnum" use="required"/>

element DependentValue

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Data
annotation |
documentation
Value of a dependent variable for this data point
source | <xsd:element name="DependentValue" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Value of a dependent variable for this data point</xsd:documentation> </xsd:annotation> </xsd:element>

element DependentVariable

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description
used by |
elements | Equation PointData
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | xsd:string | required |  |  |
dataType | xsd:string | required |  |  |
minValue | xsd:decimal |  |  |  |
documentation
Use minValue and maxValue to define constraints on the curve.
maxValue | xsd:decimal |  |  |  |
source | <xsd:element name="DependentVariable"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="unit" type="xsd:string" use="required"/> <xsd:attribute name="dataType" type="xsd:string" use="required"/> <xsd:attribute name="minValue" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Use minValue and maxValue to define constraints on the curve.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="maxValue" type="xsd:decimal"/> </xsd:complexType> </xsd:element>

attribute DependentVariable/@unit

type | xsd:string
properties |
use | required
source | <xsd:attribute name="unit" type="xsd:string" use="required"/>

attribute DependentVariable/@dataType

type | xsd:string
properties |
use | required
source | <xsd:attribute name="dataType" type="xsd:string" use="required"/>

attribute DependentVariable/@minValue

type | xsd:decimal
annotation |
documentation
Use minValue and maxValue to define constraints on the curve.
source | <xsd:attribute name="minValue" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Use minValue and maxValue to define constraints on the curve.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute DependentVariable/@maxValue

type | xsd:decimal
source | <xsd:attribute name="maxValue" type="xsd:decimal"/>

element Description

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
elements | Activity AirLoop AirLoopEquipment AirSystem AnalysisParameter Behavior Blind Building Campus Construction DaySchedule DependentVariable ExtEquip Frame Gap Glaze HolidaysModeled HydronicLoop HydronicLoopEquipment IndependentVariable IntEquip Layer Location Material Meter MovementBehavior Opening Parameter Results Schedule ShellGeometry Space Surface Weather WeekSchedule WindowType XAxis YAxis YearSchedule Zone ZoneHVACEquipment
source | <xsd:element name="Description" type="xsd:string"/>

element DesignCoolRH

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Zone
annotation |
documentation
Relative humidity set point for cooling.
source | <xsd:element name="DesignCoolRH"> <xsd:annotation> <xsd:documentation>Relative humidity set point for cooling.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"/> </xsd:simpleContent> </xsd:complexType> </xsd:element>

element DesignCoolT

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | HydronicLoop Zone
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | temperatureUnitEnum |  |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
annotation |
documentation
Design temperature for cooling
source | <xsd:element name="DesignCoolT"> <xsd:annotation> <xsd:documentation>Design temperature for cooling</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DesignCoolT/@unit

type | temperatureUnitEnum
facets |
Kind | Value | Annotation
enumeration | F |
enumeration | C |
enumeration | K |
enumeration | R |
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

attribute DesignCoolT/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element DesignFlow

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | FlowControl
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | flowUnitEnum |  |  |  |
source | <xsd:element name="DesignFlow"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="flowUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DesignFlow/@unit

type | flowUnitEnum
facets |
Kind | Value | Annotation
enumeration | CFM |
enumeration | CubicMPerHr |
enumeration | LPerSec |
enumeration | LPM |
enumeration | GPH |
enumeration | GPM |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="flowUnitEnum"/>

element DesignHeatRH

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Zone
annotation |
documentation
Relative humidity set point for heating.
source | <xsd:element name="DesignHeatRH"> <xsd:annotation> <xsd:documentation>Relative humidity set point for heating.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"/> </xsd:simpleContent> </xsd:complexType> </xsd:element>

element DesignHeatT

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Zone
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | temperatureUnitEnum |  |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
annotation |
documentation
Design temperature for heating
source | <xsd:element name="DesignHeatT"> <xsd:annotation> <xsd:documentation>Design temperature for heating</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DesignHeatT/@unit

type | temperatureUnitEnum
facets |
Kind | Value | Annotation
enumeration | F |
enumeration | C |
enumeration | K |
enumeration | R |
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

attribute DesignHeatT/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element DesignPressure

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | PressureControl
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | pressureUnitEnum |  |  |  |
source | <xsd:element name="DesignPressure"> <xsd:complexType> <xsd:attribute name="unit" type="pressureUnitEnum"/> </xsd:complexType> </xsd:element>

attribute DesignPressure/@unit

type | pressureUnitEnum
facets |
Kind | Value | Annotation
enumeration | PSI |
enumeration | kPa |
enumeration | Atmospheres |
enumeration | InchesOfH2O |
enumeration | CentimetersOfH2O |
enumeration | InchesOfMercury |
enumeration | CentimetersOfMercury |
enumeration | MillimetersOfMercury |
enumeration | Pascals |
source | <xsd:attribute name="unit" type="pressureUnitEnum"/>

element DesignTemp

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | TemperatureControl
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | temperatureUnitEnum |  |  |  |
source | <xsd:element name="DesignTemp"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute DesignTemp/@unit

type | temperatureUnitEnum
facets |
Kind | Value | Annotation
enumeration | F |
enumeration | C |
enumeration | K |
enumeration | R |
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element Dimensions

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Height Width Length
used by |
element | LightingSystem
source | <xsd:element name="Dimensions"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Height" minOccurs="0"/> <xsd:element ref="Width" minOccurs="0"/> <xsd:element ref="Length" minOccurs="0"/> </xsd:choice> </xsd:complexType> </xsd:element>

element DocumentHistory

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | CreatedBy ProgramInfo PersonInfo ModifiedBy
used by |
element | gbXML
annotation |
documentation
Contains details about people and programs that created and modified this file
source | <xsd:element name="DocumentHistory"> <xsd:annotation> <xsd:documentation>Contains details about people and programs that created and modified this file</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="2" maxOccurs="unbounded"> <xsd:element ref="CreatedBy" minOccurs="1" maxOccurs="1"/> <xsd:element ref="ProgramInfo" minOccurs="1" maxOccurs="unbounded"/> <xsd:element ref="PersonInfo" minOccurs="1" maxOccurs="unbounded"/> <xsd:element ref="ModifiedBy" minOccurs="1" maxOccurs="unbounded"/> </xsd:choice> </xsd:complexType> </xsd:element>

element Drivers

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Time Environment RoomEventType OtherConstraint
used by |
element | Behavior
annotation |
documentation
Drivers are part of the DNAS framework and represent the environmental factors that stimulate occupants to fulfill a physical, physiological or psychological need.
source | <xsd:element name="Drivers"> <xsd:annotation> <xsd:documentation>Drivers are part of the DNAS framework and represent the environmental factors that stimulate occupants to fulfill a physical, physiological or psychological need.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:sequence> <xsd:element ref="Time" minOccurs="0"/> <xsd:element ref="Environment" minOccurs="0"/> <xsd:element ref="RoomEventType" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="OtherConstraint" minOccurs="0" maxOccurs="unbounded"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element EconomizerLockout

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | AirLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | economizerLockoutEnum |  |  |  |
source | <xsd:element name="EconomizerLockout"> <xsd:complexType> <xsd:attribute name="unit" type="economizerLockoutEnum"/> </xsd:complexType> </xsd:element>

attribute EconomizerLockout/@unit

type | economizerLockoutEnum
facets |
Kind | Value | Annotation
enumeration | NoLockout |
enumeration | LockoutWithHeating |
enumeration | LockoutWithCompressor |
source | <xsd:attribute name="unit" type="economizerLockoutEnum"/>

element Education

diagram |
namespace | http://www.gbxml.org/schema
type | EducationType
properties |
content | simple
used by |
element | SocioEconomic
facets |
Kind | Value | Annotation
enumeration | High school |
enumeration | Bachelors |
enumeration | Post-graduate |
source | <xsd:element name="Education" type="EducationType"/>

element Efficiency

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | AirLoopEquipment ExtEquip HydronicLoopEquipment IntEquip
attributes |
Name | Type | Use | Default | Fixed | Annotation
standardsType | standardsTypeEnum |  |  |  |
documentation
Use the standardsType attribute when the efficiency is measured at standard conditions.
efficiencyType | efficiencyTypeEnum | required |  |  |
operationType | conditioningTypeEnum |  |  |  |
documentation
Use this attribute for conditioning units with both heating and cooling.
performanceId | xsd:IDREF |  |  |  |
documentation
Use this attribute to point to a performance curve if one is provided
source | <xsd:element name="Efficiency"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="standardsType" type="standardsTypeEnum"> <xsd:annotation> <xsd:documentation>Use the standardsType attribute when the efficiency is measured at standard conditions.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="efficiencyType" type="efficiencyTypeEnum" use="required"/> <xsd:attribute name="operationType" type="conditioningTypeEnum"> <xsd:annotation> <xsd:documentation>Use this attribute for conditioning units with both heating and cooling.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="performanceId" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Use this attribute to point to a performance curve if one is provided</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Efficiency/@standardsType

type | standardsTypeEnum
facets |
Kind | Value | Annotation
enumeration | DOE |
documentation
Department of Energy
enumeration | ARI |
documentation
Air-Conditioning and Refrigeration Institute
enumeration | ANSI |
documentation
American National Standards Institute
enumeration | NEMA |
documentation
National Electrical Manufacturers Association
annotation |
documentation
Use the standardsType attribute when the efficiency is measured at standard conditions.
source | <xsd:attribute name="standardsType" type="standardsTypeEnum"> <xsd:annotation> <xsd:documentation>Use the standardsType attribute when the efficiency is measured at standard conditions.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Efficiency/@efficiencyType

type | efficiencyTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | COP |
documentation
Coefficient of Performance
enumeration | EER |
documentation
Energy Efficiency Ratio
enumeration | SEER |
documentation
Seasonal Energy Efficiency Ratio
enumeration | AFUE |
documentation
Annual Fuel Utilization Efficiency
enumeration | HSPF |
documentation
Heating Seasonal Performance Factor
enumeration | effectiveness |
enumeration | EnergyFactor |
enumeration | ThermalEff |
documentation
Thermal Efficiency
enumeration | MotorEff |
documentation
Motor Efficiency
enumeration | FanEff |
documentation
Fan Efficiency
enumeration | MechanicalEff |
documentation
Mechanical Efficiency
enumeration | BoilerEff |
documentation
Boiler Efficiency
enumeration | kWPerTon |
enumeration | kWPerkW |
enumeration | BTUPerHourPerF |
enumeration | kWPerC |
source | <xsd:attribute name="efficiencyType" type="efficiencyTypeEnum" use="required"/>

attribute Efficiency/@operationType

type | conditioningTypeEnum
facets |
Kind | Value | Annotation
enumeration | Heating |
enumeration | Cooling |
enumeration | HeatingAndCooling |
annotation |
documentation
Use this attribute for conditioning units with both heating and cooling.
source | <xsd:attribute name="operationType" type="conditioningTypeEnum"> <xsd:annotation> <xsd:documentation>Use this attribute for conditioning units with both heating and cooling.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Efficiency/@performanceId

type | xsd:IDREF
annotation |
documentation
Use this attribute to point to a performance curve if one is provided
source | <xsd:attribute name="performanceId" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Use this attribute to point to a performance curve if one is provided</xsd:documentation> </xsd:annotation> </xsd:attribute>

element ElecLoad

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | ExtEquip IntEquip
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | powerUnitEnum | required |  |  |
annotation |
documentation
Electric load
source | <xsd:element name="ElecLoad"> <xsd:annotation> <xsd:documentation>Electric load</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="powerUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute ElecLoad/@unit

type | powerUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Watt |
enumeration | Kilowatt |
enumeration | Horsepower |
enumeration | KilogramForceMeterPerSecond |
enumeration | BtuPerSecond |
enumeration | FootPoundForcePerSecond |
enumeration | KilocaloriesPerSecond |
enumeration | BtuPerHour |
source | <xsd:attribute name="unit" type="powerUnitEnum" use="required"/>

element Elevation

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Location
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | lengthUnitEnum |  |  |  |
annotation |
documentation
Height above sea level
source | <xsd:element name="Elevation"> <xsd:annotation> <xsd:documentation>Height above sea level</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="lengthUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Elevation/@unit

type | lengthUnitEnum
facets |
Kind | Value | Annotation
enumeration | Kilometers |
enumeration | Meters |
enumeration | Centimeters |
enumeration | Millimeters |
enumeration | Miles |
enumeration | Yards |
enumeration | Feet |
enumeration | Inches |
source | <xsd:attribute name="unit" type="lengthUnitEnum"/>

element Email1Address

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | PersonInfo
source | <xsd:element name="Email1Address" type="xsd:string"/>

element EmissionRate

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | IndoorAirQuality
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | emissionUnitEnum | required |  |  |
source | <xsd:element name="EmissionRate"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="emissionUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute EmissionRate/@unit

type | emissionUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | PoundsPerHour |
enumeration | KilogramsPerHour |
enumeration | GramsPerHour |
source | <xsd:attribute name="unit" type="emissionUnitEnum" use="required"/>

element Emittance

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Blind Construction FireFace Glaze Material Opening WindowType
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | unitlessUnitEnum | required |  |  |
type | emittanceTypeEnum | required |  |  |
surfaceType | surfaceDescriptionEnum | required |  |  |
annotation |
documentation
Infra-red emissivity
source | <xsd:element name="Emittance"> <xsd:annotation> <xsd:documentation>Infra-red emissivity</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> <xsd:attribute name="type" type="emittanceTypeEnum" use="required"/> <xsd:attribute name="surfaceType" type="surfaceDescriptionEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Emittance/@unit

type | unitlessUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Percent |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

attribute Emittance/@type

type | emittanceTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | IntIR |
enumeration | ExtIR |
source | <xsd:attribute name="type" type="emittanceTypeEnum" use="required"/>

attribute Emittance/@surfaceType

type | surfaceDescriptionEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | 1 |
documentation
The surfaceDescriptionEnum allows control over the specification of material surface properties. By setting the surfaceDescriptionEnum to 1, it is implied that the attribute (e.g. - Reflectance, Emittance, etc.) is associated with Surface 1 of the material's two surfaces [it is assumed that the material is a large planar object]. Surface 1 represents the surface that points away from the building interior.
enumeration | 2 |
documentation
The surfaceDescriptionEnum allows control over the specification of material surface properties. By setting the surfaceDescriptionEnum to 2, it is implied that the attribute (e.g. - Reflectance, Emittance, etc.) is associated with Surface 2 of the material's two surfaces [it is assumed that the material is a large planar object]. Surface 2 represents the surface that points towards the building interior.
enumeration | Both |
documentation
The surfaceDescriptionEnum allows control over the specification of material surface properties. By setting the surfaceDescriptionEnum to Both, it is implied that the attribute (e.g. - Reflectance, Emittance, etc.) is associated both Surface 1 and Surface 2 of the material's 2 surfaces [it is assumed that the material is a large planar object]. See the enumerations above for a description of Surface 1 and 2.
source | <xsd:attribute name="surfaceType" type="surfaceDescriptionEnum" use="required"/>

element Employment

diagram |
namespace | http://www.gbxml.org/schema
type | EmploymentType
properties |
content | simple
used by |
element | SocioEconomic
facets |
Kind | Value | Annotation
enumeration | Unemployed |
enumeration | Employed |
enumeration | Self-employed |
source | <xsd:element name="Employment" type="EmploymentType"/>

element EndDate

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:date
properties |
content | simple
used by |
elements | YearModeled YearSchedule
annotation |
documentation
Month and day year schedule ends
source | <xsd:element name="EndDate" type="xsd:date"> <xsd:annotation> <xsd:documentation>Month and day year schedule ends</xsd:documentation> </xsd:annotation> </xsd:element>

element EndDay

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Seasons/Season
source | <xsd:element name="EndDay" type="xsd:integer"/>

element EndHour

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | TimeofDay
source | <xsd:element name="EndHour" type="xsd:integer"/>

element EndMinute

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | TimeofDay
source | <xsd:element name="EndMinute" type="xsd:integer"/>

element EndMonth

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Seasons/Season
source | <xsd:element name="EndMonth" type="xsd:integer"/>

element Energy

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | AirLoopEquipment ExtEquip HydronicLoopEquipment IntEquip
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | energyUnitEnum | required |  |  |
valueType | valueTypeEnum | required |  |  |
timePeriod | timePeriodEnum | required |  |  |
resourceType | resourceTypeEnum | required |  |  |
meterIdRef | xsd:IDREF |  |  |  |
documentation
ID for a resource meter
source | <xsd:element name="Energy"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="energyUnitEnum" use="required"/> <xsd:attribute name="valueType" type="valueTypeEnum" use="required"/> <xsd:attribute name="timePeriod" type="timePeriodEnum" use="required"/> <xsd:attribute name="resourceType" type="resourceTypeEnum" use="required"/> <xsd:attribute name="meterIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for a resource meter</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Energy/@unit

type | energyUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | KilowattHours |
enumeration | Joules |
enumeration | BTU |
enumeration | Therms |
source | <xsd:attribute name="unit" type="energyUnitEnum" use="required"/>

attribute Energy/@valueType

type | valueTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Historical |
enumeration | Simulated |
enumeration | Rated |
enumeration | Measured |
source | <xsd:attribute name="valueType" type="valueTypeEnum" use="required"/>

attribute Energy/@timePeriod

type | timePeriodEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Annual |
enumeration | Jan |
enumeration | Feb |
enumeration | Mar |
enumeration | Apr |
enumeration | May |
enumeration | Jun |
enumeration | Jul |
enumeration | Aug |
enumeration | Sep |
enumeration | Oct |
enumeration | Nov |
enumeration | Dec |
source | <xsd:attribute name="timePeriod" type="timePeriodEnum" use="required"/>

attribute Energy/@resourceType

type | resourceTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Electricity |
enumeration | NaturalGas |
enumeration | Propane |
enumeration | FuelOil1 |
enumeration | FuelOil2 |
enumeration | FuelOil4 |
enumeration | Water |
enumeration | ChilledWater |
enumeration | HotWater |
enumeration | Steam |
source | <xsd:attribute name="resourceType" type="resourceTypeEnum" use="required"/>

attribute Energy/@meterIdRef

type | xsd:IDREF
annotation |
documentation
ID for a resource meter
source | <xsd:attribute name="meterIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for a resource meter</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Enthalpy

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | AirLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | enthalpyUnitEnum | required |  |  |
enthalpyType | enthalpyTypeEnum | optional |  |  |
annotation |
documentation
Minimum enthalpy setpoint for air-side economizer.
source | <xsd:element name="Enthalpy"> <xsd:annotation> <xsd:documentation>Minimum enthalpy setpoint for air-side economizer.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="enthalpyUnitEnum" use="required"/> <xsd:attribute name="enthalpyType" type="enthalpyTypeEnum" use="optional"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Enthalpy/@unit

type | enthalpyUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | BTUPerLb |
enumeration | KJPerKg |
source | <xsd:attribute name="unit" type="enthalpyUnitEnum" use="required"/>

attribute Enthalpy/@enthalpyType

type | enthalpyTypeEnum
properties |
use | optional
facets |
Kind | Value | Annotation
enumeration | EconomizerUpperLimit |
enumeration | AirSideEconomizerMinSetpoint |
enumeration | EconomizerMaxLimit |
source | <xsd:attribute name="enthalpyType" type="enthalpyTypeEnum" use="optional"/>

element Environment

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Parameter
used by |
element | Drivers
annotation |
documentation
Environmental driver parameters can be defined.
source | <xsd:element name="Environment"> <xsd:annotation> <xsd:documentation>Environmental driver parameters can be defined.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:sequence> <xsd:element ref="Parameter" maxOccurs="unbounded"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element EnvironmentAwareness

diagram |
namespace | http://www.gbxml.org/schema
type | subjectiveValueType
properties |
content | simple
used by |
element | SubjectiveValues
facets |
Kind | Value | Annotation
enumeration | High |
enumeration | Medium |
enumeration | Low |
source | <xsd:element name="EnvironmentAwareness" type="subjectiveValueType"/>

element Equation

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Expression IndependentVariable DependentVariable
used by |
element | Performance
annotation |
documentation
The Equation element allows data for n-dimensional algebraic data to be entered. The Expression element should contain an dependent variable followed by an = sign and an equation containing independent variables. The independent and dependent variables are then defined by their respective tags. The only mathematical operations allowed are ^ (power), + (addition), - (subtraction), / (division), and * (multiplication). Example: z=x+2*y^2 would have an DependentVariable with a name = z, and two IndependentVariable(s) with names of x and y. Descriptions would be included for each variable, along with unit and dataType information identifying the variable and its role.
source | <xsd:element name="Equation"> <xsd:annotation> <xsd:documentation>The Equation element allows data for n-dimensional algebraic data to be entered. The Expression element should contain an dependent variable followed by an = sign and an equation containing independent variables. The independent and dependent variables are then defined by their respective tags. The only mathematical operations allowed are ^ (power), + (addition), - (subtraction), / (division), and * (multiplication). Example: z=x+2*y^2 would have an DependentVariable with a name = z, and two IndependentVariable(s) with names of x and y. Descriptions would be included for each variable, along with unit and dataType information identifying the variable and its role. </xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Expression"/> <xsd:element ref="IndependentVariable" maxOccurs="unbounded"/> <xsd:element ref="DependentVariable" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> </xsd:complexType> </xsd:element>

element EquipPowerPerArea

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Space
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | powerPerAreaUnitEnum | required |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
annotation |
documentation
Amount of power used by equipment in a given area
source | <xsd:element name="EquipPowerPerArea"> <xsd:annotation> <xsd:documentation>Amount of power used by equipment in a given area</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="powerPerAreaUnitEnum" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute EquipPowerPerArea/@unit

type | powerPerAreaUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | WattPerSquareMeter |
enumeration | WattPerSquareFoot |
source | <xsd:attribute name="unit" type="powerPerAreaUnitEnum" use="required"/>

attribute EquipPowerPerArea/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element EventDuration

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | NormalDurationModel
used by |
element | StatusTransitionEvent
annotation |
documentation
Duration properties of an event. If specify, the event will end after the duration.
source | <xsd:element name="EventDuration"> <xsd:annotation> <xsd:documentation>Duration properties of an event. If specify, the event will end after the duration.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:sequence> <xsd:element ref="NormalDurationModel"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element EventOccurModel

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | CustomProbabilityModel MarkovChainModel NormalProbabilityModel
used by |
element | StatusTransitionEvent
annotation |
documentation
The event occur model
source | <xsd:element name="EventOccurModel"> <xsd:annotation> <xsd:documentation>The event occur model</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice> <xsd:element ref="CustomProbabilityModel"/> <xsd:element ref="MarkovChainModel"/> <xsd:element ref="NormalProbabilityModel"/> </xsd:choice> </xsd:complexType> </xsd:element>

element Expression

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | Equation
source | <xsd:element name="Expression" type="xsd:string"/>

element ExtEquip

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Manufacturer Model ElecLoad FuelLoad LatentLoad WindSpeed Efficiency Performance Cost Weight WasteWaterHREff WaterUsePerCycle RatedFlow Power CyclesPerWeek Energy GeneralGeometry ShellGeometry IndoorAirQuality Age Reference CADObjectId
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
scheduleIdRef | xsd:IDREF |  |  |  |
documentation
ID for the schedule of transmittance of a shading surface
waterTempScheduleIdRef | xsd:IDREF |  |  |  |
hydronicLoopIdRef | xsd:IDREF |  |  |  |
documentation
ID pointing to a hydronic loop
waterScheduleIdRef | xsd:IDREF |  |  |  |
waterMeterIdRef | xsd:IDREF |  |  |  |
type | extEquipTypeEnum | required |  |  |
airLoopIdRef | xsd:IDREF |  |  |  |
documentation
ID pointing to an air loop
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
annotation |
documentation
External equipment. This is generalized to be able to contain any type of external equipment.
source | <xsd:element name="ExtEquip"> <xsd:annotation> <xsd:documentation>External equipment. This is generalized to be able to contain any type of external equipment.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Manufacturer" minOccurs="0"/> <xsd:element ref="Model" minOccurs="0"/> <xsd:element ref="ElecLoad" minOccurs="0"/> <xsd:element ref="FuelLoad" minOccurs="0"/> <xsd:element ref="LatentLoad" minOccurs="0"/> <xsd:element ref="WindSpeed" minOccurs="0"/> <xsd:element ref="Efficiency" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Performance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Cost" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Weight" minOccurs="0"/> <xsd:element ref="WasteWaterHREff" minOccurs="0"/> <xsd:element ref="WaterUsePerCycle" minOccurs="0"/> <xsd:element ref="RatedFlow" minOccurs="0"/> <xsd:element ref="Power" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="CyclesPerWeek" minOccurs="0"/> <xsd:element ref="Energy" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="GeneralGeometry" minOccurs="0"/> <xsd:element ref="ShellGeometry" minOccurs="0"/> <xsd:element ref="IndoorAirQuality" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Age" minOccurs="0"/> <xsd:element ref="Reference" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="CADObjectId" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="waterTempScheduleIdRef" type="xsd:IDREF"/> <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID pointing to a hydronic loop </xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="waterScheduleIdRef" type="xsd:IDREF"/> <xsd:attribute name="waterMeterIdRef" type="xsd:IDREF"/> <xsd:attribute name="type" type="extEquipTypeEnum" use="required"/> <xsd:attribute name="airLoopIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID pointing to an air loop</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute ExtEquip/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute ExtEquip/@scheduleIdRef

type | xsd:IDREF
annotation |
documentation
ID for the schedule of transmittance of a shading surface
source | <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute ExtEquip/@waterTempScheduleIdRef

type | xsd:IDREF
source | <xsd:attribute name="waterTempScheduleIdRef" type="xsd:IDREF"/>

attribute ExtEquip/@hydronicLoopIdRef

type | xsd:IDREF
annotation |
documentation
ID pointing to a hydronic loop
source | <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID pointing to a hydronic loop </xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute ExtEquip/@waterScheduleIdRef

type | xsd:IDREF
source | <xsd:attribute name="waterScheduleIdRef" type="xsd:IDREF"/>

attribute ExtEquip/@waterMeterIdRef

type | xsd:IDREF
source | <xsd:attribute name="waterMeterIdRef" type="xsd:IDREF"/>

attribute ExtEquip/@type

type | extEquipTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Sprinkler |
enumeration | LawnMower |
enumeration | GeneralPlugload |
enumeration | Fountain |
enumeration | Refrigerator |
enumeration | Freezer |
enumeration | Pool |
enumeration | HotTub |
enumeration | Pump |
enumeration | Sauna |
enumeration | BatteryCharger |
enumeration | Furnace |
enumeration | IndustrialEquip |
enumeration | Irrigation |
enumeration | MiscEquip |
enumeration | Vending |
enumeration | Elevator |
enumeration | Escalator |
enumeration | WindTurbine |
enumeration | Photovoltaic |
enumeration | CogenDiesel |
enumeration | CogenFuelCell |
enumeration | CogenGasTurbine |
source | <xsd:attribute name="type" type="extEquipTypeEnum" use="required"/>

attribute ExtEquip/@airLoopIdRef

type | xsd:IDREF
annotation |
documentation
ID pointing to an air loop
source | <xsd:attribute name="airLoopIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID pointing to an air loop</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute ExtEquip/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element ExtEquipId

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:string
properties |
content | complex
used by |
elements | Campus Construction WindowType
attributes |
Name | Type | Use | Default | Fixed | Annotation
extEquipIdRef | xsd:IDREF |  |  |  |
source | <xsd:element name="ExtEquipId"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:string"> <xsd:attribute name="extEquipIdRef" type="xsd:IDREF"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute ExtEquipId/@extEquipIdRef

type | xsd:IDREF
source | <xsd:attribute name="extEquipIdRef" type="xsd:IDREF"/>

element FamilyName

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | Surface
source | <xsd:element name="FamilyName" type="xsd:string"/>

element Fan

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | AirSystem
attributes |
Name | Type | Use | Default | Fixed | Annotation
fanType | fanTypeEnum | required |  |  |
id | xsd:ID | required |  |  |
source | <xsd:element name="Fan"> <xsd:complexType> <xsd:attribute name="fanType" type="fanTypeEnum" use="required"/> <xsd:attribute name="id" type="xsd:ID" use="required"/> </xsd:complexType> </xsd:element>

attribute Fan/@fanType

type | fanTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | ConstantVolume |
enumeration | VariableVolume |
source | <xsd:attribute name="fanType" type="fanTypeEnum" use="required"/>

attribute Fan/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

element FileName

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | ProjectEntity
source | <xsd:element name="FileName" type="xsd:string"/>

element Fire

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Thickness Conductivity Density SpecificHeat
used by |
element | Material
annotation |
documentation
Properties of a material under fire conditions.
source | <xsd:element name="Fire"> <xsd:annotation> <xsd:documentation>Properties of a material under fire conditions.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0"> <xsd:element ref="Thickness"/> <xsd:element ref="Conductivity"/> <xsd:element ref="Density"/> <xsd:element ref="SpecificHeat"/> </xsd:choice> </xsd:complexType> </xsd:element>

element FireFace

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Absorptance Reflectance Emittance
used by |
element | Construction
annotation |
documentation
Properties of a construction under fire conditions.
source | <xsd:element name="FireFace"> <xsd:annotation> <xsd:documentation>Properties of a construction under fire conditions.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0"> <xsd:element ref="Absorptance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Reflectance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Emittance" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> </xsd:complexType> </xsd:element>

element FirstName

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | PersonInfo
source | <xsd:element name="FirstName" type="xsd:string"/>

element FloorSlabHeatLossCoefficient

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:float
properties |
content | complex
used by |
element | LoadCalcInputParameters
attributes |
Name | Type | Use | Default | Fixed | Annotation
floorSlabPerimeterHeatLossCoefficientUnitTypeEnum | floorSlabPerimeterHeatLossCoefficientUnitTypeEnum |  |  |  |
annotation |
documentation
Specifies the heat loss from a floor in terms of the amount of heat lost per length of exposed perimeter. Used with both commercial and residential load calculation methods.
source | <xsd:element name="FloorSlabHeatLossCoefficient"> <xsd:annotation> <xsd:documentation>Specifies the heat loss from a floor in terms of the amount of heat lost per length of exposed perimeter. Used with both commercial and residential load calculation methods.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:float"> <xsd:attribute name="floorSlabPerimeterHeatLossCoefficientUnitTypeEnum" type="floorSlabPerimeterHeatLossCoefficientUnitTypeEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute FloorSlabHeatLossCoefficient/@floorSlabPerimeterHeatLossCoefficientUnitTypeEnum

type | floorSlabPerimeterHeatLossCoefficientUnitTypeEnum
facets |
Kind | Value | Annotation
enumeration | btuPerHourDegreeFPerLinearFoot |
enumeration | wattDegreeCPerLinearMeter |
source | <xsd:attribute name="floorSlabPerimeterHeatLossCoefficientUnitTypeEnum" type="floorSlabPerimeterHeatLossCoefficientUnitTypeEnum"/>

element Flow

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Zone
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | flowUnitEnum | required |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
source | <xsd:element name="Flow"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="flowUnitEnum" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Flow/@unit

type | flowUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | CFM |
enumeration | CubicMPerHr |
enumeration | LPerSec |
enumeration | LPM |
enumeration | GPH |
enumeration | GPM |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="flowUnitEnum" use="required"/>

attribute Flow/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element FlowControl

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | DesignFlow MinimumFlow MaximumFlow RecircFlow
used by |
element | HydronicLoop
attributes |
Name | Type | Use | Default | Fixed | Annotation
processScheduleId | xsd:IDREF | optional |  |  |
annotation |
documentation
Use this element to describe how the fluid flow is controlled. The temperatures specified in this element should be measured just upstream of the chiller.
source | <xsd:element name="FlowControl"> <xsd:annotation> <xsd:documentation>Use this element to describe how the fluid flow is controlled. The temperatures specified in this element should be measured just upstream of the chiller.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="DesignFlow" minOccurs="0"/> <xsd:element ref="MinimumFlow" minOccurs="0"/> <xsd:element ref="MaximumFlow" minOccurs="0"/> <xsd:element ref="RecircFlow" minOccurs="0"/> </xsd:choice> <xsd:attribute name="processScheduleId" type="xsd:IDREF" use="optional"/> </xsd:complexType> </xsd:element>

attribute FlowControl/@processScheduleId

type | xsd:IDREF
properties |
use | optional
source | <xsd:attribute name="processScheduleId" type="xsd:IDREF" use="optional"/>

element FlowPerArea

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Zone
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | flowPerAreaUnitEnum | required |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
source | <xsd:element name="FlowPerArea"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="flowPerAreaUnitEnum" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute FlowPerArea/@unit

type | flowPerAreaUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | CFMPerSquareFoot |
enumeration | LPerSecPerSquareM |
enumeration | CubicMPerSecPerSquareM |
enumeration | CubicMPerHourPerSquareM |
source | <xsd:attribute name="unit" type="flowPerAreaUnitEnum" use="required"/>

attribute FlowPerArea/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element FlowPerPerson

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Zone
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | flowUnitEnum | required |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
source | <xsd:element name="FlowPerPerson"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="flowUnitEnum" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute FlowPerPerson/@unit

type | flowUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | CFM |
enumeration | CubicMPerHr |
enumeration | LPerSec |
enumeration | LPM |
enumeration | GPH |
enumeration | GPM |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="flowUnitEnum" use="required"/>

attribute FlowPerPerson/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element FlowType

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | AirLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
flowType | flowTypeEnum | required |  |  |
source | <xsd:element name="FlowType"> <xsd:complexType> <xsd:attribute name="flowType" type="flowTypeEnum" use="required"/> </xsd:complexType> </xsd:element>

attribute FlowType/@flowType

type | flowTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Series |
enumeration | Parallel |
enumeration | SeriesFromPlenum |
enumeration | ParallelFromPlenum |
source | <xsd:attribute name="flowType" type="flowTypeEnum" use="required"/>

element Formula

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | ConstantValue Linear1D Linear2D Linear3D Quadratic1D Logit1D Logit2D Logit3D Weibull1D Logit1DQuadratic
used by |
element | Interaction
source | <xsd:element name="Formula"> <xsd:complexType> <xsd:choice> <xsd:element ref="ConstantValue" minOccurs="0"/> <xsd:element ref="Linear1D" minOccurs="0"/> <xsd:element ref="Linear2D" minOccurs="0"/> <xsd:element ref="Linear3D" minOccurs="0"/> <xsd:element ref="Quadratic1D" minOccurs="0"/> <xsd:element ref="Logit1D" minOccurs="0"/> <xsd:element ref="Logit2D" minOccurs="0"/> <xsd:element ref="Logit3D" minOccurs="0"/> <xsd:element ref="Weibull1D" minOccurs="0"/> <xsd:element ref="Logit1DQuadratic" minOccurs="0"/> </xsd:choice> </xsd:complexType> </xsd:element>

element FractionOnCyclePowerUse

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | AirLoopEquipment
annotation |
documentation
Fraction of on-cycle power use
source | <xsd:element name="FractionOnCyclePowerUse" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Fraction of on-cycle power use</xsd:documentation> </xsd:annotation> </xsd:element>

element Frame

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Width
used by |
element | WindowType
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
type | frameTypeEnum | required |  |  |
DOELibIdRef | xsd:string |  |  |  |
documentation
Use this attribute to reference objects in the DOE2 library
source | <xsd:element name="Frame"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Width" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="type" type="frameTypeEnum" use="required"/> <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Frame/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Frame/@type

type | frameTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Wood |
enumeration | Vinyl |
enumeration | Aluminum |
enumeration | AluminumWithBreak |
enumeration | Insulated |
source | <xsd:attribute name="type" type="frameTypeEnum" use="required"/>

attribute Frame/@DOELibIdRef

type | xsd:string
annotation |
documentation
Use this attribute to reference objects in the DOE2 library
source | <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute>

element FuelLoad

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | ExtEquip IntEquip
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | fuelLoadUnitEnum | required |  |  |
source | <xsd:element name="FuelLoad"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="fuelLoadUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute FuelLoad/@unit

type | fuelLoadUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | BtuPerHour |
enumeration | kBtuPerHour |
enumeration | MBtuPerHour |
enumeration | Watts |
enumeration | kW |
source | <xsd:attribute name="unit" type="fuelLoadUnitEnum" use="required"/>

element Gap

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Thickness Density DensityFofT Conductivity ConductivityFofT Viscosity ViscosityFofT PrandtlNumber PrandtlNumberFofT
used by |
element | WindowType
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
gas | gasTypeEnum | required |  |  |
DOELibIdRef | xsd:string |  |  |  |
documentation
Use this attribute to reference objects in the DOE2 library
annotation |
documentation
Space between window panes
source | <xsd:element name="Gap"> <xsd:annotation> <xsd:documentation>Space between window panes</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Thickness" minOccurs="0"/> <xsd:element ref="Density" minOccurs="0"/> <xsd:element ref="DensityFofT" minOccurs="0"/> <xsd:element ref="Conductivity" minOccurs="0"/> <xsd:element ref="ConductivityFofT" minOccurs="0"/> <xsd:element ref="Viscosity" minOccurs="0"/> <xsd:element ref="ViscosityFofT" minOccurs="0"/> <xsd:element ref="PrandtlNumber" minOccurs="0"/> <xsd:element ref="PrandtlNumberFofT" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="gas" type="gasTypeEnum" use="required"/> <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Gap/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Gap/@gas

type | gasTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Air |
enumeration | Argon |
enumeration | Krypton |
enumeration | CO2 |
enumeration | SF6 |
enumeration | Custom |
source | <xsd:attribute name="gas" type="gasTypeEnum" use="required"/>

attribute Gap/@DOELibIdRef

type | xsd:string
annotation |
documentation
Use this attribute to reference objects in the DOE2 library
source | <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute>

element GapId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
attributes |
Name | Type | Use | Default | Fixed | Annotation
gapIdRef | xsd:IDREF | required |  |  |
documentation
ID for a gap between window panes
source | <xsd:element name="GapId"> <xsd:complexType> <xsd:attribute name="gapIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID for a gap between window panes</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute GapId/@gapIdRef

type | xsd:IDREF
properties |
use | required
annotation |
documentation
ID for a gap between window panes
source | <xsd:attribute name="gapIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID for a gap between window panes</xsd:documentation> </xsd:annotation> </xsd:attribute>

element GasPreheatCoilEfficiency

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | AirLoopEquipment
annotation |
documentation
Gas preheat coil efficiency
source | <xsd:element name="GasPreheatCoilEfficiency" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Gas preheat coil efficiency</xsd:documentation> </xsd:annotation> </xsd:element>

element GasPreheatCoilParasiticElectricLoad

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | AirLoopEquipment
annotation |
documentation
Gas Preheat Coil Parasitic Electric Load
source | <xsd:element name="GasPreheatCoilParasiticElectricLoad" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Gas Preheat Coil Parasitic Electric Load</xsd:documentation> </xsd:annotation> </xsd:element>

element gbXML

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | aecXML Campus LightingSystem LightingControl Construction Layer Material WindowType Schedule WeekSchedule DaySchedule Zone AirLoop HydronicLoop AirSystem IntEquip ExtEquip Weather Meter Results DocumentHistory SimulationParameters ZoneHVACEquipment Occupants Behaviors
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID |  |  |  |
engine | derived by: xsd:NMTOKEN |  |  |  |
documentation
Analysis engine used
temperatureUnit | temperatureUnitEnum | required |  |  |
documentation
This attribute specifies the default temperature unit for the entire gbXML document, wherever the temperatureUnit simple type is used.
lengthUnit | lengthUnitEnum | required |  |  |
documentation
This attribute specifies the default length unit for the entire gbXML document, wherever the lengthUnit simple type is used.
areaUnit | areaUnitEnum | required |  |  |
documentation
This attribute specifies the default area unit for the entire gbXML document, wherever the areaUnit simple type is used.
volumeUnit | volumeUnitEnum | required |  |  |
documentation
This attribute specifies the default volume unit for the entire gbXML document, wherever the volumeUnit simple type is used.
useSIUnitsForResults | xsd:boolean | required |  |  |
documentation
Results will be given in SI or IP units. True = SI units which is the implied default. If False, results will be in english units.
version | versionEnum | required |  |  |
SurfaceReferenceLocation | surfaceReferenceLocationEnum | optional |  |  |
documentation
Use this attribute to determine what type of geometry information is included in the geometry elements. This is specified using an enumeration that includes shell/wall paper and centerline coordinates.
source | <xsd:element name="gbXML"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="aecXML" minOccurs="0"/> <xsd:element ref="Campus"/> <xsd:element ref="LightingSystem" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="LightingControl" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Construction" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Layer" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Material" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="WindowType" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Schedule" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="WeekSchedule" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="DaySchedule" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Zone" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="AirLoop" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="HydronicLoop" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="AirSystem" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="IntEquip" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="ExtEquip" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Weather" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Meter" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Results" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="DocumentHistory" minOccurs="0"/> <xsd:element ref="SimulationParameters" minOccurs="0" maxOccurs="1"/> <xsd:element ref="ZoneHVACEquipment" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Occupants"/> <xsd:element ref="Behaviors"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID"/> <xsd:attribute name="engine"> <xsd:annotation> <xsd:documentation>Analysis engine used</xsd:documentation> </xsd:annotation> <xsd:simpleType> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="DOE2.1e"/> <xsd:enumeration value="DOE2.2"/> <xsd:enumeration value="EnergyPlus"/> </xsd:restriction> </xsd:simpleType> </xsd:attribute> <xsd:attribute name="temperatureUnit" type="temperatureUnitEnum" use="required"> <xsd:annotation> <xsd:documentation>This attribute specifies the default temperature unit for the entire gbXML document, wherever the temperatureUnit simple type is used.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="lengthUnit" type="lengthUnitEnum" use="required"> <xsd:annotation> <xsd:documentation>This attribute specifies the default length unit for the entire gbXML document, wherever the lengthUnit simple type is used.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="areaUnit" type="areaUnitEnum" use="required"> <xsd:annotation> <xsd:documentation>This attribute specifies the default area unit for the entire gbXML document, wherever the areaUnit simple type is used.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="volumeUnit" type="volumeUnitEnum" use="required"> <xsd:annotation> <xsd:documentation>This attribute specifies the default volume unit for the entire gbXML document, wherever the volumeUnit simple type is used.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="useSIUnitsForResults" type="xsd:boolean" use="required"> <xsd:annotation> <xsd:documentation>Results will be given in SI or IP units. True = SI units which is the implied default. If False, results will be in english units.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="version" type="versionEnum" use="required"/> <xsd:attribute name="SurfaceReferenceLocation" type="surfaceReferenceLocationEnum" use="optional"> <xsd:annotation> <xsd:documentation>Use this attribute to determine what type of geometry information is included in the geometry elements. This is specified using an enumeration that includes shell/wall paper and centerline coordinates.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute gbXML/@id

type | xsd:ID
source | <xsd:attribute name="id" type="xsd:ID"/>

attribute gbXML/@engine

type | restriction of xsd:NMTOKEN
facets |
Kind | Value | Annotation
enumeration | DOE2.1e |
enumeration | DOE2.2 |
enumeration | EnergyPlus |
annotation |
documentation
Analysis engine used
source | <xsd:attribute name="engine"> <xsd:annotation> <xsd:documentation>Analysis engine used</xsd:documentation> </xsd:annotation> <xsd:simpleType> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="DOE2.1e"/> <xsd:enumeration value="DOE2.2"/> <xsd:enumeration value="EnergyPlus"/> </xsd:restriction> </xsd:simpleType> </xsd:attribute>

attribute gbXML/@temperatureUnit

type | temperatureUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | F |
enumeration | C |
enumeration | K |
enumeration | R |
annotation |
documentation
This attribute specifies the default temperature unit for the entire gbXML document, wherever the temperatureUnit simple type is used.
source | <xsd:attribute name="temperatureUnit" type="temperatureUnitEnum" use="required"> <xsd:annotation> <xsd:documentation>This attribute specifies the default temperature unit for the entire gbXML document, wherever the temperatureUnit simple type is used.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute gbXML/@lengthUnit

type | lengthUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Kilometers |
enumeration | Meters |
enumeration | Centimeters |
enumeration | Millimeters |
enumeration | Miles |
enumeration | Yards |
enumeration | Feet |
enumeration | Inches |
annotation |
documentation
This attribute specifies the default length unit for the entire gbXML document, wherever the lengthUnit simple type is used.
source | <xsd:attribute name="lengthUnit" type="lengthUnitEnum" use="required"> <xsd:annotation> <xsd:documentation>This attribute specifies the default length unit for the entire gbXML document, wherever the lengthUnit simple type is used.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute gbXML/@areaUnit

type | areaUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | SquareKilometers |
enumeration | SquareMeters |
enumeration | SquareCentimeters |
enumeration | SquareMillimeters |
enumeration | SquareMiles |
enumeration | SquareYards |
enumeration | SquareFeet |
enumeration | SquareInches |
annotation |
documentation
This attribute specifies the default area unit for the entire gbXML document, wherever the areaUnit simple type is used.
source | <xsd:attribute name="areaUnit" type="areaUnitEnum" use="required"> <xsd:annotation> <xsd:documentation>This attribute specifies the default area unit for the entire gbXML document, wherever the areaUnit simple type is used.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute gbXML/@volumeUnit

type | volumeUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | CubicKilometers |
enumeration | CubicMeters |
enumeration | CubicCentimeters |
enumeration | CubicMillimeters |
enumeration | CubicMiles |
enumeration | CubicYards |
enumeration | CubicFeet |
enumeration | CubicInches |
annotation |
documentation
This attribute specifies the default volume unit for the entire gbXML document, wherever the volumeUnit simple type is used.
source | <xsd:attribute name="volumeUnit" type="volumeUnitEnum" use="required"> <xsd:annotation> <xsd:documentation>This attribute specifies the default volume unit for the entire gbXML document, wherever the volumeUnit simple type is used.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute gbXML/@useSIUnitsForResults

type | xsd:boolean
properties |
use | required
annotation |
documentation
Results will be given in SI or IP units. True = SI units which is the implied default. If False, results will be in english units.
source | <xsd:attribute name="useSIUnitsForResults" type="xsd:boolean" use="required"> <xsd:annotation> <xsd:documentation>Results will be given in SI or IP units. True = SI units which is the implied default. If False, results will be in english units.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute gbXML/@version

type | versionEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | 0.35 |
enumeration | 0.36 |
enumeration | 0.37 |
enumeration | 5.00 |
enumeration | 5.01 |
enumeration | 5.10 |
enumeration | 5.11 |
enumeration | 5.12 |
enumeration | 6.00 |
enumeration | 6.01 |
source | <xsd:attribute name="version" type="versionEnum" use="required"/>

attribute gbXML/@SurfaceReferenceLocation

type | surfaceReferenceLocationEnum
properties |
use | optional
facets |
Kind | Value | Annotation
enumeration | Centerline |
enumeration | InteriorSurface |
annotation |
documentation
Use this attribute to determine what type of geometry information is included in the geometry elements. This is specified using an enumeration that includes shell/wall paper and centerline coordinates.
source | <xsd:attribute name="SurfaceReferenceLocation" type="surfaceReferenceLocationEnum" use="optional"> <xsd:annotation> <xsd:documentation>Use this attribute to determine what type of geometry information is included in the geometry elements. This is specified using an enumeration that includes shell/wall paper and centerline coordinates.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Gender

diagram |
namespace | http://www.gbxml.org/schema
type | GenderType
properties |
content | simple
used by |
element | SocioEconomic
facets |
Kind | Value | Annotation
enumeration | Male |
enumeration | Female |
source | <xsd:element name="Gender" type="GenderType"/>

element GeneralGeometry

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
elements | AirLoopEquipment ExtEquip HydronicLoopEquipment IntEquip Lighting LightingControl LightingSystem Transportation Vegetation
annotation |
documentation
This element has been left open for use with other geometry definitions, such as X3D or BLISXML.
source | <xsd:element name="GeneralGeometry"> <xsd:annotation> <xsd:documentation>This element has been left open for use with other geometry definitions, such as X3D or BLISXML.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:any namespace="##other" processContents="lax" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> </xsd:complexType> </xsd:element>

element GeographicLocation

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Country ClimateZone CommuteMode Policy Infrastructure Cost
used by |
element | Occupant
annotation |
documentation
A specific location can be assigned to each occupant.
source | <xsd:element name="GeographicLocation"> <xsd:annotation> <xsd:documentation>A specific location can be assigned to each occupant.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:sequence> <xsd:element ref="Country"/> <xsd:element ref="ClimateZone"/> <xsd:element ref="CommuteMode"/> <xsd:element ref="Policy"/> <xsd:element ref="Infrastructure"/> <xsd:element ref="Cost"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element Glare

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | ShadeControl
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | unitlessUnitEnum |  |  |  |
annotation |
documentation
Minimum amount of glare to trigger the shades to close
source | <xsd:element name="Glare"> <xsd:annotation> <xsd:documentation>Minimum amount of glare to trigger the shades to close</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Glare/@unit

type | unitlessUnitEnum
facets |
Kind | Value | Annotation
enumeration | Percent |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="unitlessUnitEnum"/>

element Glaze

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Transmittance Reflectance Emittance Thickness Conductivity Reference
used by |
element | WindowType
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
DOELibIdRef | xsd:string |  |  |  |
documentation
Use this attribute to reference objects in the DOE2 library
annotation |
documentation
Properties of one layer of a window
source | <xsd:element name="Glaze"> <xsd:annotation> <xsd:documentation>Properties of one layer of a window</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Transmittance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Reflectance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Emittance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Thickness" minOccurs="0"/> <xsd:element ref="Conductivity" minOccurs="0"/> <xsd:element ref="Reference" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Glaze/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Glaze/@DOELibIdRef

type | xsd:string
annotation |
documentation
Use this attribute to reference objects in the DOE2 library
source | <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute>

element GlazeConductivity

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Opening
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | conductivityUnitEnum | required |  |  |
source | <xsd:element name="GlazeConductivity"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="conductivityUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute GlazeConductivity/@unit

type | conductivityUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | WPerCmC |
enumeration | WPerMeterK |
enumeration | BtuPerHourFtF |
source | <xsd:attribute name="unit" type="conductivityUnitEnum" use="required"/>

element GlazeId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
attributes |
Name | Type | Use | Default | Fixed | Annotation
glazeIdRef | xsd:IDREF | required |  |  |
documentation
ID indicating the type of glaze used
source | <xsd:element name="GlazeId"> <xsd:complexType> <xsd:attribute name="glazeIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID indicating the type of glaze used</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute GlazeId/@glazeIdRef

type | xsd:IDREF
properties |
use | required
annotation |
documentation
ID indicating the type of glaze used
source | <xsd:attribute name="glazeIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID indicating the type of glaze used</xsd:documentation> </xsd:annotation> </xsd:attribute>

element GroundTemp

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | temperatureUnitEnum |  |  |  |
annotation |
documentation
Monthly ground temperatures, 12 values
source | <xsd:element name="GroundTemp"> <xsd:annotation> <xsd:documentation>Monthly ground temperatures, 12 values</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute GroundTemp/@unit

type | temperatureUnitEnum
facets |
Kind | Value | Annotation
enumeration | F |
enumeration | C |
enumeration | K |
enumeration | R |
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element GroundTempValue

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
source | <xsd:element name="GroundTempValue" type="xsd:decimal"/>

element GroupPriority

diagram |
namespace | http://www.gbxml.org/schema
type | GroupPriority
properties |
content | simple
used by |
element | Space
facets |
Kind | Value | Annotation
enumeration | Majority |
documentation
If 50% or higher proportion of occupants would like to take the same action, then the action is trigerred.
annotation |
documentation
A method can be defined how the decision is made if there are multiple people in the space.
source | <xsd:element name="GroupPriority" type="GroupPriority"> <xsd:annotation> <xsd:documentation>A method can be defined how the decision is made if there are multiple people in the space. </xsd:documentation> </xsd:annotation> </xsd:element>

element GUID

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:string
properties |
content | complex
used by |
element | ProjectEntity
attributes |
Name | Type | Use | Default | Fixed | Annotation
entity | entityTypeEnum | required |  |  |
source | <xsd:element name="GUID"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:string"> <xsd:attribute name="entity" type="entityTypeEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute GUID/@entity

type | entityTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | File |
enumeration | Model |
enumeration | Project |
enumeration | Run |
source | <xsd:attribute name="entity" type="entityTypeEnum" use="required"/>

element HDD

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Temperature HDDValue
used by |
element | Weather
annotation |
documentation
Heating degree days. HDD is calculated as the number of degrees a mean daily temperature is below a value (specified as the Temperature element), for each day. For example, if the mean temperature in a region drops to 64 degrees for four days during a year, the rest of the time staying above 65, and the Temperature element is set at 65, then HDD = 4.
source | <xsd:element name="HDD"> <xsd:annotation> <xsd:documentation>Heating degree days. HDD is calculated as the number of degrees a mean daily temperature is below a value (specified as the Temperature element), for each day. For example, if the mean temperature in a region drops to 64 degrees for four days during a year, the rest of the time staying above 65, and the Temperature element is set at 65, then HDD = 4.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Temperature"/> <xsd:element ref="HDDValue"/> </xsd:choice> </xsd:complexType> </xsd:element>

element HDDValue

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | HDD
source | <xsd:element name="HDDValue" type="xsd:decimal"/>

element HeatExchanger

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | AirSystem
attributes |
Name | Type | Use | Default | Fixed | Annotation
heatExchangerType | heatExchangerTypeEnum | required |  |  |
id | xsd:ID | required |  |  |
source | <xsd:element name="HeatExchanger"> <xsd:complexType> <xsd:attribute name="heatExchangerType" type="heatExchangerTypeEnum" use="required"/> <xsd:attribute name="id" type="xsd:ID" use="required"/> </xsd:complexType> </xsd:element>

attribute HeatExchanger/@heatExchangerType

type | heatExchangerTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Enthalpy |
enumeration | Sensible |
source | <xsd:attribute name="heatExchangerType" type="heatExchangerTypeEnum" use="required"/>

attribute HeatExchanger/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

element HeatingCoilSetpointResetType

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | AirLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | heatingCoilSetpointResetTypeEnum |  |  |  |
source | <xsd:element name="HeatingCoilSetpointResetType"> <xsd:complexType> <xsd:attribute name="unit" type="heatingCoilSetpointResetTypeEnum"/> </xsd:complexType> </xsd:element>

attribute HeatingCoilSetpointResetType/@unit

type | heatingCoilSetpointResetTypeEnum
facets |
Kind | Value | Annotation
enumeration | None |
enumeration | OutdoorAirTemperatureReset |
source | <xsd:attribute name="unit" type="heatingCoilSetpointResetTypeEnum"/>

element HeatingSizingFactor

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Zone
source | <xsd:element name="HeatingSizingFactor" type="xsd:decimal"/>

element HeatingTemperature

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | TemperatureProbabilityModel
used by |
element | ASHRAEComfortTemperatures
annotation |
documentation
A distribution of comfort heating temperature can be given where occupants and therefore, they don't carry out any actions.
source | <xsd:element name="HeatingTemperature"> <xsd:annotation> <xsd:documentation>A distribution of comfort heating temperature can be given where occupants and therefore, they don't carry out any actions. </xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice> <xsd:element ref="TemperatureProbabilityModel" minOccurs="0"/> </xsd:choice> </xsd:complexType> </xsd:element>

element HeatPumpDefrostControl

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | AirLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
defrostControlType | defrostControlEnum | required |  |  |
source | <xsd:element name="HeatPumpDefrostControl"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="defrostControlType" type="defrostControlEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute HeatPumpDefrostControl/@defrostControlType

type | defrostControlEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Timed |
enumeration | OnDemand |
source | <xsd:attribute name="defrostControlType" type="defrostControlEnum" use="required"/>

element HeatPumpDefrostStrategy

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | AirLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | defrostStrategyEnum |  |  |  |
source | <xsd:element name="HeatPumpDefrostStrategy"> <xsd:complexType> <xsd:attribute name="unit" type="defrostStrategyEnum"/> </xsd:complexType> </xsd:element>

attribute HeatPumpDefrostStrategy/@unit

type | defrostStrategyEnum
facets |
Kind | Value | Annotation
enumeration | ReverseCycle |
enumeration | Resistive |
source | <xsd:attribute name="unit" type="defrostStrategyEnum"/>

element HeatPumpFanDelayTime

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | AirLoopEquipment
annotation |
documentation
Heat pump fan delay time (s)
source | <xsd:element name="HeatPumpFanDelayTime" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Heat pump fan delay time (s)</xsd:documentation> </xsd:annotation> </xsd:element>

element HeatPumpTimeConstant

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | AirLoopEquipment
annotation |
documentation
Heat pump time constant (s)
source | <xsd:element name="HeatPumpTimeConstant" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Heat pump time constant (s)</xsd:documentation> </xsd:annotation> </xsd:element>

element HeatRecoveryType

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | AirLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | heatRecoveryTypeEnum |  |  |  |
source | <xsd:element name="HeatRecoveryType"> <xsd:complexType> <xsd:attribute name="unit" type="heatRecoveryTypeEnum"/> </xsd:complexType> </xsd:element>

attribute HeatRecoveryType/@unit

type | heatRecoveryTypeEnum
facets |
Kind | Value | Annotation
enumeration | None |
enumeration | Sensible |
enumeration | Enthalpy |
source | <xsd:attribute name="unit" type="heatRecoveryTypeEnum"/>

element HeatRejectedtoSpace

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | IntEquip
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | unitlessUnitEnum | required |  |  |
annotation |
documentation
The amount of heat from this equipment rejected to this space. For condensors exterior to building, this value will be 0.
source | <xsd:element name="HeatRejectedtoSpace"> <xsd:annotation> <xsd:documentation>The amount of heat from this equipment rejected to this space. For condensors exterior to building, this value will be 0.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute HeatRejectedtoSpace/@unit

type | unitlessUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Percent |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element Height

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Dimensions RectangularGeometry
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | lengthUnitEnum |  |  |  |
source | <xsd:element name="Height"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="lengthUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Height/@unit

type | lengthUnitEnum
facets |
Kind | Value | Annotation
enumeration | Kilometers |
enumeration | Meters |
enumeration | Centimeters |
enumeration | Millimeters |
enumeration | Miles |
enumeration | Yards |
enumeration | Feet |
enumeration | Inches |
source | <xsd:attribute name="unit" type="lengthUnitEnum"/>

element HighLimit

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | IndoorAirQuality
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | unitlessSmallUnitEnum | required |  |  |
source | <xsd:element name="HighLimit"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessSmallUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute HighLimit/@unit

type | unitlessSmallUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Percent |
enumeration | PartPerMillionByVolume |
enumeration | milliGramsPerCubicMeter |
source | <xsd:attribute name="unit" type="unitlessSmallUnitEnum" use="required"/>

element HighValue

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | conditioningUnitEnum | required |  |  |
source | <xsd:element name="HighValue"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="conditioningUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute HighValue/@unit

type | conditioningUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | kBtu |
enumeration | Btu |
enumeration | kW |
enumeration | Tons |
source | <xsd:attribute name="unit" type="conditioningUnitEnum" use="required"/>

element HolidayDate

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:date
properties |
content | simple
used by |
element | HolidaysModeled
annotation |
documentation
Date of holiday modeled
source | <xsd:element name="HolidayDate" type="xsd:date"> <xsd:annotation> <xsd:documentation>Date of holiday modeled</xsd:documentation> </xsd:annotation> </xsd:element>

element HolidaysModeled

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description HolidayDate
used by |
elements | OccupantBehavior YearModeled
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
source | <xsd:element name="HolidaysModeled"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> <xsd:complexType> <xsd:all> <xsd:element ref="Name" minOccurs="1"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="HolidayDate" minOccurs="1"/> </xsd:all> <xsd:attribute name="id" type="xsd:ID" use="required"/> </xsd:complexType> </xsd:element>

attribute HolidaysModeled/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

element HorizontalSolar

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | ShadeControl
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | powerPerAreaUnitEnum | required |  |  |
annotation |
documentation
Amount of horizontal solar radiation striking the opening before a shade is closed.
source | <xsd:element name="HorizontalSolar"> <xsd:annotation> <xsd:documentation>Amount of horizontal solar radiation striking the opening before a shade is closed.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="powerPerAreaUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute HorizontalSolar/@unit

type | powerPerAreaUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | WattPerSquareMeter |
enumeration | WattPerSquareFoot |
source | <xsd:attribute name="unit" type="powerPerAreaUnitEnum" use="required"/>

element HOutside

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:float
properties |
content | complex
used by |
elements | Layer RTSParameters
attributes |
Name | Type | Use | Default | Fixed | Annotation
hOutsideUnitTypeEnum | hOutsideUnitTypeEnum |  |  |  |
documentation
Used by the hOutsideUnitType attribute.
annotation |
documentation
h (Outside) is the combined coefficient of heat transfer by long-wave radiation and convection at outer surface, Btu/h-sf-F. See 2001 HoF Chapter 25 Table 1.
source | <xsd:element name="HOutside"> <xsd:annotation> <xsd:documentation>h (Outside) is the combined coefficient of heat transfer by long-wave radiation and convection at outer surface, Btu/h-sf-F. See 2001 HoF Chapter 25 Table 1.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:float"> <xsd:attribute name="hOutsideUnitTypeEnum" type="hOutsideUnitTypeEnum"> <xsd:annotation> <xsd:documentation>Used by the hOutsideUnitType attribute.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute HOutside/@hOutsideUnitTypeEnum

type | hOutsideUnitTypeEnum
facets |
Kind | Value | Annotation
enumeration | BTUPerHourSquareFootDegreeF |
enumeration | WattsPerSecondSquareMeterDegreeC |
annotation |
documentation
Used by the hOutsideUnitType attribute.
source | <xsd:attribute name="hOutsideUnitTypeEnum" type="hOutsideUnitTypeEnum"> <xsd:annotation> <xsd:documentation>Used by the hOutsideUnitType attribute.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element HVAC

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | HVACType
used by |
element | BuildingSystems
source | <xsd:element name="HVAC"> <xsd:complexType> <xsd:sequence> <xsd:element ref="HVACType"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element HVACType

diagram |
namespace | http://www.gbxml.org/schema
type | HVACTypeEnum
properties |
content | simple
used by |
element | HVAC
facets |
Kind | Value | Annotation
enumeration | ZoneOnOff |
source | <xsd:element name="HVACType" type="HVACTypeEnum"/>

element HydronicLoop

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Cost Reference HydronicLoopEquipment FlowControl TemperatureControl DesignCoolT CADObjectId HydronicLoopId AnalysisParameter
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | Annotation
loopType | loopTypeEnum | required |  |  |
controlZoneIdRef | xsd:IDREF |  |  |  |
primaryLoopId | xsd:IDREF |  |  |  |
fluidType | fluidTypeEnum | required |  |  |
chillerType | chillerTypeEnum | optional |  |  |
id | xsd:ID | required |  |  |
documentation
Only use this attribute for secondary loops to reference the primary loop.
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
annotation |
documentation
The HydronicLoop element represents the equipment serving one path of water, or other liquid
source | <xsd:element name="HydronicLoop"> <xsd:annotation> <xsd:documentation>The HydronicLoop element represents the equipment serving one path of water, or other liquid</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Cost" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Reference" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="HydronicLoopEquipment" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="FlowControl" minOccurs="0"/> <xsd:element ref="TemperatureControl" minOccurs="0"/> <xsd:element ref="DesignCoolT" minOccurs="0"/> <xsd:element ref="CADObjectId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="HydronicLoopId" minOccurs="0" maxOccurs="unbounded"> <xsd:annotation> <xsd:documentation>This child element is used by Revit Systems Analysis.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="AnalysisParameter" minOccurs="0" maxOccurs="unbounded"> <xsd:annotation> <xsd:documentation>This child element is used by Revit Systems Analysis.</xsd:documentation> </xsd:annotation> </xsd:element> </xsd:choice> <xsd:attribute name="loopType" type="loopTypeEnum" use="required"/> <xsd:attribute name="controlZoneIdRef" type="xsd:IDREF"/> <xsd:attribute name="primaryLoopId" type="xsd:IDREF"/> <xsd:attribute name="fluidType" type="fluidTypeEnum" use="required"/> <xsd:attribute name="chillerType" type="chillerTypeEnum" use="optional"/> <xsd:attribute name="id" type="xsd:ID" use="required"> <xsd:annotation> <xsd:documentation>Only use this attribute for secondary loops to reference the primary loop.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute HydronicLoop/@loopType

type | loopTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | PrimaryChilledWater |
enumeration | SecondaryChilledWater |
enumeration | HotWater |
enumeration | CondenserWater |
enumeration | DomesticHotWater |
enumeration | WaterLoopHeatPump |
enumeration | TwoPipe |
enumeration | PotableWaterLoop |
enumeration | VRFLoop |
source | <xsd:attribute name="loopType" type="loopTypeEnum" use="required"/>

attribute HydronicLoop/@controlZoneIdRef

type | xsd:IDREF
source | <xsd:attribute name="controlZoneIdRef" type="xsd:IDREF"/>

attribute HydronicLoop/@primaryLoopId

type | xsd:IDREF
source | <xsd:attribute name="primaryLoopId" type="xsd:IDREF"/>

attribute HydronicLoop/@fluidType

type | fluidTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Water |
enumeration | Brine |
enumeration | Glycol |
enumeration | Refrigerant |
source | <xsd:attribute name="fluidType" type="fluidTypeEnum" use="required"/>

attribute HydronicLoop/@chillerType

type | chillerTypeEnum
properties |
use | optional
facets |
Kind | Value | Annotation
enumeration | AirCooled |
enumeration | WaterCooled |
source | <xsd:attribute name="chillerType" type="chillerTypeEnum" use="optional"/>

attribute HydronicLoop/@id

type | xsd:ID
properties |
use | required
annotation |
documentation
Only use this attribute for secondary loops to reference the primary loop.
source | <xsd:attribute name="id" type="xsd:ID" use="required"> <xsd:annotation> <xsd:documentation>Only use this attribute for secondary loops to reference the primary loop.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute HydronicLoop/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element HydronicLoopEquipment

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Manufacturer Model OperationSchedule Temp ResetTemperature HydronicLoopId RatedFlow MinFlow DeltaT DeltaP Power Capacity Efficiency Control Performance Cost Weight Life RefrigerantType Energy Age Reference CADObjectId GeneralGeometry ShellGeometry
used by |
element | HydronicLoop
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
equipmentType | hydronicEquipTypeEnum | required |  |  |
waterMeterIdRef | xsd:IDREF |  |  |  |
waterScheduleIdRef | xsd:IDREF |  |  |  |
primaryLoopId | xsd:IDREF |  |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
annotation |
documentation
A piece of equipment serving a hydronic loop (most commonly a water loop). This is generalized to be able to contain any type of hydronic loop equipment.
source | <xsd:element name="HydronicLoopEquipment"> <xsd:annotation> <xsd:documentation>A piece of equipment serving a hydronic loop (most commonly a water loop). This is generalized to be able to contain any type of hydronic loop equipment.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Manufacturer" minOccurs="0"/> <xsd:element ref="Model" minOccurs="0"/> <xsd:element ref="OperationSchedule" minOccurs="0"/> <xsd:element ref="Temp" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="ResetTemperature" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="HydronicLoopId" minOccurs="0" maxOccurs="unbounded"> <xsd:annotation> <xsd:documentation>Use this element to point to another loop. For instance if this is a chiller and is a child of a chilled water loop, use this element to point at a cooling water loop.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="RatedFlow" minOccurs="0" maxOccurs="2"/> <xsd:element ref="MinFlow" minOccurs="0" maxOccurs="2"/> <xsd:element ref="DeltaT" minOccurs="0" maxOccurs="2"/> <xsd:element ref="DeltaP" minOccurs="0" maxOccurs="2"/> <xsd:element ref="Power" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Capacity" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Efficiency" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Control" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Performance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Cost" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Weight" minOccurs="0"/> <xsd:element ref="Life" minOccurs="0"/> <xsd:element ref="RefrigerantType" minOccurs="0"/> <xsd:element ref="Energy" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Age" minOccurs="0"/> <xsd:element ref="Reference" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="CADObjectId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="GeneralGeometry" minOccurs="0"/> <xsd:element ref="ShellGeometry" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="equipmentType" type="hydronicEquipTypeEnum" use="required"/> <xsd:attribute name="waterMeterIdRef" type="xsd:IDREF"/> <xsd:attribute name="waterScheduleIdRef" type="xsd:IDREF"/> <xsd:attribute name="primaryLoopId" type="xsd:IDREF"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute HydronicLoopEquipment/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute HydronicLoopEquipment/@equipmentType

type | hydronicEquipTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Chiller |
enumeration | CoolingTower |
enumeration | Condenser |
enumeration | Boiler |
enumeration | HeatExchanger |
enumeration | Pump |
enumeration | RadiantPanel |
enumeration | HotWaterHeater |
enumeration | SolarPanels |
enumeration | Earth |
enumeration | Pipe |
enumeration | Storage |
enumeration | Coil |
enumeration | Radiator |
enumeration | TwoWayValve |
enumeration | ThreeWayValve |
source | <xsd:attribute name="equipmentType" type="hydronicEquipTypeEnum" use="required"/>

attribute HydronicLoopEquipment/@waterMeterIdRef

type | xsd:IDREF
source | <xsd:attribute name="waterMeterIdRef" type="xsd:IDREF"/>

attribute HydronicLoopEquipment/@waterScheduleIdRef

type | xsd:IDREF
source | <xsd:attribute name="waterScheduleIdRef" type="xsd:IDREF"/>

attribute HydronicLoopEquipment/@primaryLoopId

type | xsd:IDREF
source | <xsd:attribute name="primaryLoopId" type="xsd:IDREF"/>

attribute HydronicLoopEquipment/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element HydronicLoopEquipmentId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | Space
attributes |
Name | Type | Use | Default | Fixed | Annotation
hydronicLoopEquipIdRef | xsd:IDREF | required |  |  |
documentation
ID pointing at a hydronic loop equipment object
source | <xsd:element name="HydronicLoopEquipmentId"> <xsd:complexType> <xsd:attribute name="hydronicLoopEquipIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID pointing at a hydronic loop equipment object</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute HydronicLoopEquipmentId/@hydronicLoopEquipIdRef

type | xsd:IDREF
properties |
use | required
annotation |
documentation
ID pointing at a hydronic loop equipment object
source | <xsd:attribute name="hydronicLoopEquipIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID pointing at a hydronic loop equipment object</xsd:documentation> </xsd:annotation> </xsd:attribute>

element HydronicLoopId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
elements | AirLoopEquipment AirSystem HydronicLoop HydronicLoopEquipment Space Zone ZoneHVACEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
hydronicLoopIdRef | xsd:IDREF | required |  |  |
documentation
ID pointing to a hydronic loop
hydronicLoopType | loopTypeEnum | required |  |  |
documentation
Type of hydronic loop
coilType | coilTypeEnum | optional |  |  |
documentation
The type of coil for the hydronic loop.
source | <xsd:element name="HydronicLoopId"> <xsd:complexType> <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID pointing to a hydronic loop </xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="hydronicLoopType" type="loopTypeEnum" use="required"> <xsd:annotation> <xsd:documentation>Type of hydronic loop </xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="coilType" type="coilTypeEnum" use="optional"> <xsd:annotation> <xsd:documentation>The type of coil for the hydronic loop.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute HydronicLoopId/@hydronicLoopIdRef

type | xsd:IDREF
properties |
use | required
annotation |
documentation
ID pointing to a hydronic loop
source | <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID pointing to a hydronic loop </xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute HydronicLoopId/@hydronicLoopType

type | loopTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | PrimaryChilledWater |
enumeration | SecondaryChilledWater |
enumeration | HotWater |
enumeration | CondenserWater |
enumeration | DomesticHotWater |
enumeration | WaterLoopHeatPump |
enumeration | TwoPipe |
enumeration | PotableWaterLoop |
enumeration | VRFLoop |
annotation |
documentation
Type of hydronic loop
source | <xsd:attribute name="hydronicLoopType" type="loopTypeEnum" use="required"> <xsd:annotation> <xsd:documentation>Type of hydronic loop </xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute HydronicLoopId/@coilType

type | coilTypeEnum
properties |
use | optional
facets |
Kind | Value | Annotation
enumeration | Preheat |
enumeration | Heating |
enumeration | Cooling |
annotation |
documentation
The type of coil for the hydronic loop.
source | <xsd:attribute name="coilType" type="coilTypeEnum" use="optional"> <xsd:annotation> <xsd:documentation>The type of coil for the hydronic loop.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element IAQ

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | ParameterRange
used by |
element | Physical
source | <xsd:element name="IAQ"> <xsd:complexType> <xsd:sequence> <xsd:element ref="ParameterRange" maxOccurs="unbounded"> <xsd:annotation> <xsd:documentation>Range of indoor air quality parameter values can be given where occupants do not feel IAQ discomfort and therefore, they don't carry out any actions. </xsd:documentation> </xsd:annotation> </xsd:element> </xsd:sequence> </xsd:complexType> </xsd:element>

element Illuminance

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | LightingControl
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | illuminanceUnitEnum | required |  |  |
source | <xsd:element name="Illuminance"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="illuminanceUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Illuminance/@unit

type | illuminanceUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Footcandles |
enumeration | Lux |
enumeration | Phot |
source | <xsd:attribute name="unit" type="illuminanceUnitEnum" use="required"/>

element ImageTexture

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | Material
attributes |
Name | Type | Use | Default | Fixed | Annotation
url | xsd:string | required |  |  |
documentation
Specifies location of the image. From X3D specification: The texture is read from the URL specified by the url field. When the url field contains no values, texturing is disabled. Browsers shall support the JPEG and PNG image file formats. In addition, browsers may support other image formats (e.g. CGM) which can be rendered into a 2D image. Support for the GIF format is also recommended (including transparency).
repeatS | xsd:boolean | required |  |  |
documentation
From X3D specification: If repeatS is TRUE, the texture map is repeated outside the [0.0, 1.0] texture coordinate range in the S direction so that it fills the shape. If repeatS is FALSE, the texture coordinates are clamped in the S direction to lie within the [0.0, 1.0] range.
repeatT | xsd:boolean | required |  |  |
documentation
From X3D specification: If repeatT is TRUE, the texture map is repeated outside the [0.0, 1.0] texture coordinate range in the T direction so that it fills the shape. If repeatT is FALSE, the texture coordinates are clamped in the T direction to lie within the [0.0, 1.0] range.
annotation |
documentation
This is an X3D element to map a texture to this material. From X3D specification: The ImageTexture node defines a texture map by specifying an image file and general parameters for mapping to geometry. Texture maps are defined in a 2D coordinate system (s, t) that ranges from [0.0, 1.0] in both directions. The bottom edge of the image corresponds to the S-axis of the texture map, and left edge of the image corresponds to the T-axis of the texture map. The lower-left pixel of the image corresponds to s=0, t=0, and the top-right pixel of the image corresponds to s=1, t=1. <!--When fixed: add type="x3d:ImageTexture"-->
source | <xsd:element name="ImageTexture"> <xsd:annotation> <xsd:documentation>This is an X3D element to map a texture to this material. From X3D specification: The ImageTexture node defines a texture map by specifying an image file and general parameters for mapping to geometry. Texture maps are defined in a 2D coordinate system (s, t) that ranges from [0.0, 1.0] in both directions. The bottom edge of the image corresponds to the S-axis of the texture map, and left edge of the image corresponds to the T-axis of the texture map. The lower-left pixel of the image corresponds to s=0, t=0, and the top-right pixel of the image corresponds to s=1, t=1. <!--When fixed: add type="x3d:ImageTexture"--> </xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:attribute name="url" type="xsd:string" use="required"> <xsd:annotation> <xsd:documentation>Specifies location of the image. From X3D specification: The texture is read from the URL specified by the url field. When the url field contains no values, texturing is disabled. Browsers shall support the JPEG and PNG image file formats. In addition, browsers may support other image formats (e.g. CGM) which can be rendered into a 2D image. Support for the GIF format is also recommended (including transparency). </xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="repeatS" type="xsd:boolean" use="required"> <xsd:annotation> <xsd:documentation>From X3D specification: If repeatS is TRUE, the texture map is repeated outside the [0.0, 1.0] texture coordinate range in the S direction so that it fills the shape. If repeatS is FALSE, the texture coordinates are clamped in the S direction to lie within the [0.0, 1.0] range. </xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="repeatT" type="xsd:boolean" use="required"> <xsd:annotation> <xsd:documentation>From X3D specification: If repeatT is TRUE, the texture map is repeated outside the [0.0, 1.0] texture coordinate range in the T direction so that it fills the shape. If repeatT is FALSE, the texture coordinates are clamped in the T direction to lie within the [0.0, 1.0] range. </xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute ImageTexture/@url

type | xsd:string
properties |
use | required
annotation |
documentation
Specifies location of the image. From X3D specification: The texture is read from the URL specified by the url field. When the url field contains no values, texturing is disabled. Browsers shall support the JPEG and PNG image file formats. In addition, browsers may support other image formats (e.g. CGM) which can be rendered into a 2D image. Support for the GIF format is also recommended (including transparency).
source | <xsd:attribute name="url" type="xsd:string" use="required"> <xsd:annotation> <xsd:documentation>Specifies location of the image. From X3D specification: The texture is read from the URL specified by the url field. When the url field contains no values, texturing is disabled. Browsers shall support the JPEG and PNG image file formats. In addition, browsers may support other image formats (e.g. CGM) which can be rendered into a 2D image. Support for the GIF format is also recommended (including transparency). </xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute ImageTexture/@repeatS

type | xsd:boolean
properties |
use | required
annotation |
documentation
From X3D specification: If repeatS is TRUE, the texture map is repeated outside the [0.0, 1.0] texture coordinate range in the S direction so that it fills the shape. If repeatS is FALSE, the texture coordinates are clamped in the S direction to lie within the [0.0, 1.0] range.
source | <xsd:attribute name="repeatS" type="xsd:boolean" use="required"> <xsd:annotation> <xsd:documentation>From X3D specification: If repeatS is TRUE, the texture map is repeated outside the [0.0, 1.0] texture coordinate range in the S direction so that it fills the shape. If repeatS is FALSE, the texture coordinates are clamped in the S direction to lie within the [0.0, 1.0] range. </xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute ImageTexture/@repeatT

type | xsd:boolean
properties |
use | required
annotation |
documentation
From X3D specification: If repeatT is TRUE, the texture map is repeated outside the [0.0, 1.0] texture coordinate range in the T direction so that it fills the shape. If repeatT is FALSE, the texture coordinates are clamped in the T direction to lie within the [0.0, 1.0] range.
source | <xsd:attribute name="repeatT" type="xsd:boolean" use="required"> <xsd:annotation> <xsd:documentation>From X3D specification: If repeatT is TRUE, the texture map is repeated outside the [0.0, 1.0] texture coordinate range in the T direction so that it fills the shape. If repeatT is FALSE, the texture coordinates are clamped in the T direction to lie within the [0.0, 1.0] range. </xsd:documentation> </xsd:annotation> </xsd:attribute>

element IncomeGroup

diagram |
namespace | http://www.gbxml.org/schema
type | IncomeGroupType
properties |
content | simple
used by |
element | SocioEconomic
facets |
Kind | Value | Annotation
enumeration | 30,000 USD-50,000 USD |
enumeration | 51,000 USD-60,000 USD |
enumeration | 61,000 USD-80,000 USD |
enumeration | Greater than 80,000 USD |
source | <xsd:element name="IncomeGroup" type="IncomeGroupType"/>

element IndependentValue

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Data
annotation |
documentation
Value of the independent variable for this data point
source | <xsd:element name="IndependentValue" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Value of the independent variable for this data point</xsd:documentation> </xsd:annotation> </xsd:element>

element IndependentVariable

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description
used by |
elements | Equation PointData
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | xsd:string | required |  |  |
dataType | xsd:string | required |  |  |
source | <xsd:element name="IndependentVariable"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> </xsd:choice> <xsd:attribute name="unit" type="xsd:string" use="required"/> <xsd:attribute name="dataType" type="xsd:string" use="required"/> </xsd:complexType> </xsd:element>

attribute IndependentVariable/@unit

type | xsd:string
properties |
use | required
source | <xsd:attribute name="unit" type="xsd:string" use="required"/>

attribute IndependentVariable/@dataType

type | xsd:string
properties |
use | required
source | <xsd:attribute name="dataType" type="xsd:string" use="required"/>

element IndoorAirQuality

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | EmissionRate SinkRate HighLimit
used by |
elements | ExtEquip IntEquip Material Zone
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
scheduleIdRef | xsd:IDREF |  |  |  |
documentation
ID for the schedule of transmittance of a shading surface
source | <xsd:element name="IndoorAirQuality"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="EmissionRate" minOccurs="0"/> <xsd:element ref="SinkRate" minOccurs="0"/> <xsd:element ref="HighLimit" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute IndoorAirQuality/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute IndoorAirQuality/@scheduleIdRef

type | xsd:IDREF
annotation |
documentation
ID for the schedule of transmittance of a shading surface
source | <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute>

element InfiltrationFlow

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | BlowerDoorValue Reference
used by |
elements | Building Space
attributes |
Name | Type | Use | Default | Fixed | Annotation
type | infiltrationTypeEnum |  |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
annotation |
documentation
Flow of air through building envelope
source | <xsd:element name="InfiltrationFlow"> <xsd:annotation> <xsd:documentation>Flow of air through building envelope</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="BlowerDoorValue" minOccurs="0"/> <xsd:element ref="Reference" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="type" type="infiltrationTypeEnum"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute InfiltrationFlow/@type

type | infiltrationTypeEnum
facets |
Kind | Value | Annotation
enumeration | Loose |
enumeration | Average |
enumeration | Tight |
source | <xsd:attribute name="type" type="infiltrationTypeEnum"/>

attribute InfiltrationFlow/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Infrastructure

diagram |
namespace | http://www.gbxml.org/schema
type | InfrastructureType
properties |
content | simple
used by |
element | GeographicLocation
facets |
Kind | Value | Annotation
enumeration | EV charging |
enumeration | Micro grid |
enumeration | Grid buyback |
source | <xsd:element name="Infrastructure" type="InfrastructureType"/>

element InputWatts

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | LightingSystem
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | powerUnitEnum | required |  |  |
source | <xsd:element name="InputWatts"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="powerUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute InputWatts/@unit

type | powerUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Watt |
enumeration | Kilowatt |
enumeration | Horsepower |
enumeration | KilogramForceMeterPerSecond |
enumeration | BtuPerSecond |
enumeration | FootPoundForcePerSecond |
enumeration | KilocaloriesPerSecond |
enumeration | BtuPerHour |
source | <xsd:attribute name="unit" type="powerUnitEnum" use="required"/>

element InsideAirFilmResistance

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Layer
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | resistanceUnitEnum | required |  |  |
annotation |
documentation
Thermal resistance of the internal air film in a layer
source | <xsd:element name="InsideAirFilmResistance"> <xsd:annotation> <xsd:documentation>Thermal resistance of the internal air film in a layer</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="resistanceUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute InsideAirFilmResistance/@unit

type | resistanceUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | SquareMeterKPerW |
enumeration | HrSquareFtFPerBTU |
source | <xsd:attribute name="unit" type="resistanceUnitEnum" use="required"/>

element IntEquip

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Manufacturer Model ElecLoad FuelLoad LatentLoad Efficiency Performance Cost Weight WasteWaterHREff WaterUsePerCycle RatedFlow HeatRejectedtoSpace Power CyclesPerWeek Energy GeneralGeometry ShellGeometry IndoorAirQuality Age Reference CADObjectId
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
scheduleIdRef | xsd:IDREF |  |  |  |
documentation
ID for the schedule of transmittance of a shading surface
waterTempScheduleIdRef | xsd:IDREF |  |  |  |
hydronicLoopIdRef | xsd:IDREF |  |  |  |
documentation
ID pointing to a hydronic loop
waterScheduleIdRef | xsd:IDREF |  |  |  |
waterMeterIdRef | xsd:IDREF |  |  |  |
type | intEquipTypeEnum | required |  |  |
airLoopIdRef | xsd:IDREF |  |  |  |
documentation
ID pointing to an air loop
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
annotation |
documentation
Interior equipment. This is generalized to be able to contain any type of internal equipment.
source | <xsd:element name="IntEquip"> <xsd:annotation> <xsd:documentation>Interior equipment. This is generalized to be able to contain any type of internal equipment.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Manufacturer" minOccurs="0"/> <xsd:element ref="Model" minOccurs="0"/> <xsd:element ref="ElecLoad" minOccurs="0"/> <xsd:element ref="FuelLoad" minOccurs="0"/> <xsd:element ref="LatentLoad" minOccurs="0"/> <xsd:element ref="Efficiency" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Performance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Cost" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Weight" minOccurs="0"/> <xsd:element ref="WasteWaterHREff" minOccurs="0"/> <xsd:element ref="WaterUsePerCycle" minOccurs="0"/> <xsd:element ref="RatedFlow" minOccurs="0"/> <xsd:element ref="HeatRejectedtoSpace" minOccurs="0"/> <xsd:element ref="Power" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="CyclesPerWeek" minOccurs="0"/> <xsd:element ref="Energy" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="GeneralGeometry" minOccurs="0"/> <xsd:element ref="ShellGeometry" minOccurs="0"/> <xsd:element ref="IndoorAirQuality" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Age" minOccurs="0"/> <xsd:element ref="Reference" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="CADObjectId" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="waterTempScheduleIdRef" type="xsd:IDREF"/> <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID pointing to a hydronic loop </xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="waterScheduleIdRef" type="xsd:IDREF"/> <xsd:attribute name="waterMeterIdRef" type="xsd:IDREF"/> <xsd:attribute name="type" type="intEquipTypeEnum" use="required"/> <xsd:attribute name="airLoopIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID pointing to an air loop</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute IntEquip/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute IntEquip/@scheduleIdRef

type | xsd:IDREF
annotation |
documentation
ID for the schedule of transmittance of a shading surface
source | <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute IntEquip/@waterTempScheduleIdRef

type | xsd:IDREF
source | <xsd:attribute name="waterTempScheduleIdRef" type="xsd:IDREF"/>

attribute IntEquip/@hydronicLoopIdRef

type | xsd:IDREF
annotation |
documentation
ID pointing to a hydronic loop
source | <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID pointing to a hydronic loop </xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute IntEquip/@waterScheduleIdRef

type | xsd:IDREF
source | <xsd:attribute name="waterScheduleIdRef" type="xsd:IDREF"/>

attribute IntEquip/@waterMeterIdRef

type | xsd:IDREF
source | <xsd:attribute name="waterMeterIdRef" type="xsd:IDREF"/>

attribute IntEquip/@type

type | intEquipTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | GeneralPlugload |
enumeration | Computer |
enumeration | Copier |
enumeration | Refrigerator |
enumeration | Stove |
enumeration | Cooktop |
enumeration | Fryer |
enumeration | Freezer |
enumeration | ClothesDryer |
enumeration | ClothesWasher |
enumeration | Dishwasher |
enumeration | TV |
enumeration | VCR |
enumeration | Microwave |
enumeration | Fan |
enumeration | AudioEquip |
enumeration | MiscEquip |
enumeration | Toilet |
enumeration | Urinal |
enumeration | Shower |
enumeration | Sink |
enumeration | Pool |
enumeration | HotTub |
enumeration | Sauna |
enumeration | BatteryCharger |
enumeration | Furnace |
enumeration | IndustrialEquip |
enumeration | Printer |
enumeration | Vending |
enumeration | Elevator |
enumeration | Escalator |
enumeration | GeneralLaundryEquip |
enumeration | GeneralKitchenEquip |
enumeration | GeneralMedicalEquip |
enumeration | GeneralOfficeEquip |
enumeration | GeneralEntertainmentEquip |
enumeration | GeneralRefrigerationEquip |
enumeration | GeneralFitnessEquip |
enumeration | GeneralVideoEquip |
enumeration | GeneralToilet |
source | <xsd:attribute name="type" type="intEquipTypeEnum" use="required"/>

attribute IntEquip/@airLoopIdRef

type | xsd:IDREF
annotation |
documentation
ID pointing to an air loop
source | <xsd:attribute name="airLoopIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID pointing to an air loop</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute IntEquip/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element IntEquipId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
elements | Building Space
attributes |
Name | Type | Use | Default | Fixed | Annotation
intEquipIdRef | xsd:IDREF | required |  |  |
documentation
ID pointing at an interior equipment object
source | <xsd:element name="IntEquipId"> <xsd:complexType> <xsd:attribute name="intEquipIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID pointing at an interior equipment object</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute IntEquipId/@intEquipIdRef

type | xsd:IDREF
properties |
use | required
annotation |
documentation
ID pointing at an interior equipment object
source | <xsd:attribute name="intEquipIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID pointing at an interior equipment object</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Interaction

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | InteractionType Formula ControlValue
used by |
element | Actions
annotation |
documentation
Interaction type and its probability model can be specified.
source | <xsd:element name="Interaction"> <xsd:annotation> <xsd:documentation>Interaction type and its probability model can be specified.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:all> <xsd:element ref="InteractionType"/> <xsd:element ref="Formula"/> <xsd:element ref="ControlValue" minOccurs="0"/> </xsd:all> </xsd:complexType> </xsd:element>

element InteractionType

diagram |
namespace | http://www.gbxml.org/schema
type | interactionType
properties |
content | simple
used by |
element | Interaction
facets |
Kind | Value | Annotation
enumeration | TurnOn |
documentation
Set the value of a parameter to 1.
enumeration | TurnOff |
documentation
Set the value of a parameter to 0.
enumeration | SetToControlValue |
documentation
Set the value of a parameter to a desired value when event occurs.
source | <xsd:element name="InteractionType" type="interactionType"/>

element IsSpecialBehavior

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:boolean
properties |
content | simple
default | false
used by |
element | Behavior
annotation |
documentation
Set to true when this is a special behavior. When the special behavior is triggered, other behaviors are ignored.
source | <xsd:element name="IsSpecialBehavior" type="xsd:boolean" default="false"> <xsd:annotation> <xsd:documentation>Set to true when this is a special behavior. When the special behavior is triggered, other behaviors are ignored.</xsd:documentation> </xsd:annotation> </xsd:element>

element JobType

diagram |
namespace | http://www.gbxml.org/schema
type | JobType
properties |
content | simple
used by |
element | SocioEconomic
facets |
Kind | Value | Annotation
enumeration | Regular staff |
enumeration | Researcher |
enumeration | Administrator |
enumeration | Manager |
enumeration | Contractor |
source | <xsd:element name="JobType" type="JobType"/>

element Lamp

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | LightingSystem
annotation |
documentation
Type of lamp used
source | <xsd:element name="Lamp" type="xsd:string"> <xsd:annotation> <xsd:documentation>Type of lamp used</xsd:documentation> </xsd:annotation> </xsd:element>

element LastName

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | PersonInfo
source | <xsd:element name="LastName" type="xsd:string"/>

element LatentHeatRecoveryEffectiveness

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | AirLoopEquipment
source | <xsd:element name="LatentHeatRecoveryEffectiveness" type="xsd:decimal"/>

element LatentLoad

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | ExtEquip IntEquip
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | loadUnitEnum | required |  |  |
source | <xsd:element name="LatentLoad"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="loadUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute LatentLoad/@unit

type | loadUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | BtuPerHour |
enumeration | Watt |
source | <xsd:attribute name="unit" type="loadUnitEnum" use="required"/>

element Latitude

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Location
annotation |
documentation
Degrees north of the equator, in decimal degrees. Locations south of the equator are negative.
source | <xsd:element name="Latitude" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Degrees north of the equator, in decimal degrees. Locations south of the equator are negative.</xsd:documentation> </xsd:annotation> </xsd:element>

element Layer

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Cost InsideAirFilmResistance MaterialId HOutside
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
DOELibIdRef | xsd:string |  |  |  |
documentation
Use this attribute to reference objects in the DOE2 library
annotation |
documentation
A Layer is a description of a material in a composite construction. Its id attribute is referenced in the Contstruction element's LayerId
source | <xsd:element name="Layer"> <xsd:annotation> <xsd:documentation>A Layer is a description of a material in a composite construction. Its id attribute is referenced in the Contstruction element's LayerId </xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Cost" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="InsideAirFilmResistance" minOccurs="0"/> <xsd:element ref="MaterialId" maxOccurs="1"/> <xsd:element ref="HOutside" minOccurs="0" maxOccurs="1"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Layer/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Layer/@DOELibIdRef

type | xsd:string
annotation |
documentation
Use this attribute to reference objects in the DOE2 library
source | <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute>

element LayerId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | Construction
attributes |
Name | Type | Use | Default | Fixed | Annotation
layerIdRef | xsd:IDREF | required |  |  |
documentation
ID identifying a layer in this construction. Multiple layers in Constructions are in order from outside to inside.
source | <xsd:element name="LayerId"> <xsd:complexType> <xsd:attribute name="layerIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID identifying a layer in this construction. Multiple layers in Constructions are in order from outside to inside.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute LayerId/@layerIdRef

type | xsd:IDREF
properties |
use | required
annotation |
documentation
ID identifying a layer in this construction. Multiple layers in Constructions are in order from outside to inside.
source | <xsd:attribute name="layerIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID identifying a layer in this construction. Multiple layers in Constructions are in order from outside to inside.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Length

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Dimensions
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | lengthUnitEnum |  |  |  |
source | <xsd:element name="Length"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="lengthUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Length/@unit

type | lengthUnitEnum
facets |
Kind | Value | Annotation
enumeration | Kilometers |
enumeration | Meters |
enumeration | Centimeters |
enumeration | Millimeters |
enumeration | Miles |
enumeration | Yards |
enumeration | Feet |
enumeration | Inches |
source | <xsd:attribute name="unit" type="lengthUnitEnum"/>

element Level

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | BuildingStorey
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | lengthUnitEnum |  |  |  |
annotation |
documentation
Building storey Local Placement Z coordinate.
source | <xsd:element name="Level"> <xsd:annotation> <xsd:documentation>Building storey Local Placement Z coordinate.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="lengthUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Level/@unit

type | lengthUnitEnum
facets |
Kind | Value | Annotation
enumeration | Kilometers |
enumeration | Meters |
enumeration | Centimeters |
enumeration | Millimeters |
enumeration | Miles |
enumeration | Yards |
enumeration | Feet |
enumeration | Inches |
source | <xsd:attribute name="unit" type="lengthUnitEnum"/>

element Life

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | AirLoopEquipment Campus HydronicLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | lifeUnitEnum | required |  |  |
source | <xsd:element name="Life"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="lifeUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Life/@unit

type | lifeUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Months |
enumeration | Years |
enumeration | Cycles |
enumeration | MillionCycles |
source | <xsd:attribute name="unit" type="lifeUnitEnum" use="required"/>

element LifeStyle

diagram |
namespace | http://www.gbxml.org/schema
type | LifeStyleType
properties |
content | simple
used by |
element | SocioEconomic
facets |
Kind | Value | Annotation
enumeration | Austerity |
enumeration | Luxury |
enumeration | Norm |
source | <xsd:element name="LifeStyle" type="LifeStyleType"/>

element LightControlId

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:string
properties |
content | complex
used by |
element | Campus
attributes |
Name | Type | Use | Default | Fixed | Annotation
scheduleIdRef | xsd:IDREF |  |  |  |
documentation
ID for the schedule of transmittance of a shading surface
source | <xsd:element name="LightControlId"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:string"> <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute LightControlId/@scheduleIdRef

type | xsd:IDREF
annotation |
documentation
ID for the schedule of transmittance of a shading surface
source | <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute>

element LightId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
attributes |
Name | Type | Use | Default | Fixed | Annotation
lightIdRef | xsd:IDREF | required |  |  |
documentation
Identifier pointing at a light object
source | <xsd:element name="LightId"> <xsd:complexType> <xsd:attribute name="lightIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>Identifier pointing at a light object</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute LightId/@lightIdRef

type | xsd:IDREF
properties |
use | required
annotation |
documentation
Identifier pointing at a light object
source | <xsd:attribute name="lightIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>Identifier pointing at a light object</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Lighting

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | GeneralGeometry ShellGeometry CoefficientOfUtilization PhotometryOrientation
used by |
elements | Building Campus Space
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
lightingSystemIdRef | xsd:IDREF |  |  |  |
lightingControlIdRef | xsd:IDREF |  |  |  |
meterIdRef | xsd:IDREF |  |  |  |
documentation
ID for a resource meter
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
source | <xsd:element name="Lighting"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="GeneralGeometry" minOccurs="0"/> <xsd:element ref="ShellGeometry" minOccurs="0"/> <xsd:element ref="CoefficientOfUtilization" minOccurs="0"/> <xsd:element ref="PhotometryOrientation" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="lightingSystemIdRef" type="xsd:IDREF"/> <xsd:attribute name="lightingControlIdRef" type="xsd:IDREF"/> <xsd:attribute name="meterIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for a resource meter</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Lighting/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Lighting/@lightingSystemIdRef

type | xsd:IDREF
source | <xsd:attribute name="lightingSystemIdRef" type="xsd:IDREF"/>

attribute Lighting/@lightingControlIdRef

type | xsd:IDREF
source | <xsd:attribute name="lightingControlIdRef" type="xsd:IDREF"/>

attribute Lighting/@meterIdRef

type | xsd:IDREF
annotation |
documentation
ID for a resource meter
source | <xsd:attribute name="meterIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for a resource meter</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Lighting/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element LightingControl

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | GeneralGeometry ShellGeometry Illuminance CartesianPoint MinPowerFrac MinLightFrac PercentAreaDaylitControlled
used by |
elements | gbXML Space
attributes |
Name | Type | Use | Default | Fixed | Annotation
type | lightControlTypeEnum | required |  |  |
id | xsd:ID | required |  |  |
lightingSystemIdRef | xsd:IDREF |  |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
source | <xsd:element name="LightingControl"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="GeneralGeometry" minOccurs="0"/> <xsd:element ref="ShellGeometry" minOccurs="0"/> <xsd:element ref="Illuminance" minOccurs="0"> <xsd:annotation> <xsd:documentation>Illuminance level that the lights are maintained if daylighting controls present (lightControlTypeEnum not equal to on off).</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="CartesianPoint" minOccurs="0"> <xsd:annotation> <xsd:documentation>Location where Illuminance value is specified.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="MinPowerFrac" minOccurs="0"/> <xsd:element ref="MinLightFrac" minOccurs="0"/> <xsd:element ref="PercentAreaDaylitControlled" minOccurs="0"/> </xsd:choice> <xsd:attribute name="type" type="lightControlTypeEnum" use="required"/> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="lightingSystemIdRef" type="xsd:IDREF"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute LightingControl/@type

type | lightControlTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Continuous |
enumeration | OnOff |
enumeration | Stepped2 |
enumeration | Stepped3 |
enumeration | Stepped4 |
enumeration | Stepped5 |
enumeration | Stepped6 |
enumeration | Stepped7 |
enumeration | Stepped8 |
enumeration | Stepped9 |
enumeration | Stepped10 |
enumeration | Stepped11 |
enumeration | Stepped12 |
enumeration | Stepped13 |
enumeration | Stepped14 |
enumeration | Stepped15 |
enumeration | Stepped16 |
enumeration | Stepped17 |
enumeration | Stepped18 |
enumeration | Stepped19 |
enumeration | Stepped20 |
enumeration | ContinuousOff |
enumeration | MotionSensor |
enumeration | Photocell |
source | <xsd:attribute name="type" type="lightControlTypeEnum" use="required"/>

attribute LightingControl/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute LightingControl/@lightingSystemIdRef

type | xsd:IDREF
source | <xsd:attribute name="lightingSystemIdRef" type="xsd:IDREF"/>

attribute LightingControl/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element LightingSystem

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Manufacturer NumberOfLamps LumensPerLamp Dimensions InputWatts Ballast Lamp Luminaire Photometry CoefficientOfUtilization Cost GeneralGeometry ShellGeometry Reference
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
source | <xsd:element name="LightingSystem"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Manufacturer" minOccurs="0"/> <xsd:element ref="NumberOfLamps" minOccurs="0"/> <xsd:element ref="LumensPerLamp" minOccurs="0"/> <xsd:element ref="Dimensions" minOccurs="0"/> <xsd:element ref="InputWatts" minOccurs="0"/> <xsd:element ref="Ballast" minOccurs="0"/> <xsd:element ref="Lamp" maxOccurs="unbounded"/> <xsd:element ref="Luminaire" minOccurs="0"/> <xsd:element ref="Photometry" minOccurs="0"/> <xsd:element ref="CoefficientOfUtilization" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Cost" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="GeneralGeometry" minOccurs="0"/> <xsd:element ref="ShellGeometry" minOccurs="0"/> <xsd:element ref="Reference" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute LightingSystem/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute LightingSystem/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element LightPowerPerArea

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Space
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | powerPerAreaUnitEnum | required |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
annotation |
documentation
Amount of power used by lighting in a given area
source | <xsd:element name="LightPowerPerArea"> <xsd:annotation> <xsd:documentation>Amount of power used by lighting in a given area</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="powerPerAreaUnitEnum" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute LightPowerPerArea/@unit

type | powerPerAreaUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | WattPerSquareMeter |
enumeration | WattPerSquareFoot |
source | <xsd:attribute name="unit" type="powerPerAreaUnitEnum" use="required"/>

attribute LightPowerPerArea/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Lights

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | LightType
used by |
element | BuildingSystems
source | <xsd:element name="Lights"> <xsd:complexType> <xsd:sequence> <xsd:element ref="LightType"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element LightType

diagram |
namespace | http://www.gbxml.org/schema
type | lightTypeEnum
properties |
content | simple
used by |
element | Lights
facets |
Kind | Value | Annotation
enumeration | OnOff |
enumeration | ContinuousControl |
source | <xsd:element name="LightType" type="lightTypeEnum"/>

element Linear1D

diagram |
namespace | http://www.gbxml.org/schema
type | eqLinear1DType
properties |
content | complex
children | Description CoefficientA CoefficientB Parameter1ID
used by |
element | Formula
source | <xsd:element name="Linear1D" type="eqLinear1DType"/>

element Linear2D

diagram |
namespace | http://www.gbxml.org/schema
type | eqLinear2DType
properties |
content | complex
children | Description CoefficientA CoefficientB CoefficientC Parameter1ID Parameter2ID
used by |
element | Formula
source | <xsd:element name="Linear2D" type="eqLinear2DType"/>

element Linear3D

diagram |
namespace | http://www.gbxml.org/schema
type | eqLinear3DType
properties |
content | complex
children | Description CoefficientA CoefficientB CoefficientC CoefficientD Parameter1ID Parameter2ID Parameter3ID
used by |
element | Formula
source | <xsd:element name="Linear3D" type="eqLinear3DType"/>

element LoadCalcInputParameters

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | RTSParameters CLTDParameters ManualJ8Parameters FloorSlabHeatLossCoefficient
used by |
element | Construction
source | <xsd:element name="LoadCalcInputParameters"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="RTSParameters" minOccurs="0"/> <xsd:element ref="CLTDParameters" minOccurs="0"/> <xsd:element ref="ManualJ8Parameters" minOccurs="0"/> <xsd:element ref="FloorSlabHeatLossCoefficient" minOccurs="0"/> </xsd:choice> </xsd:complexType> </xsd:element>

element Location

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | StationId Name Description ZipcodeOrPostalCode Longitude Latitude Elevation CADModelAzimuth
used by |
elements | Campus Weather
annotation |
documentation
The Location element describes the location of the global origin for this campus. This element can be used in a general sense by using the Name and Description elements for a physical address or landmark, or Location can be made precise by specifying the Elevation, Longitude, and Latitude of the origin.
source | <xsd:element name="Location"> <xsd:annotation> <xsd:documentation>The Location element describes the location of the global origin for this campus. This element can be used in a general sense by using the Name and Description elements for a physical address or landmark, or Location can be made precise by specifying the Elevation, Longitude, and Latitude of the origin.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:all> <xsd:element ref="StationId" minOccurs="0"/> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="ZipcodeOrPostalCode" minOccurs="1"/> <xsd:element ref="Longitude" minOccurs="0"/> <xsd:element ref="Latitude" minOccurs="0"/> <xsd:element ref="Elevation" minOccurs="0"/> <xsd:element ref="CADModelAzimuth" minOccurs="0"/> </xsd:all> </xsd:complexType> </xsd:element>

element Logit1D

diagram |
namespace | http://www.gbxml.org/schema
type | eqLogit1DLinearType
properties |
content | complex
children | Description CoefficientA CoefficientB Parameter1ID
used by |
element | Formula
source | <xsd:element name="Logit1D" type="eqLogit1DLinearType"/>

element Logit1DQuadratic

diagram |
namespace | http://www.gbxml.org/schema
type | eqLogit1DQuadraticType
properties |
content | complex
children | Description CoefficientA CoefficientB CoefficientC Parameter1ID
used by |
element | Formula
source | <xsd:element name="Logit1DQuadratic" type="eqLogit1DQuadraticType"/>

element Logit2D

diagram |
namespace | http://www.gbxml.org/schema
type | eqLogit2DLinearType
properties |
content | complex
children | Description CoefficientA CoefficientB CoefficientC Parameter1ID Parameter2ID
used by |
element | Formula
source | <xsd:element name="Logit2D" type="eqLogit2DLinearType"/>

element Logit3D

diagram |
namespace | http://www.gbxml.org/schema
type | eqLogit3DLinearType
properties |
content | complex
children | Description CoefficientA CoefficientB CoefficientC CoefficientD Parameter1ID Parameter2ID Parameter3ID
used by |
element | Formula
source | <xsd:element name="Logit3D" type="eqLogit3DLinearType"/>

element Longitude

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Location
annotation |
documentation
Degrees east of Greenwich, in decimal degrees. Locations west of Greenwich are negative.
source | <xsd:element name="Longitude" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Degrees east of Greenwich, in decimal degrees. Locations west of Greenwich are negative.</xsd:documentation> </xsd:annotation> </xsd:element>

element LowerBound

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
complexType | eqGaussianNormal1DType
source | <xsd:element name="LowerBound" type="xsd:decimal"/>

element LowerLimitValue

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | ScheduleTypeLimits
source | <xsd:element name="LowerLimitValue" type="xsd:decimal"/>

element LowValue

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | conditioningUnitEnum | required |  |  |
source | <xsd:element name="LowValue"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="conditioningUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute LowValue/@unit

type | conditioningUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | kBtu |
enumeration | Btu |
enumeration | kW |
enumeration | Tons |
source | <xsd:attribute name="unit" type="conditioningUnitEnum" use="required"/>

element LumensPerLamp

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | LightingSystem
source | <xsd:element name="LumensPerLamp" type="xsd:decimal"/>

element Luminaire

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | LightingSystem
annotation |
documentation
Type of luminaire used
source | <xsd:element name="Luminaire" type="xsd:string"> <xsd:annotation> <xsd:documentation>Type of luminaire used</xsd:documentation> </xsd:annotation> </xsd:element>

element ManualJ8Parameters

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | LoadCalcInputParameters
attributes |
Name | Type | Use | Default | Fixed | Annotation
wallGroupManualJ | wallGroupManualJEnum |  |  |  |
documentation
Specifies the group code for the wall, which determines how quickly the wall delivers heat into the space. See Table 4C, page T4C-1 ACCA Manual J Eighth Edition.
roofCLTDIndex | roofCLTDIndexEnum |  |  |  |
documentation
Specifies the array of CLTD values to use for the roof, which determines how quickly the roof delivers heat into the space. See Table 4A page T4A-18 and following, ACCA Manual J Eighth Edition.
floorIsRadiant | xsd:boolean |  |  |  |
documentation
Specifies whether or not to use a higher heating temperature difference value in calculating the heating loss for a floor (25 degrees F higher value is used in formula if floor is radiant). See Figure A5-5, page A5-8, ACCA Manual J Eighth Edition.
floorCrawlSpaceWallUValue | xsd:float |  |  |  |
documentation
Specifies the u-value of the crawl space wall that is associated with the floor, which affects both the heating and cooling load. See Figure A5-5, page A5-8, and Figure A5-17, page A5-16, ACCA Manual J Eighth Edition.
floorCrawlSpaceIsSealed | xsd:boolean |  |  |  |
documentation
Specifies whether or not the crawl space wall associated with this floor is well sealed from the outdoor air, which affects both the heating and cooling loads. See Figure A5-5, page A5-8, and Figure A5-17 page A5-16, ACCA Manual J Eighth Edition.
floorCategory | floorCategoryEnum |  |  |  |
documentation
Specifies the type of floor being considered, which affects both the heating and the cooling loads. See Table 4A, pages T4A-27 and following, ACCA Manual J Eighth Edition.
annotation |
documentation
Parameters required by the ACCA Manual J Eighth Edition load calculation method. Ignore this element and all elements under it if you are not planning to use that method.
source | <xsd:element name="ManualJ8Parameters"> <xsd:annotation> <xsd:documentation>Parameters required by the ACCA Manual J Eighth Edition load calculation method. Ignore this element and all elements under it if you are not planning to use that method.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:attribute name="wallGroupManualJ" type="wallGroupManualJEnum"> <xsd:annotation> <xsd:documentation>Specifies the group code for the wall, which determines how quickly the wall delivers heat into the space. See Table 4C, page T4C-1 ACCA Manual J Eighth Edition.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="roofCLTDIndex" type="roofCLTDIndexEnum"> <xsd:annotation> <xsd:documentation>Specifies the array of CLTD values to use for the roof, which determines how quickly the roof delivers heat into the space. See Table 4A page T4A-18 and following, ACCA Manual J Eighth Edition.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="floorIsRadiant" type="xsd:boolean"> <xsd:annotation> <xsd:documentation>Specifies whether or not to use a higher heating temperature difference value in calculating the heating loss for a floor (25 degrees F higher value is used in formula if floor is radiant). See Figure A5-5, page A5-8, ACCA Manual J Eighth Edition.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="floorCrawlSpaceWallUValue" type="xsd:float"> <xsd:annotation> <xsd:documentation>Specifies the u-value of the crawl space wall that is associated with the floor, which affects both the heating and cooling load. See Figure A5-5, page A5-8, and Figure A5-17, page A5-16, ACCA Manual J Eighth Edition.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="floorCrawlSpaceIsSealed" type="xsd:boolean"> <xsd:annotation> <xsd:documentation>Specifies whether or not the crawl space wall associated with this floor is well sealed from the outdoor air, which affects both the heating and cooling loads. See Figure A5-5, page A5-8, and Figure A5-17 page A5-16, ACCA Manual J Eighth Edition.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="floorCategory" type="floorCategoryEnum"> <xsd:annotation> <xsd:documentation>Specifies the type of floor being considered, which affects both the heating and the cooling loads. See Table 4A, pages T4A-27 and following, ACCA Manual J Eighth Edition.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute ManualJ8Parameters/@wallGroupManualJ

type | wallGroupManualJEnum
facets |
Kind | Value | Annotation
enumeration | A |
documentation
Fastest heat transfer
enumeration | B |
enumeration | C |
enumeration | D |
enumeration | E |
enumeration | F |
documentation
Medium heat transfer
enumeration | G |
enumeration | H |
enumeration | I |
enumeration | J |
enumeration | K |
documentation
Slowest heat transfer
annotation |
documentation
Specifies the group code for the wall, which determines how quickly the wall delivers heat into the space. See Table 4C, page T4C-1 ACCA Manual J Eighth Edition.
source | <xsd:attribute name="wallGroupManualJ" type="wallGroupManualJEnum"> <xsd:annotation> <xsd:documentation>Specifies the group code for the wall, which determines how quickly the wall delivers heat into the space. See Table 4C, page T4C-1 ACCA Manual J Eighth Edition.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute ManualJ8Parameters/@roofCLTDIndex

type | roofCLTDIndexEnum
facets |
Kind | Value | Annotation
enumeration | 1 |
documentation
Under attic or knee wall, U-value = 0.408 - 0.018, Unvented Attic, No Radiant Barrier, Any Roofing Material, Any Roof Color
enumeration | 2 |
documentation
Under attic or knee wall, U-value = 0.408 - 0.018, Vented Attic, No Radiant Barrier, Dark Asphalt Shingles or Dark Metal, Tar and Gravel or Membrane
enumeration | 3 |
documentation
Under attic or knee wall, U-value = 0.408 - 0.018, Vented Attic, No Radiant Barrier, White or Light Color Shingles, Any Wood Shake Light Metal, Tar and Gravel or Membrane
enumeration | 4 |
documentation
Under attic or knee wall, U-value = 0.408 - 0.02, Vented Attic, No Radiant Barrier, Dark Tile, Slate or Concrete
enumeration | 5 |
documentation
Under attic or knee wall, U-value = 0.408 - 0.02, Vented Attic, No Radiant Barrier, Light Tile, Slate or Concrete
enumeration | 6 |
documentation
Under attic or knee wall, U-value = 0.408 - 0.02, Vented Attic, No Radiant Barrier, White Tile, Slate or Concrete, White Metal or White Membrane
enumeration | 7 |
documentation
On exposed beams, U-value = 0.287 - 0.134, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 8 |
documentation
On exposed beams, U-value = 0.118 - 0.091, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 9 |
documentation
On exposed beams, U-value = 0.074 - 0.063, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 10 |
documentation
On exposed beams, U-value = 0.054, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 11 |
documentation
On exposed beams, U-value = 0.048, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 12 |
documentation
On exposed beams, U-value = 0.043 - 0.039, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 13 |
documentation
On exposed beams, U-value = 0.035, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 14 |
documentation
On exposed beams, U-value = 0.032 - 0.027, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 15 |
documentation
On exposed beams, U-value = 0.287 - 0.134, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 16 |
documentation
On exposed beams, U-value = 0.118 - 0.091, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 17 |
documentation
On exposed beams, U-value = 0.074 - 0.063, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 18 |
documentation
On exposed beams, U-value = 0.054, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 19 |
documentation
On exposed beams, U-value = 0.048, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 20 |
documentation
On exposed beams, U-value = 0.043 - 0.039, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 21 |
documentation
On exposed beams, U-value = 0.035, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 22 |
documentation
On exposed beams, U-value = 0.032 - 0.027, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 23 |
documentation
On exposed beams, U-value = 0.287 - 0.134, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane
enumeration | 24 |
documentation
On exposed beams, U-value = 0.118 - 0.091, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane
enumeration | 25 |
documentation
On exposed beams, U-value = 0.074 - 0.063, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane
enumeration | 26 |
documentation
On exposed beams, U-value = 0.054, White or Light Color Tile Slate or Concrete, White Metal, White Membrane
enumeration | 27 |
documentation
On exposed beams, U-value = 0.048, White or Light Color Tile Slate or Concrete, White Metal, White Membrane
enumeration | 28 |
documentation
On exposed beams, U-value = 0.043 - 0.039, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane
enumeration | 29 |
documentation
On exposed beams, U-value = 0.035, White or Light Color Tile Slate or Concrete, White Metal, White Membrane
enumeration | 30 |
documentation
On exposed beams, U-value = 0.032 - 0.027, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane
enumeration | 31 |
documentation
Below roof joists, U-value = 0.241 - 0.109, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 32 |
documentation
Below roof joists, U-value = 0.09 - 0.076, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 33 |
documentation
Below roof joists, U-value = 0.069, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 34 |
documentation
Below roof joists, U-value = 0.051 - 0.047, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 35 |
documentation
Below roof joists, U-value = 0.034, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 36 |
documentation
Below roof joists, U-value = 0.029, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 37 |
documentation
Below roof joists, U-value = 0.241 - 0.109, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 38 |
documentation
Below roof joists, U-value = 0.09 - 0.076, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 39 |
documentation
Below roof joists, U-value = 0.069, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 40 |
documentation
Below roof joists, U-value = 0.051 - 0.047, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 41 |
documentation
Below roof joists, U-value = 0.034, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 42 |
documentation
Below roof joists, U-value = 0.029, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 43 |
documentation
Below roof joists, U-value = 0.241 - 0.109, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane
enumeration | 44 |
documentation
Below roof joists, U-value = 0.09 - 0.076, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane
enumeration | 45 |
documentation
Below roof joists, U-value = 0.069, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane
enumeration | 46 |
documentation
Below roof joists, U-value = 0.051 - 0.034, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane
enumeration | 47 |
documentation
Below roof joists, U-value = 0.029, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane
annotation |
documentation
Specifies the array of CLTD values to use for the roof, which determines how quickly the roof delivers heat into the space. See Table 4A page T4A-18 and following, ACCA Manual J Eighth Edition.
source | <xsd:attribute name="roofCLTDIndex" type="roofCLTDIndexEnum"> <xsd:annotation> <xsd:documentation>Specifies the array of CLTD values to use for the roof, which determines how quickly the roof delivers heat into the space. See Table 4A page T4A-18 and following, ACCA Manual J Eighth Edition.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute ManualJ8Parameters/@floorIsRadiant

type | xsd:boolean
annotation |
documentation
Specifies whether or not to use a higher heating temperature difference value in calculating the heating loss for a floor (25 degrees F higher value is used in formula if floor is radiant). See Figure A5-5, page A5-8, ACCA Manual J Eighth Edition.
source | <xsd:attribute name="floorIsRadiant" type="xsd:boolean"> <xsd:annotation> <xsd:documentation>Specifies whether or not to use a higher heating temperature difference value in calculating the heating loss for a floor (25 degrees F higher value is used in formula if floor is radiant). See Figure A5-5, page A5-8, ACCA Manual J Eighth Edition.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute ManualJ8Parameters/@floorCrawlSpaceWallUValue

type | xsd:float
annotation |
documentation
Specifies the u-value of the crawl space wall that is associated with the floor, which affects both the heating and cooling load. See Figure A5-5, page A5-8, and Figure A5-17, page A5-16, ACCA Manual J Eighth Edition.
source | <xsd:attribute name="floorCrawlSpaceWallUValue" type="xsd:float"> <xsd:annotation> <xsd:documentation>Specifies the u-value of the crawl space wall that is associated with the floor, which affects both the heating and cooling load. See Figure A5-5, page A5-8, and Figure A5-17, page A5-16, ACCA Manual J Eighth Edition.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute ManualJ8Parameters/@floorCrawlSpaceIsSealed

type | xsd:boolean
annotation |
documentation
Specifies whether or not the crawl space wall associated with this floor is well sealed from the outdoor air, which affects both the heating and cooling loads. See Figure A5-5, page A5-8, and Figure A5-17 page A5-16, ACCA Manual J Eighth Edition.
source | <xsd:attribute name="floorCrawlSpaceIsSealed" type="xsd:boolean"> <xsd:annotation> <xsd:documentation>Specifies whether or not the crawl space wall associated with this floor is well sealed from the outdoor air, which affects both the heating and cooling loads. See Figure A5-5, page A5-8, and Figure A5-17 page A5-16, ACCA Manual J Eighth Edition.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute ManualJ8Parameters/@floorCategory

type | floorCategoryEnum
facets |
Kind | Value | Annotation
enumeration | OverEnclosedCrawlSpaceOrBasement |
enumeration | OverOpenCrawlSpaceOrGarage |
enumeration | Basement |
enumeration | SlabOnGrade |
annotation |
documentation
Specifies the type of floor being considered, which affects both the heating and the cooling loads. See Table 4A, pages T4A-27 and following, ACCA Manual J Eighth Edition.
source | <xsd:attribute name="floorCategory" type="floorCategoryEnum"> <xsd:annotation> <xsd:documentation>Specifies the type of floor being considered, which affects both the heating and the cooling loads. See Table 4A, pages T4A-27 and following, ACCA Manual J Eighth Edition.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Manufacturer

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
elements | AirLoopEquipment ExtEquip HydronicLoopEquipment IntEquip LightingSystem
source | <xsd:element name="Manufacturer" type="xsd:string"/>

element MaritalStatus

diagram |
namespace | http://www.gbxml.org/schema
type | MaritalStatusType
properties |
content | simple
used by |
element | SocioEconomic
facets |
Kind | Value | Annotation
enumeration | Single |
enumeration | Married |
enumeration | Partner |
source | <xsd:element name="MaritalStatus" type="MaritalStatusType"/>

element MarkovChainModel

diagram |
namespace | http://www.gbxml.org/schema
type | MarkovChainModelType
properties |
content | complex
children | EarlyOccurTime TypicalOccurTime
used by |
element | EventOccurModel
source | <xsd:element name="MarkovChainModel" type="MarkovChainModelType"/>

element Material

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Absorptance Roughness Albedo Reflectance Transmittance Emittance ImageTexture R-value Thickness Conductivity Density SpecificHeat Permeance Porosity RecycledContent Fire Cost IndoorAirQuality CADMaterialId Reference
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
DOELibIdRef | xsd:string |  |  |  |
documentation
Use this attribute to reference objects in the DOE2 library
source | <xsd:element name="Material"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Absorptance" minOccurs="0"/> <xsd:element ref="Roughness" minOccurs="0"/> <xsd:element ref="Albedo" minOccurs="0"/> <xsd:element ref="Reflectance" minOccurs="0"/> <xsd:element ref="Transmittance" minOccurs="0"/> <xsd:element ref="Emittance" minOccurs="0"/> <xsd:element ref="ImageTexture" minOccurs="0"/> <xsd:element ref="R-value" minOccurs="0"/> <xsd:element ref="Thickness" minOccurs="0"/> <xsd:element ref="Conductivity" minOccurs="0"/> <xsd:element ref="Density" minOccurs="0"/> <xsd:element ref="SpecificHeat" minOccurs="0"/> <xsd:element ref="Permeance" minOccurs="0"/> <xsd:element ref="Porosity" minOccurs="0"/> <xsd:element ref="RecycledContent" minOccurs="0"/> <xsd:element ref="Fire" minOccurs="0"/> <xsd:element ref="Cost" minOccurs="0"/> <xsd:element ref="IndoorAirQuality" minOccurs="0"/> <xsd:element ref="CADMaterialId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Reference" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Material/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Material/@DOELibIdRef

type | xsd:string
annotation |
documentation
Use this attribute to reference objects in the DOE2 library
source | <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute>

element MaterialId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | Layer
attributes |
Name | Type | Use | Default | Fixed | Annotation
materialIdRef | xsd:IDREF | required |  |  |
documentation
ID identifying a material in a Layer element.
percentOfLayer | xsd:double |  |  |  |
documentation
Percentage (1-100%) of this layer that this material is made from.
source | <xsd:element name="MaterialId"> <xsd:complexType> <xsd:attribute name="materialIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID identifying a material in a Layer element.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="percentOfLayer" type="xsd:double"> <xsd:annotation> <xsd:documentation>Percentage (1-100%) of this layer that this material is made from. </xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute MaterialId/@materialIdRef

type | xsd:IDREF
properties |
use | required
annotation |
documentation
ID identifying a material in a Layer element.
source | <xsd:attribute name="materialIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>ID identifying a material in a Layer element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute MaterialId/@percentOfLayer

type | xsd:double
annotation |
documentation
Percentage (1-100%) of this layer that this material is made from.
source | <xsd:attribute name="percentOfLayer" type="xsd:double"> <xsd:annotation> <xsd:documentation>Percentage (1-100%) of this layer that this material is made from. </xsd:documentation> </xsd:annotation> </xsd:attribute>

element MaximumFlow

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | AirLoopEquipment FlowControl
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | flowUnitEnum |  |  |  |
source | <xsd:element name="MaximumFlow"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="flowUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute MaximumFlow/@unit

type | flowUnitEnum
facets |
Kind | Value | Annotation
enumeration | CFM |
enumeration | CubicMPerHr |
enumeration | LPerSec |
enumeration | LPM |
enumeration | GPH |
enumeration | GPM |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="flowUnitEnum"/>

element MaximumFlowFractionDuringReheat

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | AirLoopEquipment
source | <xsd:element name="MaximumFlowFractionDuringReheat" type="xsd:decimal"/>

element MaxNumberOfMeetingsPerDay

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | MeetingEvent
annotation |
documentation
The maximum number of meetings per day. Uniform distribution is applied.
source | <xsd:element name="MaxNumberOfMeetingsPerDay" type="xsd:integer"> <xsd:annotation> <xsd:documentation>The maximum number of meetings per day. Uniform distribution is applied.</xsd:documentation> </xsd:annotation> </xsd:element>

element MaxNumOccupantsPerMeeting

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | MeetingEvent
annotation |
documentation
The maximum number of occupants per meeting. Uniform distribution is applied.
source | <xsd:element name="MaxNumOccupantsPerMeeting" type="xsd:integer"> <xsd:annotation> <xsd:documentation>The maximum number of occupants per meeting. Uniform distribution is applied.</xsd:documentation> </xsd:annotation> </xsd:element>

element MaxOAFlowPerZone

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Zone
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | flowUnitEnum | required |  |  |
programId | xsd:IDREF | optional |  |  |
annotation |
documentation
Maximum outdoor air flow per zone
source | <xsd:element name="MaxOAFlowPerZone"> <xsd:annotation> <xsd:documentation>Maximum outdoor air flow per zone</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="flowUnitEnum" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute MaxOAFlowPerZone/@unit

type | flowUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | CFM |
enumeration | CubicMPerHr |
enumeration | LPerSec |
enumeration | LPM |
enumeration | GPH |
enumeration | GPM |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="flowUnitEnum" use="required"/>

attribute MaxOAFlowPerZone/@programId

type | xsd:IDREF
properties |
use | optional
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"/>

element MaxPressure

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | PressureControl
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | pressureUnitEnum |  |  |  |
source | <xsd:element name="MaxPressure"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="pressureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute MaxPressure/@unit

type | pressureUnitEnum
facets |
Kind | Value | Annotation
enumeration | PSI |
enumeration | kPa |
enumeration | Atmospheres |
enumeration | InchesOfH2O |
enumeration | CentimetersOfH2O |
enumeration | InchesOfMercury |
enumeration | CentimetersOfMercury |
enumeration | MillimetersOfMercury |
enumeration | Pascals |
source | <xsd:attribute name="unit" type="pressureUnitEnum"/>

element MaxRelativeHumidity

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | AirLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | unitlessUnitEnum | required |  |  |
source | <xsd:element name="MaxRelativeHumidity"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute MaxRelativeHumidity/@unit

type | unitlessUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Percent |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element MaxTemp

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | TemperatureControl
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | temperatureUnitEnum |  |  |  |
source | <xsd:element name="MaxTemp"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute MaxTemp/@unit

type | temperatureUnitEnum
facets |
Kind | Value | Annotation
enumeration | F |
enumeration | C |
enumeration | K |
enumeration | R |
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element Mean

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
complexType | eqGaussianNormal1DType
source | <xsd:element name="Mean" type="xsd:decimal"/>

element MeetingDuration

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:duration
properties |
content | simple
used by |
complexType | MeetingDurationProbabilityType
annotation |
documentation
Potential duration of a meeting
source | <xsd:element name="MeetingDuration" type="xsd:duration"> <xsd:annotation> <xsd:documentation>Potential duration of a meeting</xsd:documentation> </xsd:annotation> </xsd:element>

element MeetingDurationProbability

diagram |
namespace | http://www.gbxml.org/schema
type | MeetingDurationProbabilityType
properties |
content | complex
children | MeetingDuration Probability
used by |
element | MeetingEvent
source | <xsd:element name="MeetingDurationProbability" type="MeetingDurationProbabilityType"/>

element MeetingEvent

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | SeasonType DayofWeek MinNumOccupantsPerMeeting MaxNumOccupantsPerMeeting MinNumberOfMeetingsPerDay MaxNumberOfMeetingsPerDay MeetingDurationProbability
used by |
element | Space
annotation |
documentation
Meeting event occurrence properties
source | <xsd:element name="MeetingEvent"> <xsd:annotation> <xsd:documentation>Meeting event occurrence properties</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:sequence> <xsd:element ref="SeasonType" minOccurs="0" maxOccurs="5"/> <xsd:element ref="DayofWeek" minOccurs="0" maxOccurs="11"/> <xsd:element ref="MinNumOccupantsPerMeeting"/> <xsd:element ref="MaxNumOccupantsPerMeeting"/> <xsd:element ref="MinNumberOfMeetingsPerDay"/> <xsd:element ref="MaxNumberOfMeetingsPerDay"/> <xsd:element ref="MeetingDurationProbability" maxOccurs="unbounded"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element Meter

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description UtilityRate
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
resourceType | resourceTypeEnum | required |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
annotation |
documentation
Description of a resource measurement
source | <xsd:element name="Meter"> <xsd:annotation> <xsd:documentation>Description of a resource measurement</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="UtilityRate" minOccurs="0"/> <xsd:any namespace="##other" processContents="lax" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="resourceType" type="resourceTypeEnum" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Meter/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Meter/@resourceType

type | resourceTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Electricity |
enumeration | NaturalGas |
enumeration | Propane |
enumeration | FuelOil1 |
enumeration | FuelOil2 |
enumeration | FuelOil4 |
enumeration | Water |
enumeration | ChilledWater |
enumeration | HotWater |
enumeration | Steam |
source | <xsd:attribute name="resourceType" type="resourceTypeEnum" use="required"/>

attribute Meter/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element MeterId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
elements | AltEnergySource Building Campus Space
attributes |
Name | Type | Use | Default | Fixed | Annotation
meterIdRef | xsd:IDREF |  |  |  |
documentation
ID for a resource meter
source | <xsd:element name="MeterId"> <xsd:complexType> <xsd:attribute name="meterIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for a resource meter</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute MeterId/@meterIdRef

type | xsd:IDREF
annotation |
documentation
ID for a resource meter
source | <xsd:attribute name="meterIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for a resource meter</xsd:documentation> </xsd:annotation> </xsd:attribute>

element MiddleName

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | PersonInfo
source | <xsd:element name="MiddleName" type="xsd:string"/>

element MinFlow

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | AirLoopEquipment HydronicLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | derived by: flowUnitEnum | required |  |  |
hydronicLoopIdRef | xsd:IDREF |  |  |  |
hydronicLoopType | loopTypeEnum |  |  |  |
annotation |
documentation
Minimum flow
source | <xsd:element name="MinFlow"> <xsd:annotation> <xsd:documentation>Minimum flow</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" use="required"> <xsd:simpleType> <xsd:union memberTypes="flowUnitEnum unitlessUnitEnum"/> </xsd:simpleType> </xsd:attribute> <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF"/> <xsd:attribute name="hydronicLoopType" type="loopTypeEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute MinFlow/@unit

type | union of (flowUnitEnum, unitlessUnitEnum)
properties |
use | required
source | <xsd:attribute name="unit" use="required"> <xsd:simpleType> <xsd:union memberTypes="flowUnitEnum unitlessUnitEnum"/> </xsd:simpleType> </xsd:attribute>

attribute MinFlow/@hydronicLoopIdRef

type | xsd:IDREF
source | <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF"/>

attribute MinFlow/@hydronicLoopType

type | loopTypeEnum
facets |
Kind | Value | Annotation
enumeration | PrimaryChilledWater |
enumeration | SecondaryChilledWater |
enumeration | HotWater |
enumeration | CondenserWater |
enumeration | DomesticHotWater |
enumeration | WaterLoopHeatPump |
enumeration | TwoPipe |
enumeration | PotableWaterLoop |
enumeration | VRFLoop |
source | <xsd:attribute name="hydronicLoopType" type="loopTypeEnum"/>

element MinimumFlow

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | FlowControl
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | flowUnitEnum |  |  |  |
source | <xsd:element name="MinimumFlow"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="flowUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute MinimumFlow/@unit

type | flowUnitEnum
facets |
Kind | Value | Annotation
enumeration | CFM |
enumeration | CubicMPerHr |
enumeration | LPerSec |
enumeration | LPM |
enumeration | GPH |
enumeration | GPM |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="flowUnitEnum"/>

element MinimumOutdoorAirControlType

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | Zone
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | minimumOutdoorAirControlTypeEnum |  |  |  |
source | <xsd:element name="MinimumOutdoorAirControlType"> <xsd:complexType> <xsd:attribute name="unit" type="minimumOutdoorAirControlTypeEnum"/> </xsd:complexType> </xsd:element>

attribute MinimumOutdoorAirControlType/@unit

type | minimumOutdoorAirControlTypeEnum
facets |
Kind | Value | Annotation
enumeration | FixedMinimum |
enumeration | ProportionalMinimum |
source | <xsd:attribute name="unit" type="minimumOutdoorAirControlTypeEnum"/>

element MinLightFrac

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | LightingControl
annotation |
documentation
Fraction of light illuminance used at minimum setting.
source | <xsd:element name="MinLightFrac" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Fraction of light illuminance used at minimum setting.</xsd:documentation> </xsd:annotation> </xsd:element>

element MinNumberOfMeetingsPerDay

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | MeetingEvent
annotation |
documentation
The minimum number of meetings per day. Uniform distribution is applied.
source | <xsd:element name="MinNumberOfMeetingsPerDay" type="xsd:integer"> <xsd:annotation> <xsd:documentation>The minimum number of meetings per day. Uniform distribution is applied.</xsd:documentation> </xsd:annotation> </xsd:element>

element MinNumOccupantsPerMeeting

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | MeetingEvent
annotation |
documentation
The minimum number of occupants per meeting. Uniform distribution is applied.
source | <xsd:element name="MinNumOccupantsPerMeeting" type="xsd:integer"> <xsd:annotation> <xsd:documentation>The minimum number of occupants per meeting. Uniform distribution is applied.</xsd:documentation> </xsd:annotation> </xsd:element>

element MinOAFlowPerZone

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Zone
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | flowUnitEnum | required |  |  |
programId | xsd:IDREF | optional |  |  |
annotation |
documentation
Minimum outdoor air flow per zone
source | <xsd:element name="MinOAFlowPerZone"> <xsd:annotation> <xsd:documentation>Minimum outdoor air flow per zone</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="flowUnitEnum" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute MinOAFlowPerZone/@unit

type | flowUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | CFM |
enumeration | CubicMPerHr |
enumeration | LPerSec |
enumeration | LPM |
enumeration | GPH |
enumeration | GPM |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="flowUnitEnum" use="required"/>

attribute MinOAFlowPerZone/@programId

type | xsd:IDREF
properties |
use | optional
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"/>

element MinPowerFrac

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | LightingControl
annotation |
documentation
Fraction of power used at minimum setting.
source | <xsd:element name="MinPowerFrac" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Fraction of power used at minimum setting.</xsd:documentation> </xsd:annotation> </xsd:element>

element MinPressure

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | PressureControl
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | pressureUnitEnum |  |  |  |
source | <xsd:element name="MinPressure"> <xsd:complexType> <xsd:attribute name="unit" type="pressureUnitEnum"/> </xsd:complexType> </xsd:element>

attribute MinPressure/@unit

type | pressureUnitEnum
facets |
Kind | Value | Annotation
enumeration | PSI |
enumeration | kPa |
enumeration | Atmospheres |
enumeration | InchesOfH2O |
enumeration | CentimetersOfH2O |
enumeration | InchesOfMercury |
enumeration | CentimetersOfMercury |
enumeration | MillimetersOfMercury |
enumeration | Pascals |
source | <xsd:attribute name="unit" type="pressureUnitEnum"/>

element MinRelativeHumidity

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | AirLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | unitlessUnitEnum | required |  |  |
source | <xsd:element name="MinRelativeHumidity"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute MinRelativeHumidity/@unit

type | unitlessUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Percent |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element MinTemp

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | TemperatureControl
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | temperatureUnitEnum |  |  |  |
source | <xsd:element name="MinTemp"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute MinTemp/@unit

type | temperatureUnitEnum
facets |
Kind | Value | Annotation
enumeration | F |
enumeration | C |
enumeration | K |
enumeration | R |
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element Model

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
elements | AirLoopEquipment ExtEquip HydronicLoopEquipment IntEquip
source | <xsd:element name="Model" type="xsd:string"/>

element ModifiedBy

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | DocumentHistory
attributes |
Name | Type | Use | Default | Fixed | Annotation
personId | xsd:IDREF | required |  |  |
programId | xsd:IDREF | required |  |  |
date | xsd:dateTime | required |  |  |
annotation |
documentation
Denotes the time this file has been modified, as well as the person and program used to modify this file.
source | <xsd:element name="ModifiedBy"> <xsd:annotation> <xsd:documentation>Denotes the time this file has been modified, as well as the person and program used to modify this file.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:attribute name="personId" type="xsd:IDREF" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="required"/> <xsd:attribute name="date" type="xsd:dateTime" use="required"/> </xsd:complexType> </xsd:element>

attribute ModifiedBy/@personId

type | xsd:IDREF
properties |
use | required
source | <xsd:attribute name="personId" type="xsd:IDREF" use="required"/>

attribute ModifiedBy/@programId

type | xsd:IDREF
properties |
use | required
source | <xsd:attribute name="programId" type="xsd:IDREF" use="required"/>

attribute ModifiedBy/@date

type | xsd:dateTime
properties |
use | required
source | <xsd:attribute name="date" type="xsd:dateTime" use="required"/>

element MotorInAirstream

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:boolean
properties |
content | simple
used by |
element | AirLoopEquipment
annotation |
documentation
Indicates if the motor is located in the path of the air stream.
source | <xsd:element name="MotorInAirstream" type="xsd:boolean"> <xsd:annotation> <xsd:documentation>Indicates if the motor is located in the path of the air stream.</xsd:documentation> </xsd:annotation> </xsd:element>

element MovementBehavior

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Description SeasonType DayofWeek RandomMovementEvent StatusTransitionEvent
used by |
element | Behaviors
attributes |
Name | Type | Use | Default | Fixed | Annotation
ID | xsd:ID | required |  |  |
Name | xsd:string | optional |  |  |
IfcGuid | xsd:string | optional |  |  |
annotation |
documentation
Behavior regarding location change of an occupant
source | <xsd:element name="MovementBehavior"> <xsd:annotation> <xsd:documentation>Behavior regarding location change of an occupant </xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:sequence> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="SeasonType" minOccurs="0" maxOccurs="5"/> <xsd:element ref="DayofWeek" minOccurs="0" maxOccurs="11"/> <xsd:element ref="RandomMovementEvent"/> <xsd:element ref="StatusTransitionEvent" maxOccurs="unbounded"/> </xsd:sequence> <xsd:attribute name="ID" type="xsd:ID" use="required"/> <xsd:attribute name="Name" type="xsd:string" use="optional"/> <xsd:attribute name="IfcGuid" type="xsd:string" use="optional"/> </xsd:complexType> </xsd:element>

attribute MovementBehavior/@ID

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="ID" type="xsd:ID" use="required"/>

attribute MovementBehavior/@Name

type | xsd:string
properties |
use | optional
source | <xsd:attribute name="Name" type="xsd:string" use="optional"/>

attribute MovementBehavior/@IfcGuid

type | xsd:string
properties |
use | optional
source | <xsd:attribute name="IfcGuid" type="xsd:string" use="optional"/>

element MovementBehaviorID

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:IDREF
properties |
content | simple
used by |
element | Occupant
source | <xsd:element name="MovementBehaviorID" type="xsd:IDREF"/>

element Name

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
elements | Activity AirLoop AirLoopEquipment AirSystem AnalysisParameter Blind Building BuildingStorey Campus Construction DaySchedule DependentVariable ExtEquip Frame Gap Glaze HolidaysModeled HydronicLoop HydronicLoopEquipment IndependentVariable IntEquip Layer Location Material Meter Opening Results Schedule ShellGeometry Space Surface Weather WeekSchedule WindowType XAxis YAxis YearSchedule Zone ZoneHVACEquipment
source | <xsd:element name="Name" type="xsd:string"/>

element NaturalVentHiTemp

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Opening
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | temperatureUnitEnum |  |  |  |
annotation |
documentation
Natural ventilation does not occur above this temperature.
source | <xsd:element name="NaturalVentHiTemp"> <xsd:annotation> <xsd:documentation>Natural ventilation does not occur above this temperature.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute NaturalVentHiTemp/@unit

type | temperatureUnitEnum
facets |
Kind | Value | Annotation
enumeration | F |
enumeration | C |
enumeration | K |
enumeration | R |
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element NaturalVentLoTemp

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Opening
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | temperatureUnitEnum |  |  |  |
annotation |
documentation
Natural ventilation does not occur below this temperature.
source | <xsd:element name="NaturalVentLoTemp"> <xsd:annotation> <xsd:documentation>Natural ventilation does not occur below this temperature.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute NaturalVentLoTemp/@unit

type | temperatureUnitEnum
facets |
Kind | Value | Annotation
enumeration | F |
enumeration | C |
enumeration | K |
enumeration | R |
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

element NaturalVentOccDep

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:boolean
properties |
content | simple
used by |
element | Opening
annotation |
documentation
Occupancy dependence of natural ventilation. If true, then natural ventilation only occurs when people are present.
source | <xsd:element name="NaturalVentOccDep" type="xsd:boolean"> <xsd:annotation> <xsd:documentation>Occupancy dependence of natural ventilation. If true, then natural ventilation only occurs when people are present.</xsd:documentation> </xsd:annotation> </xsd:element>

element Needs

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Physical
used by |
element | Behavior
source | <xsd:element name="Needs"> <xsd:complexType> <xsd:sequence> <xsd:element ref="Physical"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element NightCycleControl

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | AirLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | nightCycleControlEnum |  |  |  |
source | <xsd:element name="NightCycleControl"> <xsd:complexType> <xsd:attribute name="unit" type="nightCycleControlEnum"/> </xsd:complexType> </xsd:element>

attribute NightCycleControl/@unit

type | nightCycleControlEnum
facets |
Kind | Value | Annotation
enumeration | StayOff |
enumeration | CycleOnAny |
enumeration | CycleOnControlZone |
source | <xsd:attribute name="unit" type="nightCycleControlEnum"/>

element NormalDurationModel

diagram |
namespace | http://www.gbxml.org/schema
type | NormalDurationModelType
properties |
content | complex
children | TypicalDuration MinimumDuration
used by |
elements | ActivityDuration EventDuration
source | <xsd:element name="NormalDurationModel" type="NormalDurationModelType"/>

element NormalProbabilityModel

diagram |
namespace | http://www.gbxml.org/schema
type | NormalProbabilityModelType
properties |
content | complex
children | EarlyOccurTime TypicalOccurTime
used by |
elements | ActivityOccurModel EventOccurModel
source | <xsd:element name="NormalProbabilityModel" type="NormalProbabilityModelType"/>

element NumberOfLamps

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | LightingSystem
source | <xsd:element name="NumberOfLamps" type="xsd:integer"/>

element OAFlowPerArea

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Zone
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | flowPerAreaUnitEnum | required |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
annotation |
documentation
Outside air flow per area
source | <xsd:element name="OAFlowPerArea"> <xsd:annotation> <xsd:documentation>Outside air flow per area</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="flowPerAreaUnitEnum" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute OAFlowPerArea/@unit

type | flowPerAreaUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | CFMPerSquareFoot |
enumeration | LPerSecPerSquareM |
enumeration | CubicMPerSecPerSquareM |
enumeration | CubicMPerHourPerSquareM |
source | <xsd:attribute name="unit" type="flowPerAreaUnitEnum" use="required"/>

attribute OAFlowPerArea/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element OAFlowPerPerson

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Zone
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | flowUnitEnum | required |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
annotation |
documentation
Outside air flow per person
source | <xsd:element name="OAFlowPerPerson"> <xsd:annotation> <xsd:documentation>Outside air flow per person</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="flowUnitEnum" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute OAFlowPerPerson/@unit

type | flowUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | CFM |
enumeration | CubicMPerHr |
enumeration | LPerSec |
enumeration | LPM |
enumeration | GPH |
enumeration | GPM |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="flowUnitEnum" use="required"/>

attribute OAFlowPerPerson/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element OAFlowPerZone

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Zone
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | flowUnitEnum | required |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
annotation |
documentation
Outside air flow per zone
source | <xsd:element name="OAFlowPerZone"> <xsd:annotation> <xsd:documentation>Outside air flow per zone</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="flowUnitEnum" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute OAFlowPerZone/@unit

type | flowUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | CFM |
enumeration | CubicMPerHr |
enumeration | LPerSec |
enumeration | LPM |
enumeration | GPH |
enumeration | GPM |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="flowUnitEnum" use="required"/>

attribute OAFlowPerZone/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element ObjectId

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | Results
annotation |
documentation
Indicates which object or objects the results apply to, if any
source | <xsd:element name="ObjectId" type="xsd:string"> <xsd:annotation> <xsd:documentation>Indicates which object or objects the results apply to, if any</xsd:documentation> </xsd:annotation> </xsd:element>

element Occupant

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Priority MovementBehaviorID BehaviorID SocioEconomic GeographicLocation SubjectiveValues
used by |
element | Occupants
attributes |
Name | Type | Use | Default | Fixed | Annotation
ID | xsd:ID | required |  |  |
Name | xsd:string | optional |  |  |
IfcGuid | xsd:string | optional |  |  |
annotation |
documentation
Attributes to an occupant can be given.
source | <xsd:element name="Occupant"> <xsd:annotation> <xsd:documentation>Attributes to an occupant can be given.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:sequence> <xsd:element ref="Priority" minOccurs="0"/> <xsd:element ref="MovementBehaviorID" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="BehaviorID" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="SocioEconomic" minOccurs="0"/> <xsd:element ref="GeographicLocation" minOccurs="0"/> <xsd:element ref="SubjectiveValues" minOccurs="0"/> </xsd:sequence> <xsd:attribute name="ID" type="xsd:ID" use="required"/> <xsd:attribute name="Name" type="xsd:string" use="optional"/> <xsd:attribute name="IfcGuid" type="xsd:string" use="optional"/> </xsd:complexType> </xsd:element>

attribute Occupant/@ID

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="ID" type="xsd:ID" use="required"/>

attribute Occupant/@Name

type | xsd:string
properties |
use | optional
source | <xsd:attribute name="Name" type="xsd:string" use="optional"/>

attribute Occupant/@IfcGuid

type | xsd:string
properties |
use | optional
source | <xsd:attribute name="IfcGuid" type="xsd:string" use="optional"/>

element OccupantBehavior

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Building Occupants Behaviors Seasons TimeofDays HolidaysModeled
attributes |
Name | Type | Use | Default | Fixed | Annotation
ID |  | required |  |  |
Version |  | required |  |  |
Name | xsd:string | optional |  |  |
IfcProjectGuid | xsd:string |  |  |  |
IfcFilename | xsd:string | optional |  |  |
IfcOriginatingSystem | xsd:string | optional |  |  |
IfcCreationDate | xsd:date | optional |  |  |
IfcAuthor | xsd:string | optional |  |  |
annotation |
documentation
The occupancy behavior root node
source | <xsd:element name="OccupantBehavior"> <xsd:annotation> <xsd:documentation>The occupancy behavior root node</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:sequence> <xsd:element ref="Building" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Occupants" minOccurs="0"/> <xsd:element ref="Behaviors"/> <xsd:element ref="Seasons" minOccurs="0"/> <xsd:element ref="TimeofDays" minOccurs="0"/> <xsd:element ref="HolidaysModeled" minOccurs="0"/> </xsd:sequence> <xsd:attribute name="ID" use="required"/> <xsd:attribute name="Version" use="required"/> <xsd:attribute name="Name" type="xsd:string" use="optional"/> <xsd:attribute name="IfcProjectGuid" type="xsd:string"/> <xsd:attribute name="IfcFilename" type="xsd:string" use="optional"/> <xsd:attribute name="IfcOriginatingSystem" type="xsd:string" use="optional"/> <xsd:attribute name="IfcCreationDate" type="xsd:date" use="optional"/> <xsd:attribute name="IfcAuthor" type="xsd:string" use="optional"/> </xsd:complexType> </xsd:element>

attribute OccupantBehavior/@ID

properties |
use | required
source | <xsd:attribute name="ID" use="required"/>

attribute OccupantBehavior/@Version

properties |
use | required
source | <xsd:attribute name="Version" use="required"/>

attribute OccupantBehavior/@Name

type | xsd:string
properties |
use | optional
source | <xsd:attribute name="Name" type="xsd:string" use="optional"/>

attribute OccupantBehavior/@IfcProjectGuid

type | xsd:string
source | <xsd:attribute name="IfcProjectGuid" type="xsd:string"/>

attribute OccupantBehavior/@IfcFilename

type | xsd:string
properties |
use | optional
source | <xsd:attribute name="IfcFilename" type="xsd:string" use="optional"/>

attribute OccupantBehavior/@IfcOriginatingSystem

type | xsd:string
properties |
use | optional
source | <xsd:attribute name="IfcOriginatingSystem" type="xsd:string" use="optional"/>

attribute OccupantBehavior/@IfcCreationDate

type | xsd:date
properties |
use | optional
source | <xsd:attribute name="IfcCreationDate" type="xsd:date" use="optional"/>

attribute OccupantBehavior/@IfcAuthor

type | xsd:string
properties |
use | optional
source | <xsd:attribute name="IfcAuthor" type="xsd:string" use="optional"/>

element Occupants

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Occupant
used by |
elements | gbXML OccupantBehavior
source | <xsd:element name="Occupants"> <xsd:complexType> <xsd:sequence> <xsd:element ref="Occupant" maxOccurs="unbounded"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element Opening

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description ShadeControl U-value ShadingCoeff SolarHeatGainCoeff Transmittance Reflectance GlazeConductivity Emittance Setback NaturalVentHiTemp NaturalVentLoTemp NaturalVentOccDep RectangularGeometry PlanarGeometry CADObjectId
used by |
element | Surface
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
coordinatesAbsolute | xsd:boolean |  |  |  |
documentation
coordinatesAbsolute is a boolean value for an Opening element, which if true, specifies that the coordinates in RectangularGeometry and PlanarGeometry are relative to the origin of the project's global reference frame. If this attribute is set to false, this means the coordinates in in RectangularGeometry and PlanarGeometry are relative to a local origin, defined as the lower left hand corner of its parent wall (when viewing the wall looking towards it outward-facing normal (i.e. - "outside looking in")).
interiorShadeType | shadeOperationEnum |  |  |  |
exteriorShadeType | shadeOperationEnum |  |  |  |
windowTypeIdRef | xsd:IDREF |  |  |  |
constructionIdRef | xsd:IDREF |  |  |  |
documentation
Identifier pointing to a construction
openingType | openingTypeEnum | required |  |  |
ifcGUID | xsd:string | optional |  |  |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
source | <xsd:element name="Opening"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="ShadeControl" minOccurs="0"/> <xsd:element ref="U-value" minOccurs="0"/> <xsd:element ref="ShadingCoeff" minOccurs="0"/> <xsd:element ref="SolarHeatGainCoeff" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Transmittance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Reflectance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="GlazeConductivity" minOccurs="0"/> <xsd:element ref="Emittance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Setback" minOccurs="0"/> <xsd:element ref="NaturalVentHiTemp" minOccurs="0"/> <xsd:element ref="NaturalVentLoTemp" minOccurs="0"/> <xsd:element ref="NaturalVentOccDep" minOccurs="0"/> <xsd:element ref="RectangularGeometry"/> <xsd:element ref="PlanarGeometry"/> <xsd:element ref="CADObjectId" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="coordinatesAbsolute" type="xsd:boolean"> <xsd:annotation> <xsd:documentation>coordinatesAbsolute is a boolean value for an Opening element, which if true, specifies that the coordinates in RectangularGeometry and PlanarGeometry are relative to the origin of the project's global reference frame. If this attribute is set to false, this means the coordinates in in RectangularGeometry and PlanarGeometry are relative to a local origin, defined as the lower left hand corner of its parent wall (when viewing the wall looking towards it outward-facing normal (i.e. - "outside looking in")).</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="interiorShadeType" type="shadeOperationEnum"/> <xsd:attribute name="exteriorShadeType" type="shadeOperationEnum"/> <xsd:attribute name="windowTypeIdRef" type="xsd:IDREF"/> <xsd:attribute name="constructionIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Identifier pointing to a construction</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="openingType" type="openingTypeEnum" use="required"/> <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Opening/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Opening/@coordinatesAbsolute

type | xsd:boolean
annotation |
documentation
coordinatesAbsolute is a boolean value for an Opening element, which if true, specifies that the coordinates in RectangularGeometry and PlanarGeometry are relative to the origin of the project's global reference frame. If this attribute is set to false, this means the coordinates in in RectangularGeometry and PlanarGeometry are relative to a local origin, defined as the lower left hand corner of its parent wall (when viewing the wall looking towards it outward-facing normal (i.e. - "outside looking in")).
source | <xsd:attribute name="coordinatesAbsolute" type="xsd:boolean"> <xsd:annotation> <xsd:documentation>coordinatesAbsolute is a boolean value for an Opening element, which if true, specifies that the coordinates in RectangularGeometry and PlanarGeometry are relative to the origin of the project's global reference frame. If this attribute is set to false, this means the coordinates in in RectangularGeometry and PlanarGeometry are relative to a local origin, defined as the lower left hand corner of its parent wall (when viewing the wall looking towards it outward-facing normal (i.e. - "outside looking in")).</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Opening/@interiorShadeType

type | shadeOperationEnum
facets |
Kind | Value | Annotation
enumeration | Fixed |
enumeration | Operable |
source | <xsd:attribute name="interiorShadeType" type="shadeOperationEnum"/>

attribute Opening/@exteriorShadeType

type | shadeOperationEnum
facets |
Kind | Value | Annotation
enumeration | Fixed |
enumeration | Operable |
source | <xsd:attribute name="exteriorShadeType" type="shadeOperationEnum"/>

attribute Opening/@windowTypeIdRef

type | xsd:IDREF
source | <xsd:attribute name="windowTypeIdRef" type="xsd:IDREF"/>

attribute Opening/@constructionIdRef

type | xsd:IDREF
annotation |
documentation
Identifier pointing to a construction
source | <xsd:attribute name="constructionIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Identifier pointing to a construction</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Opening/@openingType

type | openingTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | FixedWindow |
documentation
Opening in a surface with a tilt between 45° and 149.99° with a non-operable glazed opening in it.
enumeration | OperableWindow |
documentation
Opening in a surface with a tilt between 45° and 149.99° with a operable glazed opening in it.
enumeration | FixedSkylight |
documentation
Opening in a surface with a tilt between 0° and 44.99° with a non-operable glazed opening in it.
enumeration | OperableSkylight |
documentation
Opening in a surface with a tilt between 0° and 44.99° with a operable glazed opening in it.
enumeration | SlidingDoor |
documentation
Opening in a surface with a tilt between 45° and 149.99° with a sliding door in it.
enumeration | NonSlidingDoor |
documentation
Opening in a surface with a tilt between 45° and 149.99° with a non-sliding door in it.
enumeration | Air |
documentation
Opening in a surface with a tilt between 0° and 180° with nothing in it.
source | <xsd:attribute name="openingType" type="openingTypeEnum" use="required"/>

attribute Opening/@ifcGUID

type | xsd:string
properties |
use | optional
annotation |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
source | <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element OperationSchedule

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | OperationRange
used by |
elements | AirLoopEquipment HydronicLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
scheduleIdRef | xsd:IDREF |  |  |  |
documentation
Schedule of operation for a piece of equipment. For heating and cooling equipment (such as a boiler or chiller) this is the availability schedule, the schedule of temperatures that, when reached, the piece of equipment will be available.
source | <xsd:element name="OperationSchedule"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element name="OperationRange" type="OperationRange" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Schedule of operation for a piece of equipment. For heating and cooling equipment (such as a boiler or chiller) this is the availability schedule, the schedule of temperatures that, when reached, the piece of equipment will be available.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute OperationSchedule/@scheduleIdRef

type | xsd:IDREF
annotation |
documentation
Schedule of operation for a piece of equipment. For heating and cooling equipment (such as a boiler or chiller) this is the availability schedule, the schedule of temperatures that, when reached, the piece of equipment will be available.
source | <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Schedule of operation for a piece of equipment. For heating and cooling equipment (such as a boiler or chiller) this is the availability schedule, the schedule of temperatures that, when reached, the piece of equipment will be available.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element OperationSchedule/OperationRange

diagram |
type | OperationRange
properties |
minOcc | 0
maxOcc | unbounded
content | complex
children | ParameterID Min Max
source | <xsd:element name="OperationRange" type="OperationRange" minOccurs="0" maxOccurs="unbounded"/>

element OtherConstraint

diagram |
namespace | http://www.gbxml.org/schema
type | OtherConstraintType
properties |
content | simple
used by |
element | Drivers
facets |
Kind | Value | Annotation
enumeration | NoOccupantsInRoom |
documentation
The action happens only when there is no occupant in the room. (Typically combined with leaving room events.)
source | <xsd:element name="OtherConstraint" type="OtherConstraintType"/>

element ParallelFanOnFlowFraction

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | AirLoopEquipment
annotation |
documentation
Parallel fan flow fraction
source | <xsd:element name="ParallelFanOnFlowFraction"> <xsd:annotation> <xsd:documentation>Parallel fan flow fraction</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"/> </xsd:simpleContent> </xsd:complexType> </xsd:element>

element Parameter

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Description ParameterType
used by |
element | Environment
attributes |
Name | Type | Use | Default | Fixed | Annotation
ID | xsd:ID | required |  |  |
Name | xsd:string | optional |  |  |
IfcGuid | xsd:string | optional |  |  |
annotation |
documentation
Driving parameters can be set. Units of parameters are SI: degree C, ppm, lux, W/m2.
source | <xsd:element name="Parameter"> <xsd:annotation> <xsd:documentation>Driving parameters can be set. Units of parameters are SI: degree C, ppm, lux, W/m2.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:sequence> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="ParameterType"/> </xsd:sequence> <xsd:attribute name="ID" type="xsd:ID" use="required"/> <xsd:attribute name="Name" type="xsd:string" use="optional"/> <xsd:attribute name="IfcGuid" type="xsd:string" use="optional"/> </xsd:complexType> </xsd:element>

attribute Parameter/@ID

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="ID" type="xsd:ID" use="required"/>

attribute Parameter/@Name

type | xsd:string
properties |
use | optional
source | <xsd:attribute name="Name" type="xsd:string" use="optional"/>

attribute Parameter/@IfcGuid

type | xsd:string
properties |
use | optional
source | <xsd:attribute name="IfcGuid" type="xsd:string" use="optional"/>

element Parameter1ID

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:IDREF
properties |
content | simple
used by |
complexTypes | eqLinear1DType eqLinear2DType eqLinear3DType eqLogit1DLinearType eqLogit1DQuadraticType eqLogit2DLinearType eqLogit3DLinearType eqQuadratic1DType eqWeibull1D3P
source | <xsd:element name="Parameter1ID" type="xsd:IDREF"/>

element Parameter2ID

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:IDREF
properties |
content | simple
used by |
complexTypes | eqLinear2DType eqLinear3DType eqLogit2DLinearType eqLogit3DLinearType
source | <xsd:element name="Parameter2ID" type="xsd:IDREF"/>

element Parameter3ID

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:IDREF
properties |
content | simple
used by |
complexTypes | eqLinear3DType eqLogit3DLinearType
source | <xsd:element name="Parameter3ID" type="xsd:IDREF"/>

element ParameterRange

diagram |
namespace | http://www.gbxml.org/schema
type | OperationRange
properties |
content | complex
children | ParameterID Min Max
used by |
elements | ASHRAEComfortEnvelope ASHRAECoolingAdaptiveComfort IAQ Visual
source | <xsd:element name="ParameterRange" type="OperationRange"/>

element ParameterType

diagram |
namespace | http://www.gbxml.org/schema
type | parameterType
properties |
content | simple
used by |
element | Parameter
facets |
Kind | Value | Annotation
enumeration | RoomAirTemperature |
enumeration | RoomCO2Concentration |
enumeration | RoomWorkPlaneDaylightIlluminance |
enumeration | RoomLightsPowerDensity |
enumeration | OutdoorDryBulbTemperature |
enumeration | OutdoorRainIndicator |
annotation |
documentation
Parameter type can be simple (integer, flow, boolean, string) or complex (combination of simples or equation).
source | <xsd:element name="ParameterType" type="parameterType"> <xsd:annotation> <xsd:documentation>Parameter type can be simple (integer, flow, boolean, string) or complex (combination of simples or equation).</xsd:documentation> </xsd:annotation> </xsd:element>

element ParameterValue

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | AnalysisParameter
source | <xsd:element name="ParameterValue" type="xsd:string"/>

element PastExperience

diagram |
namespace | http://www.gbxml.org/schema
type | subjectiveValueType
properties |
content | simple
used by |
element | SubjectiveValues
facets |
Kind | Value | Annotation
enumeration | High |
enumeration | Medium |
enumeration | Low |
source | <xsd:element name="PastExperience" type="subjectiveValueType"/>

element PeakDomesticHotWaterFlow

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Building
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | flowUnitEnum | required |  |  |
hydronicLoopIdRef | xsd:IDREF | required |  |  |
waterUseScheduleIdRef | xsd:IDREF | required |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
annotation |
documentation
Use this element to report overall domestic hot water use for the domestic hot water loop referenced with the hydronicLoopIdRef attribute. The schedule referenced by waterUseScheduleIdRef defines a hot water use fraction schedule, which when combined with the value of PeakDomesticHotWaterFlow fully describe the hot water use of this building.
source | <xsd:element name="PeakDomesticHotWaterFlow"> <xsd:annotation> <xsd:documentation>Use this element to report overall domestic hot water use for the domestic hot water loop referenced with the hydronicLoopIdRef attribute. The schedule referenced by waterUseScheduleIdRef defines a hot water use fraction schedule, which when combined with the value of PeakDomesticHotWaterFlow fully describe the hot water use of this building.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="flowUnitEnum" use="required"/> <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF" use="required"/> <xsd:attribute name="waterUseScheduleIdRef" type="xsd:IDREF" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute PeakDomesticHotWaterFlow/@unit

type | flowUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | CFM |
enumeration | CubicMPerHr |
enumeration | LPerSec |
enumeration | LPM |
enumeration | GPH |
enumeration | GPM |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="flowUnitEnum" use="required"/>

attribute PeakDomesticHotWaterFlow/@hydronicLoopIdRef

type | xsd:IDREF
properties |
use | required
source | <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF" use="required"/>

attribute PeakDomesticHotWaterFlow/@waterUseScheduleIdRef

type | xsd:IDREF
properties |
use | required
source | <xsd:attribute name="waterUseScheduleIdRef" type="xsd:IDREF" use="required"/>

attribute PeakDomesticHotWaterFlow/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element PeopleHeatGain

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Space
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | peopleHeatGainUnitEnum | required |  |  |
heatGainType | peopleHeatGainTypeEnum | required |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
annotation |
documentation
Amount of heat added to the space by people
source | <xsd:element name="PeopleHeatGain"> <xsd:annotation> <xsd:documentation>Amount of heat added to the space by people</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="peopleHeatGainUnitEnum" use="required"/> <xsd:attribute name="heatGainType" type="peopleHeatGainTypeEnum" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute PeopleHeatGain/@unit

type | peopleHeatGainUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | WattPerPerson |
enumeration | BtuPerHourPerson |
source | <xsd:attribute name="unit" type="peopleHeatGainUnitEnum" use="required"/>

attribute PeopleHeatGain/@heatGainType

type | peopleHeatGainTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Total |
enumeration | Sensible |
enumeration | Latent |
source | <xsd:attribute name="heatGainType" type="peopleHeatGainTypeEnum" use="required"/>

attribute PeopleHeatGain/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element PeopleNumber

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Space
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | peopleNumberUnitEnum | required |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
annotation |
documentation
Occupancy of the space
source | <xsd:element name="PeopleNumber"> <xsd:annotation> <xsd:documentation>Occupancy of the space</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="peopleNumberUnitEnum" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute PeopleNumber/@unit

type | peopleNumberUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | NumberOfPeople |
enumeration | SquareFtPerPerson |
enumeration | SquareMPerPerson |
source | <xsd:attribute name="unit" type="peopleNumberUnitEnum" use="required"/>

attribute PeopleNumber/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element PercentAreaDaylitControlled

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | LightingControl
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | unitlessUnitEnum | required |  |  |
annotation |
documentation
Percent of space area whose lights are controlled by a daylight sensor. Only applicable when LightPowerPerArea is used at the space level and not Lighting Systems.
source | <xsd:element name="PercentAreaDaylitControlled"> <xsd:annotation> <xsd:documentation>Percent of space area whose lights are controlled by a daylight sensor. Only applicable when LightPowerPerArea is used at the space level and not Lighting Systems.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute PercentAreaDaylitControlled/@unit

type | unitlessUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Percent |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element PercentExisting

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Construction
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | unitlessUnitEnum | required |  |  |
annotation |
documentation
Percent of original building shell used in renovation
source | <xsd:element name="PercentExisting"> <xsd:annotation> <xsd:documentation>Percent of original building shell used in renovation</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute PercentExisting/@unit

type | unitlessUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Percent |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element Performance

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | PointData Equation
used by |
elements | AirLoopEquipment ExtEquip HydronicLoopEquipment IntEquip
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID |  |  |  |
performanceType | xsd:string |  |  |  |
annotation |
documentation
Used to represent part-load performance and other performance metrics
source | <xsd:element name="Performance"> <xsd:annotation> <xsd:documentation>Used to represent part-load performance and other performance metrics</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="PointData" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Equation" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID"/> <xsd:attribute name="performanceType" type="xsd:string"/> </xsd:complexType> </xsd:element>

attribute Performance/@id

type | xsd:ID
source | <xsd:attribute name="id" type="xsd:ID"/>

attribute Performance/@performanceType

type | xsd:string
source | <xsd:attribute name="performanceType" type="xsd:string"/>

element Permeance

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Material
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | permUnitEnum | required |  |  |
annotation |
documentation
The rate water vapor is allowed through a surface
source | <xsd:element name="Permeance"> <xsd:annotation> <xsd:documentation>The rate water vapor is allowed through a surface</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="permUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Permeance/@unit

type | permUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | PermSI |
enumeration | PermIP |
source | <xsd:attribute name="unit" type="permUnitEnum" use="required"/>

element PersonInfo

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | FirstName LastName MiddleName Address1 Address2 City State ZipCode Country PhoneNumber Email1Address WebPage CompanyName
used by |
element | DocumentHistory
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
annotation |
documentation
Contains information about people that created and modified this file
source | <xsd:element name="PersonInfo"> <xsd:annotation> <xsd:documentation>Contains information about people that created and modified this file</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="FirstName"/> <xsd:element ref="LastName"/> <xsd:element ref="MiddleName" minOccurs="0"/> <xsd:element ref="Address1" minOccurs="0"/> <xsd:element ref="Address2" minOccurs="0"/> <xsd:element ref="City" minOccurs="0"/> <xsd:element ref="State" minOccurs="0"/> <xsd:element ref="ZipCode" minOccurs="0"/> <xsd:element ref="Country" minOccurs="0"/> <xsd:element ref="PhoneNumber" minOccurs="0"/> <xsd:element ref="Email1Address" minOccurs="0"/> <xsd:element ref="WebPage" minOccurs="0"/> <xsd:element ref="CompanyName" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> </xsd:complexType> </xsd:element>

attribute PersonInfo/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

element PhoneNumber

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | PersonInfo
source | <xsd:element name="PhoneNumber" type="xsd:string"/>

element Photometry

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | LightingSystem
annotation |
documentation
This element has been left open for use with other photometry definitions. Photometric data is required for various forms of lighting analysis. This tag provides a way for the photometric data to be passed. Since this can be done in a variety of ways (iesna LM-63, cibse TM14, ELUMDAT, etc.) a specific format is not being specified.
source | <xsd:element name="Photometry" type="xsd:string"> <xsd:annotation> <xsd:documentation>This element has been left open for use with other photometry definitions. Photometric data is required for various forms of lighting analysis. This tag provides a way for the photometric data to be passed. Since this can be done in a variety of ways (iesna LM-63, cibse TM14, ELUMDAT, etc.) a specific format is not being specified.</xsd:documentation> </xsd:annotation> </xsd:element>

element PhotometryOrientation

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | CartesianPoint
used by |
element | Lighting
annotation |
documentation
This element specifies the position and the x, y and z axis of the light source. This element must have four Coordinate elements which represent the position and the x, y and z axis in order. The first CartesianPoint element specifies the position of the light source. The second, third and fourth CartesianPoint elements specifies the displacement points for the positive x, positive y and positive z axis.
source | <xsd:element name="PhotometryOrientation"> <xsd:annotation> <xsd:documentation>This element specifies the position and the x, y and z axis of the light source. This element must have four Coordinate elements which represent the position and the x, y and z axis in order. The first CartesianPoint element specifies the position of the light source. The second, third and fourth CartesianPoint elements specifies the displacement points for the positive x, positive y and positive z axis.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0"> <xsd:element ref="CartesianPoint" minOccurs="4" maxOccurs="4"/> </xsd:choice> </xsd:complexType> </xsd:element>

element Physical

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Thermal Visual IAQ
used by |
element | Needs
source | <xsd:element name="Physical"> <xsd:complexType> <xsd:sequence> <xsd:element ref="Thermal" minOccurs="0"/> <xsd:element ref="Visual" minOccurs="0"/> <xsd:element ref="IAQ" minOccurs="0"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element PlanarGeometry

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | PolyLoop
used by |
elements | BuildingStorey Opening Space SpaceBoundary Surface
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID |  |  |  |
unit | lengthUnitEnum |  |  |  |
annotation |
documentation
List of points defining a loop. There are no repeated points in the list. All data are global, with the assumption that positive Z is up, and if CADModelAzimuth is undefined or zero, positive X is East and positive Y is North. If CADModelAzimuth is defined it is the angle of positive Y to North, positive X is the vectorial product of Y and Z. If geometry is to be precise, use Longitude, Latitude and Elevation in the Location element to define the origin. Otherwise the origin is an arbitrary point. Use PlanarGeometry to define a three dimensional polygon that lies on a plane, and has no self-intersection.
source | <xsd:element name="PlanarGeometry"> <xsd:annotation> <xsd:documentation>List of points defining a loop. There are no repeated points in the list. All data are global, with the assumption that positive Z is up, and if CADModelAzimuth is undefined or zero, positive X is East and positive Y is North. If CADModelAzimuth is defined it is the angle of positive Y to North, positive X is the vectorial product of Y and Z. If geometry is to be precise, use Longitude, Latitude and Elevation in the Location element to define the origin. Otherwise the origin is an arbitrary point. Use PlanarGeometry to define a three dimensional polygon that lies on a plane, and has no self-intersection.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="PolyLoop"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID"/> <xsd:attribute name="unit" type="lengthUnitEnum"/> </xsd:complexType> </xsd:element>

attribute PlanarGeometry/@id

type | xsd:ID
source | <xsd:attribute name="id" type="xsd:ID"/>

attribute PlanarGeometry/@unit

type | lengthUnitEnum
facets |
Kind | Value | Annotation
enumeration | Kilometers |
enumeration | Meters |
enumeration | Centimeters |
enumeration | Millimeters |
enumeration | Miles |
enumeration | Yards |
enumeration | Feet |
enumeration | Inches |
source | <xsd:attribute name="unit" type="lengthUnitEnum"/>

element Platform

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | ProgramInfo
source | <xsd:element name="Platform" type="xsd:string"/>

element PlugLoad

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | PlugLoadType
used by |
element | BuildingSystems
source | <xsd:element name="PlugLoad"> <xsd:complexType> <xsd:sequence> <xsd:element ref="PlugLoadType"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element PlugLoadType

diagram |
namespace | http://www.gbxml.org/schema
type | plugLoadTypeEnum
properties |
content | simple
used by |
element | PlugLoad
facets |
Kind | Value | Annotation
enumeration | OnOff |
enumeration | ContinuousControl |
source | <xsd:element name="PlugLoadType" type="plugLoadTypeEnum"/>

element PointData

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | IndependentVariable DependentVariable Data
used by |
element | Performance
annotation |
documentation
The PointData element allows for graph or tabular information to be entered. The data type and units of the independent and dependent variables are defined in their respective elements. Each Data element represent a data point, with each Value element representing the value of a variable - starting with the independent variable, then each dependent variable listed in the order defined.
source | <xsd:element name="PointData"> <xsd:annotation> <xsd:documentation>The PointData element allows for graph or tabular information to be entered. The data type and units of the independent and dependent variables are defined in their respective elements. Each Data element represent a data point, with each Value element representing the value of a variable - starting with the independent variable, then each dependent variable listed in the order defined.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="IndependentVariable" maxOccurs="unbounded"/> <xsd:element ref="DependentVariable" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Data" maxOccurs="unbounded"/> </xsd:choice> </xsd:complexType> </xsd:element>

element Policy

diagram |
namespace | http://www.gbxml.org/schema
type | PolicyType
properties |
content | simple
used by |
element | GeographicLocation
facets |
Kind | Value | Annotation
enumeration | Subsidies |
enumeration | Tax-cuts |
enumeration | Codes compliance |
enumeration | Insurance mandate |
source | <xsd:element name="Policy" type="PolicyType"/>

element PolyLoop

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | CartesianPoint
used by |
elements | ClosedShell PlanarGeometry RectangularGeometry
annotation |
documentation
This is a list of coordinates that make up a polygon in three-dimensional space. All coordinates must lie on the same plane. The right-hand rule applies for defining the outward normal of a surface: For every surface, points must be defined in order, such that the direction of (the average cross-product between (any point, the centroid of the surface, and the next point)) points in the direction of the outward normal, which is a vector pointing away from the first AdjacentSpaceID listed.
appinfo
<xhtml:a href="http://cig.bre.co.uk/iai_uk/documentation/IfcR2x_Final/ifctopologyresource/lexical/ifcpolyloop.html">IfcPolyLoop</xhtml:a>
source | <xsd:element name="PolyLoop"> <xsd:annotation> <xsd:documentation>This is a list of coordinates that make up a polygon in three-dimensional space. All coordinates must lie on the same plane. The right-hand rule applies for defining the outward normal of a surface: For every surface, points must be defined in order, such that the direction of (the average cross-product between (any point, the centroid of the surface, and the next point)) points in the direction of the outward normal, which is a vector pointing away from the first AdjacentSpaceID listed.</xsd:documentation> <xsd:appinfo> <xhtml:a href="http://cig.bre.co.uk/iai_uk/documentation/IfcR2x_Final/ifctopologyresource/lexical/ifcpolyloop.html">IfcPolyLoop</xhtml:a> </xsd:appinfo> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="CartesianPoint" minOccurs="3" maxOccurs="unbounded"/> </xsd:choice> </xsd:complexType> </xsd:element>

element Porosity

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Material
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | unitlessUnitEnum | required |  |  |
annotation |
documentation
the ratio of the total amount of void space in a material (due to poses, small channels, and so on) to the bulk volume occupied by the material.
source | <xsd:element name="Porosity"> <xsd:annotation> <xsd:documentation>the ratio of the total amount of void space in a material (due to poses, small channels, and so on) to the bulk volume occupied by the material. </xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Porosity/@unit

type | unitlessUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Percent |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element Power

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | AirLoopEquipment ExtEquip HydronicLoopEquipment IntEquip
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | powerUnitEnum | required |  |  |
powerType | powerTypeEnum | required |  |  |
useType | powerUseTypeEnum | required |  |  |
meterIdRef | xsd:IDREF |  |  |  |
documentation
ID for a resource meter
annotation |
documentation
Maximum consumption of energy (power input)
source | <xsd:element name="Power"> <xsd:annotation> <xsd:documentation>Maximum consumption of energy (power input)</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="powerUnitEnum" use="required"/> <xsd:attribute name="powerType" type="powerTypeEnum" use="required"/> <xsd:attribute name="useType" type="powerUseTypeEnum" use="required"/> <xsd:attribute name="meterIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for a resource meter</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Power/@unit

type | powerUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Watt |
enumeration | Kilowatt |
enumeration | Horsepower |
enumeration | KilogramForceMeterPerSecond |
enumeration | BtuPerSecond |
enumeration | FootPoundForcePerSecond |
enumeration | KilocaloriesPerSecond |
enumeration | BtuPerHour |
source | <xsd:attribute name="unit" type="powerUnitEnum" use="required"/>

attribute Power/@powerType

type | powerTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Electricity |
enumeration | NaturalGas |
enumeration | Propane |
enumeration | FuelOil1 |
enumeration | FuelOil2 |
enumeration | FuelOil4 |
enumeration | Water |
enumeration | ChilledWater |
enumeration | HotWater |
enumeration | Steam |
enumeration | Diesel |
enumeration | Biogas |
source | <xsd:attribute name="powerType" type="powerTypeEnum" use="required"/>

attribute Power/@useType

type | powerUseTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Heating |
enumeration | Cooling |
enumeration | Both |
enumeration | ElectricityGeneration |
enumeration | Other |
source | <xsd:attribute name="useType" type="powerUseTypeEnum" use="required"/>

attribute Power/@meterIdRef

type | xsd:IDREF
annotation |
documentation
ID for a resource meter
source | <xsd:attribute name="meterIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for a resource meter</xsd:documentation> </xsd:annotation> </xsd:attribute>

element PrandtlNumber

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Gap
source | <xsd:element name="PrandtlNumber" type="xsd:decimal"/>

element PrandtlNumberFofT

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Gap
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | inverseTempUnitEnum | required |  |  |
annotation |
documentation
Prandtl number as a function of temperature
source | <xsd:element name="PrandtlNumberFofT"> <xsd:annotation> <xsd:documentation>Prandtl number as a function of temperature</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="inverseTempUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute PrandtlNumberFofT/@unit

type | inverseTempUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | PerK |
enumeration | PerF |
source | <xsd:attribute name="unit" type="inverseTempUnitEnum" use="required"/>

element PreheatCoilType

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | AirLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | preheatCoilTypeEnum |  |  |  |
source | <xsd:element name="PreheatCoilType"> <xsd:complexType> <xsd:attribute name="unit" type="preheatCoilTypeEnum"/> </xsd:complexType> </xsd:element>

attribute PreheatCoilType/@unit

type | preheatCoilTypeEnum
facets |
Kind | Value | Annotation
enumeration | None |
enumeration | Electric |
enumeration | Gas |
source | <xsd:attribute name="unit" type="preheatCoilTypeEnum"/>

element PressureControl

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | DesignPressure MinPressure MaxPressure
used by |
element | AirLoop
annotation |
documentation
Use this element to describe how the air pressure is controlled. The temperatures specified in this element should be measured just upstream of the air handlers.
source | <xsd:element name="PressureControl"> <xsd:annotation> <xsd:documentation>Use this element to describe how the air pressure is controlled. The temperatures specified in this element should be measured just upstream of the air handlers.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="DesignPressure" minOccurs="0"/> <xsd:element ref="MinPressure" minOccurs="0"/> <xsd:element ref="MaxPressure" minOccurs="0"/> </xsd:choice> </xsd:complexType> </xsd:element>

element Priority

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Occupant
source | <xsd:element name="Priority" type="xsd:integer"/>

element Probability

diagram |
namespace | http://www.gbxml.org/schema
type | restriction of xsd:decimal
properties |
content | simple
used by |
element | StatusTransitionProbability
complexType | MeetingDurationProbabilityType
facets |
Kind | Value | Annotation
minInclusive | 0 |
maxInclusive | 1 |
annotation |
documentation
Probability of occurrence of a meeting with the certain corresponding duration
source | <xsd:element name="Probability"> <xsd:annotation> <xsd:documentation>Probability of occurrence of a meeting with the certain corresponding duration</xsd:documentation> </xsd:annotation> <xsd:simpleType> <xsd:restriction base="xsd:decimal"> <xsd:minInclusive value="0"/> <xsd:maxInclusive value="1"/> </xsd:restriction> </xsd:simpleType> </xsd:element>

element ProductName

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:string
properties |
content | complex
used by |
element | ProgramInfo
source | <xsd:element name="ProductName"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:string"/> </xsd:simpleContent> </xsd:complexType> </xsd:element>

element ProgramInfo

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | CompanyName ProductName Version Platform ProjectEntity
used by |
element | DocumentHistory
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
annotation |
documentation
Contains information about programs that created and modified this file
source | <xsd:element name="ProgramInfo"> <xsd:annotation> <xsd:documentation>Contains information about programs that created and modified this file</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="CompanyName" minOccurs="0"/> <xsd:element ref="ProductName" minOccurs="1"/> <xsd:element ref="Version" minOccurs="1"/> <xsd:element ref="Platform" minOccurs="1"/> <xsd:element ref="ProjectEntity" minOccurs="1"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> </xsd:complexType> </xsd:element>

attribute ProgramInfo/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

element ProjectEntity

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | FileName URI GUID
used by |
element | ProgramInfo
annotation |
documentation
Contains information about the originating or modifying file or service that created or modified this file
source | <xsd:element name="ProjectEntity"> <xsd:annotation> <xsd:documentation>Contains information about the originating or modifying file or service that created or modified this file</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="FileName" minOccurs="0"/> <xsd:element ref="URI" minOccurs="1"/> <xsd:element ref="GUID" minOccurs="1"/> </xsd:choice> </xsd:complexType> </xsd:element>

element Quadratic1D

diagram |
namespace | http://www.gbxml.org/schema
type | eqQuadratic1DType
properties |
content | complex
children | Description CoefficientA CoefficientB CoefficientC Parameter1ID
used by |
element | Formula
source | <xsd:element name="Quadratic1D" type="eqQuadratic1DType"/>

element R-value

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Material
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | resistanceUnitEnum | required |  |  |
annotation |
documentation
Resistance of material
source | <xsd:element name="R-value"> <xsd:annotation> <xsd:documentation>Resistance of material</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="resistanceUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute R-value/@unit

type | resistanceUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | SquareMeterKPerW |
enumeration | HrSquareFtFPerBTU |
source | <xsd:attribute name="unit" type="resistanceUnitEnum" use="required"/>

element RandomMovementEvent

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | SpaceOccupancy
used by |
element | MovementBehavior
annotation |
documentation
Occupant location change events inside a building
source | <xsd:element name="RandomMovementEvent"> <xsd:annotation> <xsd:documentation>Occupant location change events inside a building</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:sequence> <xsd:element ref="SpaceOccupancy" maxOccurs="unbounded"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element RatedFlow

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | AirLoopEquipment ExtEquip HydronicLoopEquipment IntEquip
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | flowUnitEnum | required |  |  |
hydronicLoopIdRef | xsd:IDREF |  |  |  |
hydronicLoopType | loopTypeEnum |  |  |  |
source | <xsd:element name="RatedFlow"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="flowUnitEnum" use="required"/> <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF"/> <xsd:attribute name="hydronicLoopType" type="loopTypeEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute RatedFlow/@unit

type | flowUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | CFM |
enumeration | CubicMPerHr |
enumeration | LPerSec |
enumeration | LPM |
enumeration | GPH |
enumeration | GPM |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="flowUnitEnum" use="required"/>

attribute RatedFlow/@hydronicLoopIdRef

type | xsd:IDREF
source | <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF"/>

attribute RatedFlow/@hydronicLoopType

type | loopTypeEnum
facets |
Kind | Value | Annotation
enumeration | PrimaryChilledWater |
enumeration | SecondaryChilledWater |
enumeration | HotWater |
enumeration | CondenserWater |
enumeration | DomesticHotWater |
enumeration | WaterLoopHeatPump |
enumeration | TwoPipe |
enumeration | PotableWaterLoop |
enumeration | VRFLoop |
source | <xsd:attribute name="hydronicLoopType" type="loopTypeEnum"/>

element RecircFlow

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | FlowControl
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | flowUnitEnum |  |  |  |
source | <xsd:element name="RecircFlow"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="flowUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute RecircFlow/@unit

type | flowUnitEnum
facets |
Kind | Value | Annotation
enumeration | CFM |
enumeration | CubicMPerHr |
enumeration | LPerSec |
enumeration | LPM |
enumeration | GPH |
enumeration | GPM |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="flowUnitEnum"/>

element RectangularGeometry

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Azimuth CartesianPoint Tilt Height Width PolyLoop
used by |
elements | Opening Surface
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID |  |  |  |
unit | lengthUnitEnum |  |  |  |
annotation |
documentation
Geometry data in a form typically used in simulation engines. For surfaces, specify the location of the bottom-left corner with the CartesianPoint element when facing it from the outside. Also for surfaces, Tilt and Azimuth must be specified. If CADModelAzimuth is defined, the Azimuth value is relative to the CADModelAzimuth value rather then North. For openings, the third Coordinate should be zero or left missing. For openings, these Coordinates represent the distance of the bottom-left of the opening to the bottom-left corner of the parent surface. Azimuth and Tilt should not be specified for opening. There is an optional PolyLoop element, which may be used for describing the polygon shape of the surface.
source | <xsd:element name="RectangularGeometry"> <xsd:annotation> <xsd:documentation>Geometry data in a form typically used in simulation engines. For surfaces, specify the location of the bottom-left corner with the CartesianPoint element when facing it from the outside. Also for surfaces, Tilt and Azimuth must be specified. If CADModelAzimuth is defined, the Azimuth value is relative to the CADModelAzimuth value rather then North. For openings, the third Coordinate should be zero or left missing. For openings, these Coordinates represent the distance of the bottom-left of the opening to the bottom-left corner of the parent surface. Azimuth and Tilt should not be specified for opening. There is an optional PolyLoop element, which may be used for describing the polygon shape of the surface.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Azimuth"/> <xsd:element ref="CartesianPoint"/> <xsd:element ref="Tilt"/> <xsd:element ref="Height"/> <xsd:element ref="Width"/> <xsd:element ref="PolyLoop" minOccurs="0"> <xsd:annotation> <xsd:documentation>This is a two-dimensional polygon, with the origin at the point specified with RectangularGeometry/CartesianPoint. </xsd:documentation> </xsd:annotation> </xsd:element> </xsd:choice> <xsd:attribute name="id" type="xsd:ID"/> <xsd:attribute name="unit" type="lengthUnitEnum"/> </xsd:complexType> </xsd:element>

attribute RectangularGeometry/@id

type | xsd:ID
source | <xsd:attribute name="id" type="xsd:ID"/>

attribute RectangularGeometry/@unit

type | lengthUnitEnum
facets |
Kind | Value | Annotation
enumeration | Kilometers |
enumeration | Meters |
enumeration | Centimeters |
enumeration | Millimeters |
enumeration | Miles |
enumeration | Yards |
enumeration | Feet |
enumeration | Inches |
source | <xsd:attribute name="unit" type="lengthUnitEnum"/>

element RecycledContent

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Material
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | unitlessUnitEnum | required |  |  |
source | <xsd:element name="RecycledContent"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute RecycledContent/@unit

type | unitlessUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Percent |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element Reference

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
elements | AirLoop AirLoopEquipment Cost ExtEquip Glaze HydronicLoop HydronicLoopEquipment InfiltrationFlow IntEquip LightingSystem Material Weather
source | <xsd:element name="Reference" type="xsd:string"/>

element Reflectance

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Blind Construction FireFace Glaze Material Opening WindowType
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | unitlessUnitEnum | required |  |  |
type | reflectanceTypeEnum | required |  |  |
surfaceType | surfaceDescriptionEnum | required |  |  |
source | <xsd:element name="Reflectance"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> <xsd:attribute name="type" type="reflectanceTypeEnum" use="required"/> <xsd:attribute name="surfaceType" type="surfaceDescriptionEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Reflectance/@unit

type | unitlessUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Percent |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

attribute Reflectance/@type

type | reflectanceTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Ground |
enumeration | IntSolar |
enumeration | IntIR |
enumeration | IntVisible |
enumeration | ExtSolar |
enumeration | ExtVisible |
enumeration | ExtIR |
source | <xsd:attribute name="type" type="reflectanceTypeEnum" use="required"/>

attribute Reflectance/@surfaceType

type | surfaceDescriptionEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | 1 |
documentation
The surfaceDescriptionEnum allows control over the specification of material surface properties. By setting the surfaceDescriptionEnum to 1, it is implied that the attribute (e.g. - Reflectance, Emittance, etc.) is associated with Surface 1 of the material's two surfaces [it is assumed that the material is a large planar object]. Surface 1 represents the surface that points away from the building interior.
enumeration | 2 |
documentation
The surfaceDescriptionEnum allows control over the specification of material surface properties. By setting the surfaceDescriptionEnum to 2, it is implied that the attribute (e.g. - Reflectance, Emittance, etc.) is associated with Surface 2 of the material's two surfaces [it is assumed that the material is a large planar object]. Surface 2 represents the surface that points towards the building interior.
enumeration | Both |
documentation
The surfaceDescriptionEnum allows control over the specification of material surface properties. By setting the surfaceDescriptionEnum to Both, it is implied that the attribute (e.g. - Reflectance, Emittance, etc.) is associated both Surface 1 and Surface 2 of the material's 2 surfaces [it is assumed that the material is a large planar object]. See the enumerations above for a description of Surface 1 and 2.
source | <xsd:attribute name="surfaceType" type="surfaceDescriptionEnum" use="required"/>

element RefrigerantType

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
elements | AirLoopEquipment HydronicLoopEquipment
source | <xsd:element name="RefrigerantType" type="xsd:string"/>

element ResetTemperature

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | AirLoopEquipment HydronicLoopEquipment TemperatureControl
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | temperatureUnitEnum | required |  |  |
type | resetTemperatureTypeEnum | required |  |  |
resetSchedIdRef | xsd:IDREF |  |  |  |
annotation |
documentation
Cooling and Heating Reset Temperature Type
source | <xsd:element name="ResetTemperature"> <xsd:annotation> <xsd:documentation>Cooling and Heating Reset Temperature Type</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum" use="required"/> <xsd:attribute name="type" type="resetTemperatureTypeEnum" use="required"/> <xsd:attribute name="resetSchedIdRef" type="xsd:IDREF"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute ResetTemperature/@unit

type | temperatureUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | F |
enumeration | C |
enumeration | K |
enumeration | R |
source | <xsd:attribute name="unit" type="temperatureUnitEnum" use="required"/>

attribute ResetTemperature/@type

type | resetTemperatureTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | None |
enumeration | Automatic |
enumeration | OutdoorAirBased |
enumeration | Scheduled |
source | <xsd:attribute name="type" type="resetTemperatureTypeEnum" use="required"/>

attribute ResetTemperature/@resetSchedIdRef

type | xsd:IDREF
source | <xsd:attribute name="resetSchedIdRef" type="xsd:IDREF"/>

element Results

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Value ObjectId CADObjectId CartesianPoint
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
unit | derived by: loadUnitEnum | required |  |  |
currency | currencyTypeEnum |  |  |  |
resultsType | resultsTypeEnum |  |  |  |
resourceType | resourceTypeEnum | required |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that generated the results using the id of the ProgramInfo element.
valueType | valueTypeEnum |  |  |  |
documentation
Please specify how the values were obtained.
startTime | xsd:dateTime | required |  |  |
documentation
Use the startTime attribute to define the start of the first Value element.
timeIncrement | xsd:duration | optional |  |  |
documentation
This specifies the duration of time between each Value element. This is required if more than one Value element exists in a this Results element.
source | <xsd:element name="Results"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Value" maxOccurs="unbounded"/> <xsd:element ref="ObjectId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="CADObjectId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="CartesianPoint" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="unit" use="required"> <xsd:simpleType> <xsd:union memberTypes="loadUnitEnum unitlessSmallUnitEnum energyUnitEnum powerUnitEnum temperatureUnitEnum unitlessUnitEnum illuminanceUnitEnum flowUnitEnum"/> </xsd:simpleType> </xsd:attribute> <xsd:attribute name="currency" type="currencyTypeEnum"/> <xsd:attribute name="resultsType" type="resultsTypeEnum"/> <xsd:attribute name="resourceType" type="resourceTypeEnum" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that generated the results using the id of the ProgramInfo element.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="valueType" type="valueTypeEnum"> <xsd:annotation> <xsd:documentation>Please specify how the values were obtained.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="startTime" type="xsd:dateTime" use="required"> <xsd:annotation> <xsd:documentation>Use the startTime attribute to define the start of the first Value element.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="timeIncrement" type="xsd:duration" use="optional"> <xsd:annotation> <xsd:documentation>This specifies the duration of time between each Value element. This is required if more than one Value element exists in a this Results element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Results/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Results/@unit

type | union of (loadUnitEnum, unitlessSmallUnitEnum, energyUnitEnum, powerUnitEnum, temperatureUnitEnum, unitlessUnitEnum, illuminanceUnitEnum, flowUnitEnum)
properties |
use | required
source | <xsd:attribute name="unit" use="required"> <xsd:simpleType> <xsd:union memberTypes="loadUnitEnum unitlessSmallUnitEnum energyUnitEnum powerUnitEnum temperatureUnitEnum unitlessUnitEnum illuminanceUnitEnum flowUnitEnum"/> </xsd:simpleType> </xsd:attribute>

attribute Results/@currency

type | currencyTypeEnum
facets |
Kind | Value | Annotation
enumeration | USDollars |
enumeration | CanadianDollars |
enumeration | Pesos |
enumeration | Euros |
enumeration | Yen |
enumeration | IndianRupee |
enumeration | Yuan |
enumeration | TaiwanDollar |
enumeration | EnglishPound |
enumeration | Mark |
enumeration | Franc |
enumeration | Ruble |
enumeration | Real |
enumeration | NewZealandDollar |
enumeration | AustralianDollar |
source | <xsd:attribute name="currency" type="currencyTypeEnum"/>

attribute Results/@resultsType

type | resultsTypeEnum
facets |
Kind | Value | Annotation
enumeration | HeatLoad |
enumeration | CoolingLoad |
enumeration | CO2 |
enumeration | SO2 |
enumeration | NOx |
enumeration | Energy |
enumeration | Power |
enumeration | Cost |
enumeration | EnergyCost |
enumeration | DemandCost |
enumeration | CommodityCost |
enumeration | TransportationCost |
enumeration | DryBulbTemperature |
enumeration | WetBulbTemperature |
enumeration | DewPointTemperature |
enumeration | FootCandles |
enumeration | Humidity |
enumeration | MoistureContent |
enumeration | Flow |
enumeration | Capacity |
source | <xsd:attribute name="resultsType" type="resultsTypeEnum"/>

attribute Results/@resourceType

type | resourceTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Electricity |
enumeration | NaturalGas |
enumeration | Propane |
enumeration | FuelOil1 |
enumeration | FuelOil2 |
enumeration | FuelOil4 |
enumeration | Water |
enumeration | ChilledWater |
enumeration | HotWater |
enumeration | Steam |
source | <xsd:attribute name="resourceType" type="resourceTypeEnum" use="required"/>

attribute Results/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that generated the results using the id of the ProgramInfo element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that generated the results using the id of the ProgramInfo element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Results/@valueType

type | valueTypeEnum
facets |
Kind | Value | Annotation
enumeration | Historical |
enumeration | Simulated |
enumeration | Rated |
enumeration | Measured |
annotation |
documentation
Please specify how the values were obtained.
source | <xsd:attribute name="valueType" type="valueTypeEnum"> <xsd:annotation> <xsd:documentation>Please specify how the values were obtained.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Results/@startTime

type | xsd:dateTime
properties |
use | required
annotation |
documentation
Use the startTime attribute to define the start of the first Value element.
source | <xsd:attribute name="startTime" type="xsd:dateTime" use="required"> <xsd:annotation> <xsd:documentation>Use the startTime attribute to define the start of the first Value element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Results/@timeIncrement

type | xsd:duration
properties |
use | optional
annotation |
documentation
This specifies the duration of time between each Value element. This is required if more than one Value element exists in a this Results element.
source | <xsd:attribute name="timeIncrement" type="xsd:duration" use="optional"> <xsd:annotation> <xsd:documentation>This specifies the duration of time between each Value element. This is required if more than one Value element exists in a this Results element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element RoomEventType

diagram |
namespace | http://www.gbxml.org/schema
type | RoomEventType
properties |
content | simple
used by |
element | Drivers
facets |
Kind | Value | Annotation
enumeration | LeavingRoom |
documentation
The occupant is in the space in the previous time-step and not in the current one.
enumeration | LeavingRoomMoreThan1Hour |
enumeration | LeavingRoomMoreThan6Hours |
enumeration | EnteringRoom |
documentation
The occupant is not in the space in the previous time-step and is in the current one.
enumeration | StayingInRoom |
annotation |
documentation
Events can be defined that are possible to happen in the building
source | <xsd:element name="RoomEventType" type="RoomEventType"> <xsd:annotation> <xsd:documentation>Events can be defined that are possible to happen in the building</xsd:documentation> </xsd:annotation> </xsd:element>

element Roughness

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
elements | Construction Material
attributes |
Name | Type | Use | Default | Fixed | Annotation
value | roughnessValueEnum | required |  |  |
annotation |
documentation
Roughness of the outside surface
source | <xsd:element name="Roughness"> <xsd:annotation> <xsd:documentation>Roughness of the outside surface</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:attribute name="value" type="roughnessValueEnum" use="required"/> </xsd:complexType> </xsd:element>

attribute Roughness/@value

type | roughnessValueEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | VeryRough |
enumeration | MediumRough |
enumeration | Rough |
enumeration | Smooth |
enumeration | MediumSmooth |
enumeration | VerySmooth |
source | <xsd:attribute name="value" type="roughnessValueEnum" use="required"/>

element RTSParameters

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | HOutside
used by |
element | LoadCalcInputParameters
attributes |
Name | Type | Use | Default | Fixed | Annotation
roofCTSType | roofCTSTypeEnum |  |  |  |
documentation
Specifies which Conduction Time Series to use for the roof. See Table 21, page 29.30, 2001 ASHRAE Handbook, Fundamentals volume. Only used if the construction is a roof and you are using the RTS calculation method.
wallCTSType | wallCTSTypeEnum |  |  |  |
documentation
Specifies which Conduction Time Series to use for the wall. See Table 20, page 29.28, 2001 ASHRAE Handbook, Fundamentals volume. Only used if the construction is a wall and you are using the RTS calculation method.
annotation |
documentation
Parameters required by RTS load calculation method, as described in pages 29.25 and following of the 2001 ASHRAE Handbook, Fundamentals volume. Ignore this element and all elements under it if you are not planning to use that method.
source | <xsd:element name="RTSParameters"> <xsd:annotation> <xsd:documentation>Parameters required by RTS load calculation method, as described in pages 29.25 and following of the 2001 ASHRAE Handbook, Fundamentals volume. Ignore this element and all elements under it if you are not planning to use that method.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice> <xsd:element ref="HOutside"/> </xsd:choice> <xsd:attribute name="roofCTSType" type="roofCTSTypeEnum"> <xsd:annotation> <xsd:documentation>Specifies which Conduction Time Series to use for the roof. See Table 21, page 29.30, 2001 ASHRAE Handbook, Fundamentals volume. Only used if the construction is a roof and you are using the RTS calculation method.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="wallCTSType" type="wallCTSTypeEnum"> <xsd:annotation> <xsd:documentation>Specifies which Conduction Time Series to use for the wall. See Table 20, page 29.28, 2001 ASHRAE Handbook, Fundamentals volume. Only used if the construction is a wall and you are using the RTS calculation method.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute RTSParameters/@roofCTSType

type | roofCTSTypeEnum
facets |
Kind | Value | Annotation
enumeration | 1 |
documentation
Metal Roof, R-19 Batt Insulation, Gyp Board
enumeration | 2 |
documentation
Metal Roof, R-19 Batt Insulation, Suspended Acoustical Ceiling
enumeration | 3 |
documentation
Metal Roof, R-19 Batt Insulation
enumeration | 4 |
documentation
Asphalt Shingles, Wood Sheathing, R-19 Batt Insulation, Gyp Board
enumeration | 5 |
documentation
Slate or Tile, Wood Sheathing, R-19 Batt Insulation, Gyp Board
enumeration | 6 |
documentation
Wood Shingles, Wood Sheathing, R-19 Batt Insulation, Gyp Board
enumeration | 7 |
documentation
Membrane, Sheathing, R-10 Insulation Board, Wood Deck
enumeration | 8 |
documentation
Membrane, Sheathing, R-10 Insulation Board, Wood Deck Suspended Acoustical Ceiling
enumeration | 9 |
documentation
Membrane, Sheathing, R-10 Insulation Board, Metal Deck
enumeration | 10 |
documentation
Membrane, Sheathing, R-10 Insulation Board, Metal Deck Suspended Acoustical Ceiling
enumeration | 11 |
documentation
Membrane, Sheathing, R-15 Insulation Board, Metal Deck
enumeration | 12 |
documentation
Membrane, Sheathing, R-10 plus R-15 Insulation Boards, Metal Deck
enumeration | 13 |
documentation
2" Concrete Roof Ballast, Membrane, Sheathing, R-15 Insulation Board, Metal Deck
enumeration | 14 |
documentation
Membrane, Sheathing, R-15 Insulation Board, 4" LW Concrete
enumeration | 15 |
documentation
Membrane, Sheathing, R-15 Insulation Board, 6" LW Concrete
enumeration | 16 |
documentation
Membrane, Sheathing, R-15 Insulation Board, 8" LW Concrete
enumeration | 17 |
documentation
Membrane, Sheathing, R-15 Insulation Board, 6" HW Concrete
enumeration | 18 |
documentation
Membrane, Sheathing, R-15 Insulation Board, 8" HW Concrete
enumeration | 19 |
documentation
Membrane, 6" HW Concrete, R-19 Batt Insulation, Suspended Acoustical Ceiling
annotation |
documentation
Specifies which Conduction Time Series to use for the roof. See Table 21, page 29.30, 2001 ASHRAE Handbook, Fundamentals volume. Only used if the construction is a roof and you are using the RTS calculation method.
source | <xsd:attribute name="roofCTSType" type="roofCTSTypeEnum"> <xsd:annotation> <xsd:documentation>Specifies which Conduction Time Series to use for the roof. See Table 21, page 29.30, 2001 ASHRAE Handbook, Fundamentals volume. Only used if the construction is a roof and you are using the RTS calculation method.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute RTSParameters/@wallCTSType

type | wallCTSTypeEnum
facets |
Kind | Value | Annotation
enumeration | 1 |
documentation
Spandrel Glass, R-10 Insulation Board, Gyp Board
enumeration | 2 |
documentation
Metal Wall Panel, R-10 Insulation Board, Gyp Board
enumeration | 3 |
documentation
1" Stone, R-10 Insulation Board, Gyp Board
enumeration | 4 |
documentation
Metal Wall Panel, Sheathing, R-11 Batt Insulation, Gyp Board
enumeration | 5 |
documentation
1" Stone, Sheathing, R-11 Batt Insulation, Gyp Board
enumeration | 6 |
documentation
Wood Siding, Sheathing, R-11 Batt Insulation, 1/2" Wood
enumeration | 7 |
documentation
1" Stucco, Sheathing, R-11 Batt Insulation, Gyp Board
enumeration | 8 |
documentation
EIFS Finish, R-5 Insulation Board, Sheathing, Gyp Board
enumeration | 9 |
documentation
EIFS Finish, R-5 Insulation Board, Sheathing, R-11 Batt Insulation, Gyp Board
enumeration | 10 |
documentation
EIFS Finish, R-5 Insulation Board, Sheathing, 8" LW CMU, Gyp Board
enumeration | 11 |
documentation
Brick, R-5 Insulation Board, Sheathing, Gyp Board
enumeration | 12 |
documentation
Brick, Sheathing, R-11 Batt Insulation, Gyp Board
enumeration | 13 |
documentation
Brick, R-5 Insulation Board, Sheathing, R-11 Batt Insulation Gyp Board
enumeration | 14 |
documentation
Brick, R-5 Insulation Board, 8" LW CMU
enumeration | 15 |
documentation
Brick, 8" LW CMU, R-11 Batt Insulation, Gyp Board
enumeration | 16 |
documentation
Brick, R-5 Insulation Board, 8" HW CMU, Gyp Board
enumeration | 17 |
documentation
Brick, R-5 Insulation Board, Brick
enumeration | 18 |
documentation
Brick, R-5 Insulation Board, 8" LW Concrete, Gyp Board
enumeration | 19 |
documentation
Brick, R-5 Insulation Board, 12" HW Concrete, Gyp Board
enumeration | 20 |
documentation
Brick, 8" HW Concrete, R-11 Batt Insulation, Gyp Board
enumeration | 21 |
documentation
8" LW CMU, R-11 Batt Insulation, Gyp Board
enumeration | 22 |
documentation
8" LW CMU w Fill Insulation, R-11 Batt Insulation, Gyp Board
enumeration | 23 |
documentation
1" Stucco, 8" HW CMU, R-11 Batt Insulation, Gyp Board
enumeration | 24 |
documentation
8" LW CMU w Fill Insulation
enumeration | 25 |
documentation
8" LW CMU w Fill Insulation, Gyp Board
enumeration | 26 |
documentation
12" LW CMU w Fill Insulation, Gyp Board
enumeration | 27 |
documentation
4" LW Concrete. R-5 Board Insulation, Gyp Board
enumeration | 28 |
documentation
4" LW Concrete. R-11 Batt Insulation, Gyp Board
enumeration | 29 |
documentation
4" LW Concrete. R-10 Board Insulation, 4" LW Concrete
enumeration | 30 |
documentation
EIFS Finish, R-5 Insulation Board, 8" LW Concrete, Gyp Board
enumeration | 31 |
documentation
8" LW Concrete. R-11 Batt Insulation, Gyp Board
enumeration | 32 |
documentation
EIFS Finish, R-10 Insulation Board, 8" HW Concrete, Gyp Board
enumeration | 33 |
documentation
8" HW Concrete. R-11 Batt Insulation, Gyp Board
enumeration | 34 |
documentation
12" HW Concrete. R-19 Batt Insulation, Gyp Board
enumeration | 35 |
documentation
12" HW Concrete
annotation |
documentation
Specifies which Conduction Time Series to use for the wall. See Table 20, page 29.28, 2001 ASHRAE Handbook, Fundamentals volume. Only used if the construction is a wall and you are using the RTS calculation method.
source | <xsd:attribute name="wallCTSType" type="wallCTSTypeEnum"> <xsd:annotation> <xsd:documentation>Specifies which Conduction Time Series to use for the wall. See Table 20, page 29.28, 2001 ASHRAE Handbook, Fundamentals volume. Only used if the construction is a wall and you are using the RTS calculation method.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Schedule

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description YearSchedule
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
type | scheduleTypeEnum | required |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
annotation |
documentation
List of year schedules that make up an entire calendar year.
source | <xsd:element name="Schedule"> <xsd:annotation> <xsd:documentation>List of year schedules that make up an entire calendar year.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="YearSchedule" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="type" type="scheduleTypeEnum" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Schedule/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Schedule/@type

type | scheduleTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Temp |
enumeration | Fraction |
enumeration | OnOff |
enumeration | ResetTemp |
enumeration | ActivityLevel |
source | <xsd:attribute name="type" type="scheduleTypeEnum" use="required"/>

attribute Schedule/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element ScheduleTypeLimits

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | LowerLimitValue UpperLimitValue
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
type | scheduleTypeLimitsEnum | required |  |  |
source | <xsd:element name="ScheduleTypeLimits"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="LowerLimitValue" minOccurs="0" maxOccurs="1"/> <xsd:element ref="UpperLimitValue" minOccurs="0" maxOccurs="1"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="type" type="scheduleTypeLimitsEnum" use="required"/> </xsd:complexType> </xsd:element>

attribute ScheduleTypeLimits/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute ScheduleTypeLimits/@type

type | scheduleTypeLimitsEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Continuous |
enumeration | Discrete |
source | <xsd:attribute name="type" type="scheduleTypeLimitsEnum" use="required"/>

element ScheduleValue

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | DaySchedule
attributes |
Name | Type | Use | Default | Fixed | Annotation
OutsideHighReset | xsd:decimal | optional |  |  |
documentation
Value of the outside drybulb temperature for when defining HVAC system lower supply reset temperature
OutsideLowReset | xsd:decimal | optional |  |  |
documentation
Value of the outside drybulb temperature for when defining HVAC system upper supply reset temperature
SupplyHighReset | xsd:decimal | optional |  |  |
documentation
Value of the upper supply air setpoint temperature for reset of cooling air or heating air temperature
SupplyLowReset | xsd:decimal | optional |  |  |
documentation
Value of the lower supply air setpoint temperature for reset of cooling air or heating air temperature
annotation |
documentation
Value for one block of time. Divides a day evenly into number of ScheduleValue elements defined in DaySchedule. Example: If 12 ScheduleValue elements are defined, each will represent two hours
source | <xsd:element name="ScheduleValue"> <xsd:annotation> <xsd:documentation>Value for one block of time. Divides a day evenly into number of ScheduleValue elements defined in DaySchedule. Example: If 12 ScheduleValue elements are defined, each will represent two hours</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="OutsideHighReset" type="xsd:decimal" use="optional"> <xsd:annotation> <xsd:documentation>Value of the outside drybulb temperature for when defining HVAC system lower supply reset temperature </xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="OutsideLowReset" type="xsd:decimal" use="optional"> <xsd:annotation> <xsd:documentation>Value of the outside drybulb temperature for when defining HVAC system upper supply reset temperature </xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="SupplyHighReset" type="xsd:decimal" use="optional"> <xsd:annotation> <xsd:documentation>Value of the upper supply air setpoint temperature for reset of cooling air or heating air temperature </xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="SupplyLowReset" type="xsd:decimal" use="optional"> <xsd:annotation> <xsd:documentation>Value of the lower supply air setpoint temperature for reset of cooling air or heating air temperature </xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute ScheduleValue/@OutsideHighReset

type | xsd:decimal
properties |
use | optional
annotation |
documentation
Value of the outside drybulb temperature for when defining HVAC system lower supply reset temperature
source | <xsd:attribute name="OutsideHighReset" type="xsd:decimal" use="optional"> <xsd:annotation> <xsd:documentation>Value of the outside drybulb temperature for when defining HVAC system lower supply reset temperature </xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute ScheduleValue/@OutsideLowReset

type | xsd:decimal
properties |
use | optional
annotation |
documentation
Value of the outside drybulb temperature for when defining HVAC system upper supply reset temperature
source | <xsd:attribute name="OutsideLowReset" type="xsd:decimal" use="optional"> <xsd:annotation> <xsd:documentation>Value of the outside drybulb temperature for when defining HVAC system upper supply reset temperature </xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute ScheduleValue/@SupplyHighReset

type | xsd:decimal
properties |
use | optional
annotation |
documentation
Value of the upper supply air setpoint temperature for reset of cooling air or heating air temperature
source | <xsd:attribute name="SupplyHighReset" type="xsd:decimal" use="optional"> <xsd:annotation> <xsd:documentation>Value of the upper supply air setpoint temperature for reset of cooling air or heating air temperature </xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute ScheduleValue/@SupplyLowReset

type | xsd:decimal
properties |
use | optional
annotation |
documentation
Value of the lower supply air setpoint temperature for reset of cooling air or heating air temperature
source | <xsd:attribute name="SupplyLowReset" type="xsd:decimal" use="optional"> <xsd:annotation> <xsd:documentation>Value of the lower supply air setpoint temperature for reset of cooling air or heating air temperature </xsd:documentation> </xsd:annotation> </xsd:attribute>

element Seasons

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Season
used by |
element | OccupantBehavior
source | <xsd:element name="Seasons"> <xsd:complexType> <xsd:sequence> <xsd:element name="Season" maxOccurs="unbounded"> <xsd:complexType> <xsd:all> <xsd:element ref="StartMonth"/> <xsd:element ref="StartDay"/> <xsd:element ref="EndMonth"/> <xsd:element ref="EndDay"/> </xsd:all> <xsd:attribute name="Type" type="SeasonType" use="required"/> </xsd:complexType> </xsd:element> </xsd:sequence> </xsd:complexType> </xsd:element>

element Seasons/Season

diagram |
properties |
minOcc | 1
maxOcc | unbounded
content | complex
children | StartMonth StartDay EndMonth EndDay
attributes |
Name | Type | Use | Default | Fixed | Annotation
Type | SeasonType | required |  |  |
source | <xsd:element name="Season" maxOccurs="unbounded"> <xsd:complexType> <xsd:all> <xsd:element ref="StartMonth"/> <xsd:element ref="StartDay"/> <xsd:element ref="EndMonth"/> <xsd:element ref="EndDay"/> </xsd:all> <xsd:attribute name="Type" type="SeasonType" use="required"/> </xsd:complexType> </xsd:element>

attribute Seasons/Season/@Type

type | SeasonType
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Spring |
documentation
March 1 to May 31
enumeration | Summer |
documentation
June 1 to August 31
enumeration | Fall |
documentation
September 1 to November 30
enumeration | Winter |
documentation
December 1 to February 28
enumeration | All |
source | <xsd:attribute name="Type" type="SeasonType" use="required"/>

element SeasonType

diagram |
namespace | http://www.gbxml.org/schema
type | SeasonType
properties |
content | simple
used by |
elements | MeetingEvent MovementBehavior Time
facets |
Kind | Value | Annotation
enumeration | Spring |
documentation
March 1 to May 31
enumeration | Summer |
documentation
June 1 to August 31
enumeration | Fall |
documentation
September 1 to November 30
enumeration | Winter |
documentation
December 1 to February 28
enumeration | All |
source | <xsd:element name="SeasonType" type="SeasonType"/>

element SecondaryFlow

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Zone
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | flowUnitEnum | required |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Secondary supply air maximum flow rate
source | <xsd:element name="SecondaryFlow"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="flowUnitEnum" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Secondary supply air maximum flow rate</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute SecondaryFlow/@unit

type | flowUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | CFM |
enumeration | CubicMPerHr |
enumeration | LPerSec |
enumeration | LPM |
enumeration | GPH |
enumeration | GPM |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="flowUnitEnum" use="required"/>

attribute SecondaryFlow/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Secondary supply air maximum flow rate
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Secondary supply air maximum flow rate</xsd:documentation> </xsd:annotation> </xsd:attribute>

element SensibleHeatRecoveryEffectiveness

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | AirLoopEquipment
source | <xsd:element name="SensibleHeatRecoveryEffectiveness" type="xsd:decimal"/>

element Setback

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Opening
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | lengthUnitEnum |  |  |  |
annotation |
documentation
Distance from outside surface of window to outside surface of wall
source | <xsd:element name="Setback"> <xsd:annotation> <xsd:documentation>Distance from outside surface of window to outside surface of wall</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="lengthUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Setback/@unit

type | lengthUnitEnum
facets |
Kind | Value | Annotation
enumeration | Kilometers |
enumeration | Meters |
enumeration | Centimeters |
enumeration | Millimeters |
enumeration | Miles |
enumeration | Yards |
enumeration | Feet |
enumeration | Inches |
source | <xsd:attribute name="unit" type="lengthUnitEnum"/>

element ShadeAndBlindType

diagram |
namespace | http://www.gbxml.org/schema
type | shadeAndBlindTypeEnum
properties |
content | simple
used by |
element | ShadesAndBlinds
facets |
Kind | Value | Annotation
enumeration | Operable |
enumeration | Fixed |
source | <xsd:element name="ShadeAndBlindType" type="shadeAndBlindTypeEnum"/>

element ShadeControl

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | ShadeSchedule SolarOnOpening HorizontalSolar AirTemperature ZoneCoolingLoad Glare
used by |
element | Opening
attributes |
Name | Type | Use | Default | Fixed | Annotation
type | shadeTypeEnum | required |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
source | <xsd:element name="ShadeControl"> <xsd:complexType> <xsd:annotation> <xsd:documentation>The ShadeControl element is a bit complex, as shading control is handled differently in different simulation engines. Each child of ShadeControl represents a criteria to help determine if the shades will be open or closed. The resulting shade action should be a union of these. Example: You have included a ShadeSchedule, which is a 1 on weekdays and a 0 on weekends, and a SolarOnOpening. The shade will be drawn when the solar radiation on this opening is greater than SolarOnOpening and it is a weekday.</xsd:documentation> </xsd:annotation> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="ShadeSchedule" minOccurs="0"/> <xsd:element ref="SolarOnOpening" minOccurs="0"/> <xsd:element ref="HorizontalSolar" minOccurs="0"/> <xsd:element ref="AirTemperature" minOccurs="0"/> <xsd:element ref="ZoneCoolingLoad" minOccurs="0"/> <xsd:element ref="Glare" minOccurs="0"/> </xsd:choice> <xsd:attribute name="type" type="shadeTypeEnum" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute ShadeControl/@type

type | shadeTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | InteriorInsulated |
enumeration | InteriorUnInsulated |
enumeration | ExternalInsulated |
enumeration | ExternalUnInsulated |
source | <xsd:attribute name="type" type="shadeTypeEnum" use="required"/>

attribute ShadeControl/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element ShadesAndBlinds

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | ShadeAndBlindType
used by |
element | BuildingSystems
source | <xsd:element name="ShadesAndBlinds"> <xsd:complexType> <xsd:sequence> <xsd:element ref="ShadeAndBlindType"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element ShadeSchedule

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | ShadeControl
attributes |
Name | Type | Use | Default | Fixed | Annotation
scheduleIdRef | xsd:ID | required |  |  |
annotation |
documentation
Use this element to define schedules for a shade.
source | <xsd:element name="ShadeSchedule"> <xsd:annotation> <xsd:documentation>Use this element to define schedules for a shade.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:attribute name="scheduleIdRef" type="xsd:ID" use="required"/> </xsd:complexType> </xsd:element>

attribute ShadeSchedule/@scheduleIdRef

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="scheduleIdRef" type="xsd:ID" use="required"/>

element ShadingCoeff

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Opening WindowType
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | unitlessUnitEnum | required |  |  |
annotation |
documentation
Shading Coefficient: The ratio of total solar transmittance for the specified glazing system to the total solar transmittance for the standard reference glazing (1/8" clear).
source | <xsd:element name="ShadingCoeff"> <xsd:annotation> <xsd:documentation>Shading Coefficient: The ratio of total solar transmittance for the specified glazing system to the total solar transmittance for the standard reference glazing (1/8" clear).</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute ShadingCoeff/@unit

type | unitlessUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Percent |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element ShellGeometry

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description ClosedShell
used by |
elements | AirLoopEquipment Building Campus ExtEquip HydronicLoopEquipment IntEquip Lighting LightingControl LightingSystem Space Transportation Vegetation
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
unit | lengthUnitEnum |  | Meters |  |
annotation |
documentation
All data are global, with the assumption that positive Z is up, and if CADModelAzimuth is undefined or zero, positive X is East and positive Y is North. If CADModelAzimuth is defined it is the angle of positive Y to North, positive X is the vectorial product of Y and Z. If geometry is to be precise, use Longitude Latitude, and Elevation in the Location element to define the origin. Otherwise the origin is an arbitrary point. ShellGeometry is used to define a union of closed shells, where there is no intersection of any two of the given shells.
source | <xsd:element name="ShellGeometry"> <xsd:annotation> <xsd:documentation>All data are global, with the assumption that positive Z is up, and if CADModelAzimuth is undefined or zero, positive X is East and positive Y is North. If CADModelAzimuth is defined it is the angle of positive Y to North, positive X is the vectorial product of Y and Z. If geometry is to be precise, use Longitude Latitude, and Elevation in the Location element to define the origin. Otherwise the origin is an arbitrary point. ShellGeometry is used to define a union of closed shells, where there is no intersection of any two of the given shells.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="ClosedShell"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="unit" type="lengthUnitEnum" default="Meters"/> </xsd:complexType> </xsd:element>

attribute ShellGeometry/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute ShellGeometry/@unit

type | lengthUnitEnum
properties |
default | Meters
facets |
Kind | Value | Annotation
enumeration | Kilometers |
enumeration | Meters |
enumeration | Centimeters |
enumeration | Millimeters |
enumeration | Miles |
enumeration | Yards |
enumeration | Feet |
enumeration | Inches |
source | <xsd:attribute name="unit" type="lengthUnitEnum" default="Meters"/>

element SimulationParameters

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | ConvergenceLimits
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | Annotation
version | xsd:string |  |  |  |
timestep | xsd:decimal |  |  |  |
annotation |
documentation
Simulation parameters refer to simulation engine settings that are used during simulation run-time. These parameters are instructions for a simulation engine to take into account features such as simulation timestep (entered as a number of minutes which should be evenly divisible into 60, see timestep attribute), convergence limits (see ConvergenceLimits), and the version of the simulation engine (version attribute). This element intends to maintain a record of the settings used to run a simulation, which may be important if gbxml stores simulation results, as a user may wish to know what settings and version of the simulation engine were used for analysis.
source | <xsd:element name="SimulationParameters"> <xsd:annotation> <xsd:documentation>Simulation parameters refer to simulation engine settings that are used during simulation run-time. These parameters are instructions for a simulation engine to take into account features such as simulation timestep (entered as a number of minutes which should be evenly divisible into 60, see timestep attribute), convergence limits (see ConvergenceLimits), and the version of the simulation engine (version attribute). This element intends to maintain a record of the settings used to run a simulation, which may be important if gbxml stores simulation results, as a user may wish to know what settings and version of the simulation engine were used for analysis.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="1"> <xsd:element ref="ConvergenceLimits" minOccurs="0" maxOccurs="1"/> </xsd:choice> <xsd:attribute name="version" type="xsd:string"/> <xsd:attribute name="timestep" type="xsd:decimal"/> </xsd:complexType> </xsd:element>

attribute SimulationParameters/@version

type | xsd:string
source | <xsd:attribute name="version" type="xsd:string"/>

attribute SimulationParameters/@timestep

type | xsd:decimal
source | <xsd:attribute name="timestep" type="xsd:decimal"/>

element SinkRate

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | IndoorAirQuality
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | sinkRateUnitEnum | required |  |  |
source | <xsd:element name="SinkRate"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="sinkRateUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute SinkRate/@unit

type | sinkRateUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | PoundsPerHour |
enumeration | KilogramsPerHour |
enumeration | GramsPerHour |
source | <xsd:attribute name="unit" type="sinkRateUnitEnum" use="required"/>

element SocialInfluence

diagram |
namespace | http://www.gbxml.org/schema
type | subjectiveValueType
properties |
content | simple
used by |
element | SubjectiveValues
facets |
Kind | Value | Annotation
enumeration | High |
enumeration | Medium |
enumeration | Low |
source | <xsd:element name="SocialInfluence" type="subjectiveValueType"/>

element SocioEconomic

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Age Gender LifeStyle JobType MaritalStatus Education IncomeGroup Employment
used by |
element | Occupant
annotation |
documentation
A specific location can be assigned to each occupant.
source | <xsd:element name="SocioEconomic"> <xsd:annotation> <xsd:documentation>A specific location can be assigned to each occupant.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:sequence> <xsd:element ref="Age" minOccurs="0"/> <xsd:element ref="Gender" minOccurs="0"/> <xsd:element ref="LifeStyle" minOccurs="0"/> <xsd:element ref="JobType" minOccurs="0"/> <xsd:element ref="MaritalStatus" minOccurs="0"/> <xsd:element ref="Education" minOccurs="0"/> <xsd:element ref="IncomeGroup" minOccurs="0"/> <xsd:element ref="Employment" minOccurs="0"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element SolarHeatGainCoeff

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Opening WindowType
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | unitlessUnitEnum | required |  |  |
solarIncidentAngle | xsd:decimal | optional |  |  |
annotation |
documentation
When element is a child of WindowType: The center of glass solar heat gain coefficient. When element is a child of Opening: The overall solar heat gain coefficient for the window assembly.
source | <xsd:element name="SolarHeatGainCoeff"> <xsd:annotation> <xsd:documentation>When element is a child of WindowType: The center of glass solar heat gain coefficient. When element is a child of Opening: The overall solar heat gain coefficient for the window assembly.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> <xsd:attribute name="solarIncidentAngle" type="xsd:decimal" use="optional"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute SolarHeatGainCoeff/@unit

type | unitlessUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Percent |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

attribute SolarHeatGainCoeff/@solarIncidentAngle

type | xsd:decimal
properties |
use | optional
source | <xsd:attribute name="solarIncidentAngle" type="xsd:decimal" use="optional"/>

element SolarOnOpening

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | ShadeControl
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | powerPerAreaUnitEnum | required |  |  |
annotation |
documentation
Amount of solar radiation striking the opening before a shade is closed.
source | <xsd:element name="SolarOnOpening"> <xsd:annotation> <xsd:documentation>Amount of solar radiation striking the opening before a shade is closed.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="powerPerAreaUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute SolarOnOpening/@unit

type | powerPerAreaUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | WattPerSquareMeter |
enumeration | WattPerSquareFoot |
source | <xsd:attribute name="unit" type="powerPerAreaUnitEnum" use="required"/>

element Space

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Lighting LightingControl InfiltrationFlow PeopleNumber PeopleHeatGain LightPowerPerArea EquipPowerPerArea AirChangesPerHour Area Temperature Volume BuildingSystems GroupPriority MeetingEvent AnalysisParameter PlanarGeometry ShellGeometry AirLoopId HydronicLoopId MeterId IntEquipId AirLoopEquipmentId HydronicLoopEquipmentId CADObjectId TypeCode SpaceBoundary OccupantID
used by |
element | Building
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
spaceType | spaceTypeEnum |  |  |  |
documentation
spaceType represents how a space is used.
appinfo
<xhtml:a href="http://206.55.31.90/cgi-bin/lpd/ShowSpaceTypes.pl">IfcPolyLoop</xhtml:a>, an IESNA and ASHRAE project for determining lighting power density for individual spaces.
zoneIdRef | xsd:IDREF |  |  |  |
scheduleIdRef | xsd:IDREF |  |  |  |
documentation
ID for the schedule of transmittance of a shading surface
lightScheduleIdRef | xsd:IDREF |  |  |  |
documentation
ID of the schedule for lights contained in this space
equipmentScheduleIdRef | xsd:IDREF |  |  |  |
documentation
ID for schedule of equipment use
peopleScheduleIdRef | xsd:IDREF |  |  |  |
documentation
ID for schedule of people in this space
conditionType | conditionTypeEnum |  |  |  |
buildingStoreyIdRef | xsd:IDREF |  |  |  |
documentation
ID for BuildingStorey this space is on.
ifcGUID | xsd:string | optional |  |  |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
annotation |
documentation
A space represents a volume enclosed by surfaces.
source | <xsd:element name="Space"> <xsd:annotation> <xsd:documentation>A space represents a volume enclosed by surfaces.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Lighting" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="LightingControl" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="InfiltrationFlow" minOccurs="0"/> <xsd:element ref="PeopleNumber" minOccurs="0"/> <xsd:element ref="PeopleHeatGain" minOccurs="0" maxOccurs="3"/> <xsd:element ref="LightPowerPerArea" minOccurs="0"/> <xsd:element ref="EquipPowerPerArea" minOccurs="0"/> <xsd:element ref="AirChangesPerHour" minOccurs="0"/> <xsd:element ref="Area" minOccurs="1"/> <xsd:element ref="Temperature" minOccurs="0"/> <xsd:element ref="Volume" minOccurs="1"/> <xsd:element ref="BuildingSystems" minOccurs="0"/> <xsd:element ref="GroupPriority" minOccurs="0"/> <xsd:element ref="MeetingEvent" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="AnalysisParameter" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="PlanarGeometry" minOccurs="0"> <xsd:annotation> <xsd:documentation>Planar polygon that represents the perimeter of space and whose area is equal to the floor area of the space.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="ShellGeometry" minOccurs="0"> <xsd:annotation> <xsd:documentation>Planar polygons that represent the interior surfaces bounding the space and whose volume is equal to the volume of the space.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="AirLoopId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="HydronicLoopId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="MeterId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="IntEquipId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="AirLoopEquipmentId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="HydronicLoopEquipmentId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="CADObjectId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="TypeCode" minOccurs="0"/> <xsd:element ref="SpaceBoundary" minOccurs="0" maxOccurs="unbounded"/> <xsd:element name="OccupantID" type="xsd:IDREF" minOccurs="0" maxOccurs="unbounded"> <xsd:annotation> <xsd:documentation>Predefined occupants can be added to the space.</xsd:documentation> </xsd:annotation> </xsd:element> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="spaceType" type="spaceTypeEnum"> <xsd:annotation> <xsd:documentation>spaceType represents how a space is used.</xsd:documentation> <xsd:appinfo> <xhtml:a href="http://206.55.31.90/cgi-bin/lpd/ShowSpaceTypes.pl">IfcPolyLoop</xhtml:a>, an IESNA and ASHRAE project for determining lighting power density for individual spaces. </xsd:appinfo> </xsd:annotation> </xsd:attribute> <xsd:attribute name="zoneIdRef" type="xsd:IDREF"/> <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="lightScheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID of the schedule for lights contained in this space</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="equipmentScheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for schedule of equipment use</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="peopleScheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for schedule of people in this space</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="conditionType" type="conditionTypeEnum"/> <xsd:attribute name="buildingStoreyIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for BuildingStorey this space is on.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Space/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Space/@spaceType

type | spaceTypeEnum
facets |
Kind | Value | Annotation
enumeration | ActiveStorage |
enumeration | ActiveStorageHospitalOrHealthcare |
enumeration | AirOrTrainOrBusBaggageArea |
enumeration | AirportConcourse |
enumeration | AtriumEachAdditionalFloor |
enumeration | AtriumFirstThreeFloors |
enumeration | AudienceOrSeatingAreaPenitentiary |
enumeration | AudienceOrSeatingAreaExerciseCenter |
enumeration | AudienceOrSeatingAreaGymnasium |
enumeration | AudienceOrSeatingAreaSportsArena |
enumeration | AudienceOrSeatingAreaConventionCenter |
enumeration | AudienceOrSeatingAreaMotionPictureTheatre |
enumeration | AudienceOrSeatingAreaPerformingArtsTheatre |
enumeration | AudienceOrSeatingAreaReligious |
enumeration | AudienceOrSeatingAreaPoliceOrFireStations |
enumeration | AudienceOrSeatingAreaCourtHouse |
enumeration | AudienceOrSeatingAreaAuditorium |
enumeration | BankCustomerArea |
enumeration | BankingActivityAreaOffice |
enumeration | BarberAndBeautyParlor |
enumeration | CardFileAndCataloguingLibrary |
enumeration | ClassroomOrLectureOrTrainingPenitentiary |
enumeration | ClassroomOrLectureOrTraining |
enumeration | ConfinementCellsPenitentiary |
enumeration | ConfinementCellsCourtHouse |
enumeration | ConferenceMeetingOrMultipurpose |
enumeration | CorridorOrTransition |
enumeration | CorridorOrTransitionManufacturingFacility |
enumeration | CorridorsWithPatientWaitingExamHospitalOrHealthcare |
enumeration | CourtSportsAreaSportsArena |
enumeration | CourtroomCourtHouse |
enumeration | DepartmentStoreSalesAreaRetail |
enumeration | DetailedManufacturingFacility |
enumeration | DiningArea |
enumeration | DiningAreaHotel |
enumeration | DiningAreaFamilyDining |
enumeration | DiningAreaLoungeOrLeisureDining |
enumeration | DiningAreaMotel |
enumeration | DiningAreaTransportation |
enumeration | DiningAreaPenitentiary |
enumeration | DiningAreaCivilServices |
enumeration | DormitoryBedroom |
enumeration | DormitoryStudyHall |
enumeration | DressingOrLockerOrFittingRoomGymnasium |
enumeration | DressingOrLockerOrFittingRoomCourtHouse |
enumeration | DressingOrLockerOrFittingRoomPerformingArtsTheatre |
enumeration | DressingOrLockerOrFittingRoomAuditorium |
enumeration | DressingOrLockerOrFittingRoomExerciseCenter |
enumeration | ElectricalOrMechanical |
enumeration | ElevatorLobbies |
enumeration | EmergencyHospitalOrHealthcare |
enumeration | EquipmentRoomManufacturingFacility |
enumeration | ExamOrTreatmentHospitalOrHealthcare |
enumeration | ExcerciseAreaExerciseCenter |
enumeration | ExcerciseAreaGymnasium |
enumeration | ExhibitSpaceConventionCenter |
enumeration | FellowshipHallReligiousBuildings |
enumeration | FineMaterialWarehouse |
enumeration | FineMerchandiseSalesAreaRetail |
enumeration | FireStationEngineRoomPoliceOrFireStation |
enumeration | FoodPreparation |
enumeration | GarageServiceOrRepairAutomotiveFacility |
enumeration | GeneralHighBayManufacturingFacility |
enumeration | GeneralLowBayManufacturingFacility |
enumeration | GeneralExhibitionMuseum |
enumeration | HospitalNurseryHospitalOrHealthcare |
enumeration | HospitalOrMedicalSuppliesHospitalOrHealthcare |
enumeration | HospitalOrRadiologyHospitalOrHealthcare |
enumeration | HotelOrConferenceCenterConferenceOrMeeting |
enumeration | InactiveStorage |
enumeration | JudgesChambersCourtHouse |
enumeration | LaboratoryOffice |
enumeration | LaundryIroningAndSorting |
enumeration | LaundryWashingHospitalOrHealthcare |
enumeration | LibraryAudioVisualLibraryAudioVisual |
enumeration | LivingQuartersDormitory |
enumeration | LivingQuartersMotel |
enumeration | LivingQuartersHotel |
enumeration | Lobby |
enumeration | LobbyReligiousBuildings |
enumeration | LobbyMotionPictureTheatre |
enumeration | LobbyAuditorium |
enumeration | LobbyPerformingArtsTheatre |
enumeration | LobbyPostOffice |
enumeration | LobbyHotel |
enumeration | LoungeOrRecreation |
enumeration | MallConcourseSalesAreaRetail |
enumeration | MassMerchandisingSalesAreaRetail |
enumeration | MediumOrBulkyMaterialWarehouse |
enumeration | MerchandisingSalesAreaRetail |
enumeration | MuseumAndGalleryStorage |
enumeration | NurseStationHospitalOrHealthcare |
enumeration | OfficeEnclosed |
enumeration | OfficeOpenPlan |
enumeration | OfficeCommonActivityAreasInactiveStorage |
enumeration | OperatingRoomHospitalOrHealthcare |
enumeration | OtherTelevisedPlayingAreaSportsArena |
enumeration | ParkingAreaAttendantOnlyParkingGarage |
enumeration | ParkingAreaPedestrianParkingGarage |
enumeration | PatientRoomHospitalOrHealthcare |
enumeration | PersonalServicesSalesAreaRetail |
enumeration | PharmacyHospitalOrHealthcare |
enumeration | PhysicalTherapyHospitalOrHealthcare |
enumeration | PlayingAreaGymnasium |
enumeration | Plenum |
enumeration | PoliceStationLaboratoryPoliceOrFireStations |
enumeration | PublicAndStaffLoungeHospitalOrHealthcare |
enumeration | ReadingAreaLibrary |
enumeration | ReceptionOrWaitingTransportation |
enumeration | ReceptionOrWaitingMotel |
enumeration | ReceptionOrWaitingHotel |
enumeration | RecoveryHospitalOrHealthcare |
enumeration | RestorationMuseum |
enumeration | Restrooms |
enumeration | RingSportsAreaSportsArena |
enumeration | ServerRoom |
enumeration | SleepingQuartersPoliceOrFireStation |
enumeration | SortingAreaPostOffice |
enumeration | SpecialtyStoreSalesAreaRetail |
enumeration | StacksLibrary |
enumeration | StairsInactive |
enumeration | Stairway |
enumeration | SupermarketSalesAreaRetail |
enumeration | TerminalTicketCounterTransportation |
enumeration | WorkshopWorkshop |
enumeration | WorshipPulpitChoirReligious |
annotation |
documentation
spaceType represents how a space is used.
appinfo
<xhtml:a href="http://206.55.31.90/cgi-bin/lpd/ShowSpaceTypes.pl">IfcPolyLoop</xhtml:a>, an IESNA and ASHRAE project for determining lighting power density for individual spaces.
source | <xsd:attribute name="spaceType" type="spaceTypeEnum"> <xsd:annotation> <xsd:documentation>spaceType represents how a space is used.</xsd:documentation> <xsd:appinfo> <xhtml:a href="http://206.55.31.90/cgi-bin/lpd/ShowSpaceTypes.pl">IfcPolyLoop</xhtml:a>, an IESNA and ASHRAE project for determining lighting power density for individual spaces. </xsd:appinfo> </xsd:annotation> </xsd:attribute>

attribute Space/@zoneIdRef

type | xsd:IDREF
source | <xsd:attribute name="zoneIdRef" type="xsd:IDREF"/>

attribute Space/@scheduleIdRef

type | xsd:IDREF
annotation |
documentation
ID for the schedule of transmittance of a shading surface
source | <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Space/@lightScheduleIdRef

type | xsd:IDREF
annotation |
documentation
ID of the schedule for lights contained in this space
source | <xsd:attribute name="lightScheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID of the schedule for lights contained in this space</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Space/@equipmentScheduleIdRef

type | xsd:IDREF
annotation |
documentation
ID for schedule of equipment use
source | <xsd:attribute name="equipmentScheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for schedule of equipment use</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Space/@peopleScheduleIdRef

type | xsd:IDREF
annotation |
documentation
ID for schedule of people in this space
source | <xsd:attribute name="peopleScheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for schedule of people in this space</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Space/@conditionType

type | conditionTypeEnum
facets |
Kind | Value | Annotation
enumeration | Heated |
enumeration | Cooled |
enumeration | HeatedAndCooled |
enumeration | Unconditioned |
enumeration | Vented |
enumeration | NaturallyVentedOnly |
source | <xsd:attribute name="conditionType" type="conditionTypeEnum"/>

attribute Space/@buildingStoreyIdRef

type | xsd:IDREF
annotation |
documentation
ID for BuildingStorey this space is on.
source | <xsd:attribute name="buildingStoreyIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for BuildingStorey this space is on.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Space/@ifcGUID

type | xsd:string
properties |
use | optional
annotation |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
source | <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Space/OccupantID

diagram |
type | xsd:IDREF
properties |
minOcc | 0
maxOcc | unbounded
content | simple
annotation |
documentation
Predefined occupants can be added to the space.
source | <xsd:element name="OccupantID" type="xsd:IDREF" minOccurs="0" maxOccurs="unbounded"> <xsd:annotation> <xsd:documentation>Predefined occupants can be added to the space.</xsd:documentation> </xsd:annotation> </xsd:element>

element SpaceBoundary

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | PlanarGeometry
used by |
elements | Building Space
attributes |
Name | Type | Use | Default | Fixed | Annotation
ifcGUID | xsd:string | optional |  |  |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
isSecondLevelBoundary | xsd:boolean | optional |  |  |
documentation
If this attribute is set to true, the boundary is important in heat flow calculation.
surfaceIdRef | xsd:IDREF | optional |  |  |
documentation
Connects the space boundary to a surface representing a building element (or representing the open air).
oppositeIdRef | xsd:IDREF | optional |  |  |
documentation
If surface referenced by SpaceBoundary is adjacent to two spaces, then this references the corresponding SpaceBoundary of the opposite space.
annotation |
documentation
This element establishes the logical relation of a given part of the space ShellGeometry such that its PlanarGeometry is part of an interior surface bounding the space.
source | <xsd:element name="SpaceBoundary"> <xsd:annotation> <xsd:documentation>This element establishes the logical relation of a given part of the space ShellGeometry such that its PlanarGeometry is part of an interior surface bounding the space.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice> <xsd:element ref="PlanarGeometry"/> </xsd:choice> <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="isSecondLevelBoundary" type="xsd:boolean" use="optional"> <xsd:annotation> <xsd:documentation>If this attribute is set to true, the boundary is important in heat flow calculation.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="surfaceIdRef" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Connects the space boundary to a surface representing a building element (or representing the open air).</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="oppositeIdRef" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>If surface referenced by SpaceBoundary is adjacent to two spaces, then this references the corresponding SpaceBoundary of the opposite space.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute SpaceBoundary/@ifcGUID

type | xsd:string
properties |
use | optional
annotation |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
source | <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute SpaceBoundary/@isSecondLevelBoundary

type | xsd:boolean
properties |
use | optional
annotation |
documentation
If this attribute is set to true, the boundary is important in heat flow calculation.
source | <xsd:attribute name="isSecondLevelBoundary" type="xsd:boolean" use="optional"> <xsd:annotation> <xsd:documentation>If this attribute is set to true, the boundary is important in heat flow calculation.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute SpaceBoundary/@surfaceIdRef

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Connects the space boundary to a surface representing a building element (or representing the open air).
source | <xsd:attribute name="surfaceIdRef" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Connects the space boundary to a surface representing a building element (or representing the open air).</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute SpaceBoundary/@oppositeIdRef

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
If surface referenced by SpaceBoundary is adjacent to two spaces, then this references the corresponding SpaceBoundary of the opposite space.
source | <xsd:attribute name="oppositeIdRef" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>If surface referenced by SpaceBoundary is adjacent to two spaces, then this references the corresponding SpaceBoundary of the opposite space.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element SpaceOccupancy

diagram |
namespace | http://www.gbxml.org/schema
type | SpaceOccupancyType
properties |
content | complex
children | SpaceCategory PercentTimePresence Duration
used by |
element | RandomMovementEvent
annotation |
documentation
Occupancy percentage of staying in a specific category in a building
source | <xsd:element name="SpaceOccupancy" type="SpaceOccupancyType"> <xsd:annotation> <xsd:documentation>Occupancy percentage of staying in a specific category in a building</xsd:documentation> </xsd:annotation> </xsd:element>

element SpecificHeat

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Fire Material
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | specificHeatUnitEnum | required |  |  |
source | <xsd:element name="SpecificHeat"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="specificHeatUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute SpecificHeat/@unit

type | specificHeatUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | JPerKgK |
enumeration | BTUPerLbF |
source | <xsd:attribute name="unit" type="specificHeatUnitEnum" use="required"/>

element StartDay

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Seasons/Season
source | <xsd:element name="StartDay" type="xsd:integer"/>

element StartHour

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | TimeofDay
source | <xsd:element name="StartHour" type="xsd:integer"/>

element StartMinute

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | TimeofDay
source | <xsd:element name="StartMinute" type="xsd:integer"/>

element StartMonth

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:integer
properties |
content | simple
used by |
element | Seasons/Season
source | <xsd:element name="StartMonth" type="xsd:integer"/>

element State

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | PersonInfo
source | <xsd:element name="State" type="xsd:string"/>

element StateOrProvince

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | Weather
source | <xsd:element name="StateOrProvince" type="xsd:string"/>

element StationId

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:string
properties |
content | complex
used by |
element | Location
attributes |
Name | Type | Use | Default | Fixed | Annotation
IDType | stationIdTypeEnum |  |  |  |
source | <xsd:element name="StationId"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:string"> <xsd:attribute name="IDType" type="stationIdTypeEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute StationId/@IDType

type | stationIdTypeEnum
facets |
Kind | Value | Annotation
enumeration | WMO |
documentation
A five-digit station identifier assigned by the World Meteorological Organization (WMO), used for international weather data exchange and station documentation.
enumeration | WBAN |
documentation
Weather-Bureau-Army-Navy station id. A five-digit station identifier used at National Climatic Data Center (NCDC) for digital data storage and general station identification purposes.
enumeration | ICAO |
documentation
A 4-letter indicator for geographical locations throughout the world, managed by the International Civil Aviation Organization (ICAO).
enumeration | NWSLI |
documentation
A 3- to 5-character alpha-numeric identifier assigned by the US National Weather Service (NWS), used for site identification in the NWS communications systems (e.g. AFOS, ROSA, SHEF, etc.).
enumeration | FAACallSign |
documentation
An alpha-numeric identifier of up to 4-characters managed by the USDT Federal Aviation Administration (FAA), used for site identification of airports, weather stations and other sites vital to navigation.
enumeration | COOP |
documentation
A 6-digit number identifying a station in the NWS Cooperative Network.
enumeration | Modeled |
documentation
A custom code identifying a virtual station for a particular grid location on the planet that was modeled by a simulation program such as MM5, WRF, or other weather simulation programs.
source | <xsd:attribute name="IDType" type="stationIdTypeEnum"/>

element StatusOfActivity

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | TimeFrequencyType ActivityOccurModel ActivityDuration
used by |
element | Activity
annotation |
documentation
Activity status in space level
source | <xsd:element name="StatusOfActivity"> <xsd:annotation> <xsd:documentation>Activity status in space level</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:sequence> <xsd:element ref="TimeFrequencyType"/> <xsd:element ref="ActivityOccurModel"/> <xsd:element ref="ActivityDuration" minOccurs="0"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element StatusTransitionEvent

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | StatusTransitionEventType EventOccurModel EventDuration
used by |
element | MovementBehavior
annotation |
documentation
Occupancy status and location change events in building level
source | <xsd:element name="StatusTransitionEvent"> <xsd:annotation> <xsd:documentation>Occupancy status and location change events in building level</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:sequence> <xsd:element ref="StatusTransitionEventType"/> <xsd:element ref="EventOccurModel"/> <xsd:element ref="EventDuration" minOccurs="0"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element StatusTransitionEventType

diagram |
namespace | http://www.gbxml.org/schema
type | statusTransitionEventType
properties |
content | simple
used by |
element | StatusTransitionEvent
facets |
Kind | Value | Annotation
enumeration | Arrival |
enumeration | Departure |
enumeration | ShortTermLeaving |
enumeration | ShortTermVisiting |
annotation |
documentation
The event type, e.g. arrival or departure
source | <xsd:element name="StatusTransitionEventType" type="statusTransitionEventType"> <xsd:annotation> <xsd:documentation>The event type, e.g. arrival or departure</xsd:documentation> </xsd:annotation> </xsd:element>

element StatusTransitionProbability

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Time Probability
used by |
complexType | CustomProbabilityModelType
source | <xsd:element name="StatusTransitionProbability"> <xsd:complexType> <xsd:sequence> <xsd:element name="Time" type="xsd:time"/> <xsd:element ref="Probability"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element StatusTransitionProbability/Time

diagram |
type | xsd:time
properties |
content | simple
source | <xsd:element name="Time" type="xsd:time"/>

element StDev

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
complexType | eqGaussianNormal1DType
source | <xsd:element name="StDev" type="xsd:decimal"/>

element StreetAddress

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | Building
source | <xsd:element name="StreetAddress" type="xsd:string"/>

element SubjectiveValues

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | PastExperience CostConscious EnvironmentAwareness TechnologyOriented Accommodating SocialInfluence
used by |
element | Occupant
annotation |
documentation
A specific belief can be assigned to each occupant.
source | <xsd:element name="SubjectiveValues"> <xsd:annotation> <xsd:documentation>A specific belief can be assigned to each occupant.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:sequence> <xsd:element ref="PastExperience" minOccurs="0"/> <xsd:element ref="CostConscious" minOccurs="0"/> <xsd:element ref="EnvironmentAwareness" minOccurs="0"/> <xsd:element ref="TechnologyOriented" minOccurs="0"/> <xsd:element ref="Accommodating" minOccurs="0"/> <xsd:element ref="SocialInfluence" minOccurs="0"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element SupplementalGasHeatingCoilEfficiency

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | AirLoopEquipment
annotation |
documentation
Supplemental heating coil efficiency
source | <xsd:element name="SupplementalGasHeatingCoilEfficiency" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Supplemental heating coil efficiency</xsd:documentation> </xsd:annotation> </xsd:element>

element SupplementalGasHeatingCoilParasiticElectricLoad

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | AirLoopEquipment
annotation |
documentation
Supplemental heating coil parasitic electric load
source | <xsd:element name="SupplementalGasHeatingCoilParasiticElectricLoad" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Supplemental heating coil parasitic electric load</xsd:documentation> </xsd:annotation> </xsd:element>

element SupplementalHeatingCoilCapacity

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | AirLoopEquipment
annotation |
documentation
Supplemental heating coil capacity.
source | <xsd:element name="SupplementalHeatingCoilCapacity" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Supplemental heating coil capacity.</xsd:documentation> </xsd:annotation> </xsd:element>

element SupplementalHeatingCoilType

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | AirLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | supplementalHeatingCoilTypeEnum |  |  |  |
source | <xsd:element name="SupplementalHeatingCoilType"> <xsd:complexType> <xsd:attribute name="unit" type="supplementalHeatingCoilTypeEnum"/> </xsd:complexType> </xsd:element>

attribute SupplementalHeatingCoilType/@unit

type | supplementalHeatingCoilTypeEnum
facets |
Kind | Value | Annotation
enumeration | Electric |
enumeration | Gas |
enumeration | HotWater |
source | <xsd:attribute name="unit" type="supplementalHeatingCoilTypeEnum"/>

element Surface

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description FamilyName AdjacentSpaceId RectangularGeometry PlanarGeometry Opening CADObjectId
used by |
element | Campus
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
surfaceType | surfaceTypeEnum | required |  |  |
constructionIdRef | xsd:IDREF | required |  |  |
documentation
Identifier pointing to a construction
scheduleShadeIdRef | xsd:IDREF |  |  |  |
documentation
ID for the schedule of transmittance of a shading surface
exposedToSun | xsd:boolean |  | true |  |
documentation
This attribute specifies whether or not direct beam radiation from the sun will ever hit this surface. Only relevant to exterior surface types.
ifcGUID | xsd:string | optional |  |  |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
source | <xsd:element name="Surface"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="FamilyName" minOccurs="0"/> <xsd:element ref="AdjacentSpaceId" minOccurs="1" maxOccurs="2"> <xsd:annotation> <xsd:documentation>First AdjacentSpaceId entered will determine how the referenced construction layers are ordered with the first construction layer being in contact with the outside or 2nd space listed and the last layer in contact with the first space listed. </xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element ref="RectangularGeometry"/> <xsd:element ref="PlanarGeometry"/> <xsd:element ref="Opening" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="CADObjectId" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="surfaceType" type="surfaceTypeEnum" use="required"/> <xsd:attribute name="constructionIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>Identifier pointing to a construction</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="scheduleShadeIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="exposedToSun" type="xsd:boolean" default="true"> <xsd:annotation> <xsd:documentation>This attribute specifies whether or not direct beam radiation from the sun will ever hit this surface. Only relevant to exterior surface types.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Surface/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Surface/@surfaceType

type | surfaceTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | InteriorWall |
documentation
The portion of the building envelope, including opaque area and fenestration, that is adjacent to two conditioned or unconditioned spaces and that is vertical or tilted at an angle of 60° from horizontal or greater.
enumeration | ExteriorWall |
documentation
The portion of the building envelope, including opaque area and fenestration, that is adjacent to one conditioned or unconditioned space and that is vertical or tilted at an angle of 60° from horizontal or greater.
enumeration | Roof |
documentation
The upper portion of the building envelope, including opaque areas and fenestration, that is adjacent to one conditioned or unconditioned space and that is horizontal or tilted at an angle of less than 60° from horizontal.
enumeration | InteriorFloor |
documentation
The lower portion of the building envelope, including opaque area and fenestration, that has conditioned or semiheated space above and is horizontal or tilted at an angle of less than 60 degrees from horizontal but excluding slab-on-grade floors.
enumeration | ExposedFloor |
documentation
The floor area exposed to non-conditioned space or outside.
enumeration | Shade |
documentation
Surface not adjacent to any spaces with tilt between 0° and 180°.
enumeration | UndergroundWall |
documentation
The portion of the building envelope, including opaque area and fenestration, that is adjacent to one conditioned or unconditioned space and earth (soil) and that is vertical or tilted at an angle of 60° from horizontal or greater.
enumeration | UndergroundSlab |
documentation
Surface adjacent to one conditioned or unconditioned space and earth (soil) below grade with a tilt between 150° and 180°.
enumeration | Ceiling |
documentation
The upper portion of the building envelope that is adjacent to two conditioned or unconditioned spaces and that is horizontal or tilted at an angle of less than 60° from horizontal.
enumeration | Air |
documentation
Air membrane between two conditioned or unconditioned spaces with a tilt between 0° and 180°.
enumeration | UndergroundCeiling |
documentation
The portion of the building envelope, including opaque area and fenestration, that is adjacent to one conditioned or unconditioned space and earth (soil) and that is horizontal or tilted at an angle of less than 60° from horizontal.
enumeration | RaisedFloor |
documentation
The lower portion of the building envelope, including opaque area and fenestration, that is adjacent to one conditioned or unconditioned space and the outside and is horizontal or tilted at an angle between 150° and 180°.
enumeration | SlabOnGrade |
documentation
The lower portion of the building envelope, including opaque area and fenestration, that is adjacent to one conditioned or unconditioned space and earth (soil) at grade with a tilt between 150° and 180°.
enumeration | FreestandingColumn |
documentation
Freestanding column in space specified by its top surface having the same ifcGUID.
enumeration | EmbeddedColumn |
documentation
Embedded column in wall specified by a surface which is coplanar with (one of) the embedding wall(s).
source | <xsd:attribute name="surfaceType" type="surfaceTypeEnum" use="required"/>

attribute Surface/@constructionIdRef

type | xsd:IDREF
properties |
use | required
annotation |
documentation
Identifier pointing to a construction
source | <xsd:attribute name="constructionIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>Identifier pointing to a construction</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Surface/@scheduleShadeIdRef

type | xsd:IDREF
annotation |
documentation
ID for the schedule of transmittance of a shading surface
source | <xsd:attribute name="scheduleShadeIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Surface/@exposedToSun

type | xsd:boolean
properties |
default | true
annotation |
documentation
This attribute specifies whether or not direct beam radiation from the sun will ever hit this surface. Only relevant to exterior surface types.
source | <xsd:attribute name="exposedToSun" type="xsd:boolean" default="true"> <xsd:annotation> <xsd:documentation>This attribute specifies whether or not direct beam radiation from the sun will ever hit this surface. Only relevant to exterior surface types.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Surface/@ifcGUID

type | xsd:string
properties |
use | optional
annotation |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
source | <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element TechnologyOriented

diagram |
namespace | http://www.gbxml.org/schema
type | subjectiveValueType
properties |
content | simple
used by |
element | SubjectiveValues
facets |
Kind | Value | Annotation
enumeration | High |
enumeration | Medium |
enumeration | Low |
source | <xsd:element name="TechnologyOriented" type="subjectiveValueType"/>

element Temp

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | AirLoopEquipment HydronicLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | temperatureUnitEnum |  |  |  |
tempType | tempTypeEnum | required |  |  |
annotation |
documentation
Temperature
source | <xsd:element name="Temp"> <xsd:annotation> <xsd:documentation>Temperature</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> <xsd:attribute name="tempType" type="tempTypeEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Temp/@unit

type | temperatureUnitEnum
facets |
Kind | Value | Annotation
enumeration | F |
enumeration | C |
enumeration | K |
enumeration | R |
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

attribute Temp/@tempType

type | tempTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Max |
enumeration | Min |
enumeration | Design |
enumeration | CoolDesign |
enumeration | HeatDesign |
enumeration | Throttle |
enumeration | Range |
enumeration | Approach |
enumeration | EnteringWetBulb |
enumeration | LeavingDryBulb |
enumeration | EnteringDryBulb |
enumeration | LeavingWetBulb |
enumeration | ChilledWaterSupply |
enumeration | CondenserWaterSupply |
enumeration | LeavingChilledWater |
enumeration | LeavingCondenserWater |
enumeration | HighTempLockout |
enumeration | LowTempLockout |
enumeration | EconomizerMaxLimitDewpoint |
enumeration | HeatPumpDefrostMaxOADryBulb |
enumeration | SupplementalHeatingCoilMaxOADryBulb |
enumeration | PreheatCoilDesignSetpoint |
source | <xsd:attribute name="tempType" type="tempTypeEnum" use="required"/>

element Temperature

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | CDD HDD Space
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | temperatureUnitEnum |  |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
source | <xsd:element name="Temperature"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Temperature/@unit

type | temperatureUnitEnum
facets |
Kind | Value | Annotation
enumeration | F |
enumeration | C |
enumeration | K |
enumeration | R |
source | <xsd:attribute name="unit" type="temperatureUnitEnum"/>

attribute Temperature/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element TemperatureControl

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | DesignTemp MinTemp MaxTemp ResetTemperature
used by |
elements | AirLoop HydronicLoop
annotation |
documentation
Use this element to describe how the temperature is controlled. The temperatures specified in this element should be measured just upstream of the most critical piece of equipment (air handlers for a chilled water and hot water loops the chiller for the cooling water loop).
source | <xsd:element name="TemperatureControl"> <xsd:annotation> <xsd:documentation>Use this element to describe how the temperature is controlled. The temperatures specified in this element should be measured just upstream of the most critical piece of equipment (air handlers for a chilled water and hot water loops the chiller for the cooling water loop).</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="DesignTemp" minOccurs="0"/> <xsd:element ref="MinTemp" minOccurs="0"/> <xsd:element ref="MaxTemp" minOccurs="0"/> <xsd:element ref="ResetTemperature" minOccurs="0"/> </xsd:choice> </xsd:complexType> </xsd:element>

element TemperatureProbabilityModel

diagram |
namespace | http://www.gbxml.org/schema
type | eqGaussianNormal1DType
properties |
content | complex
children | Description Mean StDev LowerBound UpperBound
used by |
elements | CoolingTemperature HeatingTemperature
source | <xsd:element name="TemperatureProbabilityModel" type="eqGaussianNormal1DType"/>

element Thermal

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | ASHRAEComfortTemperatures ASHRAEComfortEnvelope ASHRAECoolingAdaptiveComfort
used by |
element | Physical
source | <xsd:element name="Thermal"> <xsd:complexType> <xsd:choice> <xsd:element ref="ASHRAEComfortTemperatures"/> <xsd:element ref="ASHRAEComfortEnvelope" minOccurs="0"/> <xsd:element ref="ASHRAECoolingAdaptiveComfort" minOccurs="0"/> </xsd:choice> </xsd:complexType> </xsd:element>

element Thermostats

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | ThermostatType
used by |
element | BuildingSystems
source | <xsd:element name="Thermostats"> <xsd:complexType> <xsd:sequence> <xsd:element ref="ThermostatType"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element ThermostatType

diagram |
namespace | http://www.gbxml.org/schema
type | thermostatTypeEnum
properties |
content | simple
used by |
element | Thermostats
facets |
Kind | Value | Annotation
enumeration | Adjustable |
enumeration | Fixed |
source | <xsd:element name="ThermostatType" type="thermostatTypeEnum"/>

element Thickness

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Blind Fire Gap Glaze Material
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | lengthUnitEnum |  |  |  |
source | <xsd:element name="Thickness"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="lengthUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Thickness/@unit

type | lengthUnitEnum
facets |
Kind | Value | Annotation
enumeration | Kilometers |
enumeration | Meters |
enumeration | Centimeters |
enumeration | Millimeters |
enumeration | Miles |
enumeration | Yards |
enumeration | Feet |
enumeration | Inches |
source | <xsd:attribute name="unit" type="lengthUnitEnum"/>

element Tilt

diagram |
namespace | http://www.gbxml.org/schema
type | restriction of xsd:double
properties |
content | simple
used by |
element | RectangularGeometry
facets |
Kind | Value | Annotation
minInclusive | 0 |
maxInclusive | 180 |
annotation |
documentation
The number of degrees from up that the outside of the surface is tilted in relation to the bottom-left corner.
source | <xsd:element name="Tilt"> <xsd:annotation> <xsd:documentation>The number of degrees from up that the outside of the surface is tilted in relation to the bottom-left corner.</xsd:documentation> </xsd:annotation> <xsd:simpleType> <xsd:restriction base="xsd:double"> <xsd:minInclusive value="0"/> <xsd:maxInclusive value="180"/> </xsd:restriction> </xsd:simpleType> </xsd:element>

element Time

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | TimeofDay DayofWeek SeasonType
used by |
element | Drivers
annotation |
documentation
A time frame can be set when the specific behavior is expected to happen and when the environmental driver value is needed for simulation.
source | <xsd:element name="Time"> <xsd:annotation> <xsd:documentation>A time frame can be set when the specific behavior is expected to happen and when the environmental driver value is needed for simulation.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:sequence> <xsd:element ref="TimeofDay" minOccurs="0" maxOccurs="7"/> <xsd:element ref="DayofWeek" minOccurs="0" maxOccurs="11"/> <xsd:element ref="SeasonType" minOccurs="0" maxOccurs="5"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element TimeFrequencyType

diagram |
namespace | http://www.gbxml.org/schema
type | timeUnitEnum
properties |
content | simple
used by |
element | StatusOfActivity
facets |
Kind | Value | Annotation
enumeration | Year |
enumeration | Month |
enumeration | Week |
enumeration | Day |
enumeration | Hour |
enumeration | Minute |
annotation |
documentation
The event type, e.g. start and end
source | <xsd:element name="TimeFrequencyType" type="timeUnitEnum"> <xsd:annotation> <xsd:documentation>The event type, e.g. start and end</xsd:documentation> </xsd:annotation> </xsd:element>

element TimeIncrement

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
attributes |
Name | Type | Use | Default | Fixed | Annotation
timeUnit | timeUnitEnum | required |  |  |
annotation |
documentation
Time or period that results represent. Example: if timeType = Month and TimeIncrement = 1 the Value would be for the month of January or if timeType = Hour and TimeIncrement = 4 the 81st the Value would be for January 14 at noon.
source | <xsd:element name="TimeIncrement"> <xsd:annotation> <xsd:documentation>Time or period that results represent. Example: if timeType = Month and TimeIncrement = 1 the Value would be for the month of January or if timeType = Hour and TimeIncrement = 4 the 81st the Value would be for January 14 at noon.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="timeUnit" type="timeUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute TimeIncrement/@timeUnit

type | timeUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Year |
enumeration | Month |
enumeration | Week |
enumeration | Day |
enumeration | Hour |
enumeration | Minute |
source | <xsd:attribute name="timeUnit" type="timeUnitEnum" use="required"/>

element TimeofDay

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | StartHour StartMinute EndHour EndMinute
used by |
elements | Time TimeofDays
attributes |
Name | Type | Use | Default | Fixed | Annotation
Type | TimeofDayType | required |  |  |
source | <xsd:element name="TimeofDay"> <xsd:complexType> <xsd:all> <xsd:element ref="StartHour"/> <xsd:element ref="StartMinute"/> <xsd:element ref="EndHour"/> <xsd:element ref="EndMinute"/> </xsd:all> <xsd:attribute name="Type" type="TimeofDayType" use="required"/> </xsd:complexType> </xsd:element>

attribute TimeofDay/@Type

type | TimeofDayType
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Morning |
documentation
6am to 12pm
enumeration | Noon |
documentation
12pm
enumeration | Afternoon |
documentation
12pm to 6pm
enumeration | Evening |
documentation
6pm to 12am
enumeration | Day |
documentation
6am to 12am
enumeration | Night |
documentation
12am to 6am
enumeration | All |
source | <xsd:attribute name="Type" type="TimeofDayType" use="required"/>

element TimeofDays

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | TimeofDay
used by |
element | OccupantBehavior
source | <xsd:element name="TimeofDays"> <xsd:complexType> <xsd:sequence> <xsd:element ref="TimeofDay" maxOccurs="unbounded"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element Transmittance

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Blind Construction Glaze Material Opening WindowType
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | unitlessUnitEnum | required |  |  |
type | radiationWavelengthTypeEnum | required |  |  |
surfaceType | surfaceDescriptionEnum | required |  |  |
annotation |
documentation
Transmittance of shading surface
source | <xsd:element name="Transmittance"> <xsd:annotation> <xsd:documentation>Transmittance of shading surface</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> <xsd:attribute name="type" type="radiationWavelengthTypeEnum" use="required"/> <xsd:attribute name="surfaceType" type="surfaceDescriptionEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Transmittance/@unit

type | unitlessUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Percent |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

attribute Transmittance/@type

type | radiationWavelengthTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Solar |
enumeration | IR |
enumeration | Visible |
source | <xsd:attribute name="type" type="radiationWavelengthTypeEnum" use="required"/>

attribute Transmittance/@surfaceType

type | surfaceDescriptionEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | 1 |
documentation
The surfaceDescriptionEnum allows control over the specification of material surface properties. By setting the surfaceDescriptionEnum to 1, it is implied that the attribute (e.g. - Reflectance, Emittance, etc.) is associated with Surface 1 of the material's two surfaces [it is assumed that the material is a large planar object]. Surface 1 represents the surface that points away from the building interior.
enumeration | 2 |
documentation
The surfaceDescriptionEnum allows control over the specification of material surface properties. By setting the surfaceDescriptionEnum to 2, it is implied that the attribute (e.g. - Reflectance, Emittance, etc.) is associated with Surface 2 of the material's two surfaces [it is assumed that the material is a large planar object]. Surface 2 represents the surface that points towards the building interior.
enumeration | Both |
documentation
The surfaceDescriptionEnum allows control over the specification of material surface properties. By setting the surfaceDescriptionEnum to Both, it is implied that the attribute (e.g. - Reflectance, Emittance, etc.) is associated both Surface 1 and Surface 2 of the material's 2 surfaces [it is assumed that the material is a large planar object]. See the enumerations above for a description of Surface 1 and 2.
source | <xsd:attribute name="surfaceType" type="surfaceDescriptionEnum" use="required"/>

element Transportation

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | GeneralGeometry ShellGeometry Cost
used by |
element | Campus
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
transportationType | transportationTypeEnum | required |  |  |
scheduleIdRef | xsd:IDREF |  |  |  |
documentation
ID for the schedule of transmittance of a shading surface
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
annotation |
documentation
Public transportation
source | <xsd:element name="Transportation"> <xsd:annotation> <xsd:documentation>Public transportation</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="GeneralGeometry" minOccurs="0"/> <xsd:element ref="ShellGeometry" minOccurs="0"/> <xsd:element ref="Cost" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="transportationType" type="transportationTypeEnum" use="required"/> <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Transportation/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Transportation/@transportationType

type | transportationTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Bus |
enumeration | Train |
enumeration | Car |
enumeration | LightRail |
enumeration | Ferry |
enumeration | Airplane |
enumeration | Monorail |
enumeration | Bike |
source | <xsd:attribute name="transportationType" type="transportationTypeEnum" use="required"/>

attribute Transportation/@scheduleIdRef

type | xsd:IDREF
annotation |
documentation
ID for the schedule of transmittance of a shading surface
source | <xsd:attribute name="scheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID for the schedule of transmittance of a shading surface</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Transportation/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element TypeCode

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
elements | Space Zone
annotation |
documentation
User/project defined Code for Space or Zone.
source | <xsd:element name="TypeCode" type="xsd:string"> <xsd:annotation> <xsd:documentation>User/project defined Code for Space or Zone.</xsd:documentation> </xsd:annotation> </xsd:element>

element U-value

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Construction Opening WindowType
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | uValueUnitEnum | required |  |  |
annotation |
documentation
Overall conductance
source | <xsd:element name="U-value"> <xsd:annotation> <xsd:documentation>Overall conductance</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="uValueUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute U-value/@unit

type | uValueUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | WPerSquareMeterK |
enumeration | BtuPerHourSquareFtF |
source | <xsd:attribute name="unit" type="uValueUnitEnum" use="required"/>

element UpperBound

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
complexType | eqGaussianNormal1DType
source | <xsd:element name="UpperBound" type="xsd:decimal"/>

element UpperLimitValue

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | ScheduleTypeLimits
source | <xsd:element name="UpperLimitValue" type="xsd:decimal"/>

element URI

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | ProjectEntity
source | <xsd:element name="URI" type="xsd:string"/>

element UtilityRate

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | Meter
annotation |
documentation
We have left the UtilityRate element open to allow for use with billing schemas.
source | <xsd:element name="UtilityRate"> <xsd:annotation> <xsd:documentation>We have left the UtilityRate element open to allow for use with billing schemas.</xsd:documentation> </xsd:annotation> <xsd:complexType/> </xsd:element>

element Value

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:decimal
properties |
content | simple
used by |
element | Results
annotation |
documentation
Contains the actual numerical result value. If series result type each Value element contains the one value and is in sequential order for the series.
source | <xsd:element name="Value" type="xsd:decimal"> <xsd:annotation> <xsd:documentation>Contains the actual numerical result value. If series result type each Value element contains the one value and is in sequential order for the series.</xsd:documentation> </xsd:annotation> </xsd:element>

element Vegetation

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | GeneralGeometry ShellGeometry WaterRate BiomassDensity Cost
used by |
element | Campus
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
vegetationType | vegetationTypeEnum | required |  |  |
waterScheduleIdRef | xsd:IDREF |  |  |  |
waterMeterIdRef | xsd:IDREF |  |  |  |
shadeScheduleIdRef | xsd:IDREF |  |  |  |
documentation
Refers to a building-level surface.
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
annotation |
documentation
Plants, trees, etc. on a campus
source | <xsd:element name="Vegetation"> <xsd:annotation> <xsd:documentation>Plants, trees, etc. on a campus</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="GeneralGeometry" minOccurs="0"/> <xsd:element ref="ShellGeometry" minOccurs="0"/> <xsd:element ref="WaterRate" minOccurs="0"/> <xsd:element ref="BiomassDensity" minOccurs="0"/> <xsd:element ref="Cost" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="vegetationType" type="vegetationTypeEnum" use="required"/> <xsd:attribute name="waterScheduleIdRef" type="xsd:IDREF"/> <xsd:attribute name="waterMeterIdRef" type="xsd:IDREF"/> <xsd:attribute name="shadeScheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Refers to a building-level surface.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Vegetation/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Vegetation/@vegetationType

type | vegetationTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Trees |
enumeration | Bushes |
enumeration | Plants |
enumeration | Grass |
enumeration | Moss |
enumeration | EvergreenTrees |
enumeration | EvergreenShrubs |
enumeration | DeciduousTrees |
enumeration | DeciduousShrubs |
source | <xsd:attribute name="vegetationType" type="vegetationTypeEnum" use="required"/>

attribute Vegetation/@waterScheduleIdRef

type | xsd:IDREF
source | <xsd:attribute name="waterScheduleIdRef" type="xsd:IDREF"/>

attribute Vegetation/@waterMeterIdRef

type | xsd:IDREF
source | <xsd:attribute name="waterMeterIdRef" type="xsd:IDREF"/>

attribute Vegetation/@shadeScheduleIdRef

type | xsd:IDREF
annotation |
documentation
Refers to a building-level surface.
source | <xsd:attribute name="shadeScheduleIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Refers to a building-level surface.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Vegetation/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element Version

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | ProgramInfo
source | <xsd:element name="Version" type="xsd:string"/>

element Viscosity

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Gap
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | viscosityUnitEnum | required |  |  |
source | <xsd:element name="Viscosity"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="viscosityUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Viscosity/@unit

type | viscosityUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | KgPerMSec |
enumeration | PoundPerFootSec |
source | <xsd:attribute name="unit" type="viscosityUnitEnum" use="required"/>

element ViscosityFofT

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Gap
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | viscosityFofTUnitEnum | required |  |  |
annotation |
documentation
Viscosity as a function of temperature
source | <xsd:element name="ViscosityFofT"> <xsd:annotation> <xsd:documentation>Viscosity as a function of temperature</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="viscosityFofTUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute ViscosityFofT/@unit

type | viscosityFofTUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | KgPerMSecK |
enumeration | PoundPerFootSecF |
source | <xsd:attribute name="unit" type="viscosityFofTUnitEnum" use="required"/>

element Visual

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | ParameterRange
used by |
element | Physical
source | <xsd:element name="Visual"> <xsd:complexType> <xsd:sequence maxOccurs="unbounded"> <xsd:element ref="ParameterRange" maxOccurs="unbounded"> <xsd:annotation> <xsd:documentation>Range of indoor lighting and/or glare parameter values can be given where occupants do not feel visual discomfort and therefore, they don't carry out any actions. </xsd:documentation> </xsd:annotation> </xsd:element> </xsd:sequence> </xsd:complexType> </xsd:element>

element Volume

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Space
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | volumeUnitEnum |  |  |  |
annotation |
documentation
Specifies the volume of the space. This value should be equal to the volume enclosed by the actual physical boundaries of the space, as defined by the volumetric model's interior surfaces bounding that space.
source | <xsd:element name="Volume"> <xsd:annotation> <xsd:documentation>Specifies the volume of the space. This value should be equal to the volume enclosed by the actual physical boundaries of the space, as defined by the volumetric model's interior surfaces bounding that space.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="volumeUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Volume/@unit

type | volumeUnitEnum
facets |
Kind | Value | Annotation
enumeration | CubicKilometers |
enumeration | CubicMeters |
enumeration | CubicCentimeters |
enumeration | CubicMillimeters |
enumeration | CubicMiles |
enumeration | CubicYards |
enumeration | CubicFeet |
enumeration | CubicInches |
source | <xsd:attribute name="unit" type="volumeUnitEnum"/>

element WasteWaterHREff

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | ExtEquip IntEquip
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | unitlessUnitEnum | required |  |  |
airLoopIdRef | xsd:IDREF |  |  |  |
documentation
ID pointing to an air loop
hydronicLoopIdRef | xsd:IDREF |  |  |  |
documentation
ID pointing to a hydronic loop
annotation |
documentation
Waste water heat recovery efficiency
source | <xsd:element name="WasteWaterHREff"> <xsd:annotation> <xsd:documentation>Waste water heat recovery efficiency</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> <xsd:attribute name="airLoopIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID pointing to an air loop</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID pointing to a hydronic loop </xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute WasteWaterHREff/@unit

type | unitlessUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Percent |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

attribute WasteWaterHREff/@airLoopIdRef

type | xsd:IDREF
annotation |
documentation
ID pointing to an air loop
source | <xsd:attribute name="airLoopIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID pointing to an air loop</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute WasteWaterHREff/@hydronicLoopIdRef

type | xsd:IDREF
annotation |
documentation
ID pointing to a hydronic loop
source | <xsd:attribute name="hydronicLoopIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID pointing to a hydronic loop </xsd:documentation> </xsd:annotation> </xsd:attribute>

element WaterLoss

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | AirLoopEquipment
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | unitlessUnitEnum | required |  |  |
annotation |
documentation
This includes blowdown (draining a cooling tower to clean), drift (water loss from water sprayed), and evaporation in cooling towers.
source | <xsd:element name="WaterLoss"> <xsd:annotation> <xsd:documentation>This includes blowdown (draining a cooling tower to clean), drift (water loss from water sprayed), and evaporation in cooling towers.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute WaterLoss/@unit

type | unitlessUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Percent |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element WaterRate

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Vegetation
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | flowUnitEnum | required |  |  |
source | <xsd:element name="WaterRate"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="flowUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute WaterRate/@unit

type | flowUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | CFM |
enumeration | CubicMPerHr |
enumeration | LPerSec |
enumeration | LPM |
enumeration | GPH |
enumeration | GPM |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="flowUnitEnum" use="required"/>

element WaterUsePerCycle

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | ExtEquip IntEquip
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | waterUseUnitEnum | required |  |  |
annotation |
documentation
Amount of water used for water using equipment per cycle of operation.
source | <xsd:element name="WaterUsePerCycle"> <xsd:annotation> <xsd:documentation>Amount of water used for water using equipment per cycle of operation.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="waterUseUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute WaterUsePerCycle/@unit

type | waterUseUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | CubicMeters |
enumeration | Gallons |
enumeration | Tons |
enumeration | Kilograms |
enumeration | Liters |
source | <xsd:attribute name="unit" type="waterUseUnitEnum" use="required"/>

element Weather

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Location City StateOrProvince Country HDD CDD DDDBCool DDHiHrCool DDWBCool DDDBRangeCool DDLoHrCool DDPressureCool DDWindSpeedCool DDWindDirCool DDSkyClearnessCool DDRainCool DDSnowCool DDMonthCool DDDayCool DDDaylightCool DDGroundTCool DDDBHeat DDHiHrHeat DDWBHeat DDDBRangeHeat DDLoHrHeat DDPressureHeat DDWindSpeedHeat DDWindDirHeat DDSkyClearnessHeat DDRainHeat DDSnowHeat DDMonthHeat DDDayHeat DDDaylightHeat DDGroundTHeat GroundTemp WFTDTemp WFTDRelHumidity WFTDWindSpeed WFTDWindDir WFTDPressure Reference
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
source | <xsd:element name="Weather"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Location" minOccurs="1"/> <xsd:element ref="City" minOccurs="0"/> <xsd:element ref="StateOrProvince" minOccurs="0"/> <xsd:element ref="Country" minOccurs="0"/> <xsd:element ref="HDD" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="CDD" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="DDDBCool" minOccurs="0"/> <xsd:element ref="DDHiHrCool" minOccurs="0"/> <xsd:element ref="DDWBCool" minOccurs="0"/> <xsd:element ref="DDDBRangeCool" minOccurs="0"/> <xsd:element ref="DDLoHrCool" minOccurs="0"/> <xsd:element ref="DDPressureCool" minOccurs="0"/> <xsd:element ref="DDWindSpeedCool" minOccurs="0"/> <xsd:element ref="DDWindDirCool" minOccurs="0"/> <xsd:element ref="DDSkyClearnessCool" minOccurs="0"/> <xsd:element ref="DDRainCool" minOccurs="0"/> <xsd:element ref="DDSnowCool" minOccurs="0"/> <xsd:element ref="DDMonthCool" minOccurs="0"/> <xsd:element ref="DDDayCool" minOccurs="0"/> <xsd:element ref="DDDaylightCool" minOccurs="0"/> <xsd:element ref="DDGroundTCool" minOccurs="0"/> <xsd:element ref="DDDBHeat" minOccurs="0"/> <xsd:element ref="DDHiHrHeat" minOccurs="0"/> <xsd:element ref="DDWBHeat" minOccurs="0"/> <xsd:element ref="DDDBRangeHeat" minOccurs="0"/> <xsd:element ref="DDLoHrHeat" minOccurs="0"/> <xsd:element ref="DDPressureHeat" minOccurs="0"/> <xsd:element ref="DDWindSpeedHeat" minOccurs="0"/> <xsd:element ref="DDWindDirHeat" minOccurs="0"/> <xsd:element ref="DDSkyClearnessHeat" minOccurs="0"/> <xsd:element ref="DDRainHeat" minOccurs="0"/> <xsd:element ref="DDSnowHeat" minOccurs="0"/> <xsd:element ref="DDMonthHeat" minOccurs="0"/> <xsd:element ref="DDDayHeat" minOccurs="0"/> <xsd:element ref="DDDaylightHeat" minOccurs="0"/> <xsd:element ref="DDGroundTHeat" minOccurs="0"/> <xsd:element ref="GroundTemp" minOccurs="0"/> <xsd:element ref="WFTDTemp" minOccurs="0"/> <xsd:element ref="WFTDRelHumidity" minOccurs="0"/> <xsd:element ref="WFTDWindSpeed" minOccurs="0"/> <xsd:element ref="WFTDWindDir" minOccurs="0"/> <xsd:element ref="WFTDPressure" minOccurs="0"/> <xsd:element ref="Reference" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Weather/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Weather/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element WebPage

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | PersonInfo
source | <xsd:element name="WebPage" type="xsd:string"/>

element WeekSchedule

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Day
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
scheduleType | scheduleTypeEnum | required |  |  |
scheduleTypeLimitsId | xsd:string |  |  |  |
annotation |
documentation
Set of day schedules all assigned to a unique particular period of the week using the day type attribute. Do not schedule conflicting day types to the same week schedule.
source | <xsd:element name="WeekSchedule"> <xsd:annotation> <xsd:documentation>Set of day schedules all assigned to a unique particular period of the week using the day type attribute. Do not schedule conflicting day types to the same week schedule.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Day" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="scheduleType" type="scheduleTypeEnum" use="required"/> <xsd:attribute name="scheduleTypeLimitsId" type="xsd:string"/> </xsd:complexType> </xsd:element>

attribute WeekSchedule/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute WeekSchedule/@scheduleType

type | scheduleTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Temp |
enumeration | Fraction |
enumeration | OnOff |
enumeration | ResetTemp |
enumeration | ActivityLevel |
source | <xsd:attribute name="scheduleType" type="scheduleTypeEnum" use="required"/>

attribute WeekSchedule/@scheduleTypeLimitsId

type | xsd:string
source | <xsd:attribute name="scheduleTypeLimitsId" type="xsd:string"/>

element WeekScheduleId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | YearSchedule
attributes |
Name | Type | Use | Default | Fixed | Annotation
weekScheduleIdRef | xsd:IDREF | required |  |  |
source | <xsd:element name="WeekScheduleId"> <xsd:complexType> <xsd:attribute name="weekScheduleIdRef" type="xsd:IDREF" use="required"/> </xsd:complexType> </xsd:element>

attribute WeekScheduleId/@weekScheduleIdRef

type | xsd:IDREF
properties |
use | required
source | <xsd:attribute name="weekScheduleIdRef" type="xsd:IDREF" use="required"/>

element Weibull1D

diagram |
namespace | http://www.gbxml.org/schema
type | eqWeibull1D3P
properties |
content | complex
children | Description CoefficientA CoefficientB CoefficientC Parameter1ID
used by |
element | Formula
source | <xsd:element name="Weibull1D" type="eqWeibull1D3P"/>

element Weight

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | AirLoopEquipment ExtEquip HydronicLoopEquipment IntEquip
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | weightUnitEnum | required |  |  |
source | <xsd:element name="Weight"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="weightUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Weight/@unit

type | weightUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Pounds |
enumeration | Kilograms |
enumeration | Tons |
source | <xsd:attribute name="unit" type="weightUnitEnum" use="required"/>

element WFTDPressure

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | pressureUnitEnum | required |  |  |
annotation |
documentation
Wildfire threat design atomospheric pressure.
source | <xsd:element name="WFTDPressure"> <xsd:annotation> <xsd:documentation>Wildfire threat design atomospheric pressure.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="pressureUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute WFTDPressure/@unit

type | pressureUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | PSI |
enumeration | kPa |
enumeration | Atmospheres |
enumeration | InchesOfH2O |
enumeration | CentimetersOfH2O |
enumeration | InchesOfMercury |
enumeration | CentimetersOfMercury |
enumeration | MillimetersOfMercury |
enumeration | Pascals |
source | <xsd:attribute name="unit" type="pressureUnitEnum" use="required"/>

element WFTDRelHumidity

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | unitlessUnitEnum | required |  |  |
annotation |
documentation
Wildfire threat design relative humidity.
source | <xsd:element name="WFTDRelHumidity"> <xsd:annotation> <xsd:documentation>Wildfire threat design relative humidity.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute WFTDRelHumidity/@unit

type | unitlessUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Percent |
enumeration | Fraction |
source | <xsd:attribute name="unit" type="unitlessUnitEnum" use="required"/>

element WFTDTemp

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | temperatureUnitEnum | required |  |  |
annotation |
documentation
Wildfire threat design dry bulb temperature.
source | <xsd:element name="WFTDTemp"> <xsd:annotation> <xsd:documentation>Wildfire threat design dry bulb temperature.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="temperatureUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute WFTDTemp/@unit

type | temperatureUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | F |
enumeration | C |
enumeration | K |
enumeration | R |
source | <xsd:attribute name="unit" type="temperatureUnitEnum" use="required"/>

element WFTDWindDir

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | directionUnitEnum | required |  |  |
annotation |
documentation
Wildfire threat design wind direction
source | <xsd:element name="WFTDWindDir"> <xsd:annotation> <xsd:documentation>Wildfire threat design wind direction</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="directionUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute WFTDWindDir/@unit

type | directionUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | DegreeDecimalFromNorth |
source | <xsd:attribute name="unit" type="directionUnitEnum" use="required"/>

element WFTDWindSpeed

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | Weather
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | velocityUnitEnum | required |  |  |
annotation |
documentation
Wildfire threat design wind speed.
source | <xsd:element name="WFTDWindSpeed"> <xsd:annotation> <xsd:documentation>Wildfire threat design wind speed.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="velocityUnitEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute WFTDWindSpeed/@unit

type | velocityUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | MetersPerSecond |
enumeration | MilesPerHour |
enumeration | Knots |
source | <xsd:attribute name="unit" type="velocityUnitEnum" use="required"/>

element Width

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
elements | Dimensions Frame RectangularGeometry
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | lengthUnitEnum |  |  |  |
source | <xsd:element name="Width"> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="lengthUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute Width/@unit

type | lengthUnitEnum
facets |
Kind | Value | Annotation
enumeration | Kilometers |
enumeration | Meters |
enumeration | Centimeters |
enumeration | Millimeters |
enumeration | Miles |
enumeration | Yards |
enumeration | Feet |
enumeration | Inches |
source | <xsd:attribute name="unit" type="lengthUnitEnum"/>

element Windows

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | WindowTypeSimple
used by |
element | BuildingSystems
source | <xsd:element name="Windows"> <xsd:complexType> <xsd:sequence> <xsd:element ref="WindowTypeSimple"/> </xsd:sequence> </xsd:complexType> </xsd:element>

element WindowType

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description U-value ShadingCoeff SolarHeatGainCoeff Transmittance Reflectance Emittance Blind Frame Gap Glaze Cost ExtEquipId
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
windowTypeIsSchematic | xsd:boolean | optional |  |  |
DOELibIdRef | xsd:string |  |  |  |
documentation
Use this attribute to reference objects in the DOE2 library
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
annotation |
documentation
One WindowType should be created for each type of window. Create a Blind, Frame, and Cost for each OpeningType, and then add as many Glaze and Gaps as exist in the window. Place these Glaze and Gap elements in order from outside to inside. For instance, a two pane window will have Glaze Gap Glaze, where the first Glaze represents the outside surface.
source | <xsd:element name="WindowType"> <xsd:annotation> <xsd:documentation>One WindowType should be created for each type of window. Create a Blind, Frame, and Cost for each OpeningType, and then add as many Glaze and Gaps as exist in the window. Place these Glaze and Gap elements in order from outside to inside. For instance, a two pane window will have Glaze Gap Glaze, where the first Glaze represents the outside surface.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="U-value" minOccurs="0"/> <xsd:element ref="ShadingCoeff" minOccurs="0"/> <xsd:element ref="SolarHeatGainCoeff" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Transmittance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Reflectance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Emittance" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Blind" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Frame" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Gap" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Glaze" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="Cost" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="ExtEquipId" minOccurs="0" maxOccurs="1"> <xsd:annotation> <xsd:documentation>This element is for purposes of modeling BIPV (building integrated photovoltaics).</xsd:documentation> </xsd:annotation> </xsd:element> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="windowTypeIsSchematic" type="xsd:boolean" use="optional"/> <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute WindowType/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute WindowType/@windowTypeIsSchematic

type | xsd:boolean
properties |
use | optional
source | <xsd:attribute name="windowTypeIsSchematic" type="xsd:boolean" use="optional"/>

attribute WindowType/@DOELibIdRef

type | xsd:string
annotation |
documentation
Use this attribute to reference objects in the DOE2 library
source | <xsd:attribute name="DOELibIdRef" type="xsd:string"> <xsd:annotation> <xsd:documentation>Use this attribute to reference objects in the DOE2 library</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute WindowType/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element WindowTypeSimple

diagram |
namespace | http://www.gbxml.org/schema
type | windowTypeEnum
properties |
content | simple
used by |
element | Windows
facets |
Kind | Value | Annotation
enumeration | Operable |
enumeration | ContinuousControl |
enumeration | Fixed |
source | <xsd:element name="WindowTypeSimple" type="windowTypeEnum"/>

element WindSpeed

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | ExtEquip
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | velocityUnitEnum | required |  |  |
type | windSpeedEnum | required |  |  |
annotation |
documentation
Wind speed for wind turbine.
source | <xsd:element name="WindSpeed"> <xsd:annotation> <xsd:documentation>Wind speed for wind turbine.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="velocityUnitEnum" use="required"/> <xsd:attribute name="type" type="windSpeedEnum" use="required"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute WindSpeed/@unit

type | velocityUnitEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | MetersPerSecond |
enumeration | MilesPerHour |
enumeration | Knots |
source | <xsd:attribute name="unit" type="velocityUnitEnum" use="required"/>

attribute WindSpeed/@type

type | windSpeedEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | RatedWindSpeed |
enumeration | CutInWindSpeed |
enumeration | CutOutWindSpeed |
source | <xsd:attribute name="type" type="windSpeedEnum" use="required"/>

element XAxis

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | xsd:string | required |  |  |
dataType | xsd:string | required |  |  |
source | <xsd:element name="XAxis"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name"/> <xsd:element ref="Description" minOccurs="0"/> </xsd:choice> <xsd:attribute name="unit" type="xsd:string" use="required"/> <xsd:attribute name="dataType" type="xsd:string" use="required"/> </xsd:complexType> </xsd:element>

attribute XAxis/@unit

type | xsd:string
properties |
use | required
source | <xsd:attribute name="unit" type="xsd:string" use="required"/>

attribute XAxis/@dataType

type | xsd:string
properties |
use | required
source | <xsd:attribute name="dataType" type="xsd:string" use="required"/>

element YAxis

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | xsd:string | required |  |  |
dataType | xsd:string | required |  |  |
source | <xsd:element name="YAxis"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name"/> <xsd:element ref="Description" minOccurs="0"/> </xsd:choice> <xsd:attribute name="unit" type="xsd:string" use="required"/> <xsd:attribute name="dataType" type="xsd:string" use="required"/> </xsd:complexType> </xsd:element>

attribute YAxis/@unit

type | xsd:string
properties |
use | required
source | <xsd:attribute name="unit" type="xsd:string" use="required"/>

attribute YAxis/@dataType

type | xsd:string
properties |
use | required
source | <xsd:attribute name="dataType" type="xsd:string" use="required"/>

element YearModeled

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | BeginDate EndDate HolidaysModeled
used by |
element | Campus
annotation |
documentation
Year of simulation to use
source | <xsd:element name="YearModeled"> <xsd:annotation> <xsd:documentation>Year of simulation to use</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="2" maxOccurs="unbounded"> <xsd:element ref="BeginDate" minOccurs="1"/> <xsd:element ref="EndDate" minOccurs="1"/> <xsd:element ref="HolidaysModeled" maxOccurs="1"/> </xsd:choice> </xsd:complexType> </xsd:element>

element YearSchedule

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description BeginDate EndDate WeekScheduleId
used by |
element | Schedule
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
scheduleTypeLimitsId | xsd:string |  |  |  |
annotation |
documentation
Set of week schedules all assigned for a particular time period during the year defined by the begin and end date elements. These must not span more than one calendar year.
source | <xsd:element name="YearSchedule"> <xsd:annotation> <xsd:documentation>Set of week schedules all assigned for a particular time period during the year defined by the begin and end date elements. These must not span more than one calendar year.</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="BeginDate"/> <xsd:element ref="EndDate"/> <xsd:element ref="WeekScheduleId"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="scheduleTypeLimitsId" type="xsd:string"/> </xsd:complexType> </xsd:element>

attribute YearSchedule/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute YearSchedule/@scheduleTypeLimitsId

type | xsd:string
source | <xsd:attribute name="scheduleTypeLimitsId" type="xsd:string"/>

element ZipCode

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | PersonInfo
source | <xsd:element name="ZipCode" type="xsd:string"/>

element ZipcodeOrPostalCode

diagram |
namespace | http://www.gbxml.org/schema
type | xsd:string
properties |
content | simple
used by |
element | Location
source | <xsd:element name="ZipcodeOrPostalCode" type="xsd:string"/>

element Zone

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description Flow SecondaryFlow AirChangesPerHour FlowPerArea FlowPerPerson OAFlowPerArea OAFlowPerPerson OAFlowPerZone MaxOAFlowPerZone MinOAFlowPerZone MinimumOutdoorAirControlType DesignHeatT DesignCoolT DesignHeatRH DesignCoolRH IndoorAirQuality HydronicLoopId AirLoopId ZoneHVACEquipmentId CADObjectId TypeCode CoolingSizingFactor HeatingSizingFactor BaseboardHeatingType BaseboardHeatingCapacity
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
heatSchedIdRef | xsd:IDREF |  |  |  |
documentation
ID of heating schedule
coolSchedIdRef | xsd:IDREF |  |  |  |
documentation
Design temperature for cooling
outAirSchedIdRef | xsd:IDREF |  |  |  |
documentation
Outside air schedule ID
airChangesSchedIdRef | xsd:IDREF |  |  |  |
documentation
Air changes schedule ID
fanSchedIdRef | xsd:IDREF |  |  |  |
documentation
ID of the fan schedule for this zone
fanTempSchedIdRef | xsd:IDREF | optional |  |  |
documentation
ID of the fan temperature schedule for this zone
ifcGUID | xsd:string | optional |  |  |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
programId | xsd:IDREF | optional |  |  |
documentation
Please specify the program that added this element.
source | <xsd:element name="Zone"> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="Flow" minOccurs="0"/> <xsd:element ref="SecondaryFlow" minOccurs="0"/> <xsd:element ref="AirChangesPerHour" minOccurs="0"/> <xsd:element ref="FlowPerArea" minOccurs="0"/> <xsd:element ref="FlowPerPerson" minOccurs="0"/> <xsd:element ref="OAFlowPerArea" minOccurs="0"/> <xsd:element ref="OAFlowPerPerson" minOccurs="0"/> <xsd:element ref="OAFlowPerZone" minOccurs="0"/> <xsd:element ref="MaxOAFlowPerZone" minOccurs="0"/> <xsd:element ref="MinOAFlowPerZone" minOccurs="0"/> <xsd:element ref="MinimumOutdoorAirControlType" minOccurs="0"/> <xsd:element ref="DesignHeatT" minOccurs="0"/> <xsd:element ref="DesignCoolT" minOccurs="0"/> <xsd:element ref="DesignHeatRH" minOccurs="0"/> <xsd:element ref="DesignCoolRH" minOccurs="0"/> <xsd:element ref="IndoorAirQuality" minOccurs="0"/> <xsd:element ref="HydronicLoopId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="AirLoopId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="ZoneHVACEquipmentId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="CADObjectId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="TypeCode" minOccurs="0"/> <xsd:element ref="CoolingSizingFactor" minOccurs="0"/> <xsd:element ref="HeatingSizingFactor" minOccurs="0"/> <xsd:element ref="BaseboardHeatingType" minOccurs="0"/> <xsd:element ref="BaseboardHeatingCapacity" minOccurs="0"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="heatSchedIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID of heating schedule</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="coolSchedIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Design temperature for cooling</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="outAirSchedIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Outside air schedule ID</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="airChangesSchedIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Air changes schedule ID</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="fanSchedIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID of the fan schedule for this zone</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="fanTempSchedIdRef" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>ID of the fan temperature schedule for this zone</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute> <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute Zone/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute Zone/@heatSchedIdRef

type | xsd:IDREF
annotation |
documentation
ID of heating schedule
source | <xsd:attribute name="heatSchedIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID of heating schedule</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Zone/@coolSchedIdRef

type | xsd:IDREF
annotation |
documentation
Design temperature for cooling
source | <xsd:attribute name="coolSchedIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Design temperature for cooling</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Zone/@outAirSchedIdRef

type | xsd:IDREF
annotation |
documentation
Outside air schedule ID
source | <xsd:attribute name="outAirSchedIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Outside air schedule ID</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Zone/@airChangesSchedIdRef

type | xsd:IDREF
annotation |
documentation
Air changes schedule ID
source | <xsd:attribute name="airChangesSchedIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>Air changes schedule ID</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Zone/@fanSchedIdRef

type | xsd:IDREF
annotation |
documentation
ID of the fan schedule for this zone
source | <xsd:attribute name="fanSchedIdRef" type="xsd:IDREF"> <xsd:annotation> <xsd:documentation>ID of the fan schedule for this zone</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Zone/@fanTempSchedIdRef

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
ID of the fan temperature schedule for this zone
source | <xsd:attribute name="fanTempSchedIdRef" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>ID of the fan temperature schedule for this zone</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Zone/@ifcGUID

type | xsd:string
properties |
use | optional
annotation |
documentation
Global Unique ID from Industry Foundation Class (IFC) file.
source | <xsd:attribute name="ifcGUID" type="xsd:string" use="optional"> <xsd:annotation> <xsd:documentation>Global Unique ID from Industry Foundation Class (IFC) file.</xsd:documentation> </xsd:annotation> </xsd:attribute>

attribute Zone/@programId

type | xsd:IDREF
properties |
use | optional
annotation |
documentation
Please specify the program that added this element.
source | <xsd:attribute name="programId" type="xsd:IDREF" use="optional"> <xsd:annotation> <xsd:documentation>Please specify the program that added this element.</xsd:documentation> </xsd:annotation> </xsd:attribute>

element ZoneCoolingLoad

diagram |
namespace | http://www.gbxml.org/schema
type | extension of xsd:decimal
properties |
content | complex
used by |
element | ShadeControl
attributes |
Name | Type | Use | Default | Fixed | Annotation
unit | loadUnitEnum |  |  |  |
annotation |
documentation
Minimum cooling load that triggers the shades to close
source | <xsd:element name="ZoneCoolingLoad"> <xsd:annotation> <xsd:documentation>Minimum cooling load that triggers the shades to close</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:simpleContent> <xsd:extension base="xsd:decimal"> <xsd:attribute name="unit" type="loadUnitEnum"/> </xsd:extension> </xsd:simpleContent> </xsd:complexType> </xsd:element>

attribute ZoneCoolingLoad/@unit

type | loadUnitEnum
facets |
Kind | Value | Annotation
enumeration | BtuPerHour |
enumeration | Watt |
source | <xsd:attribute name="unit" type="loadUnitEnum"/>

element ZoneHVACEquipment

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
children | Name Description CADObjectId HydronicLoopId AirSystemId AnalysisParameter
used by |
element | gbXML
attributes |
Name | Type | Use | Default | Fixed | Annotation
id | xsd:ID | required |  |  |
zoneHVACEquipmentType | zoneHVACEquipmentTypeEnum | required |  |  |
heatingCoilType | heatingCoilTypeEnum | optional |  |  |
coolingCoilType | coolingCoilTypeEnum | optional |  |  |
drawVentilation | xsd:boolean | optional |  |  |
annotation |
documentation
Represents an early-stage equipment placeholder that provides heating or cooling to part of an air system or a water loop (EnergyPlus and Open Studio).
source | <xsd:element name="ZoneHVACEquipment"> <xsd:annotation> <xsd:documentation>Represents an early-stage equipment placeholder that provides heating or cooling to part of an air system or a water loop (EnergyPlus and Open Studio).</xsd:documentation> </xsd:annotation> <xsd:complexType> <xsd:choice minOccurs="0" maxOccurs="unbounded"> <xsd:element ref="Name" minOccurs="0"/> <xsd:element ref="Description" minOccurs="0"/> <xsd:element ref="CADObjectId" minOccurs="0"/> <xsd:element ref="HydronicLoopId" minOccurs="0" maxOccurs="unbounded"/> <xsd:element ref="AirSystemId" minOccurs="0"/> <xsd:element ref="AnalysisParameter" minOccurs="0" maxOccurs="unbounded"/> </xsd:choice> <xsd:attribute name="id" type="xsd:ID" use="required"/> <xsd:attribute name="zoneHVACEquipmentType" type="zoneHVACEquipmentTypeEnum" use="required"/> <xsd:attribute name="heatingCoilType" type="heatingCoilTypeEnum" use="optional"/> <xsd:attribute name="coolingCoilType" type="coolingCoilTypeEnum" use="optional"/> <xsd:attribute name="drawVentilation" type="xsd:boolean" use="optional"/> </xsd:complexType> </xsd:element>

attribute ZoneHVACEquipment/@id

type | xsd:ID
properties |
use | required
source | <xsd:attribute name="id" type="xsd:ID" use="required"/>

attribute ZoneHVACEquipment/@zoneHVACEquipmentType

type | zoneHVACEquipmentTypeEnum
properties |
use | required
facets |
Kind | Value | Annotation
enumeration | Undefined |
enumeration | UnConditioned |
enumeration | ChilledBeamActive |
enumeration | FourPipeFanCoil |
enumeration | PackagedTerminalAirConditioner |
enumeration | PackagedTerminalHeatPump |
enumeration | ParallelFanPoweredBox |
enumeration | VAVBox |
enumeration | BaseBoardConvective |
enumeration | BaseBoardRadiant |
enumeration | CAVBox |
enumeration | RadiantPanel |
enumeration | SeriesFanPoweredBox |
enumeration | UnitHeater |
enumeration | UnitVentilator |
enumeration | WaterSourceHeatPump |
enumeration | ChilledBeamPassive |
enumeration | VRFFanCoil |
source | <xsd:attribute name="zoneHVACEquipmentType" type="zoneHVACEquipmentTypeEnum" use="required"/>

attribute ZoneHVACEquipment/@heatingCoilType

type | heatingCoilTypeEnum
properties |
use | optional
facets |
Kind | Value | Annotation
enumeration | ElectricResistance |
enumeration | Furnace |
enumeration | HotWater |
source | <xsd:attribute name="heatingCoilType" type="heatingCoilTypeEnum" use="optional"/>

attribute ZoneHVACEquipment/@coolingCoilType

type | coolingCoilTypeEnum
properties |
use | optional
facets |
Kind | Value | Annotation
enumeration | ChilledWater |
enumeration | ChilledWaterDetailedFlatModel |
enumeration | DirectExpansion |
source | <xsd:attribute name="coolingCoilType" type="coolingCoilTypeEnum" use="optional"/>

attribute ZoneHVACEquipment/@drawVentilation

type | xsd:boolean
properties |
use | optional
source | <xsd:attribute name="drawVentilation" type="xsd:boolean" use="optional"/>

element ZoneHVACEquipmentId

diagram |
namespace | http://www.gbxml.org/schema
properties |
content | complex
used by |
element | Zone
attributes |
Name | Type | Use | Default | Fixed | Annotation
zoneHVACEquipmentIdRef | xsd:IDREF | required |  |  |
documentation
An unique identifier referencing a zone equipment.
source | <xsd:element name="ZoneHVACEquipmentId"> <xsd:complexType> <xsd:attribute name="zoneHVACEquipmentIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>An unique identifier referencing a zone equipment.</xsd:documentation> </xsd:annotation> </xsd:attribute> </xsd:complexType> </xsd:element>

attribute ZoneHVACEquipmentId/@zoneHVACEquipmentIdRef

type | xsd:IDREF
properties |
use | required
annotation |
documentation
An unique identifier referencing a zone equipment.
source | <xsd:attribute name="zoneHVACEquipmentIdRef" type="xsd:IDREF" use="required"> <xsd:annotation> <xsd:documentation>An unique identifier referencing a zone equipment.</xsd:documentation> </xsd:annotation> </xsd:attribute>

complexType CustomProbabilityModelType

diagram |
namespace | http://www.gbxml.org/schema
children | StatusTransitionProbability
used by |
element | CustomProbabilityModel
source | <xsd:complexType name="CustomProbabilityModelType"> <xsd:sequence> <xsd:element ref="StatusTransitionProbability" maxOccurs="unbounded"/> </xsd:sequence> </xsd:complexType>

complexType eqConstantValueType

diagram |
namespace | http://www.gbxml.org/schema
children | Description CoefficientA
used by |
element | ConstantValue
source | <xsd:complexType name="eqConstantValueType"> <xsd:sequence> <xsd:element name="Description" type="xsd:string" default="p=A" minOccurs="0"/> <xsd:element ref="CoefficientA"/> </xsd:sequence> </xsd:complexType>

element eqConstantValueType/Description

diagram |
type | xsd:string
properties |
minOcc | 0
maxOcc | 1
content | simple
default | p=A
source | <xsd:element name="Description" type="xsd:string" default="p=A" minOccurs="0"/>

complexType eqGaussianNormal1DType

diagram |
namespace | http://www.gbxml.org/schema
children | Description Mean StDev LowerBound UpperBound
used by |
element | TemperatureProbabilityModel
source | <xsd:complexType name="eqGaussianNormal1DType"> <xsd:sequence> <xsd:element name="Description" type="xsd:string" default="p=(1/sqrt(2*pi*StDev^2))^exp((-(x-Mean)^2)/(2*StDev^2)); where x is greater than the LowerBound and lower than the UpperBound" minOccurs="0"/> <xsd:element ref="Mean"/> <xsd:element ref="StDev"/> <xsd:element ref="LowerBound"/> <xsd:element ref="UpperBound"/> </xsd:sequence> </xsd:complexType>

element eqGaussianNormal1DType/Description

diagram |
type | xsd:string
properties |
minOcc | 0
maxOcc | 1
content | simple
default | p=(1/sqrt(2*pi*StDev^2))^exp((-(x-Mean)^2)/(2*StDev^2)); where x is greater than the LowerBound and lower than the UpperBound
source | <xsd:element name="Description" type="xsd:string" default="p=(1/sqrt(2*pi*StDev^2))^exp((-(x-Mean)^2)/(2*StDev^2)); where x is greater than the LowerBound and lower than the UpperBound" minOccurs="0"/>

complexType eqLinear1DType

diagram |
namespace | http://www.gbxml.org/schema
children | Description CoefficientA CoefficientB Parameter1ID
used by |
element | Linear1D
source | <xsd:complexType name="eqLinear1DType"> <xsd:sequence> <xsd:element name="Description" type="xsd:string" default="p=A*P1+B" minOccurs="0"/> <xsd:element ref="CoefficientA"/> <xsd:element ref="CoefficientB"/> <xsd:element ref="Parameter1ID"/> </xsd:sequence> </xsd:complexType>

element eqLinear1DType/Description

diagram |
type | xsd:string
properties |
minOcc | 0
maxOcc | 1
content | simple
default | p=A*P1+B
source | <xsd:element name="Description" type="xsd:string" default="p=A*P1+B" minOccurs="0"/>

complexType eqLinear2DType

diagram |
namespace | http://www.gbxml.org/schema
children | Description CoefficientA CoefficientB CoefficientC Parameter1ID Parameter2ID
used by |
element | Linear2D
source | <xsd:complexType name="eqLinear2DType"> <xsd:sequence> <xsd:element name="Description" type="xsd:string" default="p=A*P1+B*P2+C" minOccurs="0"/> <xsd:element ref="CoefficientA"/> <xsd:element ref="CoefficientB"/> <xsd:element ref="CoefficientC"/> <xsd:element ref="Parameter1ID"/> <xsd:element ref="Parameter2ID"/> </xsd:sequence> </xsd:complexType>

element eqLinear2DType/Description

diagram |
type | xsd:string
properties |
minOcc | 0
maxOcc | 1
content | simple
default | p=A*P1+B*P2+C
source | <xsd:element name="Description" type="xsd:string" default="p=A*P1+B*P2+C" minOccurs="0"/>

complexType eqLinear3DType

diagram |
namespace | http://www.gbxml.org/schema
children | Description CoefficientA CoefficientB CoefficientC CoefficientD Parameter1ID Parameter2ID Parameter3ID
used by |
element | Linear3D
source | <xsd:complexType name="eqLinear3DType"> <xsd:sequence> <xsd:element name="Description" type="xsd:string" default="p=A*P1+B*P2+C*P3+D" minOccurs="0"/> <xsd:element ref="CoefficientA"/> <xsd:element ref="CoefficientB"/> <xsd:element ref="CoefficientC"/> <xsd:element ref="CoefficientD"/> <xsd:element ref="Parameter1ID"/> <xsd:element ref="Parameter2ID"/> <xsd:element ref="Parameter3ID"/> </xsd:sequence> </xsd:complexType>

element eqLinear3DType/Description

diagram |
type | xsd:string
properties |
minOcc | 0
maxOcc | 1
content | simple
default | p=A*P1+B*P2+C*P3+D
source | <xsd:element name="Description" type="xsd:string" default="p=A*P1+B*P2+C*P3+D" minOccurs="0"/>

complexType eqLogit1DLinearType

diagram |
namespace | http://www.gbxml.org/schema
children | Description CoefficientA CoefficientB Parameter1ID
used by |
element | Logit1D
source | <xsd:complexType name="eqLogit1DLinearType"> <xsd:sequence> <xsd:element name="Description" default="log(p/(1-p)) = A*P1+B or p = exp(A*P1+B) / { exp(A*P1+B) + 1}" minOccurs="0"/> <xsd:element ref="CoefficientA"/> <xsd:element ref="CoefficientB"/> <xsd:element ref="Parameter1ID"/> </xsd:sequence> </xsd:complexType>

element eqLogit1DLinearType/Description

diagram |
properties |
minOcc | 0
maxOcc | 1
default | log(p/(1-p)) = A*P1+B or p = exp(A*P1+B) / { exp(A*P1+B) + 1}
source | <xsd:element name="Description" default="log(p/(1-p)) = A*P1+B or p = exp(A*P1+B) / { exp(A*P1+B) + 1}" minOccurs="0"/>

complexType eqLogit1DQuadraticType

diagram |
namespace | http://www.gbxml.org/schema
children | Description CoefficientA CoefficientB CoefficientC Parameter1ID
used by |
element | Logit1DQuadratic
source | <xsd:complexType name="eqLogit1DQuadraticType"> <xsd:sequence> <xsd:element name="Description" default="p = A + C / {1 + exp(-B*[log10(P1)-D]}" minOccurs="0"/> <xsd:element ref="CoefficientA"/> <xsd:element ref="CoefficientB"/> <xsd:element ref="CoefficientC"/> <xsd:element ref="Parameter1ID"/> </xsd:sequence> </xsd:complexType>

element eqLogit1DQuadraticType/Description

diagram |
properties |
minOcc | 0
maxOcc | 1
default | p = A + C / {1 + exp(-B*[log10(P1)-D]}
source | <xsd:element name="Description" default="p = A + C / {1 + exp(-B*[log10(P1)-D]}" minOccurs="0"/>

complexType eqLogit2DLinearType

diagram |
namespace | http://www.gbxml.org/schema
children | Description CoefficientA CoefficientB CoefficientC Parameter1ID Parameter2ID
used by |
element | Logit2D
source | <xsd:complexType name="eqLogit2DLinearType"> <xsd:sequence> <xsd:element name="Description" default="log(p/(1-p)) = A*P1+B*P2+C or p = exp(A*P1+B*P2+C) / { exp(A*P1+B*P2+C) + 1}" minOccurs="0"/> <xsd:element ref="CoefficientA"/> <xsd:element ref="CoefficientB"/> <xsd:element ref="CoefficientC"/> <xsd:element ref="Parameter1ID"/> <xsd:element ref="Parameter2ID"/> </xsd:sequence> </xsd:complexType>

element eqLogit2DLinearType/Description

diagram |
properties |
minOcc | 0
maxOcc | 1
default | log(p/(1-p)) = A*P1+B*P2+C or p = exp(A*P1+B*P2+C) / { exp(A*P1+B*P2+C) + 1}
source | <xsd:element name="Description" default="log(p/(1-p)) = A*P1+B*P2+C or p = exp(A*P1+B*P2+C) / { exp(A*P1+B*P2+C) + 1}" minOccurs="0"/>

complexType eqLogit3DLinearType

diagram |
namespace | http://www.gbxml.org/schema
children | Description CoefficientA CoefficientB CoefficientC CoefficientD Parameter1ID Parameter2ID Parameter3ID
used by |
element | Logit3D
source | <xsd:complexType name="eqLogit3DLinearType"> <xsd:sequence> <xsd:element name="Description" default="log(p/(1-p)) = A*P1+B*P2+C*P3+D or p = exp(A*P1+B*P2+C*P3+D) / { exp(A*P1+B*P2+C*P3+D) + 1}" minOccurs="0"/> <xsd:element ref="CoefficientA"/> <xsd:element ref="CoefficientB"/> <xsd:element ref="CoefficientC"/> <xsd:element ref="CoefficientD"/> <xsd:element ref="Parameter1ID"/> <xsd:element ref="Parameter2ID"/> <xsd:element ref="Parameter3ID"/> </xsd:sequence> </xsd:complexType>

element eqLogit3DLinearType/Description

diagram |
properties |
minOcc | 0
maxOcc | 1
default | log(p/(1-p)) = A*P1+B*P2+C*P3+D or p = exp(A*P1+B*P2+C*P3+D) / { exp(A*P1+B*P2+C*P3+D) + 1}
source | <xsd:element name="Description" default="log(p/(1-p)) = A*P1+B*P2+C*P3+D or p = exp(A*P1+B*P2+C*P3+D) / { exp(A*P1+B*P2+C*P3+D) + 1}" minOccurs="0"/>

complexType eqQuadratic1DType

diagram |
namespace | http://www.gbxml.org/schema
children | Description CoefficientA CoefficientB CoefficientC Parameter1ID
used by |
element | Quadratic1D
source | <xsd:complexType name="eqQuadratic1DType"> <xsd:sequence> <xsd:element name="Description" default="p=A*P1*P1+B*P1+C" minOccurs="0"/> <xsd:element ref="CoefficientA"/> <xsd:element ref="CoefficientB"/> <xsd:element ref="CoefficientC"/> <xsd:element ref="Parameter1ID"/> </xsd:sequence> </xsd:complexType>

element eqQuadratic1DType/Description

diagram |
properties |
minOcc | 0
maxOcc | 1
default | p=A*P1*P1+B*P1+C
source | <xsd:element name="Description" default="p=A*P1*P1+B*P1+C" minOccurs="0"/>

complexType eqWeibull1D3P

diagram |
namespace | http://www.gbxml.org/schema
children | Description CoefficientA CoefficientB CoefficientC Parameter1ID
used by |
element | Weibull1D
source | <xsd:complexType name="eqWeibull1D3P"> <xsd:sequence> <xsd:element name="Description" type="xsd:string" default="p=1-exp( - dT * ( (P1-A)/B)^C)) if (P1-A)/B is large than 0; p=0 if (P1-A)/B is less or equals to 0" minOccurs="0"/> <xsd:element ref="CoefficientA"/> <xsd:element ref="CoefficientB"/> <xsd:element ref="CoefficientC"/> <xsd:element ref="Parameter1ID"/> </xsd:sequence> </xsd:complexType>

element eqWeibull1D3P/Description

diagram |
type | xsd:string
properties |
minOcc | 0
maxOcc | 1
content | simple
default | p=1-exp( - dT * ( (P1-A)/B)^C)) if (P1-A)/B is large than 0; p=0 if (P1-A)/B is less or equals to 0
source | <xsd:element name="Description" type="xsd:string" default="p=1-exp( - dT * ( (P1-A)/B)^C)) if (P1-A)/B is large than 0; p=0 if (P1-A)/B is less or equals to 0" minOccurs="0"/>

complexType MarkovChainModelType

diagram |
namespace | http://www.gbxml.org/schema
children | EarlyOccurTime TypicalOccurTime
used by |
element | MarkovChainModel
source | <xsd:complexType name="MarkovChainModelType"> <xsd:sequence> <xsd:element name="EarlyOccurTime" type="xsd:time"> <xsd:annotation> <xsd:documentation>Earliest occurrence time of a status transition event</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="TypicalOccurTime" type="xsd:time"> <xsd:annotation> <xsd:documentation>Typical occurrence time of a status transition event</xsd:documentation> </xsd:annotation> </xsd:element> </xsd:sequence> </xsd:complexType>

element MarkovChainModelType/EarlyOccurTime

diagram |
type | xsd:time
properties |
content | simple
annotation |
documentation
Earliest occurrence time of a status transition event
source | <xsd:element name="EarlyOccurTime" type="xsd:time"> <xsd:annotation> <xsd:documentation>Earliest occurrence time of a status transition event</xsd:documentation> </xsd:annotation> </xsd:element>

element MarkovChainModelType/TypicalOccurTime

diagram |
type | xsd:time
properties |
content | simple
annotation |
documentation
Typical occurrence time of a status transition event
source | <xsd:element name="TypicalOccurTime" type="xsd:time"> <xsd:annotation> <xsd:documentation>Typical occurrence time of a status transition event</xsd:documentation> </xsd:annotation> </xsd:element>

complexType MeetingDurationProbabilityType

diagram |
namespace | http://www.gbxml.org/schema
children | MeetingDuration Probability
used by |
element | MeetingDurationProbability
source | <xsd:complexType name="MeetingDurationProbabilityType"> <xsd:sequence> <xsd:element ref="MeetingDuration"/> <xsd:element ref="Probability"/> </xsd:sequence> </xsd:complexType>

complexType NormalDurationModelType

diagram |
namespace | http://www.gbxml.org/schema
children | TypicalDuration MinimumDuration
used by |
element | NormalDurationModel
source | <xsd:complexType name="NormalDurationModelType"> <xsd:sequence> <xsd:element name="TypicalDuration" type="xsd:duration"/> <xsd:element name="MinimumDuration" type="xsd:duration"/> </xsd:sequence> </xsd:complexType>

element NormalDurationModelType/TypicalDuration

diagram |
type | xsd:duration
properties |
content | simple
source | <xsd:element name="TypicalDuration" type="xsd:duration"/>

element NormalDurationModelType/MinimumDuration

diagram |
type | xsd:duration
properties |
content | simple
source | <xsd:element name="MinimumDuration" type="xsd:duration"/>

complexType NormalProbabilityModelType

diagram |
namespace | http://www.gbxml.org/schema
children | EarlyOccurTime TypicalOccurTime
used by |
element | NormalProbabilityModel
source | <xsd:complexType name="NormalProbabilityModelType"> <xsd:sequence> <xsd:element name="EarlyOccurTime" type="xsd:time"> <xsd:annotation> <xsd:documentation>Earliest occurrence time of a status transition event. The duration between the early occur time and the typical occur time is 3 times of the standard deviation.</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="TypicalOccurTime" type="xsd:time"> <xsd:annotation> <xsd:documentation>Typical occurrence time of a status transition event, the mean of the distribution.</xsd:documentation> </xsd:annotation> </xsd:element> </xsd:sequence> </xsd:complexType>

element NormalProbabilityModelType/EarlyOccurTime

diagram |
type | xsd:time
properties |
content | simple
annotation |
documentation
Earliest occurrence time of a status transition event. The duration between the early occur time and the typical occur time is 3 times of the standard deviation.
source | <xsd:element name="EarlyOccurTime" type="xsd:time"> <xsd:annotation> <xsd:documentation>Earliest occurrence time of a status transition event. The duration between the early occur time and the typical occur time is 3 times of the standard deviation.</xsd:documentation> </xsd:annotation> </xsd:element>

element NormalProbabilityModelType/TypicalOccurTime

diagram |
type | xsd:time
properties |
content | simple
annotation |
documentation
Typical occurrence time of a status transition event, the mean of the distribution.
source | <xsd:element name="TypicalOccurTime" type="xsd:time"> <xsd:annotation> <xsd:documentation>Typical occurrence time of a status transition event, the mean of the distribution.</xsd:documentation> </xsd:annotation> </xsd:element>

complexType OperationRange

diagram |
namespace | http://www.gbxml.org/schema
children | ParameterID Min Max
used by |
elements | OperationSchedule/OperationRange ParameterRange
source | <xsd:complexType name="OperationRange"> <xsd:choice> <xsd:element name="ParameterID"/> <xsd:element name="Min" minOccurs="0"/> <xsd:element name="Max" minOccurs="0"/> </xsd:choice> </xsd:complexType>

element OperationRange/ParameterID

diagram |
source | <xsd:element name="ParameterID"/>

element OperationRange/Min

diagram |
properties |
minOcc | 0
maxOcc | 1
source | <xsd:element name="Min" minOccurs="0"/>

element OperationRange/Max

diagram |
properties |
minOcc | 0
maxOcc | 1
source | <xsd:element name="Max" minOccurs="0"/>

complexType SpaceOccupancyType

diagram |
namespace | http://www.gbxml.org/schema
children | SpaceCategory PercentTimePresence Duration
used by |
element | SpaceOccupancy
source | <xsd:complexType name="SpaceOccupancyType"> <xsd:all> <xsd:element name="SpaceCategory" type="SpaceCategory"> <xsd:annotation> <xsd:documentation>Space category for random movement events in a building</xsd:documentation> </xsd:annotation> </xsd:element> <xsd:element name="PercentTimePresence"> <xsd:annotation> <xsd:documentation>Percentage of time of staying in a specific space category</xsd:documentation> </xsd:annotation> <xsd:simpleType> <xsd:restriction base="xsd:decimal"> <xsd:minInclusive value="0"/> <xsd:maxInclusive value="100"/> </xsd:restriction> </xsd:simpleType> </xsd:element> <xsd:element name="Duration" type="xsd:duration"> <xsd:annotation> <xsd:documentation>Average duration of staying in a space category</xsd:documentation> </xsd:annotation> </xsd:element> </xsd:all> </xsd:complexType>

element SpaceOccupancyType/SpaceCategory

diagram |
type | SpaceCategory
properties |
content | simple
facets |
Kind | Value | Annotation
enumeration | OwnOffice |
enumeration | OtherOffice |
enumeration | MeetingRoom |
enumeration | AuxRoom |
documentation
All other rooms
enumeration | Outdoor |
annotation |
documentation
Space category for random movement events in a building
source | <xsd:element name="SpaceCategory" type="SpaceCategory"> <xsd:annotation> <xsd:documentation>Space category for random movement events in a building</xsd:documentation> </xsd:annotation> </xsd:element>

element SpaceOccupancyType/PercentTimePresence

diagram |
type | restriction of xsd:decimal
properties |
content | simple
facets |
Kind | Value | Annotation
minInclusive | 0 |
maxInclusive | 100 |
annotation |
documentation
Percentage of time of staying in a specific space category
source | <xsd:element name="PercentTimePresence"> <xsd:annotation> <xsd:documentation>Percentage of time of staying in a specific space category</xsd:documentation> </xsd:annotation> <xsd:simpleType> <xsd:restriction base="xsd:decimal"> <xsd:minInclusive value="0"/> <xsd:maxInclusive value="100"/> </xsd:restriction> </xsd:simpleType> </xsd:element>

element SpaceOccupancyType/Duration

diagram |
type | xsd:duration
properties |
content | simple
annotation |
documentation
Average duration of staying in a space category
source | <xsd:element name="Duration" type="xsd:duration"> <xsd:annotation> <xsd:documentation>Average duration of staying in a space category</xsd:documentation> </xsd:annotation> </xsd:element>

simpleType absorptanceUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Absorptance/@type
facets |
Kind | Value | Annotation
enumeration | IntIR |
enumeration | IntSolar |
enumeration | IntVisible |
enumeration | IntTotal |
enumeration | ExtIR |
enumeration | ExtSolar |
enumeration | ExtVisible |
enumeration | ExtTotal |
source | <xsd:simpleType name="absorptanceUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="IntIR"/> <xsd:enumeration value="IntSolar"/> <xsd:enumeration value="IntVisible"/> <xsd:enumeration value="IntTotal"/> <xsd:enumeration value="ExtIR"/> <xsd:enumeration value="ExtSolar"/> <xsd:enumeration value="ExtVisible"/> <xsd:enumeration value="ExtTotal"/> </xsd:restriction> </xsd:simpleType>

simpleType airTemperatureTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | AirTemperature/@type
facets |
Kind | Value | Annotation
enumeration | Outside |
enumeration | Zone |
source | <xsd:simpleType name="airTemperatureTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Outside"/> <xsd:enumeration value="Zone"/> </xsd:restriction> </xsd:simpleType>

simpleType areaUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | gbXML/@areaUnit Area/@unit
facets |
Kind | Value | Annotation
enumeration | SquareKilometers |
enumeration | SquareMeters |
enumeration | SquareCentimeters |
enumeration | SquareMillimeters |
enumeration | SquareMiles |
enumeration | SquareYards |
enumeration | SquareFeet |
enumeration | SquareInches |
source | <xsd:simpleType name="areaUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="SquareKilometers"/> <xsd:enumeration value="SquareMeters"/> <xsd:enumeration value="SquareCentimeters"/> <xsd:enumeration value="SquareMillimeters"/> <xsd:enumeration value="SquareMiles"/> <xsd:enumeration value="SquareYards"/> <xsd:enumeration value="SquareFeet"/> <xsd:enumeration value="SquareInches"/> </xsd:restriction> </xsd:simpleType>

simpleType baseboardHeatingTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | BaseboardHeatingType/@unit
facets |
Kind | Value | Annotation
enumeration | ACH |
enumeration | HotWater |
enumeration | Electric |
source | <xsd:simpleType name="baseboardHeatingTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="ACH"/> <xsd:enumeration value="HotWater"/> <xsd:enumeration value="Electric"/> </xsd:restriction> </xsd:simpleType>

simpleType blowerDoorUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | BlowerDoorValue/@unit
facets |
Kind | Value | Annotation
enumeration | ACH |
enumeration | AirChangesPerHour |
enumeration | SquareFeet |
enumeration | SquareMeter |
source | <xsd:simpleType name="blowerDoorUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="ACH"/> <xsd:enumeration value="AirChangesPerHour"/> <xsd:enumeration value="SquareFeet"/> <xsd:enumeration value="SquareMeter"/> </xsd:restriction> </xsd:simpleType>

simpleType buildingSystemTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
attribute | Behavior/@SystemType
facets |
Kind | Value | Annotation
enumeration | HVAC |
enumeration | Lights |
enumeration | Windows |
enumeration | PlugLoad |
enumeration | Thermostats |
enumeration | ShadesAndBlinds |
source | <xsd:simpleType name="buildingSystemTypeEnum"> <xsd:restriction base="xsd:string"> <xsd:enumeration value="HVAC"/> <xsd:enumeration value="Lights"/> <xsd:enumeration value="Windows"/> <xsd:enumeration value="PlugLoad"/> <xsd:enumeration value="Thermostats"/> <xsd:enumeration value="ShadesAndBlinds"/> </xsd:restriction> </xsd:simpleType>

simpleType buildingTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | Behavior/@AppliedBuildingType Building/@buildingType
facets |
Kind | Value | Annotation
enumeration | AutomotiveFacility |
enumeration | ConventionCenter |
enumeration | Courthouse |
enumeration | DataCenter |
enumeration | DiningBarLoungeOrLeisure |
enumeration | DiningCafeteriaFastFood |
enumeration | DiningFamily |
enumeration | Dormitory |
enumeration | ExerciseCenter |
enumeration | FireStation |
enumeration | Gymnasium |
enumeration | HospitalOrHealthcare |
enumeration | Hotel |
enumeration | Library |
enumeration | Manufacturing |
enumeration | Motel |
enumeration | MotionPictureTheatre |
enumeration | MultiFamily |
enumeration | Museum |
enumeration | Office |
enumeration | ParkingGarage |
enumeration | Penitentiary |
enumeration | PerformingArtsTheater |
enumeration | PoliceStation |
enumeration | PostOffice |
enumeration | ReligiousBuilding |
enumeration | Retail |
enumeration | SchoolOrUniversity |
enumeration | SingleFamily |
enumeration | SportsArena |
enumeration | TownHall |
enumeration | Transportation |
enumeration | Unknown |
documentation
Enumeration value to be used when there is no building type information available.
enumeration | Warehouse |
enumeration | Workshop |
annotation |
documentation
Use to specify the most predominant building use type.
source | <xsd:simpleType name="buildingTypeEnum"> <xsd:annotation> <xsd:documentation>Use to specify the most predominant building use type.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="AutomotiveFacility"/> <xsd:enumeration value="ConventionCenter"/> <xsd:enumeration value="Courthouse"/> <xsd:enumeration value="DataCenter"/> <xsd:enumeration value="DiningBarLoungeOrLeisure"/> <xsd:enumeration value="DiningCafeteriaFastFood"/> <xsd:enumeration value="DiningFamily"/> <xsd:enumeration value="Dormitory"/> <xsd:enumeration value="ExerciseCenter"/> <xsd:enumeration value="FireStation"/> <xsd:enumeration value="Gymnasium"/> <xsd:enumeration value="HospitalOrHealthcare"/> <xsd:enumeration value="Hotel"/> <xsd:enumeration value="Library"/> <xsd:enumeration value="Manufacturing"/> <xsd:enumeration value="Motel"/> <xsd:enumeration value="MotionPictureTheatre"/> <xsd:enumeration value="MultiFamily"/> <xsd:enumeration value="Museum"/> <xsd:enumeration value="Office"/> <xsd:enumeration value="ParkingGarage"/> <xsd:enumeration value="Penitentiary"/> <xsd:enumeration value="PerformingArtsTheater"/> <xsd:enumeration value="PoliceStation"/> <xsd:enumeration value="PostOffice"/> <xsd:enumeration value="ReligiousBuilding"/> <xsd:enumeration value="Retail"/> <xsd:enumeration value="SchoolOrUniversity"/> <xsd:enumeration value="SingleFamily"/> <xsd:enumeration value="SportsArena"/> <xsd:enumeration value="TownHall"/> <xsd:enumeration value="Transportation"/> <xsd:enumeration value="Unknown"> <xsd:annotation> <xsd:documentation>Enumeration value to be used when there is no building type information available.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Warehouse"/> <xsd:enumeration value="Workshop"/> </xsd:restriction> </xsd:simpleType>

simpleType capacityTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Capacity/@capacityType
facets |
Kind | Value | Annotation
enumeration | Heating |
enumeration | CoolingTotal |
enumeration | CoolingSensible |
enumeration | CoolingLatent |
enumeration | CoolingSHR |
enumeration | Volume |
source | <xsd:simpleType name="capacityTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Heating"/> <xsd:enumeration value="CoolingTotal"/> <xsd:enumeration value="CoolingSensible"/> <xsd:enumeration value="CoolingLatent"/> <xsd:enumeration value="CoolingSHR"/> <xsd:enumeration value="Volume"/> </xsd:restriction> </xsd:simpleType>

simpleType capacityUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Capacity/@unit
facets |
Kind | Value | Annotation
enumeration | Tons |
enumeration | kW |
enumeration | BtuPerHour |
enumeration | kBtuPerHour |
enumeration | Gallons |
enumeration | Liters |
enumeration | CubicMeters |
enumeration | CubicFeet |
source | <xsd:simpleType name="capacityUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Tons"/> <xsd:enumeration value="kW"/> <xsd:enumeration value="BtuPerHour"/> <xsd:enumeration value="kBtuPerHour"/> <xsd:enumeration value="Gallons"/> <xsd:enumeration value="Liters"/> <xsd:enumeration value="CubicMeters"/> <xsd:enumeration value="CubicFeet"/> </xsd:restriction> </xsd:simpleType>

simpleType chillerTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | HydronicLoop/@chillerType
facets |
Kind | Value | Annotation
enumeration | AirCooled |
enumeration | WaterCooled |
source | <xsd:simpleType name="chillerTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="AirCooled"/> <xsd:enumeration value="WaterCooled"/> </xsd:restriction> </xsd:simpleType>

simpleType ClimateZoneType

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | ClimateZone
facets |
Kind | Value | Annotation
enumeration | 1 |
enumeration | 2 |
enumeration | 3 |
enumeration | 4 |
enumeration | 5 |
enumeration | 6 |
enumeration | 7 |
source | <xsd:simpleType name="ClimateZoneType"> <xsd:restriction base="xsd:string"> <xsd:enumeration value="1"/> <xsd:enumeration value="2"/> <xsd:enumeration value="3"/> <xsd:enumeration value="4"/> <xsd:enumeration value="5"/> <xsd:enumeration value="6"/> <xsd:enumeration value="7"/> </xsd:restriction> </xsd:simpleType>

simpleType coilTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | HydronicLoopId/@coilType
facets |
Kind | Value | Annotation
enumeration | Preheat |
enumeration | Heating |
enumeration | Cooling |
source | <xsd:simpleType name="coilTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Preheat"/> <xsd:enumeration value="Heating"/> <xsd:enumeration value="Cooling"/> </xsd:restriction> </xsd:simpleType>

simpleType CommuteModeType

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | CommuteMode
facets |
Kind | Value | Annotation
enumeration | Walk |
enumeration | Cycle |
enumeration | Car |
enumeration | Transit |
source | <xsd:simpleType name="CommuteModeType"> <xsd:restriction base="xsd:string"> <xsd:enumeration value="Walk"/> <xsd:enumeration value="Cycle"/> <xsd:enumeration value="Car"/> <xsd:enumeration value="Transit"/> </xsd:restriction> </xsd:simpleType>

simpleType conditioningTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | DeltaP/@conditioningType DeltaT/@conditioningType Efficiency/@operationType
facets |
Kind | Value | Annotation
enumeration | Heating |
enumeration | Cooling |
enumeration | HeatingAndCooling |
source | <xsd:simpleType name="conditioningTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Heating"/> <xsd:enumeration value="Cooling"/> <xsd:enumeration value="HeatingAndCooling"/> </xsd:restriction> </xsd:simpleType>

simpleType conditioningUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | HighValue/@unit LowValue/@unit
facets |
Kind | Value | Annotation
enumeration | kBtu |
enumeration | Btu |
enumeration | kW |
enumeration | Tons |
source | <xsd:simpleType name="conditioningUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="kBtu"/> <xsd:enumeration value="Btu"/> <xsd:enumeration value="kW"/> <xsd:enumeration value="Tons"/> </xsd:restriction> </xsd:simpleType>

simpleType conditionTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Space/@conditionType
facets |
Kind | Value | Annotation
enumeration | Heated |
enumeration | Cooled |
enumeration | HeatedAndCooled |
enumeration | Unconditioned |
enumeration | Vented |
enumeration | NaturallyVentedOnly |
source | <xsd:simpleType name="conditionTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Heated"/> <xsd:enumeration value="Cooled"/> <xsd:enumeration value="HeatedAndCooled"/> <xsd:enumeration value="Unconditioned"/> <xsd:enumeration value="Vented"/> <xsd:enumeration value="NaturallyVentedOnly"/> </xsd:restriction> </xsd:simpleType>

simpleType conductivityFofTUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | ConductivityFofT/@unit
facets |
Kind | Value | Annotation
enumeration | WPerMSquareK |
enumeration | BtuPerHourFtSquareF |
source | <xsd:simpleType name="conductivityFofTUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="WPerMSquareK"/> <xsd:enumeration value="BtuPerHourFtSquareF"/> </xsd:restriction> </xsd:simpleType>

simpleType conductivityUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | Conductivity/@unit GlazeConductivity/@unit
facets |
Kind | Value | Annotation
enumeration | WPerCmC |
enumeration | WPerMeterK |
enumeration | BtuPerHourFtF |
source | <xsd:simpleType name="conductivityUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="WPerCmC"/> <xsd:enumeration value="WPerMeterK"/> <xsd:enumeration value="BtuPerHourFtF"/> </xsd:restriction> </xsd:simpleType>

simpleType controlTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Control/@controlType
facets |
Kind | Value | Annotation
enumeration | Boiler |
enumeration | Chiller |
enumeration | Damper |
enumeration | Fan |
enumeration | Pump |
enumeration | Valve |
source | <xsd:simpleType name="controlTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Boiler"/> <xsd:enumeration value="Chiller"/> <xsd:enumeration value="Damper"/> <xsd:enumeration value="Fan"/> <xsd:enumeration value="Pump"/> <xsd:enumeration value="Valve"/> </xsd:restriction> </xsd:simpleType>

simpleType coolingCoilSetpointResetTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | CoolingCoilSetpointResetType/@unit
facets |
Kind | Value | Annotation
enumeration | None |
enumeration | Warmest |
enumeration | OutdoorAirTemperatureReset |
enumeration | WarmestTemperatureFirst |
source | <xsd:simpleType name="coolingCoilSetpointResetTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="None"/> <xsd:enumeration value="Warmest"/> <xsd:enumeration value="OutdoorAirTemperatureReset"/> <xsd:enumeration value="WarmestTemperatureFirst"/> </xsd:restriction> </xsd:simpleType>

simpleType coolingCoilTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | AirSystem/@coolingCoilType ZoneHVACEquipment/@coolingCoilType CoolingCoilType/@unit
facets |
Kind | Value | Annotation
enumeration | ChilledWater |
enumeration | ChilledWaterDetailedFlatModel |
enumeration | DirectExpansion |
source | <xsd:simpleType name="coolingCoilTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="ChilledWater"/> <xsd:enumeration value="ChilledWaterDetailedFlatModel"/> <xsd:enumeration value="DirectExpansion"/> </xsd:restriction> </xsd:simpleType>

simpleType costTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Cost/@costType
facets |
Kind | Value | Annotation
enumeration | CO2 |
enumeration | SOx |
enumeration | NOx |
enumeration | EmbodiedEnergyTransportation |
enumeration | EmbodiedEnergyManufacture |
enumeration | EmbodiedEnergyInstallation |
enumeration | EmbodiedEnergyTotal |
enumeration | PurchaseCost |
enumeration | DeliveryCost |
enumeration | FirstCost |
enumeration | MonthlyCost |
enumeration | AnnualCost |
enumeration | MaintenanceCost |
enumeration | OverhaulCost |
enumeration | InstallationCost |
enumeration | ServiceFees |
source | <xsd:simpleType name="costTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="CO2"/> <xsd:enumeration value="SOx"/> <xsd:enumeration value="NOx"/> <xsd:enumeration value="EmbodiedEnergyTransportation"/> <xsd:enumeration value="EmbodiedEnergyManufacture"/> <xsd:enumeration value="EmbodiedEnergyInstallation"/> <xsd:enumeration value="EmbodiedEnergyTotal"/> <xsd:enumeration value="PurchaseCost"/> <xsd:enumeration value="DeliveryCost"/> <xsd:enumeration value="FirstCost"/> <xsd:enumeration value="MonthlyCost"/> <xsd:enumeration value="AnnualCost"/> <xsd:enumeration value="MaintenanceCost"/> <xsd:enumeration value="OverhaulCost"/> <xsd:enumeration value="InstallationCost"/> <xsd:enumeration value="ServiceFees"/> </xsd:restriction> </xsd:simpleType>

simpleType currencyTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | CostValue/@currency Results/@currency
facets |
Kind | Value | Annotation
enumeration | USDollars |
enumeration | CanadianDollars |
enumeration | Pesos |
enumeration | Euros |
enumeration | Yen |
enumeration | IndianRupee |
enumeration | Yuan |
enumeration | TaiwanDollar |
enumeration | EnglishPound |
enumeration | Mark |
enumeration | Franc |
enumeration | Ruble |
enumeration | Real |
enumeration | NewZealandDollar |
enumeration | AustralianDollar |
source | <xsd:simpleType name="currencyTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="USDollars"/> <xsd:enumeration value="CanadianDollars"/> <xsd:enumeration value="Pesos"/> <xsd:enumeration value="Euros"/> <xsd:enumeration value="Yen"/> <xsd:enumeration value="IndianRupee"/> <xsd:enumeration value="Yuan"/> <xsd:enumeration value="TaiwanDollar"/> <xsd:enumeration value="EnglishPound"/> <xsd:enumeration value="Mark"/> <xsd:enumeration value="Franc"/> <xsd:enumeration value="Ruble"/> <xsd:enumeration value="Real"/> <xsd:enumeration value="NewZealandDollar"/> <xsd:enumeration value="AustralianDollar"/> </xsd:restriction> </xsd:simpleType>

simpleType damperHeatingActionEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | DamperHeatingAction/@unit
facets |
Kind | Value | Annotation
enumeration | Normal |
enumeration | Reverse |
source | <xsd:simpleType name="damperHeatingActionEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Normal"/> <xsd:enumeration value="Reverse"/> </xsd:restriction> </xsd:simpleType>

simpleType dayTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
element | DayofWeek
attribute | Day/@dayType
facets |
Kind | Value | Annotation
enumeration | Weekday |
enumeration | Weekend |
enumeration | Holiday |
enumeration | WeekendOrHoliday |
enumeration | HeatingDesignDay |
enumeration | CoolingDesignDay |
enumeration | Sun |
enumeration | Mon |
enumeration | Tue |
enumeration | Wed |
enumeration | Thu |
enumeration | Fri |
enumeration | Sat |
enumeration | Custom |
enumeration | All |
source | <xsd:simpleType name="dayTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Weekday"/> <xsd:enumeration value="Weekend"/> <xsd:enumeration value="Holiday"/> <xsd:enumeration value="WeekendOrHoliday"/> <xsd:enumeration value="HeatingDesignDay"/> <xsd:enumeration value="CoolingDesignDay"/> <xsd:enumeration value="Sun"/> <xsd:enumeration value="Mon"/> <xsd:enumeration value="Tue"/> <xsd:enumeration value="Wed"/> <xsd:enumeration value="Thu"/> <xsd:enumeration value="Fri"/> <xsd:enumeration value="Sat"/> <xsd:enumeration value="Custom"/> <xsd:enumeration value="All"/> </xsd:restriction> </xsd:simpleType>

simpleType defrostControlEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | HeatPumpDefrostControl/@defrostControlType
facets |
Kind | Value | Annotation
enumeration | Timed |
enumeration | OnDemand |
source | <xsd:simpleType name="defrostControlEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Timed"/> <xsd:enumeration value="OnDemand"/> </xsd:restriction> </xsd:simpleType>

simpleType defrostStrategyEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | HeatPumpDefrostStrategy/@unit
facets |
Kind | Value | Annotation
enumeration | ReverseCycle |
enumeration | Resistive |
source | <xsd:simpleType name="defrostStrategyEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="ReverseCycle"/> <xsd:enumeration value="Resistive"/> </xsd:restriction> </xsd:simpleType>

simpleType deltaPUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | DeltaP/@unit
facets |
Kind | Value | Annotation
enumeration | PSI |
enumeration | kPa |
enumeration | Atmospheres |
enumeration | InchesOfH2O |
enumeration | CentimetersOfH2O |
enumeration | InchesOfMercury |
enumeration | CentimetersOfMercury |
enumeration | MillimetersOfMercury |
enumeration | Pascals |
source | <xsd:simpleType name="deltaPUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="PSI"/> <xsd:enumeration value="kPa"/> <xsd:enumeration value="Atmospheres"/> <xsd:enumeration value="InchesOfH2O"/> <xsd:enumeration value="CentimetersOfH2O"/> <xsd:enumeration value="InchesOfMercury"/> <xsd:enumeration value="CentimetersOfMercury"/> <xsd:enumeration value="MillimetersOfMercury"/> <xsd:enumeration value="Pascals"/> </xsd:restriction> </xsd:simpleType>

simpleType densityFofTUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | DensityFofT/@unit
facets |
Kind | Value | Annotation
enumeration | LbsPerCubicFtF |
enumeration | KgPerCubicMK |
source | <xsd:simpleType name="densityFofTUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="LbsPerCubicFtF"/> <xsd:enumeration value="KgPerCubicMK"/> </xsd:restriction> </xsd:simpleType>

simpleType densityUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | BiomassDensity/@unit Density/@unit
facets |
Kind | Value | Annotation
enumeration | GramsPerCubicCm |
enumeration | LbsPerCubicIn |
enumeration | LbsPerCubicFt |
enumeration | KgPerCubicM |
source | <xsd:simpleType name="densityUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="GramsPerCubicCm"/> <xsd:enumeration value="LbsPerCubicIn"/> <xsd:enumeration value="LbsPerCubicFt"/> <xsd:enumeration value="KgPerCubicM"/> </xsd:restriction> </xsd:simpleType>

simpleType directionUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | DDWindDirCool/@unit DDWindDirHeat/@unit WFTDWindDir/@unit
facets |
Kind | Value | Annotation
enumeration | DegreeDecimalFromNorth |
source | <xsd:simpleType name="directionUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="DegreeDecimalFromNorth"/> </xsd:restriction> </xsd:simpleType>

simpleType economizerLockoutEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | EconomizerLockout/@unit
facets |
Kind | Value | Annotation
enumeration | NoLockout |
enumeration | LockoutWithHeating |
enumeration | LockoutWithCompressor |
source | <xsd:simpleType name="economizerLockoutEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="NoLockout"/> <xsd:enumeration value="LockoutWithHeating"/> <xsd:enumeration value="LockoutWithCompressor"/> </xsd:restriction> </xsd:simpleType>

simpleType EducationType

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | Education
facets |
Kind | Value | Annotation
enumeration | High school |
enumeration | Bachelors |
enumeration | Post-graduate |
source | <xsd:simpleType name="EducationType"> <xsd:restriction base="xsd:string"> <xsd:enumeration value="High school"/> <xsd:enumeration value="Bachelors"/> <xsd:enumeration value="Post-graduate"/> </xsd:restriction> </xsd:simpleType>

simpleType efficiencyTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Efficiency/@efficiencyType
facets |
Kind | Value | Annotation
enumeration | COP |
documentation
Coefficient of Performance
enumeration | EER |
documentation
Energy Efficiency Ratio
enumeration | SEER |
documentation
Seasonal Energy Efficiency Ratio
enumeration | AFUE |
documentation
Annual Fuel Utilization Efficiency
enumeration | HSPF |
documentation
Heating Seasonal Performance Factor
enumeration | effectiveness |
enumeration | EnergyFactor |
enumeration | ThermalEff |
documentation
Thermal Efficiency
enumeration | MotorEff |
documentation
Motor Efficiency
enumeration | FanEff |
documentation
Fan Efficiency
enumeration | MechanicalEff |
documentation
Mechanical Efficiency
enumeration | BoilerEff |
documentation
Boiler Efficiency
enumeration | kWPerTon |
enumeration | kWPerkW |
enumeration | BTUPerHourPerF |
enumeration | kWPerC |
source | <xsd:simpleType name="efficiencyTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="COP"> <xsd:annotation> <xsd:documentation>Coefficient of Performance</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="EER"> <xsd:annotation> <xsd:documentation>Energy Efficiency Ratio</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="SEER"> <xsd:annotation> <xsd:documentation>Seasonal Energy Efficiency Ratio</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="AFUE"> <xsd:annotation> <xsd:documentation>Annual Fuel Utilization Efficiency</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="HSPF"> <xsd:annotation> <xsd:documentation>Heating Seasonal Performance Factor</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="effectiveness"/> <xsd:enumeration value="EnergyFactor"/> <xsd:enumeration value="ThermalEff"> <xsd:annotation> <xsd:documentation>Thermal Efficiency</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="MotorEff"> <xsd:annotation> <xsd:documentation>Motor Efficiency</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="FanEff"> <xsd:annotation> <xsd:documentation>Fan Efficiency</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="MechanicalEff"> <xsd:annotation> <xsd:documentation>Mechanical Efficiency</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="BoilerEff"> <xsd:annotation> <xsd:documentation>Boiler Efficiency</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="kWPerTon"/> <xsd:enumeration value="kWPerkW"/> <xsd:enumeration value="BTUPerHourPerF"/> <xsd:enumeration value="kWPerC"/> </xsd:restriction> </xsd:simpleType>

simpleType emissionUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | EmissionRate/@unit
facets |
Kind | Value | Annotation
enumeration | PoundsPerHour |
enumeration | KilogramsPerHour |
enumeration | GramsPerHour |
source | <xsd:simpleType name="emissionUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="PoundsPerHour"/> <xsd:enumeration value="KilogramsPerHour"/> <xsd:enumeration value="GramsPerHour"/> </xsd:restriction> </xsd:simpleType>

simpleType emittanceTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Emittance/@type
facets |
Kind | Value | Annotation
enumeration | IntIR |
enumeration | ExtIR |
source | <xsd:simpleType name="emittanceTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="IntIR"/> <xsd:enumeration value="ExtIR"/> </xsd:restriction> </xsd:simpleType>

simpleType EmploymentType

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | Employment
facets |
Kind | Value | Annotation
enumeration | Unemployed |
enumeration | Employed |
enumeration | Self-employed |
source | <xsd:simpleType name="EmploymentType"> <xsd:restriction base="xsd:string"> <xsd:enumeration value="Unemployed"/> <xsd:enumeration value="Employed"/> <xsd:enumeration value="Self-employed"/> </xsd:restriction> </xsd:simpleType>

simpleType energyUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | Energy/@unit Results/@unit
facets |
Kind | Value | Annotation
enumeration | KilowattHours |
enumeration | Joules |
enumeration | BTU |
enumeration | Therms |
source | <xsd:simpleType name="energyUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="KilowattHours"/> <xsd:enumeration value="Joules"/> <xsd:enumeration value="BTU"/> <xsd:enumeration value="Therms"/> </xsd:restriction> </xsd:simpleType>

simpleType enthalpyTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Enthalpy/@enthalpyType
facets |
Kind | Value | Annotation
enumeration | EconomizerUpperLimit |
enumeration | AirSideEconomizerMinSetpoint |
enumeration | EconomizerMaxLimit |
source | <xsd:simpleType name="enthalpyTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="EconomizerUpperLimit"/> <xsd:enumeration value="AirSideEconomizerMinSetpoint"/> <xsd:enumeration value="EconomizerMaxLimit"/> </xsd:restriction> </xsd:simpleType>

simpleType enthalpyUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Enthalpy/@unit
facets |
Kind | Value | Annotation
enumeration | BTUPerLb |
enumeration | KJPerKg |
source | <xsd:simpleType name="enthalpyUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="BTUPerLb"/> <xsd:enumeration value="KJPerKg"/> </xsd:restriction> </xsd:simpleType>

simpleType entityTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | GUID/@entity
facets |
Kind | Value | Annotation
enumeration | File |
enumeration | Model |
enumeration | Project |
enumeration | Run |
source | <xsd:simpleType name="entityTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="File"/> <xsd:enumeration value="Model"/> <xsd:enumeration value="Project"/> <xsd:enumeration value="Run"/> </xsd:restriction> </xsd:simpleType>

simpleType equipmentTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | AirLoopEquipment/@equipmentType
facets |
Kind | Value | Annotation
enumeration | Fan |
enumeration | HeatExchanger |
enumeration | Coil |
enumeration | Furnace |
enumeration | Evaporative |
enumeration | Radiant |
enumeration | Economizer |
enumeration | Duct |
enumeration | Humidifier |
enumeration | Dehumidifier |
enumeration | UnitaryAC |
enumeration | UnitaryHP |
enumeration | SplitAC |
enumeration | SplitHP |
enumeration | TerminalUnit |
enumeration | Register |
enumeration | VAVBox |
enumeration | EvaporativePreCooler |
enumeration | PreheatCoil |
source | <xsd:simpleType name="equipmentTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Fan"/> <xsd:enumeration value="HeatExchanger"/> <xsd:enumeration value="Coil"/> <xsd:enumeration value="Furnace"/> <xsd:enumeration value="Evaporative"/> <xsd:enumeration value="Radiant"/> <xsd:enumeration value="Economizer"/> <xsd:enumeration value="Duct"/> <xsd:enumeration value="Humidifier"/> <xsd:enumeration value="Dehumidifier"/> <xsd:enumeration value="UnitaryAC"/> <xsd:enumeration value="UnitaryHP"/> <xsd:enumeration value="SplitAC"/> <xsd:enumeration value="SplitHP"/> <xsd:enumeration value="TerminalUnit"/> <xsd:enumeration value="Register"/> <xsd:enumeration value="VAVBox"/> <xsd:enumeration value="EvaporativePreCooler"/> <xsd:enumeration value="PreheatCoil"/> </xsd:restriction> </xsd:simpleType>

simpleType extEquipTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | ExtEquip/@type
facets |
Kind | Value | Annotation
enumeration | Sprinkler |
enumeration | LawnMower |
enumeration | GeneralPlugload |
enumeration | Fountain |
enumeration | Refrigerator |
enumeration | Freezer |
enumeration | Pool |
enumeration | HotTub |
enumeration | Pump |
enumeration | Sauna |
enumeration | BatteryCharger |
enumeration | Furnace |
enumeration | IndustrialEquip |
enumeration | Irrigation |
enumeration | MiscEquip |
enumeration | Vending |
enumeration | Elevator |
enumeration | Escalator |
enumeration | WindTurbine |
enumeration | Photovoltaic |
enumeration | CogenDiesel |
enumeration | CogenFuelCell |
enumeration | CogenGasTurbine |
source | <xsd:simpleType name="extEquipTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Sprinkler"/> <xsd:enumeration value="LawnMower"/> <xsd:enumeration value="GeneralPlugload"/> <xsd:enumeration value="Fountain"/> <xsd:enumeration value="Refrigerator"/> <xsd:enumeration value="Freezer"/> <xsd:enumeration value="Pool"/> <xsd:enumeration value="HotTub"/> <xsd:enumeration value="Pump"/> <xsd:enumeration value="Sauna"/> <xsd:enumeration value="BatteryCharger"/> <xsd:enumeration value="Furnace"/> <xsd:enumeration value="IndustrialEquip"/> <xsd:enumeration value="Irrigation"/> <xsd:enumeration value="MiscEquip"/> <xsd:enumeration value="Vending"/> <xsd:enumeration value="Elevator"/> <xsd:enumeration value="Escalator"/> <xsd:enumeration value="WindTurbine"/> <xsd:enumeration value="Photovoltaic"/> <xsd:enumeration value="CogenDiesel"/> <xsd:enumeration value="CogenFuelCell"/> <xsd:enumeration value="CogenGasTurbine"/> </xsd:restriction> </xsd:simpleType>

simpleType fanTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Fan/@fanType
facets |
Kind | Value | Annotation
enumeration | ConstantVolume |
enumeration | VariableVolume |
source | <xsd:simpleType name="fanTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="ConstantVolume"/> <xsd:enumeration value="VariableVolume"/> </xsd:restriction> </xsd:simpleType>

simpleType floorCategoryEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | ManualJ8Parameters/@floorCategory
facets |
Kind | Value | Annotation
enumeration | OverEnclosedCrawlSpaceOrBasement |
enumeration | OverOpenCrawlSpaceOrGarage |
enumeration | Basement |
enumeration | SlabOnGrade |
annotation |
documentation
Used with the floorCategory attribute.
source | <xsd:simpleType name="floorCategoryEnum"> <xsd:annotation> <xsd:documentation>Used with the floorCategory attribute.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="OverEnclosedCrawlSpaceOrBasement"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="OverOpenCrawlSpaceOrGarage"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Basement"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="SlabOnGrade"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType floorSlabPerimeterHeatLossCoefficientUnitTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | FloorSlabHeatLossCoefficient/@floorSlabPerimeterHeatLossCoefficientUnitTypeEnum
facets |
Kind | Value | Annotation
enumeration | btuPerHourDegreeFPerLinearFoot |
enumeration | wattDegreeCPerLinearMeter |
annotation |
documentation
Used with the floorSlabPerimeterHeatLossCoefficientUnitType attribute.
source | <xsd:simpleType name="floorSlabPerimeterHeatLossCoefficientUnitTypeEnum"> <xsd:annotation> <xsd:documentation>Used with the floorSlabPerimeterHeatLossCoefficientUnitType attribute.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="btuPerHourDegreeFPerLinearFoot"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="wattDegreeCPerLinearMeter"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType flowPerAreaUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | FlowPerArea/@unit OAFlowPerArea/@unit
facets |
Kind | Value | Annotation
enumeration | CFMPerSquareFoot |
enumeration | LPerSecPerSquareM |
enumeration | CubicMPerSecPerSquareM |
enumeration | CubicMPerHourPerSquareM |
source | <xsd:simpleType name="flowPerAreaUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="CFMPerSquareFoot"/> <xsd:enumeration value="LPerSecPerSquareM"/> <xsd:enumeration value="CubicMPerSecPerSquareM"/> <xsd:enumeration value="CubicMPerHourPerSquareM"/> </xsd:restriction> </xsd:simpleType>

simpleType flowTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | FlowType/@flowType
facets |
Kind | Value | Annotation
enumeration | Series |
enumeration | Parallel |
enumeration | SeriesFromPlenum |
enumeration | ParallelFromPlenum |
source | <xsd:simpleType name="flowTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Series"/> <xsd:enumeration value="Parallel"/> <xsd:enumeration value="SeriesFromPlenum"/> <xsd:enumeration value="ParallelFromPlenum"/> </xsd:restriction> </xsd:simpleType>

simpleType flowUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | DesignFlow/@unit RecircFlow/@unit Flow/@unit FlowPerPerson/@unit MaxOAFlowPerZone/@unit MaximumFlow/@unit MinFlow/@unit MinimumFlow/@unit MinOAFlowPerZone/@unit OAFlowPerPerson/@unit OAFlowPerZone/@unit PeakDomesticHotWaterFlow/@unit RatedFlow/@unit Results/@unit SecondaryFlow/@unit WaterRate/@unit
facets |
Kind | Value | Annotation
enumeration | CFM |
enumeration | CubicMPerHr |
enumeration | LPerSec |
enumeration | LPM |
enumeration | GPH |
enumeration | GPM |
enumeration | Fraction |
source | <xsd:simpleType name="flowUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="CFM"/> <xsd:enumeration value="CubicMPerHr"/> <xsd:enumeration value="LPerSec"/> <xsd:enumeration value="LPM"/> <xsd:enumeration value="GPH"/> <xsd:enumeration value="GPM"/> <xsd:enumeration value="Fraction"/> </xsd:restriction> </xsd:simpleType>

simpleType fluidTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | HydronicLoop/@fluidType
facets |
Kind | Value | Annotation
enumeration | Water |
enumeration | Brine |
enumeration | Glycol |
enumeration | Refrigerant |
source | <xsd:simpleType name="fluidTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Water"/> <xsd:enumeration value="Brine"/> <xsd:enumeration value="Glycol"/> <xsd:enumeration value="Refrigerant"/> </xsd:restriction> </xsd:simpleType>

simpleType frameTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Frame/@type
facets |
Kind | Value | Annotation
enumeration | Wood |
enumeration | Vinyl |
enumeration | Aluminum |
enumeration | AluminumWithBreak |
enumeration | Insulated |
source | <xsd:simpleType name="frameTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Wood"/> <xsd:enumeration value="Vinyl"/> <xsd:enumeration value="Aluminum"/> <xsd:enumeration value="AluminumWithBreak"/> <xsd:enumeration value="Insulated"/> </xsd:restriction> </xsd:simpleType>

simpleType fuelLoadUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | FuelLoad/@unit
facets |
Kind | Value | Annotation
enumeration | BtuPerHour |
enumeration | kBtuPerHour |
enumeration | MBtuPerHour |
enumeration | Watts |
enumeration | kW |
source | <xsd:simpleType name="fuelLoadUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="BtuPerHour"/> <xsd:enumeration value="kBtuPerHour"/> <xsd:enumeration value="MBtuPerHour"/> <xsd:enumeration value="Watts"/> <xsd:enumeration value="kW"/> </xsd:restriction> </xsd:simpleType>

simpleType gasTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Gap/@gas
facets |
Kind | Value | Annotation
enumeration | Air |
enumeration | Argon |
enumeration | Krypton |
enumeration | CO2 |
enumeration | SF6 |
enumeration | Custom |
source | <xsd:simpleType name="gasTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Air"/> <xsd:enumeration value="Argon"/> <xsd:enumeration value="Krypton"/> <xsd:enumeration value="CO2"/> <xsd:enumeration value="SF6"/> <xsd:enumeration value="Custom"/> </xsd:restriction> </xsd:simpleType>

simpleType GenderType

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | Gender
facets |
Kind | Value | Annotation
enumeration | Male |
enumeration | Female |
source | <xsd:simpleType name="GenderType"> <xsd:restriction base="xsd:string"> <xsd:enumeration value="Male"/> <xsd:enumeration value="Female"/> </xsd:restriction> </xsd:simpleType>

simpleType GroupPriority

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | GroupPriority
facets |
Kind | Value | Annotation
enumeration | Majority |
documentation
If 50% or higher proportion of occupants would like to take the same action, then the action is trigerred.
source | <xsd:simpleType name="GroupPriority"> <xsd:restriction base="xsd:string"> <xsd:enumeration value="Majority"> <xsd:annotation> <xsd:documentation>If 50% or higher proportion of occupants would like to take the same action, then the action is trigerred.</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType heatExchangerTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | HeatExchanger/@heatExchangerType
facets |
Kind | Value | Annotation
enumeration | Enthalpy |
enumeration | Sensible |
source | <xsd:simpleType name="heatExchangerTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Enthalpy"/> <xsd:enumeration value="Sensible"/> </xsd:restriction> </xsd:simpleType>

simpleType heatingCoilSetpointResetTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | HeatingCoilSetpointResetType/@unit
facets |
Kind | Value | Annotation
enumeration | None |
enumeration | OutdoorAirTemperatureReset |
source | <xsd:simpleType name="heatingCoilSetpointResetTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="None"/> <xsd:enumeration value="OutdoorAirTemperatureReset"/> </xsd:restriction> </xsd:simpleType>

simpleType heatingCoilTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | AirSystem/@heatingCoilType ZoneHVACEquipment/@heatingCoilType AirSystem/@preheatCoilType
facets |
Kind | Value | Annotation
enumeration | ElectricResistance |
enumeration | Furnace |
enumeration | HotWater |
annotation |
documentation
The type of heating coil.
source | <xsd:simpleType name="heatingCoilTypeEnum"> <xsd:annotation> <xsd:documentation>The type of heating coil.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="ElectricResistance"/> <xsd:enumeration value="Furnace"/> <xsd:enumeration value="HotWater"/> </xsd:restriction> </xsd:simpleType>

simpleType heatRecoveryTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | HeatRecoveryType/@unit
facets |
Kind | Value | Annotation
enumeration | None |
enumeration | Sensible |
enumeration | Enthalpy |
source | <xsd:simpleType name="heatRecoveryTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="None"/> <xsd:enumeration value="Sensible"/> <xsd:enumeration value="Enthalpy"/> </xsd:restriction> </xsd:simpleType>

simpleType hOutsideUnitTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | HOutside/@hOutsideUnitTypeEnum
facets |
Kind | Value | Annotation
enumeration | BTUPerHourSquareFootDegreeF |
enumeration | WattsPerSecondSquareMeterDegreeC |
annotation |
documentation
Used with the hOutsideUnitType attribute.
source | <xsd:simpleType name="hOutsideUnitTypeEnum"> <xsd:annotation> <xsd:documentation>Used with the hOutsideUnitType attribute.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="BTUPerHourSquareFootDegreeF"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="WattsPerSecondSquareMeterDegreeC"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType HVACTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | HVACType
facets |
Kind | Value | Annotation
enumeration | ZoneOnOff |
annotation |
documentation
HVAC can be controlled in a continuous scale or on/off (1/0).
source | <xsd:simpleType name="HVACTypeEnum"> <xsd:annotation> <xsd:documentation>HVAC can be controlled in a continuous scale or on/off (1/0).</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:string"> <xsd:enumeration value="ZoneOnOff"/> </xsd:restriction> </xsd:simpleType>

simpleType hydronicEquipTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | HydronicLoopEquipment/@equipmentType
facets |
Kind | Value | Annotation
enumeration | Chiller |
enumeration | CoolingTower |
enumeration | Condenser |
enumeration | Boiler |
enumeration | HeatExchanger |
enumeration | Pump |
enumeration | RadiantPanel |
enumeration | HotWaterHeater |
enumeration | SolarPanels |
enumeration | Earth |
enumeration | Pipe |
enumeration | Storage |
enumeration | Coil |
enumeration | Radiator |
enumeration | TwoWayValve |
enumeration | ThreeWayValve |
source | <xsd:simpleType name="hydronicEquipTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Chiller"/> <xsd:enumeration value="CoolingTower"/> <xsd:enumeration value="Condenser"/> <xsd:enumeration value="Boiler"/> <xsd:enumeration value="HeatExchanger"/> <xsd:enumeration value="Pump"/> <xsd:enumeration value="RadiantPanel"/> <xsd:enumeration value="HotWaterHeater"/> <xsd:enumeration value="SolarPanels"/> <xsd:enumeration value="Earth"/> <xsd:enumeration value="Pipe"/> <xsd:enumeration value="Storage"/> <xsd:enumeration value="Coil"/> <xsd:enumeration value="Radiator"/> <xsd:enumeration value="TwoWayValve"/> <xsd:enumeration value="ThreeWayValve"/> </xsd:restriction> </xsd:simpleType>

simpleType illuminanceUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | Illuminance/@unit Results/@unit
facets |
Kind | Value | Annotation
enumeration | Footcandles |
enumeration | Lux |
enumeration | Phot |
source | <xsd:simpleType name="illuminanceUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Footcandles"/> <xsd:enumeration value="Lux"/> <xsd:enumeration value="Phot"/> </xsd:restriction> </xsd:simpleType>

simpleType IncomeGroupType

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | IncomeGroup
facets |
Kind | Value | Annotation
enumeration | 30,000 USD-50,000 USD |
enumeration | 51,000 USD-60,000 USD |
enumeration | 61,000 USD-80,000 USD |
enumeration | Greater than 80,000 USD |
source | <xsd:simpleType name="IncomeGroupType"> <xsd:restriction base="xsd:string"> <xsd:enumeration value="30,000 USD-50,000 USD"/> <xsd:enumeration value="51,000 USD-60,000 USD"/> <xsd:enumeration value="61,000 USD-80,000 USD"/> <xsd:enumeration value="Greater than 80,000 USD"/> </xsd:restriction> </xsd:simpleType>

simpleType infiltrationTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | InfiltrationFlow/@type
facets |
Kind | Value | Annotation
enumeration | Loose |
enumeration | Average |
enumeration | Tight |
source | <xsd:simpleType name="infiltrationTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Loose"/> <xsd:enumeration value="Average"/> <xsd:enumeration value="Tight"/> </xsd:restriction> </xsd:simpleType>

simpleType InfrastructureType

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | Infrastructure
facets |
Kind | Value | Annotation
enumeration | EV charging |
enumeration | Micro grid |
enumeration | Grid buyback |
source | <xsd:simpleType name="InfrastructureType"> <xsd:restriction base="xsd:string"> <xsd:enumeration value="EV charging"/> <xsd:enumeration value="Micro grid"/> <xsd:enumeration value="Grid buyback"/> </xsd:restriction> </xsd:simpleType>

simpleType intEquipTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | IntEquip/@type
facets |
Kind | Value | Annotation
enumeration | GeneralPlugload |
enumeration | Computer |
enumeration | Copier |
enumeration | Refrigerator |
enumeration | Stove |
enumeration | Cooktop |
enumeration | Fryer |
enumeration | Freezer |
enumeration | ClothesDryer |
enumeration | ClothesWasher |
enumeration | Dishwasher |
enumeration | TV |
enumeration | VCR |
enumeration | Microwave |
enumeration | Fan |
enumeration | AudioEquip |
enumeration | MiscEquip |
enumeration | Toilet |
enumeration | Urinal |
enumeration | Shower |
enumeration | Sink |
enumeration | Pool |
enumeration | HotTub |
enumeration | Sauna |
enumeration | BatteryCharger |
enumeration | Furnace |
enumeration | IndustrialEquip |
enumeration | Printer |
enumeration | Vending |
enumeration | Elevator |
enumeration | Escalator |
enumeration | GeneralLaundryEquip |
enumeration | GeneralKitchenEquip |
enumeration | GeneralMedicalEquip |
enumeration | GeneralOfficeEquip |
enumeration | GeneralEntertainmentEquip |
enumeration | GeneralRefrigerationEquip |
enumeration | GeneralFitnessEquip |
enumeration | GeneralVideoEquip |
enumeration | GeneralToilet |
source | <xsd:simpleType name="intEquipTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="GeneralPlugload"/> <xsd:enumeration value="Computer"/> <xsd:enumeration value="Copier"/> <xsd:enumeration value="Refrigerator"/> <xsd:enumeration value="Stove"/> <xsd:enumeration value="Cooktop"/> <xsd:enumeration value="Fryer"/> <xsd:enumeration value="Freezer"/> <xsd:enumeration value="ClothesDryer"/> <xsd:enumeration value="ClothesWasher"/> <xsd:enumeration value="Dishwasher"/> <xsd:enumeration value="TV"/> <xsd:enumeration value="VCR"/> <xsd:enumeration value="Microwave"/> <xsd:enumeration value="Fan"/> <xsd:enumeration value="AudioEquip"/> <xsd:enumeration value="MiscEquip"/> <xsd:enumeration value="Toilet"/> <xsd:enumeration value="Urinal"/> <xsd:enumeration value="Shower"/> <xsd:enumeration value="Sink"/> <xsd:enumeration value="Pool"/> <xsd:enumeration value="HotTub"/> <xsd:enumeration value="Sauna"/> <xsd:enumeration value="BatteryCharger"/> <xsd:enumeration value="Furnace"/> <xsd:enumeration value="IndustrialEquip"/> <xsd:enumeration value="Printer"/> <xsd:enumeration value="Vending"/> <xsd:enumeration value="Elevator"/> <xsd:enumeration value="Escalator"/> <xsd:enumeration value="GeneralLaundryEquip"/> <xsd:enumeration value="GeneralKitchenEquip"/> <xsd:enumeration value="GeneralMedicalEquip"/> <xsd:enumeration value="GeneralOfficeEquip"/> <xsd:enumeration value="GeneralEntertainmentEquip"/> <xsd:enumeration value="GeneralRefrigerationEquip"/> <xsd:enumeration value="GeneralFitnessEquip"/> <xsd:enumeration value="GeneralVideoEquip"/> <xsd:enumeration value="GeneralToilet"/> </xsd:restriction> </xsd:simpleType>

simpleType interactionType

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | InteractionType
attribute | Behavior/@ActionType
facets |
Kind | Value | Annotation
enumeration | TurnOn |
documentation
Set the value of a parameter to 1.
enumeration | TurnOff |
documentation
Set the value of a parameter to 0.
enumeration | SetToControlValue |
documentation
Set the value of a parameter to a desired value when event occurs.
annotation |
documentation
There are three types of interactions: TurnOn: set the value of a parameter to 1; TurnOff: set the value of a parameter to 0; and SetToControlValue: set the value of a parameter to a desired value.
source | <xsd:simpleType name="interactionType"> <xsd:annotation> <xsd:documentation>There are three types of interactions: TurnOn: set the value of a parameter to 1; TurnOff: set the value of a parameter to 0; and SetToControlValue: set the value of a parameter to a desired value.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:string"> <xsd:enumeration value="TurnOn"> <xsd:annotation> <xsd:documentation>Set the value of a parameter to 1.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="TurnOff"> <xsd:annotation> <xsd:documentation>Set the value of a parameter to 0.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="SetToControlValue"> <xsd:annotation> <xsd:documentation>Set the value of a parameter to a desired value when event occurs.</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType inverseTempUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | PrandtlNumberFofT/@unit
facets |
Kind | Value | Annotation
enumeration | PerK |
enumeration | PerF |
source | <xsd:simpleType name="inverseTempUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="PerK"/> <xsd:enumeration value="PerF"/> </xsd:restriction> </xsd:simpleType>

simpleType JobType

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | JobType
facets |
Kind | Value | Annotation
enumeration | Regular staff |
enumeration | Researcher |
enumeration | Administrator |
enumeration | Manager |
enumeration | Contractor |
source | <xsd:simpleType name="JobType"> <xsd:restriction base="xsd:string"> <xsd:enumeration value="Regular staff"/> <xsd:enumeration value="Researcher"/> <xsd:enumeration value="Administrator"/> <xsd:enumeration value="Manager"/> <xsd:enumeration value="Contractor"/> </xsd:restriction> </xsd:simpleType>

simpleType lengthUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | gbXML/@lengthUnit Elevation/@unit Height/@unit Length/@unit Level/@unit PlanarGeometry/@unit RectangularGeometry/@unit Setback/@unit ShellGeometry/@unit Thickness/@unit Width/@unit
facets |
Kind | Value | Annotation
enumeration | Kilometers |
enumeration | Meters |
enumeration | Centimeters |
enumeration | Millimeters |
enumeration | Miles |
enumeration | Yards |
enumeration | Feet |
enumeration | Inches |
source | <xsd:simpleType name="lengthUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Kilometers"/> <xsd:enumeration value="Meters"/> <xsd:enumeration value="Centimeters"/> <xsd:enumeration value="Millimeters"/> <xsd:enumeration value="Miles"/> <xsd:enumeration value="Yards"/> <xsd:enumeration value="Feet"/> <xsd:enumeration value="Inches"/> </xsd:restriction> </xsd:simpleType>

simpleType LifeStyleType

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | LifeStyle
facets |
Kind | Value | Annotation
enumeration | Austerity |
enumeration | Luxury |
enumeration | Norm |
source | <xsd:simpleType name="LifeStyleType"> <xsd:restriction base="xsd:string"> <xsd:enumeration value="Austerity"/> <xsd:enumeration value="Luxury"/> <xsd:enumeration value="Norm"/> </xsd:restriction> </xsd:simpleType>

simpleType lifeUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Life/@unit
facets |
Kind | Value | Annotation
enumeration | Months |
enumeration | Years |
enumeration | Cycles |
enumeration | MillionCycles |
source | <xsd:simpleType name="lifeUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Months"/> <xsd:enumeration value="Years"/> <xsd:enumeration value="Cycles"/> <xsd:enumeration value="MillionCycles"/> </xsd:restriction> </xsd:simpleType>

simpleType lightControlTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | LightingControl/@type
facets |
Kind | Value | Annotation
enumeration | Continuous |
enumeration | OnOff |
enumeration | Stepped2 |
enumeration | Stepped3 |
enumeration | Stepped4 |
enumeration | Stepped5 |
enumeration | Stepped6 |
enumeration | Stepped7 |
enumeration | Stepped8 |
enumeration | Stepped9 |
enumeration | Stepped10 |
enumeration | Stepped11 |
enumeration | Stepped12 |
enumeration | Stepped13 |
enumeration | Stepped14 |
enumeration | Stepped15 |
enumeration | Stepped16 |
enumeration | Stepped17 |
enumeration | Stepped18 |
enumeration | Stepped19 |
enumeration | Stepped20 |
enumeration | ContinuousOff |
enumeration | MotionSensor |
enumeration | Photocell |
source | <xsd:simpleType name="lightControlTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Continuous"/> <xsd:enumeration value="OnOff"/> <xsd:enumeration value="Stepped2"/> <xsd:enumeration value="Stepped3"/> <xsd:enumeration value="Stepped4"/> <xsd:enumeration value="Stepped5"/> <xsd:enumeration value="Stepped6"/> <xsd:enumeration value="Stepped7"/> <xsd:enumeration value="Stepped8"/> <xsd:enumeration value="Stepped9"/> <xsd:enumeration value="Stepped10"/> <xsd:enumeration value="Stepped11"/> <xsd:enumeration value="Stepped12"/> <xsd:enumeration value="Stepped13"/> <xsd:enumeration value="Stepped14"/> <xsd:enumeration value="Stepped15"/> <xsd:enumeration value="Stepped16"/> <xsd:enumeration value="Stepped17"/> <xsd:enumeration value="Stepped18"/> <xsd:enumeration value="Stepped19"/> <xsd:enumeration value="Stepped20"/> <xsd:enumeration value="ContinuousOff"/> <xsd:enumeration value="MotionSensor"/> <xsd:enumeration value="Photocell"/> </xsd:restriction> </xsd:simpleType>

simpleType lightTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | LightType
facets |
Kind | Value | Annotation
enumeration | OnOff |
enumeration | ContinuousControl |
annotation |
documentation
Lights can be controlled in a continuous scale or on/off (1/0).
source | <xsd:simpleType name="lightTypeEnum"> <xsd:annotation> <xsd:documentation>Lights can be controlled in a continuous scale or on/off (1/0).</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:string"> <xsd:enumeration value="OnOff"/> <xsd:enumeration value="ContinuousControl"/> </xsd:restriction> </xsd:simpleType>

simpleType loadUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | LatentLoad/@unit Results/@unit ZoneCoolingLoad/@unit
facets |
Kind | Value | Annotation
enumeration | BtuPerHour |
enumeration | Watt |
source | <xsd:simpleType name="loadUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="BtuPerHour"/> <xsd:enumeration value="Watt"/> </xsd:restriction> </xsd:simpleType>

simpleType loopTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | DeltaP/@hydronicLoopType HydronicLoopId/@hydronicLoopType MinFlow/@hydronicLoopType RatedFlow/@hydronicLoopType HydronicLoop/@loopType
facets |
Kind | Value | Annotation
enumeration | PrimaryChilledWater |
enumeration | SecondaryChilledWater |
enumeration | HotWater |
enumeration | CondenserWater |
enumeration | DomesticHotWater |
enumeration | WaterLoopHeatPump |
enumeration | TwoPipe |
enumeration | PotableWaterLoop |
enumeration | VRFLoop |
source | <xsd:simpleType name="loopTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="PrimaryChilledWater"/> <xsd:enumeration value="SecondaryChilledWater"/> <xsd:enumeration value="HotWater"/> <xsd:enumeration value="CondenserWater"/> <xsd:enumeration value="DomesticHotWater"/> <xsd:enumeration value="WaterLoopHeatPump"/> <xsd:enumeration value="TwoPipe"/> <xsd:enumeration value="PotableWaterLoop"/> <xsd:enumeration value="VRFLoop"/> </xsd:restriction> </xsd:simpleType>

simpleType MaritalStatusType

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | MaritalStatus
facets |
Kind | Value | Annotation
enumeration | Single |
enumeration | Married |
enumeration | Partner |
source | <xsd:simpleType name="MaritalStatusType"> <xsd:restriction base="xsd:string"> <xsd:enumeration value="Single"/> <xsd:enumeration value="Married"/> <xsd:enumeration value="Partner"/> </xsd:restriction> </xsd:simpleType>

simpleType minimumOutdoorAirControlTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | MinimumOutdoorAirControlType/@unit
facets |
Kind | Value | Annotation
enumeration | FixedMinimum |
enumeration | ProportionalMinimum |
source | <xsd:simpleType name="minimumOutdoorAirControlTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="FixedMinimum"/> <xsd:enumeration value="ProportionalMinimum"/> </xsd:restriction> </xsd:simpleType>

simpleType nightCycleControlEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | NightCycleControl/@unit
facets |
Kind | Value | Annotation
enumeration | StayOff |
enumeration | CycleOnAny |
enumeration | CycleOnControlZone |
source | <xsd:simpleType name="nightCycleControlEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="StayOff"/> <xsd:enumeration value="CycleOnAny"/> <xsd:enumeration value="CycleOnControlZone"/> </xsd:restriction> </xsd:simpleType>

simpleType openingTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Opening/@openingType
facets |
Kind | Value | Annotation
enumeration | FixedWindow |
documentation
Opening in a surface with a tilt between 45° and 149.99° with a non-operable glazed opening in it.
enumeration | OperableWindow |
documentation
Opening in a surface with a tilt between 45° and 149.99° with a operable glazed opening in it.
enumeration | FixedSkylight |
documentation
Opening in a surface with a tilt between 0° and 44.99° with a non-operable glazed opening in it.
enumeration | OperableSkylight |
documentation
Opening in a surface with a tilt between 0° and 44.99° with a operable glazed opening in it.
enumeration | SlidingDoor |
documentation
Opening in a surface with a tilt between 45° and 149.99° with a sliding door in it.
enumeration | NonSlidingDoor |
documentation
Opening in a surface with a tilt between 45° and 149.99° with a non-sliding door in it.
enumeration | Air |
documentation
Opening in a surface with a tilt between 0° and 180° with nothing in it.
source | <xsd:simpleType name="openingTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="FixedWindow"> <xsd:annotation> <xsd:documentation>Opening in a surface with a tilt between 45° and 149.99° with a non-operable glazed opening in it. </xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="OperableWindow"> <xsd:annotation> <xsd:documentation>Opening in a surface with a tilt between 45° and 149.99° with a operable glazed opening in it. </xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="FixedSkylight"> <xsd:annotation> <xsd:documentation>Opening in a surface with a tilt between 0° and 44.99° with a non-operable glazed opening in it. </xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="OperableSkylight"> <xsd:annotation> <xsd:documentation>Opening in a surface with a tilt between 0° and 44.99° with a operable glazed opening in it. </xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="SlidingDoor"> <xsd:annotation> <xsd:documentation>Opening in a surface with a tilt between 45° and 149.99° with a sliding door in it. </xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="NonSlidingDoor"> <xsd:annotation> <xsd:documentation>Opening in a surface with a tilt between 45° and 149.99° with a non-sliding door in it. </xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Air"> <xsd:annotation> <xsd:documentation>Opening in a surface with a tilt between 0° and 180° with nothing in it. </xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType operationTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Control/@operationType
facets |
Kind | Value | Annotation
enumeration | Cycling |
enumeration | Continuous |
source | <xsd:simpleType name="operationTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Cycling"/> <xsd:enumeration value="Continuous"/> </xsd:restriction> </xsd:simpleType>

simpleType OtherConstraintType

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | OtherConstraint
facets |
Kind | Value | Annotation
enumeration | NoOccupantsInRoom |
documentation
The action happens only when there is no occupant in the room. (Typically combined with leaving room events.)
source | <xsd:simpleType name="OtherConstraintType"> <xsd:restriction base="xsd:string"> <xsd:enumeration value="NoOccupantsInRoom"> <xsd:annotation> <xsd:documentation>The action happens only when there is no occupant in the room. (Typically combined with leaving room events.)</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType parameterType

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | ParameterType
facets |
Kind | Value | Annotation
enumeration | RoomAirTemperature |
enumeration | RoomCO2Concentration |
enumeration | RoomWorkPlaneDaylightIlluminance |
enumeration | RoomLightsPowerDensity |
enumeration | OutdoorDryBulbTemperature |
enumeration | OutdoorRainIndicator |
source | <xsd:simpleType name="parameterType"> <xsd:restriction base="xsd:string"> <xsd:enumeration value="RoomAirTemperature"/> <xsd:enumeration value="RoomCO2Concentration"/> <xsd:enumeration value="RoomWorkPlaneDaylightIlluminance"/> <xsd:enumeration value="RoomLightsPowerDensity"/> <xsd:enumeration value="OutdoorDryBulbTemperature"/> <xsd:enumeration value="OutdoorRainIndicator"/> </xsd:restriction> </xsd:simpleType>

simpleType peopleHeatGainTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | PeopleHeatGain/@heatGainType
facets |
Kind | Value | Annotation
enumeration | Total |
enumeration | Sensible |
enumeration | Latent |
source | <xsd:simpleType name="peopleHeatGainTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Total"/> <xsd:enumeration value="Sensible"/> <xsd:enumeration value="Latent"/> </xsd:restriction> </xsd:simpleType>

simpleType peopleHeatGainUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | PeopleHeatGain/@unit
facets |
Kind | Value | Annotation
enumeration | WattPerPerson |
enumeration | BtuPerHourPerson |
source | <xsd:simpleType name="peopleHeatGainUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="WattPerPerson"/> <xsd:enumeration value="BtuPerHourPerson"/> </xsd:restriction> </xsd:simpleType>

simpleType peopleNumberUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | PeopleNumber/@unit
facets |
Kind | Value | Annotation
enumeration | NumberOfPeople |
enumeration | SquareFtPerPerson |
enumeration | SquareMPerPerson |
source | <xsd:simpleType name="peopleNumberUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="NumberOfPeople"/> <xsd:enumeration value="SquareFtPerPerson"/> <xsd:enumeration value="SquareMPerPerson"/> </xsd:restriction> </xsd:simpleType>

simpleType permUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Permeance/@unit
facets |
Kind | Value | Annotation
enumeration | PermSI |
enumeration | PermIP |
source | <xsd:simpleType name="permUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="PermSI"/> <xsd:enumeration value="PermIP"/> </xsd:restriction> </xsd:simpleType>

simpleType plugLoadTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | PlugLoadType
facets |
Kind | Value | Annotation
enumeration | OnOff |
enumeration | ContinuousControl |
annotation |
documentation
Plug loads can be controlled in a continuous scale or on/off (1/0).
source | <xsd:simpleType name="plugLoadTypeEnum"> <xsd:annotation> <xsd:documentation>Plug loads can be controlled in a continuous scale or on/off (1/0).</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:string"> <xsd:enumeration value="OnOff"/> <xsd:enumeration value="ContinuousControl"/> </xsd:restriction> </xsd:simpleType>

simpleType PolicyType

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | Policy
facets |
Kind | Value | Annotation
enumeration | Subsidies |
enumeration | Tax-cuts |
enumeration | Codes compliance |
enumeration | Insurance mandate |
source | <xsd:simpleType name="PolicyType"> <xsd:restriction base="xsd:string"> <xsd:enumeration value="Subsidies"/> <xsd:enumeration value="Tax-cuts"/> <xsd:enumeration value="Codes compliance"/> <xsd:enumeration value="Insurance mandate"/> </xsd:restriction> </xsd:simpleType>

simpleType powerPerAreaUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | EquipPowerPerArea/@unit HorizontalSolar/@unit LightPowerPerArea/@unit SolarOnOpening/@unit
facets |
Kind | Value | Annotation
enumeration | WattPerSquareMeter |
enumeration | WattPerSquareFoot |
source | <xsd:simpleType name="powerPerAreaUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="WattPerSquareMeter"/> <xsd:enumeration value="WattPerSquareFoot"/> </xsd:restriction> </xsd:simpleType>

simpleType powerTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Power/@powerType
facets |
Kind | Value | Annotation
enumeration | Electricity |
enumeration | NaturalGas |
enumeration | Propane |
enumeration | FuelOil1 |
enumeration | FuelOil2 |
enumeration | FuelOil4 |
enumeration | Water |
enumeration | ChilledWater |
enumeration | HotWater |
enumeration | Steam |
enumeration | Diesel |
enumeration | Biogas |
source | <xsd:simpleType name="powerTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Electricity"/> <xsd:enumeration value="NaturalGas"/> <xsd:enumeration value="Propane"/> <xsd:enumeration value="FuelOil1"/> <xsd:enumeration value="FuelOil2"/> <xsd:enumeration value="FuelOil4"/> <xsd:enumeration value="Water"/> <xsd:enumeration value="ChilledWater"/> <xsd:enumeration value="HotWater"/> <xsd:enumeration value="Steam"/> <xsd:enumeration value="Diesel"/> <xsd:enumeration value="Biogas"/> </xsd:restriction> </xsd:simpleType>

simpleType powerUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | ElecLoad/@unit InputWatts/@unit Power/@unit Results/@unit
facets |
Kind | Value | Annotation
enumeration | Watt |
enumeration | Kilowatt |
enumeration | Horsepower |
enumeration | KilogramForceMeterPerSecond |
enumeration | BtuPerSecond |
enumeration | FootPoundForcePerSecond |
enumeration | KilocaloriesPerSecond |
enumeration | BtuPerHour |
source | <xsd:simpleType name="powerUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Watt"/> <xsd:enumeration value="Kilowatt"/> <xsd:enumeration value="Horsepower"/> <xsd:enumeration value="KilogramForceMeterPerSecond"/> <xsd:enumeration value="BtuPerSecond"/> <xsd:enumeration value="FootPoundForcePerSecond"/> <xsd:enumeration value="KilocaloriesPerSecond"/> <xsd:enumeration value="BtuPerHour"/> </xsd:restriction> </xsd:simpleType>

simpleType powerUseTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Power/@useType
facets |
Kind | Value | Annotation
enumeration | Heating |
enumeration | Cooling |
enumeration | Both |
enumeration | ElectricityGeneration |
enumeration | Other |
source | <xsd:simpleType name="powerUseTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Heating"/> <xsd:enumeration value="Cooling"/> <xsd:enumeration value="Both"/> <xsd:enumeration value="ElectricityGeneration"/> <xsd:enumeration value="Other"/> </xsd:restriction> </xsd:simpleType>

simpleType preheatCoilTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | PreheatCoilType/@unit
facets |
Kind | Value | Annotation
enumeration | None |
enumeration | Electric |
enumeration | Gas |
source | <xsd:simpleType name="preheatCoilTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="None"/> <xsd:enumeration value="Electric"/> <xsd:enumeration value="Gas"/> </xsd:restriction> </xsd:simpleType>

simpleType pressureUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | DDPressureCool/@unit DDPressureHeat/@unit DesignPressure/@unit MaxPressure/@unit MinPressure/@unit WFTDPressure/@unit
facets |
Kind | Value | Annotation
enumeration | PSI |
enumeration | kPa |
enumeration | Atmospheres |
enumeration | InchesOfH2O |
enumeration | CentimetersOfH2O |
enumeration | InchesOfMercury |
enumeration | CentimetersOfMercury |
enumeration | MillimetersOfMercury |
enumeration | Pascals |
source | <xsd:simpleType name="pressureUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="PSI"/> <xsd:enumeration value="kPa"/> <xsd:enumeration value="Atmospheres"/> <xsd:enumeration value="InchesOfH2O"/> <xsd:enumeration value="CentimetersOfH2O"/> <xsd:enumeration value="InchesOfMercury"/> <xsd:enumeration value="CentimetersOfMercury"/> <xsd:enumeration value="MillimetersOfMercury"/> <xsd:enumeration value="Pascals"/> </xsd:restriction> </xsd:simpleType>

simpleType radiationWavelengthTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Transmittance/@type
facets |
Kind | Value | Annotation
enumeration | Solar |
enumeration | IR |
enumeration | Visible |
source | <xsd:simpleType name="radiationWavelengthTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Solar"/> <xsd:enumeration value="IR"/> <xsd:enumeration value="Visible"/> </xsd:restriction> </xsd:simpleType>

simpleType reflectanceTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Reflectance/@type
facets |
Kind | Value | Annotation
enumeration | Ground |
enumeration | IntSolar |
enumeration | IntIR |
enumeration | IntVisible |
enumeration | ExtSolar |
enumeration | ExtVisible |
enumeration | ExtIR |
source | <xsd:simpleType name="reflectanceTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Ground"/> <xsd:enumeration value="IntSolar"/> <xsd:enumeration value="IntIR"/> <xsd:enumeration value="IntVisible"/> <xsd:enumeration value="ExtSolar"/> <xsd:enumeration value="ExtVisible"/> <xsd:enumeration value="ExtIR"/> </xsd:restriction> </xsd:simpleType>

simpleType resetTemperatureTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | ResetTemperature/@type
facets |
Kind | Value | Annotation
enumeration | None |
enumeration | Automatic |
enumeration | OutdoorAirBased |
enumeration | Scheduled |
source | <xsd:simpleType name="resetTemperatureTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="None"/> <xsd:enumeration value="Automatic"/> <xsd:enumeration value="OutdoorAirBased"/> <xsd:enumeration value="Scheduled"/> </xsd:restriction> </xsd:simpleType>

simpleType resistanceUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | InsideAirFilmResistance/@unit R-value/@unit
facets |
Kind | Value | Annotation
enumeration | SquareMeterKPerW |
enumeration | HrSquareFtFPerBTU |
source | <xsd:simpleType name="resistanceUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="SquareMeterKPerW"/> <xsd:enumeration value="HrSquareFtFPerBTU"/> </xsd:restriction> </xsd:simpleType>

simpleType resourceTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | AltEnergySource/@resourceType Energy/@resourceType Meter/@resourceType Results/@resourceType
facets |
Kind | Value | Annotation
enumeration | Electricity |
enumeration | NaturalGas |
enumeration | Propane |
enumeration | FuelOil1 |
enumeration | FuelOil2 |
enumeration | FuelOil4 |
enumeration | Water |
enumeration | ChilledWater |
enumeration | HotWater |
enumeration | Steam |
source | <xsd:simpleType name="resourceTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Electricity"/> <xsd:enumeration value="NaturalGas"/> <xsd:enumeration value="Propane"/> <xsd:enumeration value="FuelOil1"/> <xsd:enumeration value="FuelOil2"/> <xsd:enumeration value="FuelOil4"/> <xsd:enumeration value="Water"/> <xsd:enumeration value="ChilledWater"/> <xsd:enumeration value="HotWater"/> <xsd:enumeration value="Steam"/> </xsd:restriction> </xsd:simpleType>

simpleType resultsExtraResourceTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
facets |
Kind | Value | Annotation
enumeration | Thermal |
enumeration | Light |
enumeration | Moisture |
enumeration | Air |
enumeration | Contaminant |
source | <xsd:simpleType name="resultsExtraResourceTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Thermal"/> <xsd:enumeration value="Light"/> <xsd:enumeration value="Moisture"/> <xsd:enumeration value="Air"/> <xsd:enumeration value="Contaminant"/> </xsd:restriction> </xsd:simpleType>

simpleType resultsTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Results/@resultsType
facets |
Kind | Value | Annotation
enumeration | HeatLoad |
enumeration | CoolingLoad |
enumeration | CO2 |
enumeration | SO2 |
enumeration | NOx |
enumeration | Energy |
enumeration | Power |
enumeration | Cost |
enumeration | EnergyCost |
enumeration | DemandCost |
enumeration | CommodityCost |
enumeration | TransportationCost |
enumeration | DryBulbTemperature |
enumeration | WetBulbTemperature |
enumeration | DewPointTemperature |
enumeration | FootCandles |
enumeration | Humidity |
enumeration | MoistureContent |
enumeration | Flow |
enumeration | Capacity |
source | <xsd:simpleType name="resultsTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="HeatLoad"/> <xsd:enumeration value="CoolingLoad"/> <xsd:enumeration value="CO2"/> <xsd:enumeration value="SO2"/> <xsd:enumeration value="NOx"/> <xsd:enumeration value="Energy"/> <xsd:enumeration value="Power"/> <xsd:enumeration value="Cost"/> <xsd:enumeration value="EnergyCost"/> <xsd:enumeration value="DemandCost"/> <xsd:enumeration value="CommodityCost"/> <xsd:enumeration value="TransportationCost"/> <xsd:enumeration value="DryBulbTemperature"/> <xsd:enumeration value="WetBulbTemperature"/> <xsd:enumeration value="DewPointTemperature"/> <xsd:enumeration value="FootCandles"/> <xsd:enumeration value="Humidity"/> <xsd:enumeration value="MoistureContent"/> <xsd:enumeration value="Flow"/> <xsd:enumeration value="Capacity"/> </xsd:restriction> </xsd:simpleType>

simpleType roofASHRAENumberEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | CLTDParameters/@roofASHRAENumber
facets |
Kind | Value | Annotation
enumeration | 0 |
documentation
Undefined
enumeration | 1 |
documentation
Steel sheet with 1 or 2 inches insulation
enumeration | 2 |
documentation
One inch wood with 1 inch insulation
enumeration | 3 |
documentation
Four inch light weight concrete
enumeration | 4 |
documentation
Two inch heavy weight concrete
enumeration | 5 |
documentation
One inch wood with 2 inch insulation
enumeration | 6 |
documentation
Six inch light weight concrete
enumeration | 7 |
documentation
2.5 inch wood with 1 inch insulation
enumeration | 8 |
documentation
Eight inch light weight concrete
enumeration | 9 |
documentation
4 inch hvy wt concrete with 1-2 inch insulation
enumeration | 10 |
documentation
2.5 inch wood with 2 inches of insulation
enumeration | 11 |
documentation
Roof Terrace System
enumeration | 12 |
documentation
6 inch hvy wt concrete with 1-2 inch insulation
enumeration | 13 |
documentation
4 inch wood with 1-2 inches of insulation
annotation |
documentation
Used with the roofASHRAENumber attribute. Each annotation for the values is only one example of many possible constructions for that ASHRAE roof number. The user should select the one that best matches the thermal characteristics of the roof, not necessarily the one closest to the example description.
source | <xsd:simpleType name="roofASHRAENumberEnum"> <xsd:annotation> <xsd:documentation>Used with the roofASHRAENumber attribute. Each annotation for the values is only one example of many possible constructions for that ASHRAE roof number. The user should select the one that best matches the thermal characteristics of the roof, not necessarily the one closest to the example description.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="0"> <xsd:annotation> <xsd:documentation>Undefined</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="1"> <xsd:annotation> <xsd:documentation>Steel sheet with 1 or 2 inches insulation</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="2"> <xsd:annotation> <xsd:documentation>One inch wood with 1 inch insulation</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="3"> <xsd:annotation> <xsd:documentation>Four inch light weight concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="4"> <xsd:annotation> <xsd:documentation>Two inch heavy weight concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="5"> <xsd:annotation> <xsd:documentation>One inch wood with 2 inch insulation</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="6"> <xsd:annotation> <xsd:documentation>Six inch light weight concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="7"> <xsd:annotation> <xsd:documentation>2.5 inch wood with 1 inch insulation</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="8"> <xsd:annotation> <xsd:documentation>Eight inch light weight concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="9"> <xsd:annotation> <xsd:documentation>4 inch hvy wt concrete with 1-2 inch insulation</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="10"> <xsd:annotation> <xsd:documentation>2.5 inch wood with 2 inches of insulation</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="11"> <xsd:annotation> <xsd:documentation>Roof Terrace System</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="12"> <xsd:annotation> <xsd:documentation>6 inch hvy wt concrete with 1-2 inch insulation</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="13"> <xsd:annotation> <xsd:documentation>4 inch wood with 1-2 inches of insulation</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType roofCLTDIndexEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | ManualJ8Parameters/@roofCLTDIndex
facets |
Kind | Value | Annotation
enumeration | 1 |
documentation
Under attic or knee wall, U-value = 0.408 - 0.018, Unvented Attic, No Radiant Barrier, Any Roofing Material, Any Roof Color
enumeration | 2 |
documentation
Under attic or knee wall, U-value = 0.408 - 0.018, Vented Attic, No Radiant Barrier, Dark Asphalt Shingles or Dark Metal, Tar and Gravel or Membrane
enumeration | 3 |
documentation
Under attic or knee wall, U-value = 0.408 - 0.018, Vented Attic, No Radiant Barrier, White or Light Color Shingles, Any Wood Shake Light Metal, Tar and Gravel or Membrane
enumeration | 4 |
documentation
Under attic or knee wall, U-value = 0.408 - 0.02, Vented Attic, No Radiant Barrier, Dark Tile, Slate or Concrete
enumeration | 5 |
documentation
Under attic or knee wall, U-value = 0.408 - 0.02, Vented Attic, No Radiant Barrier, Light Tile, Slate or Concrete
enumeration | 6 |
documentation
Under attic or knee wall, U-value = 0.408 - 0.02, Vented Attic, No Radiant Barrier, White Tile, Slate or Concrete, White Metal or White Membrane
enumeration | 7 |
documentation
On exposed beams, U-value = 0.287 - 0.134, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 8 |
documentation
On exposed beams, U-value = 0.118 - 0.091, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 9 |
documentation
On exposed beams, U-value = 0.074 - 0.063, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 10 |
documentation
On exposed beams, U-value = 0.054, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 11 |
documentation
On exposed beams, U-value = 0.048, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 12 |
documentation
On exposed beams, U-value = 0.043 - 0.039, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 13 |
documentation
On exposed beams, U-value = 0.035, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 14 |
documentation
On exposed beams, U-value = 0.032 - 0.027, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 15 |
documentation
On exposed beams, U-value = 0.287 - 0.134, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 16 |
documentation
On exposed beams, U-value = 0.118 - 0.091, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 17 |
documentation
On exposed beams, U-value = 0.074 - 0.063, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 18 |
documentation
On exposed beams, U-value = 0.054, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 19 |
documentation
On exposed beams, U-value = 0.048, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 20 |
documentation
On exposed beams, U-value = 0.043 - 0.039, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 21 |
documentation
On exposed beams, U-value = 0.035, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 22 |
documentation
On exposed beams, U-value = 0.032 - 0.027, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 23 |
documentation
On exposed beams, U-value = 0.287 - 0.134, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane
enumeration | 24 |
documentation
On exposed beams, U-value = 0.118 - 0.091, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane
enumeration | 25 |
documentation
On exposed beams, U-value = 0.074 - 0.063, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane
enumeration | 26 |
documentation
On exposed beams, U-value = 0.054, White or Light Color Tile Slate or Concrete, White Metal, White Membrane
enumeration | 27 |
documentation
On exposed beams, U-value = 0.048, White or Light Color Tile Slate or Concrete, White Metal, White Membrane
enumeration | 28 |
documentation
On exposed beams, U-value = 0.043 - 0.039, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane
enumeration | 29 |
documentation
On exposed beams, U-value = 0.035, White or Light Color Tile Slate or Concrete, White Metal, White Membrane
enumeration | 30 |
documentation
On exposed beams, U-value = 0.032 - 0.027, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane
enumeration | 31 |
documentation
Below roof joists, U-value = 0.241 - 0.109, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 32 |
documentation
Below roof joists, U-value = 0.09 - 0.076, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 33 |
documentation
Below roof joists, U-value = 0.069, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 34 |
documentation
Below roof joists, U-value = 0.051 - 0.047, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 35 |
documentation
Below roof joists, U-value = 0.034, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 36 |
documentation
Below roof joists, U-value = 0.029, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel
enumeration | 37 |
documentation
Below roof joists, U-value = 0.241 - 0.109, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 38 |
documentation
Below roof joists, U-value = 0.09 - 0.076, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 39 |
documentation
Below roof joists, U-value = 0.069, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 40 |
documentation
Below roof joists, U-value = 0.051 - 0.047, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 41 |
documentation
Below roof joists, U-value = 0.034, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 42 |
documentation
Below roof joists, U-value = 0.029, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel
enumeration | 43 |
documentation
Below roof joists, U-value = 0.241 - 0.109, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane
enumeration | 44 |
documentation
Below roof joists, U-value = 0.09 - 0.076, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane
enumeration | 45 |
documentation
Below roof joists, U-value = 0.069, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane
enumeration | 46 |
documentation
Below roof joists, U-value = 0.051 - 0.034, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane
enumeration | 47 |
documentation
Below roof joists, U-value = 0.029, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane
annotation |
documentation
Used with the roofCLTDIndex attribute.
source | <xsd:simpleType name="roofCLTDIndexEnum"> <xsd:annotation> <xsd:documentation>Used with the roofCLTDIndex attribute.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="1"> <xsd:annotation> <xsd:documentation>Under attic or knee wall, U-value = 0.408 - 0.018, Unvented Attic, No Radiant Barrier, Any Roofing Material, Any Roof Color</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="2"> <xsd:annotation> <xsd:documentation>Under attic or knee wall, U-value = 0.408 - 0.018, Vented Attic, No Radiant Barrier, Dark Asphalt Shingles or Dark Metal, Tar and Gravel or Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="3"> <xsd:annotation> <xsd:documentation>Under attic or knee wall, U-value = 0.408 - 0.018, Vented Attic, No Radiant Barrier, White or Light Color Shingles, Any Wood Shake Light Metal, Tar and Gravel or Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="4"> <xsd:annotation> <xsd:documentation>Under attic or knee wall, U-value = 0.408 - 0.02, Vented Attic, No Radiant Barrier, Dark Tile, Slate or Concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="5"> <xsd:annotation> <xsd:documentation>Under attic or knee wall, U-value = 0.408 - 0.02, Vented Attic, No Radiant Barrier, Light Tile, Slate or Concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="6"> <xsd:annotation> <xsd:documentation>Under attic or knee wall, U-value = 0.408 - 0.02, Vented Attic, No Radiant Barrier, White Tile, Slate or Concrete, White Metal or White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="7"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.287 - 0.134, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="8"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.118 - 0.091, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="9"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.074 - 0.063, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="10"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.054, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="11"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.048, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="12"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.043 - 0.039, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="13"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.035, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="14"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.032 - 0.027, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="15"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.287 - 0.134, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="16"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.118 - 0.091, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="17"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.074 - 0.063, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="18"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.054, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="19"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.048, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="20"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.043 - 0.039, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="21"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.035, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="22"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.032 - 0.027, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="23"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.287 - 0.134, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="24"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.118 - 0.091, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="25"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.074 - 0.063, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="26"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.054, White or Light Color Tile Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="27"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.048, White or Light Color Tile Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="28"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.043 - 0.039, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="29"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.035, White or Light Color Tile Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="30"> <xsd:annotation> <xsd:documentation>On exposed beams, U-value = 0.032 - 0.027, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="31"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.241 - 0.109, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="32"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.09 - 0.076, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="33"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.069, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="34"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.051 - 0.047, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="35"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.034, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="36"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.029, Dark or Bold-Color Asphalt Shingle, Dark Metal, Dark Membrane, Dark Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="37"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.241 - 0.109, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="38"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.09 - 0.076, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="39"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.069, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="40"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.051 - 0.047, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="41"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.034, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="42"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.029, White or Light Color Asphalt Shingle, Any Wood Shake, Dark or Medium Color Tile, Slate or Concrete, Light or Unpainted Metal, Light or Silver Membrane, Light Tar and Gravel</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="43"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.241 - 0.109, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="44"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.09 - 0.076, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="45"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.069, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="46"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.051 - 0.034, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="47"> <xsd:annotation> <xsd:documentation>Below roof joists, U-value = 0.029, White or Light Color Tile, Slate or Concrete, White Metal, White Membrane</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType roofColorEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | CLTDParameters/@roofColor
facets |
Kind | Value | Annotation
enumeration | Dark |
documentation
Dark colored or light colored in an industrial area
enumeration | Light |
documentation
Permanently light colored and in a rural area
annotation |
documentation
Used with the roofColor attribute. Only enter Light if the construction is a roof and if it's in a rural location.
source | <xsd:simpleType name="roofColorEnum"> <xsd:annotation> <xsd:documentation>Used with the roofColor attribute. Only enter Light if the construction is a roof and if it's in a rural location.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Dark"> <xsd:annotation> <xsd:documentation>Dark colored or light colored in an industrial area</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Light"> <xsd:annotation> <xsd:documentation>Permanently light colored and in a rural area</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType roofCTSTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | RTSParameters/@roofCTSType
facets |
Kind | Value | Annotation
enumeration | 1 |
documentation
Metal Roof, R-19 Batt Insulation, Gyp Board
enumeration | 2 |
documentation
Metal Roof, R-19 Batt Insulation, Suspended Acoustical Ceiling
enumeration | 3 |
documentation
Metal Roof, R-19 Batt Insulation
enumeration | 4 |
documentation
Asphalt Shingles, Wood Sheathing, R-19 Batt Insulation, Gyp Board
enumeration | 5 |
documentation
Slate or Tile, Wood Sheathing, R-19 Batt Insulation, Gyp Board
enumeration | 6 |
documentation
Wood Shingles, Wood Sheathing, R-19 Batt Insulation, Gyp Board
enumeration | 7 |
documentation
Membrane, Sheathing, R-10 Insulation Board, Wood Deck
enumeration | 8 |
documentation
Membrane, Sheathing, R-10 Insulation Board, Wood Deck Suspended Acoustical Ceiling
enumeration | 9 |
documentation
Membrane, Sheathing, R-10 Insulation Board, Metal Deck
enumeration | 10 |
documentation
Membrane, Sheathing, R-10 Insulation Board, Metal Deck Suspended Acoustical Ceiling
enumeration | 11 |
documentation
Membrane, Sheathing, R-15 Insulation Board, Metal Deck
enumeration | 12 |
documentation
Membrane, Sheathing, R-10 plus R-15 Insulation Boards, Metal Deck
enumeration | 13 |
documentation
2" Concrete Roof Ballast, Membrane, Sheathing, R-15 Insulation Board, Metal Deck
enumeration | 14 |
documentation
Membrane, Sheathing, R-15 Insulation Board, 4" LW Concrete
enumeration | 15 |
documentation
Membrane, Sheathing, R-15 Insulation Board, 6" LW Concrete
enumeration | 16 |
documentation
Membrane, Sheathing, R-15 Insulation Board, 8" LW Concrete
enumeration | 17 |
documentation
Membrane, Sheathing, R-15 Insulation Board, 6" HW Concrete
enumeration | 18 |
documentation
Membrane, Sheathing, R-15 Insulation Board, 8" HW Concrete
enumeration | 19 |
documentation
Membrane, 6" HW Concrete, R-19 Batt Insulation, Suspended Acoustical Ceiling
annotation |
documentation
Used with the roofCTSType attribute. Each annotation for the values is only one example of many possible constructions for that CTS type. The user should select the one that best matches the thermal characteristics of the roof, not necessarily the one closest to the example description.
source | <xsd:simpleType name="roofCTSTypeEnum"> <xsd:annotation> <xsd:documentation>Used with the roofCTSType attribute. Each annotation for the values is only one example of many possible constructions for that CTS type. The user should select the one that best matches the thermal characteristics of the roof, not necessarily the one closest to the example description.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="1"> <xsd:annotation> <xsd:documentation>Metal Roof, R-19 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="2"> <xsd:annotation> <xsd:documentation>Metal Roof, R-19 Batt Insulation, Suspended Acoustical Ceiling </xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="3"> <xsd:annotation> <xsd:documentation>Metal Roof, R-19 Batt Insulation</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="4"> <xsd:annotation> <xsd:documentation>Asphalt Shingles, Wood Sheathing, R-19 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="5"> <xsd:annotation> <xsd:documentation>Slate or Tile, Wood Sheathing, R-19 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="6"> <xsd:annotation> <xsd:documentation>Wood Shingles, Wood Sheathing, R-19 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="7"> <xsd:annotation> <xsd:documentation>Membrane, Sheathing, R-10 Insulation Board, Wood Deck</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="8"> <xsd:annotation> <xsd:documentation>Membrane, Sheathing, R-10 Insulation Board, Wood Deck Suspended Acoustical Ceiling</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="9"> <xsd:annotation> <xsd:documentation>Membrane, Sheathing, R-10 Insulation Board, Metal Deck</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="10"> <xsd:annotation> <xsd:documentation>Membrane, Sheathing, R-10 Insulation Board, Metal Deck Suspended Acoustical Ceiling</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="11"> <xsd:annotation> <xsd:documentation>Membrane, Sheathing, R-15 Insulation Board, Metal Deck</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="12"> <xsd:annotation> <xsd:documentation>Membrane, Sheathing, R-10 plus R-15 Insulation Boards, Metal Deck</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="13"> <xsd:annotation> <xsd:documentation>2" Concrete Roof Ballast, Membrane, Sheathing, R-15 Insulation Board, Metal Deck</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="14"> <xsd:annotation> <xsd:documentation>Membrane, Sheathing, R-15 Insulation Board, 4" LW Concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="15"> <xsd:annotation> <xsd:documentation>Membrane, Sheathing, R-15 Insulation Board, 6" LW Concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="16"> <xsd:annotation> <xsd:documentation>Membrane, Sheathing, R-15 Insulation Board, 8" LW Concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="17"> <xsd:annotation> <xsd:documentation>Membrane, Sheathing, R-15 Insulation Board, 6" HW Concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="18"> <xsd:annotation> <xsd:documentation>Membrane, Sheathing, R-15 Insulation Board, 8" HW Concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="19"> <xsd:annotation> <xsd:documentation>Membrane, 6" HW Concrete, R-19 Batt Insulation, Suspended Acoustical Ceiling</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType RoomEventType

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | RoomEventType
facets |
Kind | Value | Annotation
enumeration | LeavingRoom |
documentation
The occupant is in the space in the previous time-step and not in the current one.
enumeration | LeavingRoomMoreThan1Hour |
enumeration | LeavingRoomMoreThan6Hours |
enumeration | EnteringRoom |
documentation
The occupant is not in the space in the previous time-step and is in the current one.
enumeration | StayingInRoom |
source | <xsd:simpleType name="RoomEventType"> <xsd:restriction base="xsd:string"> <xsd:enumeration value="LeavingRoom"> <xsd:annotation> <xsd:documentation>The occupant is in the space in the previous time-step and not in the current one.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="LeavingRoomMoreThan1Hour"/> <xsd:enumeration value="LeavingRoomMoreThan6Hours"/> <xsd:enumeration value="EnteringRoom"> <xsd:annotation> <xsd:documentation>The occupant is not in the space in the previous time-step and is in the current one.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="StayingInRoom"/> </xsd:restriction> </xsd:simpleType>

simpleType roughnessValueEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Roughness/@value
facets |
Kind | Value | Annotation
enumeration | VeryRough |
enumeration | MediumRough |
enumeration | Rough |
enumeration | Smooth |
enumeration | MediumSmooth |
enumeration | VerySmooth |
source | <xsd:simpleType name="roughnessValueEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="VeryRough"/> <xsd:enumeration value="MediumRough"/> <xsd:enumeration value="Rough"/> <xsd:enumeration value="Smooth"/> <xsd:enumeration value="MediumSmooth"/> <xsd:enumeration value="VerySmooth"/> </xsd:restriction> </xsd:simpleType>

simpleType scheduleTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | DaySchedule/@scheduleType WeekSchedule/@scheduleType Schedule/@type
facets |
Kind | Value | Annotation
enumeration | Temp |
enumeration | Fraction |
enumeration | OnOff |
enumeration | ResetTemp |
enumeration | ActivityLevel |
source | <xsd:simpleType name="scheduleTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Temp"/> <xsd:enumeration value="Fraction"/> <xsd:enumeration value="OnOff"/> <xsd:enumeration value="ResetTemp"/> <xsd:enumeration value="ActivityLevel"/> </xsd:restriction> </xsd:simpleType>

simpleType scheduleTypeLimitsEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | ScheduleTypeLimits/@type
facets |
Kind | Value | Annotation
enumeration | Continuous |
enumeration | Discrete |
source | <xsd:simpleType name="scheduleTypeLimitsEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Continuous"/> <xsd:enumeration value="Discrete"/> </xsd:restriction> </xsd:simpleType>

simpleType SeasonType

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | SeasonType
attribute | Seasons/Season/@Type
facets |
Kind | Value | Annotation
enumeration | Spring |
documentation
March 1 to May 31
enumeration | Summer |
documentation
June 1 to August 31
enumeration | Fall |
documentation
September 1 to November 30
enumeration | Winter |
documentation
December 1 to February 28
enumeration | All |
source | <xsd:simpleType name="SeasonType"> <xsd:restriction base="xsd:string"> <xsd:enumeration value="Spring"> <xsd:annotation> <xsd:documentation>March 1 to May 31</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Summer"> <xsd:annotation> <xsd:documentation>June 1 to August 31</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Fall"> <xsd:annotation> <xsd:documentation>September 1 to November 30</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Winter"> <xsd:annotation> <xsd:documentation>December 1 to February 28</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="All"/> </xsd:restriction> </xsd:simpleType>

simpleType shadeAndBlindTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | ShadeAndBlindType
facets |
Kind | Value | Annotation
enumeration | Operable |
enumeration | Fixed |
source | <xsd:simpleType name="shadeAndBlindTypeEnum"> <xsd:restriction base="xsd:string"> <xsd:enumeration value="Operable"/> <xsd:enumeration value="Fixed"/> </xsd:restriction> </xsd:simpleType>

simpleType shadeOperationEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | Opening/@exteriorShadeType Opening/@interiorShadeType
facets |
Kind | Value | Annotation
enumeration | Fixed |
enumeration | Operable |
source | <xsd:simpleType name="shadeOperationEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Fixed"/> <xsd:enumeration value="Operable"/> </xsd:restriction> </xsd:simpleType>

simpleType shadeScheduleTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
facets |
Kind | Value | Annotation
enumeration | Shade |
enumeration | Blind |
enumeration | Operation |
enumeration | Probability |
enumeration | MaxSolar |
source | <xsd:simpleType name="shadeScheduleTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Shade"/> <xsd:enumeration value="Blind"/> <xsd:enumeration value="Operation"/> <xsd:enumeration value="Probability"/> <xsd:enumeration value="MaxSolar"/> </xsd:restriction> </xsd:simpleType>

simpleType shadeTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | ShadeControl/@type
facets |
Kind | Value | Annotation
enumeration | InteriorInsulated |
enumeration | InteriorUnInsulated |
enumeration | ExternalInsulated |
enumeration | ExternalUnInsulated |
source | <xsd:simpleType name="shadeTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="InteriorInsulated"/> <xsd:enumeration value="InteriorUnInsulated"/> <xsd:enumeration value="ExternalInsulated"/> <xsd:enumeration value="ExternalUnInsulated"/> </xsd:restriction> </xsd:simpleType>

simpleType sinkRateUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | SinkRate/@unit
facets |
Kind | Value | Annotation
enumeration | PoundsPerHour |
enumeration | KilogramsPerHour |
enumeration | GramsPerHour |
source | <xsd:simpleType name="sinkRateUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="PoundsPerHour"/> <xsd:enumeration value="KilogramsPerHour"/> <xsd:enumeration value="GramsPerHour"/> </xsd:restriction> </xsd:simpleType>

simpleType SpaceCategory

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | SpaceOccupancyType/SpaceCategory
facets |
Kind | Value | Annotation
enumeration | OwnOffice |
enumeration | OtherOffice |
enumeration | MeetingRoom |
enumeration | AuxRoom |
documentation
All other rooms
enumeration | Outdoor |
source | <xsd:simpleType name="SpaceCategory"> <xsd:restriction base="xsd:string"> <xsd:enumeration value="OwnOffice"/> <xsd:enumeration value="OtherOffice"/> <xsd:enumeration value="MeetingRoom"/> <xsd:enumeration value="AuxRoom"> <xsd:annotation> <xsd:documentation>All other rooms</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Outdoor"/> </xsd:restriction> </xsd:simpleType>

simpleType spaceTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Space/@spaceType
facets |
Kind | Value | Annotation
enumeration | ActiveStorage |
enumeration | ActiveStorageHospitalOrHealthcare |
enumeration | AirOrTrainOrBusBaggageArea |
enumeration | AirportConcourse |
enumeration | AtriumEachAdditionalFloor |
enumeration | AtriumFirstThreeFloors |
enumeration | AudienceOrSeatingAreaPenitentiary |
enumeration | AudienceOrSeatingAreaExerciseCenter |
enumeration | AudienceOrSeatingAreaGymnasium |
enumeration | AudienceOrSeatingAreaSportsArena |
enumeration | AudienceOrSeatingAreaConventionCenter |
enumeration | AudienceOrSeatingAreaMotionPictureTheatre |
enumeration | AudienceOrSeatingAreaPerformingArtsTheatre |
enumeration | AudienceOrSeatingAreaReligious |
enumeration | AudienceOrSeatingAreaPoliceOrFireStations |
enumeration | AudienceOrSeatingAreaCourtHouse |
enumeration | AudienceOrSeatingAreaAuditorium |
enumeration | BankCustomerArea |
enumeration | BankingActivityAreaOffice |
enumeration | BarberAndBeautyParlor |
enumeration | CardFileAndCataloguingLibrary |
enumeration | ClassroomOrLectureOrTrainingPenitentiary |
enumeration | ClassroomOrLectureOrTraining |
enumeration | ConfinementCellsPenitentiary |
enumeration | ConfinementCellsCourtHouse |
enumeration | ConferenceMeetingOrMultipurpose |
enumeration | CorridorOrTransition |
enumeration | CorridorOrTransitionManufacturingFacility |
enumeration | CorridorsWithPatientWaitingExamHospitalOrHealthcare |
enumeration | CourtSportsAreaSportsArena |
enumeration | CourtroomCourtHouse |
enumeration | DepartmentStoreSalesAreaRetail |
enumeration | DetailedManufacturingFacility |
enumeration | DiningArea |
enumeration | DiningAreaHotel |
enumeration | DiningAreaFamilyDining |
enumeration | DiningAreaLoungeOrLeisureDining |
enumeration | DiningAreaMotel |
enumeration | DiningAreaTransportation |
enumeration | DiningAreaPenitentiary |
enumeration | DiningAreaCivilServices |
enumeration | DormitoryBedroom |
enumeration | DormitoryStudyHall |
enumeration | DressingOrLockerOrFittingRoomGymnasium |
enumeration | DressingOrLockerOrFittingRoomCourtHouse |
enumeration | DressingOrLockerOrFittingRoomPerformingArtsTheatre |
enumeration | DressingOrLockerOrFittingRoomAuditorium |
enumeration | DressingOrLockerOrFittingRoomExerciseCenter |
enumeration | ElectricalOrMechanical |
enumeration | ElevatorLobbies |
enumeration | EmergencyHospitalOrHealthcare |
enumeration | EquipmentRoomManufacturingFacility |
enumeration | ExamOrTreatmentHospitalOrHealthcare |
enumeration | ExcerciseAreaExerciseCenter |
enumeration | ExcerciseAreaGymnasium |
enumeration | ExhibitSpaceConventionCenter |
enumeration | FellowshipHallReligiousBuildings |
enumeration | FineMaterialWarehouse |
enumeration | FineMerchandiseSalesAreaRetail |
enumeration | FireStationEngineRoomPoliceOrFireStation |
enumeration | FoodPreparation |
enumeration | GarageServiceOrRepairAutomotiveFacility |
enumeration | GeneralHighBayManufacturingFacility |
enumeration | GeneralLowBayManufacturingFacility |
enumeration | GeneralExhibitionMuseum |
enumeration | HospitalNurseryHospitalOrHealthcare |
enumeration | HospitalOrMedicalSuppliesHospitalOrHealthcare |
enumeration | HospitalOrRadiologyHospitalOrHealthcare |
enumeration | HotelOrConferenceCenterConferenceOrMeeting |
enumeration | InactiveStorage |
enumeration | JudgesChambersCourtHouse |
enumeration | LaboratoryOffice |
enumeration | LaundryIroningAndSorting |
enumeration | LaundryWashingHospitalOrHealthcare |
enumeration | LibraryAudioVisualLibraryAudioVisual |
enumeration | LivingQuartersDormitory |
enumeration | LivingQuartersMotel |
enumeration | LivingQuartersHotel |
enumeration | Lobby |
enumeration | LobbyReligiousBuildings |
enumeration | LobbyMotionPictureTheatre |
enumeration | LobbyAuditorium |
enumeration | LobbyPerformingArtsTheatre |
enumeration | LobbyPostOffice |
enumeration | LobbyHotel |
enumeration | LoungeOrRecreation |
enumeration | MallConcourseSalesAreaRetail |
enumeration | MassMerchandisingSalesAreaRetail |
enumeration | MediumOrBulkyMaterialWarehouse |
enumeration | MerchandisingSalesAreaRetail |
enumeration | MuseumAndGalleryStorage |
enumeration | NurseStationHospitalOrHealthcare |
enumeration | OfficeEnclosed |
enumeration | OfficeOpenPlan |
enumeration | OfficeCommonActivityAreasInactiveStorage |
enumeration | OperatingRoomHospitalOrHealthcare |
enumeration | OtherTelevisedPlayingAreaSportsArena |
enumeration | ParkingAreaAttendantOnlyParkingGarage |
enumeration | ParkingAreaPedestrianParkingGarage |
enumeration | PatientRoomHospitalOrHealthcare |
enumeration | PersonalServicesSalesAreaRetail |
enumeration | PharmacyHospitalOrHealthcare |
enumeration | PhysicalTherapyHospitalOrHealthcare |
enumeration | PlayingAreaGymnasium |
enumeration | Plenum |
enumeration | PoliceStationLaboratoryPoliceOrFireStations |
enumeration | PublicAndStaffLoungeHospitalOrHealthcare |
enumeration | ReadingAreaLibrary |
enumeration | ReceptionOrWaitingTransportation |
enumeration | ReceptionOrWaitingMotel |
enumeration | ReceptionOrWaitingHotel |
enumeration | RecoveryHospitalOrHealthcare |
enumeration | RestorationMuseum |
enumeration | Restrooms |
enumeration | RingSportsAreaSportsArena |
enumeration | ServerRoom |
enumeration | SleepingQuartersPoliceOrFireStation |
enumeration | SortingAreaPostOffice |
enumeration | SpecialtyStoreSalesAreaRetail |
enumeration | StacksLibrary |
enumeration | StairsInactive |
enumeration | Stairway |
enumeration | SupermarketSalesAreaRetail |
enumeration | TerminalTicketCounterTransportation |
enumeration | WorkshopWorkshop |
enumeration | WorshipPulpitChoirReligious |
source | <xsd:simpleType name="spaceTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="ActiveStorage"/> <xsd:enumeration value="ActiveStorageHospitalOrHealthcare"/> <xsd:enumeration value="AirOrTrainOrBusBaggageArea"/> <xsd:enumeration value="AirportConcourse"/> <xsd:enumeration value="AtriumEachAdditionalFloor"/> <xsd:enumeration value="AtriumFirstThreeFloors"/> <xsd:enumeration value="AudienceOrSeatingAreaPenitentiary"/> <xsd:enumeration value="AudienceOrSeatingAreaExerciseCenter"/> <xsd:enumeration value="AudienceOrSeatingAreaGymnasium"/> <xsd:enumeration value="AudienceOrSeatingAreaSportsArena"/> <xsd:enumeration value="AudienceOrSeatingAreaConventionCenter"/> <xsd:enumeration value="AudienceOrSeatingAreaMotionPictureTheatre"/> <xsd:enumeration value="AudienceOrSeatingAreaPerformingArtsTheatre"/> <xsd:enumeration value="AudienceOrSeatingAreaReligious"/> <xsd:enumeration value="AudienceOrSeatingAreaPoliceOrFireStations"/> <xsd:enumeration value="AudienceOrSeatingAreaCourtHouse"/> <xsd:enumeration value="AudienceOrSeatingAreaAuditorium"/> <xsd:enumeration value="BankCustomerArea"/> <xsd:enumeration value="BankingActivityAreaOffice"/> <xsd:enumeration value="BarberAndBeautyParlor"/> <xsd:enumeration value="CardFileAndCataloguingLibrary"/> <xsd:enumeration value="ClassroomOrLectureOrTrainingPenitentiary"/> <xsd:enumeration value="ClassroomOrLectureOrTraining"/> <xsd:enumeration value="ConfinementCellsPenitentiary"/> <xsd:enumeration value="ConfinementCellsCourtHouse"/> <xsd:enumeration value="ConferenceMeetingOrMultipurpose"/> <xsd:enumeration value="CorridorOrTransition"/> <xsd:enumeration value="CorridorOrTransitionManufacturingFacility"/> <xsd:enumeration value="CorridorsWithPatientWaitingExamHospitalOrHealthcare"/> <xsd:enumeration value="CourtSportsAreaSportsArena"/> <xsd:enumeration value="CourtroomCourtHouse"/> <xsd:enumeration value="DepartmentStoreSalesAreaRetail"/> <xsd:enumeration value="DetailedManufacturingFacility"/> <xsd:enumeration value="DiningArea"/> <xsd:enumeration value="DiningAreaHotel"/> <xsd:enumeration value="DiningAreaFamilyDining"/> <xsd:enumeration value="DiningAreaLoungeOrLeisureDining"/> <xsd:enumeration value="DiningAreaMotel"/> <xsd:enumeration value="DiningAreaTransportation"/> <xsd:enumeration value="DiningAreaPenitentiary"/> <xsd:enumeration value="DiningAreaCivilServices"/> <xsd:enumeration value="DormitoryBedroom"/> <xsd:enumeration value="DormitoryStudyHall"/> <xsd:enumeration value="DressingOrLockerOrFittingRoomGymnasium"/> <xsd:enumeration value="DressingOrLockerOrFittingRoomCourtHouse"/> <xsd:enumeration value="DressingOrLockerOrFittingRoomPerformingArtsTheatre"/> <xsd:enumeration value="DressingOrLockerOrFittingRoomAuditorium"/> <xsd:enumeration value="DressingOrLockerOrFittingRoomExerciseCenter"/> <xsd:enumeration value="ElectricalOrMechanical"/> <xsd:enumeration value="ElevatorLobbies"/> <xsd:enumeration value="EmergencyHospitalOrHealthcare"/> <xsd:enumeration value="EquipmentRoomManufacturingFacility"/> <xsd:enumeration value="ExamOrTreatmentHospitalOrHealthcare"/> <xsd:enumeration value="ExcerciseAreaExerciseCenter"/> <xsd:enumeration value="ExcerciseAreaGymnasium"/> <xsd:enumeration value="ExhibitSpaceConventionCenter"/> <xsd:enumeration value="FellowshipHallReligiousBuildings"/> <xsd:enumeration value="FineMaterialWarehouse"/> <xsd:enumeration value="FineMerchandiseSalesAreaRetail"/> <xsd:enumeration value="FireStationEngineRoomPoliceOrFireStation"/> <xsd:enumeration value="FoodPreparation"/> <xsd:enumeration value="GarageServiceOrRepairAutomotiveFacility"/> <xsd:enumeration value="GeneralHighBayManufacturingFacility"/> <xsd:enumeration value="GeneralLowBayManufacturingFacility"/> <xsd:enumeration value="GeneralExhibitionMuseum"/> <xsd:enumeration value="HospitalNurseryHospitalOrHealthcare"/> <xsd:enumeration value="HospitalOrMedicalSuppliesHospitalOrHealthcare"/> <xsd:enumeration value="HospitalOrRadiologyHospitalOrHealthcare"/> <xsd:enumeration value="HotelOrConferenceCenterConferenceOrMeeting"/> <xsd:enumeration value="InactiveStorage"/> <xsd:enumeration value="JudgesChambersCourtHouse"/> <xsd:enumeration value="LaboratoryOffice"/> <xsd:enumeration value="LaundryIroningAndSorting"/> <xsd:enumeration value="LaundryWashingHospitalOrHealthcare"/> <xsd:enumeration value="LibraryAudioVisualLibraryAudioVisual"/> <xsd:enumeration value="LivingQuartersDormitory"/> <xsd:enumeration value="LivingQuartersMotel"/> <xsd:enumeration value="LivingQuartersHotel"/> <xsd:enumeration value="Lobby"/> <xsd:enumeration value="LobbyReligiousBuildings"/> <xsd:enumeration value="LobbyMotionPictureTheatre"/> <xsd:enumeration value="LobbyAuditorium"/> <xsd:enumeration value="LobbyPerformingArtsTheatre"/> <xsd:enumeration value="LobbyPostOffice"/> <xsd:enumeration value="LobbyHotel"/> <xsd:enumeration value="LoungeOrRecreation"/> <xsd:enumeration value="MallConcourseSalesAreaRetail"/> <xsd:enumeration value="MassMerchandisingSalesAreaRetail"/> <xsd:enumeration value="MediumOrBulkyMaterialWarehouse"/> <xsd:enumeration value="MerchandisingSalesAreaRetail"/> <xsd:enumeration value="MuseumAndGalleryStorage"/> <xsd:enumeration value="NurseStationHospitalOrHealthcare"/> <xsd:enumeration value="OfficeEnclosed"/> <xsd:enumeration value="OfficeOpenPlan"/> <xsd:enumeration value="OfficeCommonActivityAreasInactiveStorage"/> <xsd:enumeration value="OperatingRoomHospitalOrHealthcare"/> <xsd:enumeration value="OtherTelevisedPlayingAreaSportsArena"/> <xsd:enumeration value="ParkingAreaAttendantOnlyParkingGarage"/> <xsd:enumeration value="ParkingAreaPedestrianParkingGarage"/> <xsd:enumeration value="PatientRoomHospitalOrHealthcare"/> <xsd:enumeration value="PersonalServicesSalesAreaRetail"/> <xsd:enumeration value="PharmacyHospitalOrHealthcare"/> <xsd:enumeration value="PhysicalTherapyHospitalOrHealthcare"/> <xsd:enumeration value="PlayingAreaGymnasium"/> <xsd:enumeration value="Plenum"/> <xsd:enumeration value="PoliceStationLaboratoryPoliceOrFireStations"/> <xsd:enumeration value="PublicAndStaffLoungeHospitalOrHealthcare"/> <xsd:enumeration value="ReadingAreaLibrary"/> <xsd:enumeration value="ReceptionOrWaitingTransportation"/> <xsd:enumeration value="ReceptionOrWaitingMotel"/> <xsd:enumeration value="ReceptionOrWaitingHotel"/> <xsd:enumeration value="RecoveryHospitalOrHealthcare"/> <xsd:enumeration value="RestorationMuseum"/> <xsd:enumeration value="Restrooms"/> <xsd:enumeration value="RingSportsAreaSportsArena"/> <xsd:enumeration value="ServerRoom"/> <xsd:enumeration value="SleepingQuartersPoliceOrFireStation"/> <xsd:enumeration value="SortingAreaPostOffice"/> <xsd:enumeration value="SpecialtyStoreSalesAreaRetail"/> <xsd:enumeration value="StacksLibrary"/> <xsd:enumeration value="StairsInactive"/> <xsd:enumeration value="Stairway"/> <xsd:enumeration value="SupermarketSalesAreaRetail"/> <xsd:enumeration value="TerminalTicketCounterTransportation"/> <xsd:enumeration value="WorkshopWorkshop"/> <xsd:enumeration value="WorshipPulpitChoirReligious"/> </xsd:restriction> </xsd:simpleType>

simpleType specificHeatUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | SpecificHeat/@unit
facets |
Kind | Value | Annotation
enumeration | JPerKgK |
enumeration | BTUPerLbF |
source | <xsd:simpleType name="specificHeatUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="JPerKgK"/> <xsd:enumeration value="BTUPerLbF"/> </xsd:restriction> </xsd:simpleType>

simpleType stageTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Control/@stages
facets |
Kind | Value | Annotation
enumeration | 1Stage |
enumeration | 2Stage |
enumeration | Variable |
source | <xsd:simpleType name="stageTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="1Stage"/> <xsd:enumeration value="2Stage"/> <xsd:enumeration value="Variable"/> </xsd:restriction> </xsd:simpleType>

simpleType standardsTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Efficiency/@standardsType
facets |
Kind | Value | Annotation
enumeration | DOE |
documentation
Department of Energy
enumeration | ARI |
documentation
Air-Conditioning and Refrigeration Institute
enumeration | ANSI |
documentation
American National Standards Institute
enumeration | NEMA |
documentation
National Electrical Manufacturers Association
source | <xsd:simpleType name="standardsTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="DOE"> <xsd:annotation> <xsd:documentation>Department of Energy</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="ARI"> <xsd:annotation> <xsd:documentation>Air-Conditioning and Refrigeration Institute</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="ANSI"> <xsd:annotation> <xsd:documentation>American National Standards Institute</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="NEMA"> <xsd:annotation> <xsd:documentation>National Electrical Manufacturers Association</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType stationIdTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | StationId/@IDType
facets |
Kind | Value | Annotation
enumeration | WMO |
documentation
A five-digit station identifier assigned by the World Meteorological Organization (WMO), used for international weather data exchange and station documentation.
enumeration | WBAN |
documentation
Weather-Bureau-Army-Navy station id. A five-digit station identifier used at National Climatic Data Center (NCDC) for digital data storage and general station identification purposes.
enumeration | ICAO |
documentation
A 4-letter indicator for geographical locations throughout the world, managed by the International Civil Aviation Organization (ICAO).
enumeration | NWSLI |
documentation
A 3- to 5-character alpha-numeric identifier assigned by the US National Weather Service (NWS), used for site identification in the NWS communications systems (e.g. AFOS, ROSA, SHEF, etc.).
enumeration | FAACallSign |
documentation
An alpha-numeric identifier of up to 4-characters managed by the USDT Federal Aviation Administration (FAA), used for site identification of airports, weather stations and other sites vital to navigation.
enumeration | COOP |
documentation
A 6-digit number identifying a station in the NWS Cooperative Network.
enumeration | Modeled |
documentation
A custom code identifying a virtual station for a particular grid location on the planet that was modeled by a simulation program such as MM5, WRF, or other weather simulation programs.
source | <xsd:simpleType name="stationIdTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="WMO"> <xsd:annotation> <xsd:documentation>A five-digit station identifier assigned by the World Meteorological Organization (WMO), used for international weather data exchange and station documentation.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="WBAN"> <xsd:annotation> <xsd:documentation>Weather-Bureau-Army-Navy station id. A five-digit station identifier used at National Climatic Data Center (NCDC) for digital data storage and general station identification purposes.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="ICAO"> <xsd:annotation> <xsd:documentation>A 4-letter indicator for geographical locations throughout the world, managed by the International Civil Aviation Organization (ICAO).</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="NWSLI"> <xsd:annotation> <xsd:documentation>A 3- to 5-character alpha-numeric identifier assigned by the US National Weather Service (NWS), used for site identification in the NWS communications systems (e.g. AFOS, ROSA, SHEF, etc.).</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="FAACallSign"> <xsd:annotation> <xsd:documentation>An alpha-numeric identifier of up to 4-characters managed by the USDT Federal Aviation Administration (FAA), used for site identification of airports, weather stations and other sites vital to navigation.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="COOP"> <xsd:annotation> <xsd:documentation>A 6-digit number identifying a station in the NWS Cooperative Network.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Modeled"> <xsd:annotation> <xsd:documentation>A custom code identifying a virtual station for a particular grid location on the planet that was modeled by a simulation program such as MM5, WRF, or other weather simulation programs.</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType statusTransitionEventType

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | StatusTransitionEventType
facets |
Kind | Value | Annotation
enumeration | Arrival |
enumeration | Departure |
enumeration | ShortTermLeaving |
enumeration | ShortTermVisiting |
annotation |
documentation
One time event involving occupancy status transition in building level
source | <xsd:simpleType name="statusTransitionEventType"> <xsd:annotation> <xsd:documentation> One time event involving occupancy status transition in building level</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:string"> <xsd:enumeration value="Arrival"/> <xsd:enumeration value="Departure"/> <xsd:enumeration value="ShortTermLeaving"/> <xsd:enumeration value="ShortTermVisiting"/> </xsd:restriction> </xsd:simpleType>

simpleType subjectiveValueType

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
elements | Accommodating CostConscious EnvironmentAwareness PastExperience SocialInfluence TechnologyOriented
facets |
Kind | Value | Annotation
enumeration | High |
enumeration | Medium |
enumeration | Low |
source | <xsd:simpleType name="subjectiveValueType"> <xsd:restriction base="xsd:string"> <xsd:enumeration value="High"/> <xsd:enumeration value="Medium"/> <xsd:enumeration value="Low"/> </xsd:restriction> </xsd:simpleType>

simpleType supplementalHeatingCoilTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | SupplementalHeatingCoilType/@unit
facets |
Kind | Value | Annotation
enumeration | Electric |
enumeration | Gas |
enumeration | HotWater |
source | <xsd:simpleType name="supplementalHeatingCoilTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Electric"/> <xsd:enumeration value="Gas"/> <xsd:enumeration value="HotWater"/> </xsd:restriction> </xsd:simpleType>

simpleType surfaceDescriptionEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | Emittance/@surfaceType Reflectance/@surfaceType Transmittance/@surfaceType
facets |
Kind | Value | Annotation
enumeration | 1 |
documentation
The surfaceDescriptionEnum allows control over the specification of material surface properties. By setting the surfaceDescriptionEnum to 1, it is implied that the attribute (e.g. - Reflectance, Emittance, etc.) is associated with Surface 1 of the material's two surfaces [it is assumed that the material is a large planar object]. Surface 1 represents the surface that points away from the building interior.
enumeration | 2 |
documentation
The surfaceDescriptionEnum allows control over the specification of material surface properties. By setting the surfaceDescriptionEnum to 2, it is implied that the attribute (e.g. - Reflectance, Emittance, etc.) is associated with Surface 2 of the material's two surfaces [it is assumed that the material is a large planar object]. Surface 2 represents the surface that points towards the building interior.
enumeration | Both |
documentation
The surfaceDescriptionEnum allows control over the specification of material surface properties. By setting the surfaceDescriptionEnum to Both, it is implied that the attribute (e.g. - Reflectance, Emittance, etc.) is associated both Surface 1 and Surface 2 of the material's 2 surfaces [it is assumed that the material is a large planar object]. See the enumerations above for a description of Surface 1 and 2.
source | <xsd:simpleType name="surfaceDescriptionEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="1"> <xsd:annotation> <xsd:documentation>The surfaceDescriptionEnum allows control over the specification of material surface properties. By setting the surfaceDescriptionEnum to 1, it is implied that the attribute (e.g. - Reflectance, Emittance, etc.) is associated with Surface 1 of the material's two surfaces [it is assumed that the material is a large planar object]. Surface 1 represents the surface that points away from the building interior.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="2"> <xsd:annotation> <xsd:documentation>The surfaceDescriptionEnum allows control over the specification of material surface properties. By setting the surfaceDescriptionEnum to 2, it is implied that the attribute (e.g. - Reflectance, Emittance, etc.) is associated with Surface 2 of the material's two surfaces [it is assumed that the material is a large planar object]. Surface 2 represents the surface that points towards the building interior.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Both"> <xsd:annotation> <xsd:documentation>The surfaceDescriptionEnum allows control over the specification of material surface properties. By setting the surfaceDescriptionEnum to Both, it is implied that the attribute (e.g. - Reflectance, Emittance, etc.) is associated both Surface 1 and Surface 2 of the material's 2 surfaces [it is assumed that the material is a large planar object]. See the enumerations above for a description of Surface 1 and 2.</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType surfaceReferenceLocationEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | gbXML/@SurfaceReferenceLocation
facets |
Kind | Value | Annotation
enumeration | Centerline |
enumeration | InteriorSurface |
source | <xsd:simpleType name="surfaceReferenceLocationEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Centerline"/> <xsd:enumeration value="InteriorSurface"/> </xsd:restriction> </xsd:simpleType>

simpleType surfaceTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | AdjacentSpaceId/@surfaceType Surface/@surfaceType
facets |
Kind | Value | Annotation
enumeration | InteriorWall |
documentation
The portion of the building envelope, including opaque area and fenestration, that is adjacent to two conditioned or unconditioned spaces and that is vertical or tilted at an angle of 60° from horizontal or greater.
enumeration | ExteriorWall |
documentation
The portion of the building envelope, including opaque area and fenestration, that is adjacent to one conditioned or unconditioned space and that is vertical or tilted at an angle of 60° from horizontal or greater.
enumeration | Roof |
documentation
The upper portion of the building envelope, including opaque areas and fenestration, that is adjacent to one conditioned or unconditioned space and that is horizontal or tilted at an angle of less than 60° from horizontal.
enumeration | InteriorFloor |
documentation
The lower portion of the building envelope, including opaque area and fenestration, that has conditioned or semiheated space above and is horizontal or tilted at an angle of less than 60 degrees from horizontal but excluding slab-on-grade floors.
enumeration | ExposedFloor |
documentation
The floor area exposed to non-conditioned space or outside.
enumeration | Shade |
documentation
Surface not adjacent to any spaces with tilt between 0° and 180°.
enumeration | UndergroundWall |
documentation
The portion of the building envelope, including opaque area and fenestration, that is adjacent to one conditioned or unconditioned space and earth (soil) and that is vertical or tilted at an angle of 60° from horizontal or greater.
enumeration | UndergroundSlab |
documentation
Surface adjacent to one conditioned or unconditioned space and earth (soil) below grade with a tilt between 150° and 180°.
enumeration | Ceiling |
documentation
The upper portion of the building envelope that is adjacent to two conditioned or unconditioned spaces and that is horizontal or tilted at an angle of less than 60° from horizontal.
enumeration | Air |
documentation
Air membrane between two conditioned or unconditioned spaces with a tilt between 0° and 180°.
enumeration | UndergroundCeiling |
documentation
The portion of the building envelope, including opaque area and fenestration, that is adjacent to one conditioned or unconditioned space and earth (soil) and that is horizontal or tilted at an angle of less than 60° from horizontal.
enumeration | RaisedFloor |
documentation
The lower portion of the building envelope, including opaque area and fenestration, that is adjacent to one conditioned or unconditioned space and the outside and is horizontal or tilted at an angle between 150° and 180°.
enumeration | SlabOnGrade |
documentation
The lower portion of the building envelope, including opaque area and fenestration, that is adjacent to one conditioned or unconditioned space and earth (soil) at grade with a tilt between 150° and 180°.
enumeration | FreestandingColumn |
documentation
Freestanding column in space specified by its top surface having the same ifcGUID.
enumeration | EmbeddedColumn |
documentation
Embedded column in wall specified by a surface which is coplanar with (one of) the embedding wall(s).
source | <xsd:simpleType name="surfaceTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="InteriorWall"> <xsd:annotation> <xsd:documentation>The portion of the building envelope, including opaque area and fenestration, that is adjacent to two conditioned or unconditioned spaces and that is vertical or tilted at an angle of 60° from horizontal or greater.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="ExteriorWall"> <xsd:annotation> <xsd:documentation>The portion of the building envelope, including opaque area and fenestration, that is adjacent to one conditioned or unconditioned space and that is vertical or tilted at an angle of 60° from horizontal or greater.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Roof"> <xsd:annotation> <xsd:documentation>The upper portion of the building envelope, including opaque areas and fenestration, that is adjacent to one conditioned or unconditioned space and that is horizontal or tilted at an angle of less than 60° from horizontal.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="InteriorFloor"> <xsd:annotation> <xsd:documentation>The lower portion of the building envelope, including opaque area and fenestration, that has conditioned or semiheated space above and is horizontal or tilted at an angle of less than 60 degrees from horizontal but excluding slab-on-grade floors.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="ExposedFloor"> <xsd:annotation> <xsd:documentation>The floor area exposed to non-conditioned space or outside.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Shade"> <xsd:annotation> <xsd:documentation>Surface not adjacent to any spaces with tilt between 0° and 180°.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="UndergroundWall"> <xsd:annotation> <xsd:documentation>The portion of the building envelope, including opaque area and fenestration, that is adjacent to one conditioned or unconditioned space and earth (soil) and that is vertical or tilted at an angle of 60° from horizontal or greater.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="UndergroundSlab"> <xsd:annotation> <xsd:documentation>Surface adjacent to one conditioned or unconditioned space and earth (soil) below grade with a tilt between 150° and 180°.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Ceiling"> <xsd:annotation> <xsd:documentation>The upper portion of the building envelope that is adjacent to two conditioned or unconditioned spaces and that is horizontal or tilted at an angle of less than 60° from horizontal.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Air"> <xsd:annotation> <xsd:documentation>Air membrane between two conditioned or unconditioned spaces with a tilt between 0° and 180°. </xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="UndergroundCeiling"> <xsd:annotation> <xsd:documentation>The portion of the building envelope, including opaque area and fenestration, that is adjacent to one conditioned or unconditioned space and earth (soil) and that is horizontal or tilted at an angle of less than 60° from horizontal.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="RaisedFloor"> <xsd:annotation> <xsd:documentation>The lower portion of the building envelope, including opaque area and fenestration, that is adjacent to one conditioned or unconditioned space and the outside and is horizontal or tilted at an angle between 150° and 180°.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="SlabOnGrade"> <xsd:annotation> <xsd:documentation>The lower portion of the building envelope, including opaque area and fenestration, that is adjacent to one conditioned or unconditioned space and earth (soil) at grade with a tilt between 150° and 180°.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="FreestandingColumn"> <xsd:annotation> <xsd:documentation>Freestanding column in space specified by its top surface having the same ifcGUID.</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="EmbeddedColumn"> <xsd:annotation> <xsd:documentation>Embedded column in wall specified by a surface which is coplanar with (one of) the embedding wall(s).</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType systemTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | AirLoop/@systemType
facets |
Kind | Value | Annotation
enumeration | SingleZoneReheat |
documentation
Variable Temperature
enumeration | PackagedSingleZone |
documentation
Packaged Single-zone
enumeration | SingleZoneCeilingInduction |
documentation
Ceiling Induction
enumeration | ReheatFan |
documentation
Constant-volume Reheat Fan
enumeration | VariableAirVolume |
documentation
Variable-volume Fan
enumeration | PoweredInductionUnit |
documentation
Powered Induction Unit
enumeration | PackagedVariableAirVolume |
documentation
Packaged Variable Air Volume
enumeration | PackagedVariableVolumeVariableTemperature |
documentation
Packaged Variable-Volume Variable-Temperature
enumeration | CeilingBypassVariableAirVolume |
documentation
Ceiling Bypass
enumeration | EvaporativeCooling |
documentation
Evaporative Cooling
enumeration | MultiZone |
documentation
Multizone Fan
enumeration | PackagedMultiZone |
documentation
Packaged Multizone
enumeration | DualDuct |
documentation
Dual-duct Fan
enumeration | FanCoil |
documentation
Fan Coil
enumeration | InductionUnit |
documentation
Induction Unit
enumeration | PackagedTerminalAirConditioner |
documentation
Packaged Terminal Air Conditioner
enumeration | WaterLoopHeatPump |
documentation
Water Loop Heat Pump
enumeration | ResidentialCyclingFurnaceCyclingAC |
documentation
Residential with cycling furnace and cycling air-conditioner
enumeration | ResidentialVariableAirVolumeVariableTemperature |
documentation
Residential Variable-Volume Variable-Temperature
enumeration | FloorPanelHeating |
documentation
Floor Panel Heating
enumeration | HeatingAndVentilating |
documentation
Heating and Ventilating
enumeration | UnitHeater |
documentation
Unit Heater
enumeration | UnitVentilator |
documentation
Unit Ventilator
enumeration | CentralHeatingRadiators |
documentation
Central Heating Radiators
enumeration | CentralHeatingConvectors |
documentation
Central Heating Convectors
enumeration | CentralHeatingRadiantFloor |
documentation
Central Heating Radiant Floor
enumeration | CentralHeatingHotAir |
documentation
Central Heating Hot Air
enumeration | OtherRoomHeater |
documentation
Other Room Heater
enumeration | RadiantHeaterNoFlue |
documentation
Radiant Heater No Flue
enumeration | RadiantHeaterFlue |
documentation
Radiant Heater Flue
enumeration | RadiantHeaterMultiburner |
documentation
Radiant Heater Multiburner
enumeration | ForcedConvectionHeaterFlue |
documentation
Forced Convection Heater Flue
enumeration | ForcedConvectionHeaterNoFlue |
documentation
Forced Convection Heater No Flue
enumeration | VAVSingleDuct |
documentation
VAV Single Duct
enumeration | VAVDualDuct |
documentation
VAV Dual Duct
enumeration | VAVReheatFan |
documentation
VAV Reheat Fan
enumeration | VAVIndoorPackagedCabinet |
documentation
VAV Indoor Packaged Cabinet
enumeration | ConstantVolumeFixedOA |
documentation
Constant Volume Fixed OA
enumeration | ConstantVolumeVariableOA |
documentation
Constant Volume Variable OA
enumeration | ConstantVolumeTerminalReheat |
documentation
Constant Volume Terminal Reheat
enumeration | MultizoneHotDeckColdDeck |
documentation
Multizone Hot Deck Cold Deck
enumeration | ConstantVolumeDualDuct |
documentation
Constant Volume Dual Duct
enumeration | RadiantCooledCeilings |
documentation
Radiant Cooled Ceilings
enumeration | ActiveChilledBeams |
documentation
Active Chilled Beams
enumeration | VariableRefrigerantFlow |
documentation
Variable Refrigerant Flow
enumeration | SplitSystemsWithNaturalVentilation |
documentation
Split Systems With Natural Ventilation
enumeration | SplitSystemsWithMechanicalVentilation |
documentation
Split Systems With Mechanical Ventilation
enumeration | SplitSystemsWithMechanicalVentilationWithCooling |
documentation
Split Systems With Mechanical Ventilation With Cooling
enumeration | Exhaust |
documentation
Exhaust Air Systems
source | <xsd:simpleType name="systemTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="SingleZoneReheat"> <xsd:annotation> <xsd:documentation>Variable Temperature</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="PackagedSingleZone"> <xsd:annotation> <xsd:documentation>Packaged Single-zone</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="SingleZoneCeilingInduction"> <xsd:annotation> <xsd:documentation>Ceiling Induction</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="ReheatFan"> <xsd:annotation> <xsd:documentation>Constant-volume Reheat Fan</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="VariableAirVolume"> <xsd:annotation> <xsd:documentation>Variable-volume Fan</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="PoweredInductionUnit"> <xsd:annotation> <xsd:documentation>Powered Induction Unit</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="PackagedVariableAirVolume"> <xsd:annotation> <xsd:documentation>Packaged Variable Air Volume</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="PackagedVariableVolumeVariableTemperature"> <xsd:annotation> <xsd:documentation>Packaged Variable-Volume Variable-Temperature</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="CeilingBypassVariableAirVolume"> <xsd:annotation> <xsd:documentation>Ceiling Bypass</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="EvaporativeCooling"> <xsd:annotation> <xsd:documentation>Evaporative Cooling</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="MultiZone"> <xsd:annotation> <xsd:documentation>Multizone Fan</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="PackagedMultiZone"> <xsd:annotation> <xsd:documentation>Packaged Multizone</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="DualDuct"> <xsd:annotation> <xsd:documentation>Dual-duct Fan</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="FanCoil"> <xsd:annotation> <xsd:documentation>Fan Coil</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="InductionUnit"> <xsd:annotation> <xsd:documentation>Induction Unit</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="PackagedTerminalAirConditioner"> <xsd:annotation> <xsd:documentation>Packaged Terminal Air Conditioner</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="WaterLoopHeatPump"> <xsd:annotation> <xsd:documentation>Water Loop Heat Pump</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="ResidentialCyclingFurnaceCyclingAC"> <xsd:annotation> <xsd:documentation>Residential with cycling furnace and cycling air-conditioner</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="ResidentialVariableAirVolumeVariableTemperature"> <xsd:annotation> <xsd:documentation>Residential Variable-Volume Variable-Temperature</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="FloorPanelHeating"> <xsd:annotation> <xsd:documentation>Floor Panel Heating</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="HeatingAndVentilating"> <xsd:annotation> <xsd:documentation>Heating and Ventilating</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="UnitHeater"> <xsd:annotation> <xsd:documentation>Unit Heater</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="UnitVentilator"> <xsd:annotation> <xsd:documentation>Unit Ventilator</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="CentralHeatingRadiators"> <xsd:annotation> <xsd:documentation>Central Heating Radiators</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="CentralHeatingConvectors"> <xsd:annotation> <xsd:documentation>Central Heating Convectors</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="CentralHeatingRadiantFloor"> <xsd:annotation> <xsd:documentation>Central Heating Radiant Floor</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="CentralHeatingHotAir"> <xsd:annotation> <xsd:documentation>Central Heating Hot Air</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="OtherRoomHeater"> <xsd:annotation> <xsd:documentation>Other Room Heater</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="RadiantHeaterNoFlue"> <xsd:annotation> <xsd:documentation>Radiant Heater No Flue</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="RadiantHeaterFlue"> <xsd:annotation> <xsd:documentation>Radiant Heater Flue</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="RadiantHeaterMultiburner"> <xsd:annotation> <xsd:documentation>Radiant Heater Multiburner</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="ForcedConvectionHeaterFlue"> <xsd:annotation> <xsd:documentation>Forced Convection Heater Flue</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="ForcedConvectionHeaterNoFlue"> <xsd:annotation> <xsd:documentation>Forced Convection Heater No Flue</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="VAVSingleDuct"> <xsd:annotation> <xsd:documentation>VAV Single Duct</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="VAVDualDuct"> <xsd:annotation> <xsd:documentation>VAV Dual Duct</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="VAVReheatFan"> <xsd:annotation> <xsd:documentation>VAV Reheat Fan</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="VAVIndoorPackagedCabinet"> <xsd:annotation> <xsd:documentation>VAV Indoor Packaged Cabinet</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="ConstantVolumeFixedOA"> <xsd:annotation> <xsd:documentation>Constant Volume Fixed OA</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="ConstantVolumeVariableOA"> <xsd:annotation> <xsd:documentation>Constant Volume Variable OA</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="ConstantVolumeTerminalReheat"> <xsd:annotation> <xsd:documentation>Constant Volume Terminal Reheat</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="MultizoneHotDeckColdDeck"> <xsd:annotation> <xsd:documentation>Multizone Hot Deck Cold Deck</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="ConstantVolumeDualDuct"> <xsd:annotation> <xsd:documentation>Constant Volume Dual Duct</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="RadiantCooledCeilings"> <xsd:annotation> <xsd:documentation>Radiant Cooled Ceilings</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="ActiveChilledBeams"> <xsd:annotation> <xsd:documentation>Active Chilled Beams</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="VariableRefrigerantFlow"> <xsd:annotation> <xsd:documentation>Variable Refrigerant Flow</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="SplitSystemsWithNaturalVentilation"> <xsd:annotation> <xsd:documentation>Split Systems With Natural Ventilation</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="SplitSystemsWithMechanicalVentilation"> <xsd:annotation> <xsd:documentation>Split Systems With Mechanical Ventilation</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="SplitSystemsWithMechanicalVentilationWithCooling"> <xsd:annotation> <xsd:documentation>Split Systems With Mechanical Ventilation With Cooling</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Exhaust"> <xsd:annotation> <xsd:documentation>Exhaust Air Systems</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType temperatureUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | gbXML/@temperatureUnit AirTemperature/@unit ResetTemperature/@unit DDDBCool/@unit DDDBHeat/@unit DDDBRangeCool/@unit DDDBRangeHeat/@unit DDGroundTCool/@unit DDGroundTHeat/@unit DDWBCool/@unit DDWBHeat/@unit DeltaT/@unit DesignCoolT/@unit DesignHeatT/@unit DesignTemp/@unit GroundTemp/@unit MaxTemp/@unit MinTemp/@unit NaturalVentHiTemp/@unit NaturalVentLoTemp/@unit Results/@unit Temp/@unit Temperature/@unit WFTDTemp/@unit
facets |
Kind | Value | Annotation
enumeration | F |
enumeration | C |
enumeration | K |
enumeration | R |
source | <xsd:simpleType name="temperatureUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="F"/> <xsd:enumeration value="C"/> <xsd:enumeration value="K"/> <xsd:enumeration value="R"/> </xsd:restriction> </xsd:simpleType>

simpleType tempTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Temp/@tempType
facets |
Kind | Value | Annotation
enumeration | Max |
enumeration | Min |
enumeration | Design |
enumeration | CoolDesign |
enumeration | HeatDesign |
enumeration | Throttle |
enumeration | Range |
enumeration | Approach |
enumeration | EnteringWetBulb |
enumeration | LeavingDryBulb |
enumeration | EnteringDryBulb |
enumeration | LeavingWetBulb |
enumeration | ChilledWaterSupply |
enumeration | CondenserWaterSupply |
enumeration | LeavingChilledWater |
enumeration | LeavingCondenserWater |
enumeration | HighTempLockout |
enumeration | LowTempLockout |
enumeration | EconomizerMaxLimitDewpoint |
enumeration | HeatPumpDefrostMaxOADryBulb |
enumeration | SupplementalHeatingCoilMaxOADryBulb |
enumeration | PreheatCoilDesignSetpoint |
source | <xsd:simpleType name="tempTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Max"/> <xsd:enumeration value="Min"/> <xsd:enumeration value="Design"/> <xsd:enumeration value="CoolDesign"/> <xsd:enumeration value="HeatDesign"/> <xsd:enumeration value="Throttle"/> <xsd:enumeration value="Range"/> <xsd:enumeration value="Approach"/> <xsd:enumeration value="EnteringWetBulb"/> <xsd:enumeration value="LeavingDryBulb"/> <xsd:enumeration value="EnteringDryBulb"/> <xsd:enumeration value="LeavingWetBulb"/> <xsd:enumeration value="ChilledWaterSupply"/> <xsd:enumeration value="CondenserWaterSupply"/> <xsd:enumeration value="LeavingChilledWater"/> <xsd:enumeration value="LeavingCondenserWater"/> <xsd:enumeration value="HighTempLockout"/> <xsd:enumeration value="LowTempLockout"/> <xsd:enumeration value="EconomizerMaxLimitDewpoint"/> <xsd:enumeration value="HeatPumpDefrostMaxOADryBulb"/> <xsd:enumeration value="SupplementalHeatingCoilMaxOADryBulb"/> <xsd:enumeration value="PreheatCoilDesignSetpoint"/> </xsd:restriction> </xsd:simpleType>

simpleType thermostatTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | ThermostatType
facets |
Kind | Value | Annotation
enumeration | Adjustable |
enumeration | Fixed |
source | <xsd:simpleType name="thermostatTypeEnum"> <xsd:restriction base="xsd:string"> <xsd:enumeration value="Adjustable"/> <xsd:enumeration value="Fixed"/> </xsd:restriction> </xsd:simpleType>

simpleType TimeofDayType

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
attribute | TimeofDay/@Type
facets |
Kind | Value | Annotation
enumeration | Morning |
documentation
6am to 12pm
enumeration | Noon |
documentation
12pm
enumeration | Afternoon |
documentation
12pm to 6pm
enumeration | Evening |
documentation
6pm to 12am
enumeration | Day |
documentation
6am to 12am
enumeration | Night |
documentation
12am to 6am
enumeration | All |
source | <xsd:simpleType name="TimeofDayType"> <xsd:restriction base="xsd:string"> <xsd:enumeration value="Morning"> <xsd:annotation> <xsd:documentation>6am to 12pm</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Noon"> <xsd:annotation> <xsd:documentation>12pm</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Afternoon"> <xsd:annotation> <xsd:documentation>12pm to 6pm</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Evening"> <xsd:annotation> <xsd:documentation>6pm to 12am</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Day"> <xsd:annotation> <xsd:documentation>6am to 12am</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Night"> <xsd:annotation> <xsd:documentation>12am to 6am</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="All"/> </xsd:restriction> </xsd:simpleType>

simpleType timePeriodEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Energy/@timePeriod
facets |
Kind | Value | Annotation
enumeration | Annual |
enumeration | Jan |
enumeration | Feb |
enumeration | Mar |
enumeration | Apr |
enumeration | May |
enumeration | Jun |
enumeration | Jul |
enumeration | Aug |
enumeration | Sep |
enumeration | Oct |
enumeration | Nov |
enumeration | Dec |
source | <xsd:simpleType name="timePeriodEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Annual"/> <xsd:enumeration value="Jan"/> <xsd:enumeration value="Feb"/> <xsd:enumeration value="Mar"/> <xsd:enumeration value="Apr"/> <xsd:enumeration value="May"/> <xsd:enumeration value="Jun"/> <xsd:enumeration value="Jul"/> <xsd:enumeration value="Aug"/> <xsd:enumeration value="Sep"/> <xsd:enumeration value="Oct"/> <xsd:enumeration value="Nov"/> <xsd:enumeration value="Dec"/> </xsd:restriction> </xsd:simpleType>

simpleType timeUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
element | TimeFrequencyType
attribute | TimeIncrement/@timeUnit
facets |
Kind | Value | Annotation
enumeration | Year |
enumeration | Month |
enumeration | Week |
enumeration | Day |
enumeration | Hour |
enumeration | Minute |
source | <xsd:simpleType name="timeUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Year"/> <xsd:enumeration value="Month"/> <xsd:enumeration value="Week"/> <xsd:enumeration value="Day"/> <xsd:enumeration value="Hour"/> <xsd:enumeration value="Minute"/> </xsd:restriction> </xsd:simpleType>

simpleType transportationTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Transportation/@transportationType
facets |
Kind | Value | Annotation
enumeration | Bus |
enumeration | Train |
enumeration | Car |
enumeration | LightRail |
enumeration | Ferry |
enumeration | Airplane |
enumeration | Monorail |
enumeration | Bike |
source | <xsd:simpleType name="transportationTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Bus"/> <xsd:enumeration value="Train"/> <xsd:enumeration value="Car"/> <xsd:enumeration value="LightRail"/> <xsd:enumeration value="Ferry"/> <xsd:enumeration value="Airplane"/> <xsd:enumeration value="Monorail"/> <xsd:enumeration value="Bike"/> </xsd:restriction> </xsd:simpleType>

simpleType TypesDataCollectedList

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
attributes | Behavior/@TypesDataCollected1 Behavior/@TypesDataCollected2 Behavior/@TypesDataCollected3
facets |
Kind | Value | Annotation
enumeration | CrossSectionSurvey |
enumeration | LongitudinalSurvey |
enumeration | IEQmeasurements |
source | <xsd:simpleType name="TypesDataCollectedList"> <xsd:restriction base="xsd:string"> <xsd:enumeration value="CrossSectionSurvey"/> <xsd:enumeration value="LongitudinalSurvey"/> <xsd:enumeration value="IEQmeasurements"/> </xsd:restriction> </xsd:simpleType>

simpleType unitlessSmallUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | HighLimit/@unit Results/@unit
facets |
Kind | Value | Annotation
enumeration | Percent |
enumeration | PartPerMillionByVolume |
enumeration | milliGramsPerCubicMeter |
source | <xsd:simpleType name="unitlessSmallUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Percent"/> <xsd:enumeration value="PartPerMillionByVolume"/> <xsd:enumeration value="milliGramsPerCubicMeter"/> </xsd:restriction> </xsd:simpleType>

simpleType unitlessUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | Absorptance/@unit Albedo/@unit DDSkyClearnessCool/@unit DDSkyClearnessHeat/@unit Emittance/@unit Glare/@unit MaxRelativeHumidity/@unit MinFlow/@unit MinRelativeHumidity/@unit PercentAreaDaylitControlled/@unit PercentExisting/@unit Porosity/@unit RecycledContent/@unit Reflectance/@unit Results/@unit ShadingCoeff/@unit SolarHeatGainCoeff/@unit Transmittance/@unit WasteWaterHREff/@unit WaterLoss/@unit HeatRejectedtoSpace/@unit WFTDRelHumidity/@unit
facets |
Kind | Value | Annotation
enumeration | Percent |
enumeration | Fraction |
source | <xsd:simpleType name="unitlessUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Percent"/> <xsd:enumeration value="Fraction"/> </xsd:restriction> </xsd:simpleType>

simpleType uValueUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | U-value/@unit
facets |
Kind | Value | Annotation
enumeration | WPerSquareMeterK |
enumeration | BtuPerHourSquareFtF |
source | <xsd:simpleType name="uValueUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="WPerSquareMeterK"/> <xsd:enumeration value="BtuPerHourSquareFtF"/> </xsd:restriction> </xsd:simpleType>

simpleType valueTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | Energy/@valueType Results/@valueType
facets |
Kind | Value | Annotation
enumeration | Historical |
enumeration | Simulated |
enumeration | Rated |
enumeration | Measured |
source | <xsd:simpleType name="valueTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Historical"/> <xsd:enumeration value="Simulated"/> <xsd:enumeration value="Rated"/> <xsd:enumeration value="Measured"/> </xsd:restriction> </xsd:simpleType>

simpleType vegetationTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Vegetation/@vegetationType
facets |
Kind | Value | Annotation
enumeration | Trees |
enumeration | Bushes |
enumeration | Plants |
enumeration | Grass |
enumeration | Moss |
enumeration | EvergreenTrees |
enumeration | EvergreenShrubs |
enumeration | DeciduousTrees |
enumeration | DeciduousShrubs |
source | <xsd:simpleType name="vegetationTypeEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Trees"/> <xsd:enumeration value="Bushes"/> <xsd:enumeration value="Plants"/> <xsd:enumeration value="Grass"/> <xsd:enumeration value="Moss"/> <xsd:enumeration value="EvergreenTrees"/> <xsd:enumeration value="EvergreenShrubs"/> <xsd:enumeration value="DeciduousTrees"/> <xsd:enumeration value="DeciduousShrubs"/> </xsd:restriction> </xsd:simpleType>

simpleType velocityUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | DDWindSpeedCool/@unit DDWindSpeedHeat/@unit WFTDWindSpeed/@unit WindSpeed/@unit
facets |
Kind | Value | Annotation
enumeration | MetersPerSecond |
enumeration | MilesPerHour |
enumeration | Knots |
source | <xsd:simpleType name="velocityUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="MetersPerSecond"/> <xsd:enumeration value="MilesPerHour"/> <xsd:enumeration value="Knots"/> </xsd:restriction> </xsd:simpleType>

simpleType versionEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | gbXML/@version
facets |
Kind | Value | Annotation
enumeration | 0.35 |
enumeration | 0.36 |
enumeration | 0.37 |
enumeration | 5.00 |
enumeration | 5.01 |
enumeration | 5.10 |
enumeration | 5.11 |
enumeration | 5.12 |
enumeration | 6.00 |
enumeration | 6.01 |
source | <xsd:simpleType name="versionEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="0.35"/> <xsd:enumeration value="0.36"/> <xsd:enumeration value="0.37"/> <xsd:enumeration value="5.00"/> <xsd:enumeration value="5.01"/> <xsd:enumeration value="5.10"/> <xsd:enumeration value="5.11"/> <xsd:enumeration value="5.12"/> <xsd:enumeration value="6.00"/> <xsd:enumeration value="6.01"/> </xsd:restriction> </xsd:simpleType>

simpleType viscosityFofTUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | ViscosityFofT/@unit
facets |
Kind | Value | Annotation
enumeration | KgPerMSecK |
enumeration | PoundPerFootSecF |
source | <xsd:simpleType name="viscosityFofTUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="KgPerMSecK"/> <xsd:enumeration value="PoundPerFootSecF"/> </xsd:restriction> </xsd:simpleType>

simpleType viscosityUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Viscosity/@unit
facets |
Kind | Value | Annotation
enumeration | KgPerMSec |
enumeration | PoundPerFootSec |
source | <xsd:simpleType name="viscosityUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="KgPerMSec"/> <xsd:enumeration value="PoundPerFootSec"/> </xsd:restriction> </xsd:simpleType>

simpleType volumeUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attributes | Volume/@unit gbXML/@volumeUnit
facets |
Kind | Value | Annotation
enumeration | CubicKilometers |
enumeration | CubicMeters |
enumeration | CubicCentimeters |
enumeration | CubicMillimeters |
enumeration | CubicMiles |
enumeration | CubicYards |
enumeration | CubicFeet |
enumeration | CubicInches |
source | <xsd:simpleType name="volumeUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="CubicKilometers"/> <xsd:enumeration value="CubicMeters"/> <xsd:enumeration value="CubicCentimeters"/> <xsd:enumeration value="CubicMillimeters"/> <xsd:enumeration value="CubicMiles"/> <xsd:enumeration value="CubicYards"/> <xsd:enumeration value="CubicFeet"/> <xsd:enumeration value="CubicInches"/> </xsd:restriction> </xsd:simpleType>

simpleType wallASHRAEGroupEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | CLTDParameters/@wallASHRAEGroup
facets |
Kind | Value | Annotation
enumeration | A |
documentation
4-in. face brick, insulation + 8-in. com. brick
enumeration | B |
documentation
4-in. face brick, 2-in. insul., 4-in. com. brick
enumeration | C |
documentation
4-in. face brick, air space + 4-in. face brick
enumeration | D |
documentation
4-in. face brick + 4-in. common brick
enumeration | E |
documentation
4-in. face brick + 4-in. block
enumeration | F |
documentation
4-in. block + air space or insulation
enumeration | G |
documentation
Metal curtain wall + 1 to 3-in. insulation
annotation |
documentation
Used with the wallASHRAEGroup attribute. Each annotation for the values is only one example of many possible constructions for that ASHRAE wall group. The user should select the one that best matches the thermal characteristics of the wall, not necessarily the one closest to the example description.
source | <xsd:simpleType name="wallASHRAEGroupEnum"> <xsd:annotation> <xsd:documentation>Used with the wallASHRAEGroup attribute. Each annotation for the values is only one example of many possible constructions for that ASHRAE wall group. The user should select the one that best matches the thermal characteristics of the wall, not necessarily the one closest to the example description.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="A"> <xsd:annotation> <xsd:documentation>4-in. face brick, insulation + 8-in. com. brick</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="B"> <xsd:annotation> <xsd:documentation>4-in. face brick, 2-in. insul., 4-in. com. brick</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="C"> <xsd:annotation> <xsd:documentation>4-in. face brick, air space + 4-in. face brick</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="D"> <xsd:annotation> <xsd:documentation>4-in. face brick + 4-in. common brick</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="E"> <xsd:annotation> <xsd:documentation>4-in. face brick + 4-in. block</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="F"> <xsd:annotation> <xsd:documentation>4-in. block + air space or insulation</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="G"> <xsd:annotation> <xsd:documentation>Metal curtain wall + 1 to 3-in. insulation</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType wallColorEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | CLTDParameters/@wallColor
facets |
Kind | Value | Annotation
enumeration | Dark |
documentation
Dark colored or light colored in an industrial area
enumeration | Medium |
documentation
Permanently medium colored and in a rural area
enumeration | Light |
documentation
Permanently light colored and in a rural area
annotation |
documentation
Used with the wallColor attribute. Only enter Light or Medium if the construction is a wall and if it's in a rural location.
source | <xsd:simpleType name="wallColorEnum"> <xsd:annotation> <xsd:documentation>Used with the wallColor attribute. Only enter Light or Medium if the construction is a wall and if it's in a rural location.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Dark"> <xsd:annotation> <xsd:documentation>Dark colored or light colored in an industrial area</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Medium"> <xsd:annotation> <xsd:documentation>Permanently medium colored and in a rural area</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="Light"> <xsd:annotation> <xsd:documentation>Permanently light colored and in a rural area</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType wallCTSTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | RTSParameters/@wallCTSType
facets |
Kind | Value | Annotation
enumeration | 1 |
documentation
Spandrel Glass, R-10 Insulation Board, Gyp Board
enumeration | 2 |
documentation
Metal Wall Panel, R-10 Insulation Board, Gyp Board
enumeration | 3 |
documentation
1" Stone, R-10 Insulation Board, Gyp Board
enumeration | 4 |
documentation
Metal Wall Panel, Sheathing, R-11 Batt Insulation, Gyp Board
enumeration | 5 |
documentation
1" Stone, Sheathing, R-11 Batt Insulation, Gyp Board
enumeration | 6 |
documentation
Wood Siding, Sheathing, R-11 Batt Insulation, 1/2" Wood
enumeration | 7 |
documentation
1" Stucco, Sheathing, R-11 Batt Insulation, Gyp Board
enumeration | 8 |
documentation
EIFS Finish, R-5 Insulation Board, Sheathing, Gyp Board
enumeration | 9 |
documentation
EIFS Finish, R-5 Insulation Board, Sheathing, R-11 Batt Insulation, Gyp Board
enumeration | 10 |
documentation
EIFS Finish, R-5 Insulation Board, Sheathing, 8" LW CMU, Gyp Board
enumeration | 11 |
documentation
Brick, R-5 Insulation Board, Sheathing, Gyp Board
enumeration | 12 |
documentation
Brick, Sheathing, R-11 Batt Insulation, Gyp Board
enumeration | 13 |
documentation
Brick, R-5 Insulation Board, Sheathing, R-11 Batt Insulation Gyp Board
enumeration | 14 |
documentation
Brick, R-5 Insulation Board, 8" LW CMU
enumeration | 15 |
documentation
Brick, 8" LW CMU, R-11 Batt Insulation, Gyp Board
enumeration | 16 |
documentation
Brick, R-5 Insulation Board, 8" HW CMU, Gyp Board
enumeration | 17 |
documentation
Brick, R-5 Insulation Board, Brick
enumeration | 18 |
documentation
Brick, R-5 Insulation Board, 8" LW Concrete, Gyp Board
enumeration | 19 |
documentation
Brick, R-5 Insulation Board, 12" HW Concrete, Gyp Board
enumeration | 20 |
documentation
Brick, 8" HW Concrete, R-11 Batt Insulation, Gyp Board
enumeration | 21 |
documentation
8" LW CMU, R-11 Batt Insulation, Gyp Board
enumeration | 22 |
documentation
8" LW CMU w Fill Insulation, R-11 Batt Insulation, Gyp Board
enumeration | 23 |
documentation
1" Stucco, 8" HW CMU, R-11 Batt Insulation, Gyp Board
enumeration | 24 |
documentation
8" LW CMU w Fill Insulation
enumeration | 25 |
documentation
8" LW CMU w Fill Insulation, Gyp Board
enumeration | 26 |
documentation
12" LW CMU w Fill Insulation, Gyp Board
enumeration | 27 |
documentation
4" LW Concrete. R-5 Board Insulation, Gyp Board
enumeration | 28 |
documentation
4" LW Concrete. R-11 Batt Insulation, Gyp Board
enumeration | 29 |
documentation
4" LW Concrete. R-10 Board Insulation, 4" LW Concrete
enumeration | 30 |
documentation
EIFS Finish, R-5 Insulation Board, 8" LW Concrete, Gyp Board
enumeration | 31 |
documentation
8" LW Concrete. R-11 Batt Insulation, Gyp Board
enumeration | 32 |
documentation
EIFS Finish, R-10 Insulation Board, 8" HW Concrete, Gyp Board
enumeration | 33 |
documentation
8" HW Concrete. R-11 Batt Insulation, Gyp Board
enumeration | 34 |
documentation
12" HW Concrete. R-19 Batt Insulation, Gyp Board
enumeration | 35 |
documentation
12" HW Concrete
annotation |
documentation
Used with the wallCTSType attribute. Each annotation for the values is only one example of many possible constructions for that CTS type. The user should select the one that best matches the thermal characteristics of the wall, not necessarily the one closest to the example description.
source | <xsd:simpleType name="wallCTSTypeEnum"> <xsd:annotation> <xsd:documentation>Used with the wallCTSType attribute. Each annotation for the values is only one example of many possible constructions for that CTS type. The user should select the one that best matches the thermal characteristics of the wall, not necessarily the one closest to the example description.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="1"> <xsd:annotation> <xsd:documentation>Spandrel Glass, R-10 Insulation Board, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="2"> <xsd:annotation> <xsd:documentation>Metal Wall Panel, R-10 Insulation Board, Gyp Board </xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="3"> <xsd:annotation> <xsd:documentation>1" Stone, R-10 Insulation Board, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="4"> <xsd:annotation> <xsd:documentation>Metal Wall Panel, Sheathing, R-11 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="5"> <xsd:annotation> <xsd:documentation>1" Stone, Sheathing, R-11 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="6"> <xsd:annotation> <xsd:documentation>Wood Siding, Sheathing, R-11 Batt Insulation, 1/2" Wood</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="7"> <xsd:annotation> <xsd:documentation>1" Stucco, Sheathing, R-11 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="8"> <xsd:annotation> <xsd:documentation>EIFS Finish, R-5 Insulation Board, Sheathing, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="9"> <xsd:annotation> <xsd:documentation>EIFS Finish, R-5 Insulation Board, Sheathing, R-11 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="10"> <xsd:annotation> <xsd:documentation>EIFS Finish, R-5 Insulation Board, Sheathing, 8" LW CMU, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="11"> <xsd:annotation> <xsd:documentation>Brick, R-5 Insulation Board, Sheathing, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="12"> <xsd:annotation> <xsd:documentation>Brick, Sheathing, R-11 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="13"> <xsd:annotation> <xsd:documentation>Brick, R-5 Insulation Board, Sheathing, R-11 Batt Insulation Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="14"> <xsd:annotation> <xsd:documentation>Brick, R-5 Insulation Board, 8" LW CMU</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="15"> <xsd:annotation> <xsd:documentation>Brick, 8" LW CMU, R-11 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="16"> <xsd:annotation> <xsd:documentation>Brick, R-5 Insulation Board, 8" HW CMU, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="17"> <xsd:annotation> <xsd:documentation>Brick, R-5 Insulation Board, Brick</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="18"> <xsd:annotation> <xsd:documentation>Brick, R-5 Insulation Board, 8" LW Concrete, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="19"> <xsd:annotation> <xsd:documentation>Brick, R-5 Insulation Board, 12" HW Concrete, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="20"> <xsd:annotation> <xsd:documentation>Brick, 8" HW Concrete, R-11 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="21"> <xsd:annotation> <xsd:documentation>8" LW CMU, R-11 Batt Insulation, Gyp Board </xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="22"> <xsd:annotation> <xsd:documentation>8" LW CMU w Fill Insulation, R-11 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="23"> <xsd:annotation> <xsd:documentation>1" Stucco, 8" HW CMU, R-11 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="24"> <xsd:annotation> <xsd:documentation>8" LW CMU w Fill Insulation</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="25"> <xsd:annotation> <xsd:documentation>8" LW CMU w Fill Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="26"> <xsd:annotation> <xsd:documentation>12" LW CMU w Fill Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="27"> <xsd:annotation> <xsd:documentation>4" LW Concrete. R-5 Board Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="28"> <xsd:annotation> <xsd:documentation>4" LW Concrete. R-11 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="29"> <xsd:annotation> <xsd:documentation>4" LW Concrete. R-10 Board Insulation, 4" LW Concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="30"> <xsd:annotation> <xsd:documentation>EIFS Finish, R-5 Insulation Board, 8" LW Concrete, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="31"> <xsd:annotation> <xsd:documentation>8" LW Concrete. R-11 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="32"> <xsd:annotation> <xsd:documentation>EIFS Finish, R-10 Insulation Board, 8" HW Concrete, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="33"> <xsd:annotation> <xsd:documentation>8" HW Concrete. R-11 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="34"> <xsd:annotation> <xsd:documentation>12" HW Concrete. R-19 Batt Insulation, Gyp Board</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="35"> <xsd:annotation> <xsd:documentation>12" HW Concrete</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType wallGroupManualJEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | ManualJ8Parameters/@wallGroupManualJ
facets |
Kind | Value | Annotation
enumeration | A |
documentation
Fastest heat transfer
enumeration | B |
enumeration | C |
enumeration | D |
enumeration | E |
enumeration | F |
documentation
Medium heat transfer
enumeration | G |
enumeration | H |
enumeration | I |
enumeration | J |
enumeration | K |
documentation
Slowest heat transfer
annotation |
documentation
Used with the wallGroupManualJ attribute.
source | <xsd:simpleType name="wallGroupManualJEnum"> <xsd:annotation> <xsd:documentation>Used with the wallGroupManualJ attribute.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="A"> <xsd:annotation> <xsd:documentation>Fastest heat transfer</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="B"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="C"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="D"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="E"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="F"> <xsd:annotation> <xsd:documentation>Medium heat transfer</xsd:documentation> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="G"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="H"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="I"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="J"> <xsd:annotation> <xsd:documentation/> </xsd:annotation> </xsd:enumeration> <xsd:enumeration value="K"> <xsd:annotation> <xsd:documentation>Slowest heat transfer</xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType>

simpleType waterUseUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | WaterUsePerCycle/@unit
facets |
Kind | Value | Annotation
enumeration | CubicMeters |
enumeration | Gallons |
enumeration | Tons |
enumeration | Kilograms |
enumeration | Liters |
source | <xsd:simpleType name="waterUseUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="CubicMeters"/> <xsd:enumeration value="Gallons"/> <xsd:enumeration value="Tons"/> <xsd:enumeration value="Kilograms"/> <xsd:enumeration value="Liters"/> </xsd:restriction> </xsd:simpleType>

simpleType weightUnitEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | Weight/@unit
facets |
Kind | Value | Annotation
enumeration | Pounds |
enumeration | Kilograms |
enumeration | Tons |
source | <xsd:simpleType name="weightUnitEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Pounds"/> <xsd:enumeration value="Kilograms"/> <xsd:enumeration value="Tons"/> </xsd:restriction> </xsd:simpleType>

simpleType windowTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:string
properties |
base | xsd:string
used by |
element | WindowTypeSimple
facets |
Kind | Value | Annotation
enumeration | Operable |
enumeration | ContinuousControl |
enumeration | Fixed |
source | <xsd:simpleType name="windowTypeEnum"> <xsd:restriction base="xsd:string"> <xsd:enumeration value="Operable"/> <xsd:enumeration value="ContinuousControl"/> <xsd:enumeration value="Fixed"/> </xsd:restriction> </xsd:simpleType>

simpleType windSpeedEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | WindSpeed/@type
facets |
Kind | Value | Annotation
enumeration | RatedWindSpeed |
enumeration | CutInWindSpeed |
enumeration | CutOutWindSpeed |
source | <xsd:simpleType name="windSpeedEnum"> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="RatedWindSpeed"/> <xsd:enumeration value="CutInWindSpeed"/> <xsd:enumeration value="CutOutWindSpeed"/> </xsd:restriction> </xsd:simpleType>

simpleType zoneHVACEquipmentTypeEnum

namespace | http://www.gbxml.org/schema
type | restriction of xsd:NMTOKEN
properties |
base | xsd:NMTOKEN
used by |
attribute | ZoneHVACEquipment/@zoneHVACEquipmentType
facets |
Kind | Value | Annotation
enumeration | Undefined |
enumeration | UnConditioned |
enumeration | ChilledBeamActive |
enumeration | FourPipeFanCoil |
enumeration | PackagedTerminalAirConditioner |
enumeration | PackagedTerminalHeatPump |
enumeration | ParallelFanPoweredBox |
enumeration | VAVBox |
enumeration | BaseBoardConvective |
enumeration | BaseBoardRadiant |
enumeration | CAVBox |
enumeration | RadiantPanel |
enumeration | SeriesFanPoweredBox |
enumeration | UnitHeater |
enumeration | UnitVentilator |
enumeration | WaterSourceHeatPump |
enumeration | ChilledBeamPassive |
enumeration | VRFFanCoil |
annotation |
documentation
The type of zone equipment.
source | <xsd:simpleType name="zoneHVACEquipmentTypeEnum"> <xsd:annotation> <xsd:documentation>The type of zone equipment.</xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:NMTOKEN"> <xsd:enumeration value="Undefined"/> <xsd:enumeration value="UnConditioned"/> <xsd:enumeration value="ChilledBeamActive"/> <xsd:enumeration value="FourPipeFanCoil"/> <xsd:enumeration value="PackagedTerminalAirConditioner"/> <xsd:enumeration value="PackagedTerminalHeatPump"/> <xsd:enumeration value="ParallelFanPoweredBox"/> <xsd:enumeration value="VAVBox"/> <xsd:enumeration value="BaseBoardConvective"/> <xsd:enumeration value="BaseBoardRadiant"/> <xsd:enumeration value="CAVBox"/> <xsd:enumeration value="RadiantPanel"/> <xsd:enumeration value="SeriesFanPoweredBox"/> <xsd:enumeration value="UnitHeater"/> <xsd:enumeration value="UnitVentilator"/> <xsd:enumeration value="WaterSourceHeatPump"/> <xsd:enumeration value="ChilledBeamPassive"/> <xsd:enumeration value="VRFFanCoil"/> </xsd:restriction> </xsd:simpleType>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy